{"text_format":"1","workbook":"xlsx","n_sheets":33,"sheets":["Cover Page","READ ME","Contents","Project Summary","Process Map","System Boundary Activities","Assumptions","Primary EF Database","Secondary EF Database","Proxy EF Database","IPCC Characterisation Factors","EF Library","A0 - Preconstruction","A1-A3 - Production","A4-A5 -Transport & Construction","B1-B8 - Use","C1-C5 - End-of-Life","Data Quality & Uncertainty","Conversions","Results","Graphs","PER Export","Lists","Taxonomies","Dynamic Dropdowns>>","EF L1 List","EF L2 List","EF L3 List","EF L4 List","EF Unit List","Asset Taxonomy","Geographies","Activity Taxonomy"],"not_rendered":{"charts":10,"images":9,"macros":1,"external_links":0,"defined_names":4585,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover Page","index":0,"n_rows":27,"n_cols":3,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,"COVER PAGE "]
[]
[]
[null,"Title:","Offshore Wind Footprinting Tool"]
[]
[null,"Author(s):","Cormac Dineen (The Carbon Trust)"]
[null,null,"Lucie Shackley (The Carbon Trust)"]
[]
[null,"Date:",45540]
[]
[null,"Version","V1"]
[]
[null,"Description:","This tool may be used to assess the Project Carbon Footprint (PCF) of an Offshore Wind development, with the functional unit of \"1 kWh electricity, net, generated by the OSW development and delivered to the grid at the PoI with the grid at the onshore substation\". It may also be used to assess the absolute carbon footprint associated with the different lifecycle stages of an OSW development, including preconstruction, production, construction and installation, operations and maintenance, and End-of decommissioning stages."]
[]
[null,"Licence:","The Offshore Wind Footprinting Tool by Carbon Trust is licensed under CC BY-SA 4.0. To view a copy of this license, visit https://creativecommons.org/licenses/by-sa/4.0/"]
[]
[null,"Disclaimer:","This tool has been developed as part of the Offshore Wind Sustainability Joint Industry Programme (SUS-JIP) phase 1 project to standardise the assessment of the carbon footprint of Offshore Wind developments in accordance to the methodology described in the SUS-JIP OSW Industry PCF Guidance. Any results generated by it are the sole responsibility of each user and are not considered to be verified by the Carbon Trust. Assessors may engage 3rd parties to verify the results of their assessment in compliance with relevant assurance standards. Any information and results derived from the use of this model are subject to the accuracy of data inputs supplied during the modelling process. This model has not yet been subject to any external independent audit. All results should be checked and challenged before any reliance, publication or use."]
[null,null,"While the tool has been prepared in good faith, no representation, warranty, assurance or undertaking (express or implied) is or will be made, and no responsibility or liability is or will be accepted by The Carbon Trust or any of its subsidiaries or by any of their respective officers, employees or agents in relation to the adequacy, accuracy, completeness or reasonableness of the model or of any information or results derived from it. All and any such responsibility and liability (including in the case of negligence) is expressly disclaimed to the fullest extent permitted by law."]
[null,null,"All trademarks, service marks and logos in the model, and copyright in it, are the property of The Carbon Trust. Nothing in the model shall be construed as granting any licence or right to use or reproduce any of the trademarks, services marks, logos, copyright or any proprietary information in any way without The Carbon Trust’s prior written permission. "]
[]
[null,null,"Any use of this model indicates your acceptance of the terms set out in this disclaimer. "]
[]
[null,null,"The Carbon Trust is a company limited by guarantee and registered in England and Wales under company number 4190230 with its registered office at Level 5, Arbor, 255 Blackfriars Road, London SE1 9AX, UK."]
[]
[null,null,"© The Carbon Trust 2023. All rights reserved."]

{"sheet":"READ ME","index":1,"n_rows":39,"n_cols":3,"rows_kept":39,"cut":false,"hidden":false,"merged":[[17,1,19,1],[20,1,21,1],[22,1,27,1],[35,1,36,1],[28,1,31,1]]}
[]
[null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,"READ ME"]
[]
[]
[null,"About:","This tool has been designed for the estimation of the lifecycle carbon footprint of an Offshore Wind development. The user can use the data input sheets to enter known or estimated data about the development to estimate the total carbon impact for the project.  "]
[]
[null,"Tab Key:","Introductory Tabs"]
[null,null,"Project Overview Tabs"]
[null,null,"SUS-JIP Emission Factor Database"]
[null,null,"Footprint Calculation Tabs"]
[null,null,"Results Tabs"]
[]
[null,"Methodology","The tool is designed to assess the footprint in alignment with the SUS-JIP \"Offshore Wind Industry Product Carbon Footprinting (PCF) Guidance\". The guidance document has been prepared by the SUS-JIP consortium to provide specific guidance for the application of existing standards for carbon footprinting to Offshore Wind development.\n\nFootprints prepared correctly in accordance with the guidance are compliant with the following core standards:\n•\tISO14067: Carbon footprint of products. Requirements and guidelines for quantification\n•\tGHGP Product Lifecycle Accounting and Reporting standard.\n•\tISO 14040 - Environmental management — Life cycle assessment — Principles and framework\n•\tISO 14044 Environmental management — Life cycle assessment — Requirements and guidelines\n\nFootprints prepared correctly in accordance with the guidance will also be aligned to the terminology and requirements outlined in the following supplementary standards, where not in contravention of the core standards:\n•\tISO 21931-2: Sustainability in buildings and civil engineering works — Framework for methods of assessment of the environmental, social and economic performance of construction works as a basis for sustainability assessment — Part 2: Civil engineering works\n•\tISO 21930:2017: Sustainability in buildings and civil engineering works — Core rules for environmental product declarations of construction products and services\n•\tEN 15978: Sustainability of construction works. Assessment of environmental performance of buildings. Calculation method\n•\tEN 15804: Sustainability of construction works - Environmental product declarations - Core rules for the product category of construction products.\n•\tEN 17472:2022: Sustainability of construction works. Sustainability assessment of civil engineering works. Calculation methods\n•\tISO 14025 Environmental labels and declarations — type iii environmental declarations — principles and procedures\n•\tInternational Reference Life Cycle Data System (ILCD) Handbook - General guide for Life Cycle Assessment\n•\tEuropean Commission: Product Environmental Footprint\n•\tPAS 2080:2023 Carbon management in buildings and infrastructure\n•\tPCR 2007:08: electricity, steam and hot/cold water generation and distribution\n•\tRICS: Whole life carbon assessment for the built environment v2\n•\tCarbon Trust: Product carbon footprints requirements for assurance – Part 1: Technical, v3.0\n•\tEPD International: General Programme Instructions for the International EPD system\n•\tWBCSD PACT Pathfinder Framework v2"]
[]
[null,"Mandatory Lifecycle Stages:","Mandatory Lifecycle Modules:"]
[null,"Preconstruction (A0)","A0: Preconstruction activities"]
[null,"Production Stage (A1-A3)","A1: Raw material supply"]
[null,null,"A2: Transport (to manufacturer)"]
[null,null,"A3: Manufacturing"]
[null,"Construction Stage (A4-A5)","A4: Transport (to OSW site)"]
[null,null,"A5: Construction & installation of the OSW development"]
[null,"Use of OSW development Stage (B1-B8)","B1: Use (direct emissions)"]
[null,null,"B2: Maintenance"]
[null,null,"B3: Repair"]
[null,null,"B4: Replacement"]
[null,null,"B5: Refurbishment"]
[null,null,"B6-B8: Operational use of energy, materials and water and waste management"]
[null,"End-of life of OSW development Stage (C1-C5)","C1: De-construction & Demolition"]
[null,null,"C2: Transport"]
[null,null,"C3: Waste Processing"]
[null,null,"C4: Disposal"]
[null,null,"C5: Relandscaping"]
[]
[null,"Optional Lifecycle Stages:","Optional Lifecycle Modules:"]
[null,"Benefits & Loads beyond the system boundary (D1-D2)","D1: Displacement of downstream materials due to recycling of OSW development materials & components at EoL"]
[null,null,"D2:  Displacement of other electricity with non-renewable electricity with renewable electricity from the OSW Development"]
[]
[null,null,"Source: SUS-JIP OSW Industry PCF Guidance"]

{"sheet":"Contents","index":2,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
[]
[null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,"CONTENTS"]
[]
[]
[]
[null,"Section","Sheet","Description"]
[null,"Project information","Project Summary","This Tab shall be populated by the user with information relating to the development under study. If this tab is not populated with the reference flow parameters, the assessor will not be able to calculate all of the relevant results."]
[null,null,"Process Map","This tab shows a generic process overview in the form of a flow diagram. This diagram may be used by the assessor to visually represent the activities included in the OSW development. The assessor should add information where required."]
[null,null,"System Boundary Activities","This tab provides a list of mandatory emissions sources to be captured in the footprint and a list of potential OSW development activities to be included in the footprint."]
[null,null,"Assumptions","This tab is the central table of assumptions which have been made by the user during the completion of the carbon footprint assessment. This should be updated by the user every time an assumption has been made to ensure the approach taken in the assessment is transparent."]
[null,"SUS-JIP Emission Factor Database","Primary EF database","This tab contains the Primary EF Database. The Primary EF database is where the assessor may add primary emission factors, sourced from suppliers of goods and services for the development. The assessor shall use the user form to add data."]
[null,null,"Secondary EF database","This tab contains the Secondary EF Database (Ecoinvent). The Secondary EF database contains a curated list of EFs relevant to the OSW lifecycle. The assessor must follow the guidance to import the data from a local copy of the database."]
[null,null,"Proxy EF database","This tab contains the Proxy EF Database. This is a list of other relevant EFs, taken from other sources such as EPDs, Government stats, etc to represent the activities included in the OSW lifecycle. The assessor shall use the user form to add data."]
[null,null,"IPCC Characterisation Factors","This tab contains the IPCC AR6 Characterisation factors for greenhouse gasses. These factors underpin the Secondary EF database, and may also be used to represent direct emissions."]
[null,null,"Emission Factor Library","This tab is the central table of Emission Factors to used in the footprint calculations that is compiled from the four other databases. The Data Input & Calculation tabs draw Emission Factors from this table only. It may be compiled by using the user controls."]
[null,"Data Input & Calculation ","A0 - Preconstruction","This tab is for calculating the emissions associated with preconstruction activities, including fuel, energy & materials used in surveys and other development preparation activities."]
[null,null,"A1-A3 - Production","This tab is for calculating the emissions associated with production activities, including fuel & energy used in the extraction and processing of raw materials, and manufacturing of assets and sub-components"]
[null,null,"A4 - Transportation","This tab is for calculating the emissions associated with the fuel & energy used in the transportation of assets, subcomponents and materials from the supplier manufacturing site to the OSW development site."]
[null,null,"A5 - Construction ","This tab is for calculating the emissions associated with the fuel & energy used in the  construction of the OSW development, including foundation & turbine installation, cable laying and balance of plant."]
[null,null,"B1-B8 - Use of infrastructure","This tab is for calculating the emissions associated with fuel, energy & material use, as well as any direct emissions or removals occurring during the operational phase of the OSW development, including maintenance & repair activities."]
[null,null,"C1-C4 - End-of-Life of infrastructure","This tab is for calculating the emissions associated with the fuel & energy used in the decommissioning of the OSW development, including transport to waste treatment site and eventual disposal of development materials."]
[null,null,"Conversions","This tab allows the user to convert units for standard measurement types such as distance, mass, volume and area which may be used to convert native activity data into the appropriate unit for the emissions calculation."]
[null,null,"Data Quality & Uncertainty","This tab allows the user to assess Data Quality for the assessment and estimate an uncertainty range for each lifecycle stage, which may be propagated to the overall result for the assessment"]
[null,"Results","Results Summary","The Results Summary is the central results tab drawing data from the calculation tabs & project summary. This shows the absolute emissions associated with the OSW development, broken down by lifecycle stage, asset & subcomponent type, and activity type. It also shows the results per reference unit"]
[null,null,"Graphs","This tab shows a series of visual representations of the  results contained in the results summary which may be used by the assessor to generate insights and drive analysis."]
[null,null,"PER Export","The PER Export is a simplified results sheet drawing data from the results summary and project summary. The assessor may use the user controls to directly export a PDF version of the assessment results."]

{"sheet":"Project Summary","index":3,"n_rows":67,"n_cols":5,"rows_kept":67,"cut":false,"hidden":false,"merged":[[19,1,19,2],[59,1,59,2],[7,1,7,4]]}
[]
[null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,"PROJECT SUMMARY"]
[]
[]
[null,"Project Summary Guidance"]
[]
[null,"The project summary tab shall be populated by the user with information and data relating to the assessed OSW development and is mandatory. It consists of  data which describes the OSW development being studied such that the assessment may be properly interpreted, as well as specific operational parameters that are required to calculate the assessment criteria that will flow through to the results worksheets. \n\nThe user shall populate the tables below before beginning their carbon footprint assessment on the Calculation tabs. The populated data will be used to calculate and report the result of the assessment.\n"]
[]
[null,"READ ME"]
[]
[]
[null,"Description cell"]
[null,"Guidance"]
[null,"Input cell"]
[null,"Calculation Cell"]
[null,"Preset Cell"]
[]
[null,"Assessment details & methodology"]
[null,"Please provide the details required about the assessment and the methodology used for calculations."]
[]
[null,"Assessment Details ","Assessor provided:"]
[null,"Assessor name"]
[null,"Assessor email"]
[null,"Development name"]
[null,"Development location"]
[null,"Development distance from shore (km)"]
[null,"Development water depth (m)"]
[null,"Windspeed (m/s) average hub height"]
[null,"Assessment type:"]
[null,"Scope of assessment:",{"$f":"IF(ISBLANK(Development_name),_xlfn.CONCAT(\"A PCF assessment of Offshore Wind development, \"&\"[ENTER DEVELOPMENT NAME (C25)]\"&\", built for renewable electricity generation, covering the full lifecycle of the infrastructure development.\"),_xlfn.CONCAT(\"A PCF assessment of Offshore Wind development, \"&Development_name&\", built for renewable electricity generation, covering the full lifecycle of the infrastructure development.\"))","v":"A PCF assessment of Offshore Wind development, [ENTER DEVELOPMENT NAME (C25)], built for renewable electricity generation, covering the full lifecycle of the infrastructure development."}]
[null,"Carbon footprinting standards:","ISO14067: Carbon footprint of products. Requirements and guidelines for quantification.\n\nGHG Protocol Product Lifecycle Accounting and Reporting standard."]
[null,"Name of the independent, third-party validator/verifier (optional)"]
[null,"Level of assurance achieved (optional)"]
[null,"Date of validation/verification (optional)"]
[null,"PCF calculation date (DD/MM/YYYY)"]
[null,"OSW development construction period (DD/MM/YYYY)-(DD/MM/YYYY)"]
[null,"OSW development operational expected lifetime (DD/MM/YYYY)-(DD/MM/YYYY)"]
[]
[null,"Assessment Methodology","Assessor provided: "]
[null,"OSW development description","e.g. The development is a 800MW site, consisting of 80, 10 MW turbines with fixed bottom, MP/TP foundations."]
[null,"System boundary","The system boundary shall include all lifecycle activities associated with the infrastructure development, including preconstruction, construction, operation, decommissioning and EoL. The system boundary ends at the point at which electricity is delivered at the Point of Interconnection (PoI) with the grid at the onshore substation."]
[null,"Cut-off criteria","Operational assessment:\n\n•\tNon-material contributors may be excluded for practical reasons (data availability, data quality, or other stated justification) if the highest reasonable estimate for that source of emissions does not exceed 0.2% of the total footprint. Aggregate exclusions should not exceed 2% of estimated the total footprint. \n•\tPlease refer to Appendix 1 for a list of activities for mandatory inclusion for an assessment of an operational development.\n•\tExclusions shall be stated clearly in the assumptions along with their GHG emissions estimates. The organisation shall document a simple justification for these exclusions. If exclusion exceed the thresholds listed above due to practical limitations the assessor shall clearly describe the exclusions and justify the approach footprint. Aggregate exclusions should not exceed 2% of estimated the total footprint. "]
[null,"Methodology applied","OSW Industry PCF Guidance"]
[null,"     -Key methodological choices (description)","Refer to \"Assumptions\" Table"]
[null,"     -Assumptions","Refer to \"Assumptions\" Table"]
[null,"     -Exclusions","Refer to \"Assumptions\" Table"]
[null,"     -Allocation – Input, Outputs & Recycling","Refer to \"Assumptions\" Table"]
[null,"     -Grouping","Refer to \"Assumptions\" Table"]
[null,"Methodological changes since the previous assessment"]
[null,"Calculation methodology by lifecycle stage"]
[null,"     - A0: Preconstruction","Methodology aligned to \"OSW Industry PCF Guidance\""]
[null,"     - A1 - A3: Production and manufacturing","Methodology aligned to \"OSW Industry PCF Guidance\""]
[null,"     - A4 - A5: Transportation, installation & construction","Methodology aligned to \"OSW Industry PCF Guidance\""]
[null,"     - B1 - B7: Operations & Maintenance","Methodology aligned to \"OSW Industry PCF Guidance\""]
[null,"     - C1 - C4: End-of-life","Methodology aligned to \"OSW Industry PCF Guidance\""]
[null,"     - D: Optional information outside of the system boundary","Methodology aligned to \"OSW Industry PCF Guidance\""]
[]
[null,"Reference flow parameters"]
[null,"Please provide parameter values for the calculation of the reference flow. Default values are given for capacity factor, assumed service life, and electrical losses in line with the OSW Industry PCF Guidance. Please provide justification and additional comment where the reference flow parameters diverge from default values.\n\nThe reference flow is also calculated using default values for sensitivity analysis. "]
[]
[null,"Reference flow parameters:","Assessor values:","Assessor comment:","Default values for sensitivity analysis:"]
[null,"Installed capacity (MW)",880,null,{"$f":"Installed_capacity__MW","v":880}]
[null,"Assumed capacity factor (%)",0.5,"Please provide justification and supporting evidence where the capacity factor provided diverges from the default values provided in the OSW Industry PCF Guidance",0.5]
[null,"Assumed service life (Years)",25,"Please provide justification and supporting evidence in this cell where the service life provided diverges from the default values provided in the OSW Industry PCF Guidance",25]
[null,"Assumed electrical losses in system boundary (%)",0.02,"Please provide justification and supporting evidence in this cell where the electrical losses in system value provided diverges from the default values provided in the OSW Industry PCF Guidance",0.05]
[null,"Reference flow (kWh) - electricity delivered at metered PoI with the grid ",{"$f":"(Installed_capacity__MW*1000)*(Assumed_capacity_factor)*(Assumed_service_life_Years*365*24)*(1-Assumed_electrical_losses_in_system_boundary)","v":94432800000},null,{"$f":"(Installed_capacity__MW*1000)*(Assumed_capacity_factor_SA)*(Assumed_service_life_Years_SA*365*24)*(1-Assumed_electrical_losses_in_system_boundary_SA)","v":91542000000}]

{"sheet":"Process Map","index":4,"n_rows":3,"n_cols":2,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
[]
[null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,"PROCESS MAP"]

{"sheet":"System Boundary Activities","index":5,"n_rows":119,"n_cols":7,"rows_kept":119,"cut":false,"hidden":false,"merged":[[8,3,8,6],[30,3,35,3],[30,4,32,4],[30,5,32,5],[33,4,35,4],[13,3,14,3],[15,3,23,3],[15,4,17,4],[15,5,17,5],[18,4,19,4],[18,5,19,5],[20,4,21,4],[20,5,21,5],[22,4,23,4],[22,5,23,5],[57,3,68,3],[57,4,68,4],[58,5,63,5],[64,5,65,5],[66,5,68,5],[40,3,49,3],[50,3,52,3],[33,5,35,5],[24,3,29,3],[36,3,39,3],[69,3,91,3],[69,4,91,4],[69,5,72,5],[73,5,76,5],[77,5,80,5],[81,5,82,5],[83,5,85,5],[86,5,88,5],[89,5,91,5],[112,3,118,3],[112,4,118,4],[113,5,115,5],[92,3,103,3],[92,4,103,4],[92,5,94,5],[95,5,103,5],[104,3,111,3],[104,4,111,4],[104,5,105,5],[106,5,107,5],[108,5,111,5]]}
[]
[null,null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,null,"Offshore Wind Footprinting Tool"]
[null,null,null,"System boundary activities for PCF of Offshore Wind"]
[]
[]
[null,null,null,"Relevant emissions sources and activities to include in system boundary - guidance"]
[]
[null,null,null,"This tab provides additional guidance to  support the calculation of a PCF for an OSW development and should be referred to when completing the calculation tabs A0 - C1-C4. Each OSW farm may have activities within the boundary that are based on design and technology choices that are specific to the wind farm being assessed. We have provided Tables 1 and 1on this tab as guidance to cover the list of the relevant activities that should be considered in the system boundary.\n\nTable 1 provides a list of the mandatory emission sources that must be included within the system boundary for a PCF assessment of an OSW development. The relevant emission sources remain consistent regardless of the type of assessment being conducted. However, data availability may vary, particularly when specific activities have not yet occurred at the time of the assessment resulting in the absence of primary data for the assessor. Table 1 begins by describing each relevant emission source or \"activity\" within the system boundary, based on the activity taxonomy described in the OSW Industry PCF Guidance. It also provides examples of where these emissions might arise in an OSW development and recommends the appropriate emission factors to use.\n\nFollowing this, Table 2 offers a non-exhaustive list of specific development activities that may need to be considered in an OSW development PCF assessment, organised by lifecycle stage. Each OSW development will have its own set of relevant activities, determined by the design and technical specifications of the project. Where activities listed are not relevant to the development under study, they may be excluded from the assessment. Conversely, if specific activities relevant to the OSW development being studied are not included in the list, the assessor should add them."]
[]
[null,1,null,"Mandatory emissions sources"]
[]
[null,null,null,"L1: Activity Category","L2: Activity subcategory","OSW development emissions source","Recommended emission factor"]
[null,null,null,"1.     Direct emissions and removals","a.     Fugitive emissions","Emissions of insulating GHGs (e.g., SF6) from substation equipment during regular operation or blow-outs.","IPCC (2021) emission factor for specific GHG (GWP100)"]
[null,null,null,null,"b.     Process emissions","Emissions of GHGs from chemical processes (e.g., use of coolants, chemicals in maintenance).","IPCC (2021) emission factor for GHG (GWP100)"]
[null,null,null,"2.     Freight and transportation","a.     Air freight and transportation","Emissions from transport of infrastructure components, parts, and maintenance personnel to site using freight planes, drones, or transport helicopters.","Emission factor for specific fuel combusted in the aircraft, typically jet fuel, or kerosene (kgCO2e/litre, tonne, MJ, etc.)"]
[null,null,null,null,null,null,"Weight distance-based emission factor for aircraft type (kgCO2e/tonne.km)"]
[null,null,null,null,null,null,"Journey-based emission factor for aircraft type (kgCO2e/hour, LTO)"]
[null,null,null,null,"b.     Rail freight and transportation","Emissions from transport of components and materials using trains.","Emission factor for specific fuel combusted in the train, typically diesel (kgCO2e/litre or tonne or MJ, etc.)"]
[null,null,null,null,null,null,"Weight-distance based factor for train type (kgCO2e/tonne.km)"]
[null,null,null,null,"c.     Road freight and transportation","Emissions from transport of components, materials, and maintenance personnel using trucks, lorries, vans, cars, and specialised vehicles.","Emission factor for specific fuel combusted in the vehicle, typically diesel, petrol, bio-based alternative, or electricity (kgCO2e/litre or tonne or MJ, etc.)"]
[null,null,null,null,null,null,"Weight-distance based factor for vehicle type (kgCO2e/tonne.km) "]
[null,null,null,null,"d.     Sea freight and transportation","Emissions from transport of infrastructure assets, components, materials, and personnel via sea, using freight vessels, specialist vessels (e.g., Turbine Installation).","Emission factor for specific fuel combusted in the vehicle, typically marine fuel oil, marine diesel, bio-based alternative, or electricity (kgCO2e/litre or tonne or MJ, etc.)"]
[null,null,null,null,null,null,"Weight-distance based for vessel type (kgCO2e/tonne.km)"]
[null,null,null,"                 3.     Electricity, fuels and other utilities","a.     Biofuels lifecycle","Emissions from the production, transport, and use of biofuels for OSW operations not otherwise captured in Freight and Transportation.","Emission factor for specific biofuel combusted, may be derived from PCF or LCA report (biofuel certification) or from secondary database. Typically, biodiesel, bioethanol, biogas, etc. (kgCO2e/litre or tonne or MJ, etc.)"]
[null,null,null,null,"b.     Electricity lifecycle","Emissions from the production, transmission, and use of electricity imported from the grid to support OSW development operations such as onshore operation sites.","Emission factor for electricity generation for the grid region where the OSW development is operating may be derived from secondary database (kgCO2e/kWh)."]
[null,null,null,null,"c.     Gaseous fuels lifecycle","Emissions from the production, transport, and use of gaseous fuels to support OSW development operations such as heating onshore operation sites.","Emission factor for specific gas combusted, typically natural gas (kgCO2e/litre or tonne or MJ, etc.)"]
[null,null,null,null,"d.     Liquid fuels lifecycle","Emissions from the production, transport, and use of fossil-based liquid fuels for OSW operations not otherwise captured in Freight and Transportation. ","Emission factor for specific fuel combusted, typically diesel, petrol, marine fuel oil, etc (kgCO2e/litre or tonne or MJ, etc.)"]
[null,null,null,null,"e.     Solid fuels lifecycle","Emissions from the production, transport, and use of solid fuels for OSW operations not otherwise captured in Freight and Transportation. Unlikely to be relevant.","Emission factor for specific fuel combusted, may include coal or other solid fuels (kgCO2e/litre or tonne or MJ, etc.)"]
[null,null,null,null,"f.     Water supply","Emissions from the supply of freshwater used in OSW operations.","Emission factor for mains water for the consumption region where the OSW development is operating (kgCO2e/litre or tonne or MJ, etc.)"]
[null,null,null,"4.     Fully manufactured assets and components","a.     Assets","Emissions from the production and manufacturing of infrastructure assets procured for the OSW development (e.g. WTG, foundations, cables etc (refer to Table 15 for list of assets)). Covers all cradle-to-gate (supplier gate) emissions from manufacturing the asset including materials, upstream transportation, manufacturing energy use and waste.","Emission factor for the finished asset may be derived from a supplier PCF, LCA or EPD report for the asset (kgCO2e/unit (e.g. 1 WTG specific manufacturer model, MW capacity))"]
[null,null,null,null,null,null,"Emissions factor for generic finished asset may be derived from secondary database (kgCO2e/unit (e.g. 1 generic WTG, MW capacity)) "]
[null,null,null,null,null,null,"Assessors may combine a full asset approach for some assets (e.g. WTG, cables) with a material composition approach for others (e.g. steel quantities for foundations)"]
[null,null,null,null,"b.     Subcomponents","Emissions from the production and manufacturing of subcomponents procured for the OSW development (e.g. blades for WTG, transformers for substation, etc (refer to Table 15 for list of asset subcomponents)). Covers all cradle to gate (supplier gate) emissions from manufacturing the asset including materials, upstream transportation, manufacturing energy use and waste.","Emission factor for the finished subcomponent may be derived from a supplier PCF, LCA or EPD report for the asset (kgCO2e/unit (e.g. 1 WTG blade, specific manufacturer model, material grade))"]
[null,null,null,null,null,null,"Emissions factor for generic finished asset may be derived from secondary database (kgCO2e/unit (e.g. 1 generic WTG blade, specific manufacturer model, material grade)) "]
[null,null,null,null,null,null,"Assessors may combine a full asset approach for some assets (e.g. WTG, cables) with a material composition approach for others (e.g. steel quantities for foundations)"]
[null,null,null,"5.     Manufacturing processes","a.     Coating and galvanising processes","Emissions from coating, galvanizing, or other surface treatment processes used in the manufacturing of OSW components, where not already included in assessment of fully manufactured assets or components assessment. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets","Emission factor for specific coating or galvanizing process used, typically derived from secondary databases (kgCO2e/unit or per process step)."]
[null,null,null,null,"b.     Joining and welding processes","Emissions from welding, joining, or other assembly processes used in the manufacturing of OSW components, where not already included in assessment of fully manufactured assets or components assessment. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets","Emission factor for specific joining or welding process used, typically derived from secondary databases (kgCO2e/unit or per process step)."]
[null,null,null,null,"c.     Material processing","Emissions from processing raw materials into components or parts for OSW manufacturing (e.g., cutting, forming, shaping materials), where not already included in assessment of fully manufactured assets or components assessment. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets","Emission factor for specific material processing step, typically derived from secondary databases (kgCO2e/unit or per process step)."]
[null,null,null,null,"d.     Other manufacturing processes","Emissions from additional manufacturing processes not covered in other subcategories.","Emission factor for the specific manufacturing process, typically derived from secondary databases (kgCO2e/unit or per process step)."]
[null,null,null,"6.     Materials","a.     Aluminium","Emissions from the production, processing, and use of aluminium, or aluminium alloys in OSW components, including WTG towers, nacelle, cable conductors, substation, and electrical equipment, where not already included in assessment of fully manufactured assets or components assessment. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for aluminium production (cradle-to-gate), referencing specific grade required for asset or component. Typically, derived from supplier LCA, PCF or EPD report, or secondary databases (kgCO2e/kg or tonne of aluminium)."]
[null,null,null,null,"b.     Biogenic materials","Emissions from the production, processing, and use of biogenic materials (e.g., wood, natural fibres) in OSW components, potentially used in blades, insulation, composite materials, where not already included in assessment of fully manufactured assets or components assessment. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for biogenic material production (cradle-to-gate). Typically, derived from supplier LCA, PCF or EPD report, or secondary databases (kgCO2e/kg or tonne of biogenic material)."]
[null,null,null,null,"c.     Carbon fibre","Emissions from the production, processing, and use of carbon fibre in OSW components, particularly in WTG blades and other high-strength, lightweight structures where not already included in assessment of fully manufactured assets or components assessment. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for carbon fibre production. Typically, derived from supplier LCA, PCF or EPD report, or secondary databases (kgCO2e/kg or tonne of carbon fibre)."]
[null,null,null,null,"d.     Concrete","Emissions from the production, processing, and use of concrete in OSW components, including foundations, platforms, and other structures, where not already included in assessment of fully manufactured assets or components assessment. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for concrete production, referencing specific concrete type and grade. Typically, derived from supplier LCA, PCF or EPD report, or secondary databases (kgCO2e/kg or tonne of concrete)."]
[null,null,null,null,"e.     Copper","Emissions from the production, processing, and use of copper or copper alloys in OSW components, notably in cables, transformers, and other electrical equipment. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for copper production, referencing specific copper grade. Typically, derived from supplier LCA, PCF or EPD report, or secondary databases (kgCO2e/kg or tonne of copper)."]
[null,null,null,null,"f.      Fibreglass","Emissions from the production, processing, and use of fibreglass in OSW components, particularly in WTG blades and nacelles. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for fibreglass production. Typically derived from supplier LCA, PCF, or EPD report, or secondary databases (kgCO2e/kg or tonne of fibreglass)."]
[null,null,null,null,"g.     Oils and lubricants","Emissions from the production, processing, and use of oils and lubricants in OSW components and machinery. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for oils and lubricants. Typically derived from supplier LCA, PCF, or EPD report, or secondary databases (kgCO2e/kg or litre of oil or lubricant)."]
[null,null,null,null,"h.     Other materials","Emissions from the production, processing, and use of other materials in OSW components not covered in other subcategories. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for other materials. Typically derived from supplier LCA, PCF, or EPD report, or secondary databases (kgCO2e/kg or tonne of material)."]
[null,null,null,null,"i.       Polymers","Emissions from the production, processing, and use of polymers in OSW components, particularly in cables, insulation, and composite materials. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for polymer production. Typically derived from supplier LCA, PCF, or EPD report, or secondary databases (kgCO2e/kg or tonne of polymer)."]
[null,null,null,null,"j.       Steel","Emissions from the production, processing, and use of steel in OSW components, including towers, foundations, and other structural elements. Typically, relevant where assessor uses a material composition approach to measure emissions from infrastructure assets. Covers all cradle-to-gate (supplier gate) emissions from production of the material.","Emission factor for steel production, referencing specific steel grade. Typically derived from supplier LCA, PCF, or EPD report, or secondary databases (kgCO2e/kg or tonne of steel)."]
[null,null,null,"7.     Waste treatment","a.     Incineration","Emissions from the incineration, without energy recovery, of waste generated during OSW development lifecycle activities.","Emission factor for waste incineration. Typically derived from LCA or secondary databases (kgCO2e/kg or tonne of waste)."]
[null,null,null,null,"b.     Landfill","Emissions from the disposal of waste in landfills, generated during OSW development and operations.","Emission factor for landfill disposal. Typically derived from LCA or secondary databases (kgCO2e/kg or tonne of waste)."]
[null,null,null,null,"c.     Processing, sorting for recycling and reuse","Emissions from the processing and sorting of waste for recycling and reuse, generated during OSW development and operations. ","Emission factor for recycling and reuse processes. Typically derived from LCA or secondary databases (kgCO2e/kg or tonne of waste)."]
[]
[null,2,null,"List of potential emissions generating activities in OSW development"]
[]
[null,null,null,"Lifecycle stage ","Emissions sources","Relevant development area","Specific development activity"]
[null,null,null,"A0: Preconstruction Stage","Emissions from fuels and energy consumed in preconstruction activities and emissions from the production of preconstruction infrastructure","A0: Development and consenting services","Environmental impact assessment"]
[null,null,null,null,null,"A0: Environmental surveys","Benthic environmental surveys"]
[null,null,null,null,null,null,"Fish and shellfish surveys"]
[null,null,null,null,null,null,"Ornithological environmental surveys"]
[null,null,null,null,null,null,"Marine mammal environmental surveys"]
[null,null,null,null,null,null,"Onshore environmental surveys"]
[null,null,null,null,null,null,"Human impact studies"]
[null,null,null,null,null,"A0: Metocean assessment","Survey infrastructure, including:\n•\tFoundation\n•\tPlatform\n•\tMast\n•\tBuoys"]
[null,null,null,null,null,null,"Survey sensors including:\n•\tMeteorological sensors \n•\tAnemometers \n•\tMetocean sensors \n•\tData loggers"]
[null,null,null,null,null,"A0: Geological and hydrological surveys","Geophysical surveys"]
[null,null,null,null,null,null,"Geotechnical Surveys"]
[null,null,null,null,null,null,"Hydrographic surveys"]
[null,null,null,"A1-A3: Production Stage","Emissions from fuel and energy, and materials used in production activities for assets, sub-components and materials used in the OSW development. This includes extraction, transportation, and processing of materials up to supplier gate (tier 1).","A1-A3: WTG","Nacelle and internals\n•\tBedplate\n•\tMain bearing\n•\tMain shaft\n•\tGearbox\n•\tGenerator\n•\tPower take-off\n•\tControl system\n•\tYaw system\n•\tYaw bearing\n•\tNacelle auxiliary systems\n•\tNacelle cover\n•\tSmall engineering components"]
[null,null,null,null,null,null,"Blades, hub, and rotor system\n•\tStructural fasteners\n•\tCondition monitoring system\n•\tHub casting\n•\tBlades\n•\tBlade bearings\n•\tPitch system\n•\tSpinner\n•\tRotor auxiliary systems\n•\tFabricated steel components\n•\tStructural fasteners"]
[null,null,null,null,null,null,"Turbine transformer"]
[null,null,null,null,null,null,"Turbine tower\n•\tSteel\n•\tTower internals"]
[null,null,null,null,null,"A1-A3: Fixed Foundations","Monopile\n•\tSteel plates \n•\tFlange \n•\tJoints\n•\tCorrosion protection materials and coatings, including galvanisation materials.\n•\tScour protection materials"]
[null,null,null,null,null,null,"Transition piece\n•\tCrew access system and work platform\n•\tInternal platforms\n•\tDavit crane\n•\tJ-tubes, I-tube or monopile entry point"]
[null,null,null,null,null,null,"Jacket\n•\tSteel lattice\n•\tStruts \n•\tNodes \n•\tPin piles \n•\tCrew access system and work platform\n•\tInternal platforms\n•\tDavit crane\n•\tJ-tubes\n•\tCorrosion protection materials and coatings, including galvanisation materials.\n•\tScour protection materials"]
[null,null,null,null,null,null,"Other fixed foundation technologies\n•\tGravity base\n•\tHybrid foundations\n•\tSuction bucket foundations\n•\tComposite materials \n•\tInnovative scour protection techniques"]
[null,null,null,null,null,"A1:A3: Floating foundations","Platform\n•\tSemi-submersible (steel structure)\n•\tSpar Buoy (steel structure)\n•\tTension Leg Platform (TLP)"]
[null,null,null,null,null,null,"Mooring\n•\tAnchors \n•\tMooring Lines \n•\tMooring Connectors"]
[null,null,null,null,null,null,"Ballast\n•\tBallast Tanks\n•\tWater Ballast\n•\tConcrete Ballast"]
[null,null,null,null,null,null,"Other fixed foundation technologies\n•\tBarges \n•\tPontoon systems\n•\tHybrid floating structures\n•\tAlternative mooring systems "]
[null,null,null,null,null,"A1-A3: Cables","Inter Array Cables\n•\tCable core\n•\tCable outer\n•\tCable accessories\n•\tCable jointing"]
[null,null,null,null,null,null,"Export Cables\n•\tCable core\n•\tCable outers\n•\tCable accessories\n•\tCable jointing"]
[null,null,null,null,null,"A1-A3: Offshore Substation","Electrical Systems\n•\tHVAC and HVDC systems:\n•\tHV AC and DC switchgear\n•\tTransformers\n•\tConverters\n•\tPassive and active power compensation\n•\tEarthing systems\n•\tAuxiliary electrical, control and monitoring systems\n•\tIndustrial waterproof enclosures\n•\tCable trays, tracks, clamps, and supports to protect electrical items"]
[null,null,null,null,null,null,"Facilities\n•\tAuxiliary electrical systems \n•\tMonitoring systems \n•\tCommunication system \n•\tFire and blast protection systems \n•\tStandby generator (normally for HVDC substations) \n•\tCrane \n•\tControl room and refuge \n•\tClean and black water systems (normally for HVDC substations) \n•\tFuel tanks (normally for HVDC substations) \n•\tHeating, ventilation and air conditioning equipment"]
[null,null,null,null,null,null,"Structure\n•\tSteel structure\n•\tHelideck and/or heliwinch "]
[null,null,null,null,null,"A1-A3: Onshore substation","Electrical Systems\n•\tHVAC and HVDC systems:\n•\tHV AC and DC switchgear\n•\tTransformers\n•\tConverters\n•\tPassive and active power compensation\n•\tEarthing systems\n•\tAuxiliary electrical, control and monitoring systems\n•\tIndustrial waterproof enclosures\n•\tCable trays, tracks, clamps, and supports to protect electrical items"]
[null,null,null,null,null,null,"Facilities\n•\tAuxiliary electrical systems \n•\tMonitoring systems \n•\tCommunication system \n•\tFire and blast protection systems \n•\tStandby generator (normally for HVDC substations) \n•\tCrane \n•\tControl room and refuge \n•\tClean and black water systems (normally for HVDC substations) \n•\tFuel tanks (normally for HVDC substations) \n•\tHeating, ventilation and air conditioning equipment"]
[null,null,null,null,null,null,"Structure\n•\tSteel structure\n•\tHelideck and/or heliwinch "]
[null,null,null,null,null,"A1-A3: Operations base","Vessel berths"]
[null,null,null,null,null,null,"Warehouse"]
[null,null,null,null,null,null,"Workshop"]
[null,null,null,"A4-A5: Construction and Installation stage","Emissions from fuel and energy consumed in the transportation of assets, sub-components and materials to the Offshore Wind development site and emissions and emissions from fuel and energy in the construction of the Offshore Wind development.","A4: Transportation to site","Sea freight \n•\tContainer ships\n•\tTanker ships\n•\tOther vessels"]
[null,null,null,null,null,null,"Land freight \n•\tHeavy goods vehicles (HGV)\n•\tLight goods vehicles (LGV)\n•\tFreight train"]
[null,null,null,null,null,null,"Air freight \n•\tFreight planes"]
[null,null,null,null,null,"A5: Construction and installation at site","Turbine installation vessel"]
[null,null,null,null,null,null,"Foundation Installation vessel"]
[null,null,null,null,null,null,"Cable laying vessels"]
[null,null,null,null,null,null,"Substation installation vessels"]
[null,null,null,null,null,null,"Onshore substation installation"]
[null,null,null,null,null,null,"Support vessels\n•\tBarges\n•\tCrew transfer vessels\n•\tRemotely operated vehicle"]
[null,null,null,null,null,null,"Other construction vessels"]
[null,null,null,null,null,null,"Onshore plant and construction equipment"]
[null,null,null,null,null,null,"Transport, processing, disposal of construction and installation waste"]
[null,null,null,"B1-B8: Use of development stage ","Direct emissions and removals from use of the infrastructure, emissions from fuel and energy consumption in the infrastructure, and emissions the production of consumable materials used in the infrastructure including maintenance, repair, and replacement activities.","B1: Direct emissions and removals from the use of the infrastructure","Direct, leakage or venting of greenhouse gasses.\n•\tInsulating gas (e.g. SF6, etc)\n•\tRefrigerant gasses\n•\tProcess gasses"]
[null,null,null,null,null,null,"Absorption of carbon dioxide or other greenhouse through natural or technical processes\n•\tCarbonation of cementitious materials\n•\tTechnological removals"]
[null,null,null,null,null,"B2-B5: Maintenance, repair, replacement, and refurbishment activities for OSW development","Maintenance and repair services, including fuel and energy consumed by vessels for maintaining development infrastructure\n•\tTurbine inspection and repair\n•\tFoundation inspection and repair\n•\tCable inspection and repair\n•\tScour monitoring and management\n•\tSubstation maintenance and service"]
[null,null,null,null,null,null,"Material procurement for maintenance, repair, and refurbishment:\n•\tFinished parts and components.\n•\tMaintenance materials."]
[null,null,null,null,null,"B6-B8 Direct use of energy, use of materials, use of water or waste generated by the OSW development","Consumption of grid electricity by the OSW development, or assets, during start up or down time."]
[null,null,null,null,null,null,"Consumption of fuels in backup generators used by the OSW development or assets during start up or down time"]
[null,null,null,null,null,null,"Consumption of mains or utility water by the OSW development, or specific assets during operation."]
[null,null,null,null,null,null,"Transport, processing and disposal of waste generated by the OSW development during regular operation."]
[null,null,null,"C1-C5: End of life of infrastructure Stage","Emissions from fuel and energy consumed in the deconstruction and demolition of the OSW development site, transport of waste to treatment site, processing of sorting of waste before end-of-waste state, disposal and relandscaping activities","C1: Decommissioning and deconstructing OSW development","Decommissioning and deconstruction vessel activities\n•\tAll offshore and onshore infrastructure assets and components\n•\tOther decommissioning activities"]
[null,null,null,null,null,"C2: Transportation of OSW development waste materials to processing facility","Sea freight \n•\tContainer ships\n•\tTanker ships\n•\tOther vessels"]
[null,null,null,null,null,null,"Land freight \n•\tHeavy goods vehicles (HGV)\n•\tLight goods vehicles (LGV)\n•\tFreight train"]
[null,null,null,null,null,null,"Air freight \n•\tFreight planes"]
[null,null,null,null,null,"C3: Waste processing and treatment","Waste processing:\n•\tDismantling of assets components not otherwise assessed in module C1\n•\tProcessing and sorting of recyclable materials up to end-of-waste state\n•\tProcessing of non-recyclable materials before disposal"]
[null,null,null,null,null,"C4: Waste disposal","Waste disposal activities:\n•\tIncineration without energy recovery\n•\tLandfill"]
[null,null,null,null,null,"C5: Relandscaping","Return of land and seabed to original condition\n•\tVessels and equipment"]

{"sheet":"Assumptions","index":6,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[[7,1,7,5]]}
[]
[null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,"ASSUMPTIONS"]
[]
[]
[null,"Assumptions Guidance"]
[]
[null,"The assumptions guidance tab shall be populated by the user to describe and track any methodological assumptions that were made in the calculation of the footprint. Assumptions should be documented and logged as they are made.\n"]
[]
[null,"Assumptions Table"]
[]
[null,"Assumption ID","Lifecycle stage","Assumption Description","Worksheet","Comment"]
[null,1,"Reference Flow Parameters","e.g. We have assumed a 30 year lifecycle based on the manufacturer specifications for the WTGs, evidence for this provided at x","All"]
[null,2,"Reference Flow Parameters","e.g. We have assumed a capacity factor of 45%","All"]

{"sheet":"Primary EF Database","index":7,"n_rows":21,"n_cols":26,"rows_kept":21,"cut":false,"hidden":false,"merged":[[19,1,19,15],[7,1,7,14],[19,16,19,25]]}
[]
[null,"SUS-JIP  |  Offshore Wind Footprinting Tool"]
[null,"PRIMARY EMISSION FACTOR DATABASE"]
[]
[]
[null,"Primary Emission Factor Database Guidance"]
[]
[null,"The Primary Emission Factor Database may be updated by the user to add primary EFs related to the OSW project under study to use those EFs in the emissions calculation.\n\n“Primary EF” refers to an LCIA result that has been calculated for specific activities in the system boundary. Primary EFs are typically produced by the organisation or entity that has operational control over the activity. Primary emission factors are the most accurate type of emission factor as they are an expression of the carbon intensity of a specific activity, which may be measured and verified by the company with operational control of the activity. \n\nIf you have collected primary EFs for your OSW PCF assessment, for example, an EF for the specific type of steel used in the foundations, or a Primary EF for the whole turbine, which has been provided in the form of an LCA report by your turbine supplier, you may enter it into this table. Once the data has been entered into the table, and the EF Library has been compiled, the dataset will become available to use in the assessment.\n\nThis worksheet and table cannot be directly manipulated by the users outside of using the user controls below, which allows the user to enter a Primary EF into the database through a user form, which will request data from the user. A separate button is available to delete the previous row of the table in the event that the user makes a mistake in data entry. The purple guidance boxes are provided to describe the data that should be populated in each column using the user form.\n\nAfter adding data to this database please go to the EF library and click 'compile EF library' to make EFs available for use in the calculation sheets."]
[]
[null,"User Controls"]
[]
[]
[]
[]
[]
[]
[null,"Data input column guidance"]
[null,"Emission Factor ID is automatically populated","For first version of a factor please enter \"V1\". If you update the study and provide a new values, please up the version number.","The name of the EF source. This may be a supplier or other entity who conducted the study and produced the data.","Native database identifier (e.g. ID in EPD database). If not available please state \"NA\".","The type of assessment that factor is derived from (PCF, LCA, EPD, OCF allocation)","A short description of the activity/process the factor represents. E.g. \"This factor represents the production of cables\"","UN classification code for the activity. If not available please state \"NA\"","Boundary of the factor, e.g. cradle-to-gate, A1-A3.","Background LCI dataset and version used for assessment, if unknown please state \"NA\" (Ecoinvent, GaBi, US EPA, etc.)","Impact methodology used for assessment (e.g. IPCC 2021, CML, EF, ReCiPi)","Impact indicator. This must be GWP100.","Reporting standard for the underlying assessment (ISO 14067, ISO 14040/44, GHGP). If unknown please state \"NA","Product Category Rules (PCR) used for the assessment. If none used please state \"NA\"","Has the assessment been verified by a 3rd party (Yes or No)","When is the assessment valid until (MM-YY), if unknown please state \"NA\" ","OSW EF Factor Category is autopopulated","OSW Activity Taxonomy L1 (please select from  the dropdown)","OSW Activity Taxonomy L2 (please select from dropdown)","Name of Emission Factor process. E.g. \"Steel production, heavy-plate, produced via BOF\"","The geographical location of the activity","The Unit of Measure for the factor (the reference unit for the assessment)","Greenhouse gas emissions for factor from fossil origin. If split is not available, leave blank.","Greenhouse gas emissions for factor from biogenic origin. If split is not available, leave blank.","Greenhouse gas emissions for factor from land use change. If split is not available, leave blank.","Total greenhouse gas emissions for the activity. If split is not available, populate the total, or net, in this column."]
[]
[null,"EMISSION FACTOR METADATA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EMISSION FACTOR"]
[null,"Emission Factor ID","Emission Factor version number","EF source name","Native database ID (optional)","Assessment Type","Activity Description","UN CPC 2.1 Code (optional)","Emission Factor Boundary","Background Dataset Used","Impact Methodology Used","Impact Indicator","Reporting Standard used ","PCR used (optional)","Verified","Valid until","OSW EF Category","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Geography","Emissions Factor Unit","climate change: fossil (kgCO2e/unit)","climate change: biogenic (kgCO2e/unit)","climate change: land use (kgCO2e/unit)","Emissions Factor Net (kgCO2e/unit)"]

{"sheet":"Secondary EF Database","index":8,"n_rows":803,"n_cols":26,"rows_kept":803,"cut":false,"hidden":false,"merged":[[7,1,8,14],[17,1,17,15],[17,16,17,25]]}
[]
[null,"SUS-JIP  |  Offshore Wind Footprinting Tool"]
[null,"SECONDARY EF DATABASE"]
[]
[]
[null,"Secondary EF Database Guidance"]
[]
[null,"The Secondary Emission Factor Database is a selection of curated datasets from the Ecoinvent LCI database which are relevant to the activities included in the system boundary for the OSW PCF guidance. Where primary factors are not available for the specific activity being footprinted, secondary emission factors should be used by the assessor. There is no Ecoinvent life cycle data on this templated sheet before it is imported by the user, to use the data import function on this tab you must hold a valid Ecoinvent licence. If you do not, please navigate to the Proxy EF Database tab and import other sources of data there.\n\nEcoinvent is a widely used lifecycle inventory database, which contains lifecycle inventory data for a large number of human processes. Ecoinvent also includes an LCIA inventory for these processes, which may be used as secondary emission factors (IPCC 2021, GWP100) for the purpose of carbon footprinting. The Ecoinvent database is commercially protected, and must be licenced by the user to allow for use of the data. The table below has been populated with Ecoinvent Database IDs for the curated datasets relevant to OSW development assessments. \n\nTo import the data to the tool, the assessor must first login to the Ecoinvent data portal using their login credentials, which will be issued when the assessor takes out a user licence with Ecoinvent. Once the assessor has logged in, they may take the following steps:\n\n1. In the Ecoinvent \"ecoQuery\" data portal, navigate to the \"Files\" button on the main site ribbon\n2. In the Files section, navigate to the database 3.10. The database will be updated to reflect the latest Ecoinvent data during the review cycle for this tool.\n3. In 3.10, navigate to the section \"Allocation cut-off by classification\" and click on the file \"ecoinvent 3.10_cutoff_cumulative_lcia_xlsx.7z\". This should begin your download of the relevant dataset.\n4. Store the file locally on your device, in a location you can easily access through the file browser. Where the file stores a zip folder, please extract the contents.\n\nOnce you have followed the steps outline and have stored the file locally, you may now use the user controls below to add the emission factor data to the tool. This worksheet and table cannot be directly manipulated by the users outside of using the user controls below. The \"Import Ecoinvent Data\" button will prompt the assessor to navigate to their locally stored copy of the using the file explorer. When you click on the file, the import will begin. Please ensure you have carefully followed steps 1-4 above, and imported the correct database or the user controls will not import the data successfully. The \"Clear Table\" button allows the user to clear the table in the event that the import was unsuccessful. When the data is imported and the EF Library is compiled, the secondary EFs will become available for use in the calculation sheets. \n\nAfter adding data to this database please go to the EF library and click 'compile EF library' to make EFs available for use in the calculation sheets."]
[]
[]
[null,"User Controls"]
[]
[]
[]
[]
[]
[]
[null,"EMISSION FACTOR METADATA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EMISSION FACTOR"]
[null,"Emission Factor ID","Emission Factor version number","EF source name","Native database ID (optional)","Assessment Type","Activity Description","UN CPC 2.1 Code (optional)","Emission Factor Boundary","Background Dataset Used","Impact Methodology Used","Impact Indicator","Reporting Standard used ","PCR used (optional)","Verified","Valid until","OSW EF Category","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Geography","Emissions Factor Unit","climate change: fossil (kgCO2e/unit)","climate change: biogenic (kgCO2e/unit)","climate change: land use (kgCO2e/unit)","Emissions Factor Net (kgCO2e/unit)"]
[null,"OSW_SE_1","N/A","Ecoinvent  3.10, cut-off by allocation version","0d88960c-7038-525c-8d90-194b3ba5d604_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_2","N/A","Ecoinvent  3.10, cut-off by allocation version","4e959cbd-4b18-5f8d-9eb6-1c347ea2c2ff_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_3","N/A","Ecoinvent  3.10, cut-off by allocation version","d7bb4e4f-49d6-5054-aff8-6290f98f8205_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_4","N/A","Ecoinvent  3.10, cut-off by allocation version","efe8be91-2ffc-533f-bcd6-22e70a11d008_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_5","N/A","Ecoinvent  3.10, cut-off by allocation version","bd1a994e-9b13-5afb-9b86-9880dc35a62a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_6","N/A","Ecoinvent  3.10, cut-off by allocation version","a6f17f0f-8b94-5475-9f13-1a6f4e54218f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_7","N/A","Ecoinvent  3.10, cut-off by allocation version","bc019df7-0f00-59c7-9538-67ce8a4b0081_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_8","N/A","Ecoinvent  3.10, cut-off by allocation version","bcf870ca-7662-5fab-88e1-05f0fae4f45e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_9","N/A","Ecoinvent  3.10, cut-off by allocation version","867301f4-8db2-5bd4-95d5-52404f98c69f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_10","N/A","Ecoinvent  3.10, cut-off by allocation version","c5362e7d-fc80-5c74-a13d-1cc248ea169f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_11","N/A","Ecoinvent  3.10, cut-off by allocation version","d2ad7d45-9fab-59eb-ae32-e34aba958ba6_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_12","N/A","Ecoinvent  3.10, cut-off by allocation version","e305c073-d9bd-5bb9-89ea-6987758a00d7_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_13","N/A","Ecoinvent  3.10, cut-off by allocation version","5c309945-5358-5228-bfbe-9edd9e3f5e20_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_14","N/A","Ecoinvent  3.10, cut-off by allocation version","4b5ababf-cb44-59ed-9f92-bb4492ec52b5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_15","N/A","Ecoinvent  3.10, cut-off by allocation version","c6931985-d821-5ad0-bb60-b08fa52f62d9_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_16","N/A","Ecoinvent  3.10, cut-off by allocation version","1e48c229-e40a-5bb9-9509-e5513c1437dd_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_17","N/A","Ecoinvent  3.10, cut-off by allocation version","eebad817-5f9a-5572-b361-8009c47698db_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_18","N/A","Ecoinvent  3.10, cut-off by allocation version","c9a2346c-4228-574d-a767-fd01a981bb80_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_19","N/A","Ecoinvent  3.10, cut-off by allocation version","2f1625c1-a80d-5264-96b1-929f3d5d513c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_20","N/A","Ecoinvent  3.10, cut-off by allocation version","920c3004-54f6-5f18-9d9b-3d6c4f9bcd6d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_21","N/A","Ecoinvent  3.10, cut-off by allocation version","e53e0491-6ca1-5901-8674-cb18ad0287e8_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_22","N/A","Ecoinvent  3.10, cut-off by allocation version","8814190a-62d5-5294-a961-ebc78ccdfc5c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_23","N/A","Ecoinvent  3.10, cut-off by allocation version","fbe35edd-e62e-525a-8cb8-fca983b2019b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_24","N/A","Ecoinvent  3.10, cut-off by allocation version","f490b95e-5a62-5064-9c34-7c77c1805c76_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_25","N/A","Ecoinvent  3.10, cut-off by allocation version","ee1bb605-5372-5e41-a497-fcbaf6d2e9d5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_26","N/A","Ecoinvent  3.10, cut-off by allocation version","bf8effe2-d954-51ae-ad2e-b0115b455211_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_27","N/A","Ecoinvent  3.10, cut-off by allocation version","bb151bdb-a8a1-554b-922e-625822c50dce_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_28","N/A","Ecoinvent  3.10, cut-off by allocation version","275f5839-90f3-50ab-8971-89cbd9fc793d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_29","N/A","Ecoinvent  3.10, cut-off by allocation version","11c0049d-e481-52b2-bd7b-72a491ad7ed3_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_30","N/A","Ecoinvent  3.10, cut-off by allocation version","91d8acb4-e0a7-51a8-85b8-0792e4e2c492_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_31","N/A","Ecoinvent  3.10, cut-off by allocation version","80e62ca3-236c-5e43-b007-942e61757853_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_32","N/A","Ecoinvent  3.10, cut-off by allocation version","b5cf1a85-ab39-5145-9544-155be6ca6d43_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_33","N/A","Ecoinvent  3.10, cut-off by allocation version","a8df3de1-1915-54cc-85aa-451e018d8332_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_34","N/A","Ecoinvent  3.10, cut-off by allocation version","581af806-d4f7-532f-99f5-46b495724400_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_35","N/A","Ecoinvent  3.10, cut-off by allocation version","dd9c8cc4-f857-51a9-a4ac-62b4b96f3bdf_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_36","N/A","Ecoinvent  3.10, cut-off by allocation version","9996f97c-69b6-5e77-a2b6-20d2253e137d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_37","N/A","Ecoinvent  3.10, cut-off by allocation version","a2b3c97a-e5f8-596d-adbe-b53627f210c3_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_38","N/A","Ecoinvent  3.10, cut-off by allocation version","c518da90-0362-54fe-913d-57118042bb09_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_39","N/A","Ecoinvent  3.10, cut-off by allocation version","2484baaa-e415-5fbc-9c33-c6a2ccd2e6ce_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_40","N/A","Ecoinvent  3.10, cut-off by allocation version","4d9f590b-bf4c-510b-b899-a83f138d78ea_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_41","N/A","Ecoinvent  3.10, cut-off by allocation version","da8aa9b5-cf46-5519-9159-0468958cae27_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_42","N/A","Ecoinvent  3.10, cut-off by allocation version","3e3d2f61-6803-57be-b6cd-73cd8a888f8e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_43","N/A","Ecoinvent  3.10, cut-off by allocation version","a228a463-f671-5180-af65-d2afe362f0fa_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_44","N/A","Ecoinvent  3.10, cut-off by allocation version","1bba7748-a22d-5ef3-ac7b-9f84e6376db2_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_45","N/A","Ecoinvent  3.10, cut-off by allocation version","75a39532-1863-5b57-bdfa-1d767b4ccf78_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_46","N/A","Ecoinvent  3.10, cut-off by allocation version","6c3d75b9-34ab-5e29-bcd1-e87b11908d96_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_47","N/A","Ecoinvent  3.10, cut-off by allocation version","9baa4e58-25c6-558f-abf1-9f796c57ab81_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_48","N/A","Ecoinvent  3.10, cut-off by allocation version","68f01316-97bb-5702-aa86-bbdd8414e490_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_49","N/A","Ecoinvent  3.10, cut-off by allocation version","7537f6a4-8e59-5766-bbb3-50e404fcca23_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_50","N/A","Ecoinvent  3.10, cut-off by allocation version","f0596e75-2d5f-5910-a974-af2f0267df23_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_51","N/A","Ecoinvent  3.10, cut-off by allocation version","4e32e3bd-b3a8-5d45-89b4-4f62c6c8c139_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_52","N/A","Ecoinvent  3.10, cut-off by allocation version","4b751597-0cf6-5cbc-af97-6068af6f1c09_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_53","N/A","Ecoinvent  3.10, cut-off by allocation version","1a8d13b2-87ac-5c43-aa62-4f1ceb9c9b54_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_54","N/A","Ecoinvent  3.10, cut-off by allocation version","a044fcb0-673d-54d9-a33a-fa8751352510_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_55","N/A","Ecoinvent  3.10, cut-off by allocation version","02f0edec-9d38-563d-bbfb-17d34b844ae1_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_56","N/A","Ecoinvent  3.10, cut-off by allocation version","2ad5c0a5-7831-5f5c-9b65-ed34e996d85a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_57","N/A","Ecoinvent  3.10, cut-off by allocation version","3eb03656-f9be-55f3-94cb-f421abfc38f5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_58","N/A","Ecoinvent  3.10, cut-off by allocation version","beef6691-f62f-5282-b8fe-c5d3f67fc624_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_59","N/A","Ecoinvent  3.10, cut-off by allocation version","8fae52c3-23ea-5d05-9aef-207d988fa26f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_60","N/A","Ecoinvent  3.10, cut-off by allocation version","2efd189f-472d-5931-89c0-57799674b9bf_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_61","N/A","Ecoinvent  3.10, cut-off by allocation version","2d5fbeac-02e0-5777-bb55-de3ab2d769ce_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_62","N/A","Ecoinvent  3.10, cut-off by allocation version","fc09fb1b-5219-5605-9f56-07f491033a59_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_63","N/A","Ecoinvent  3.10, cut-off by allocation version","ac460e8b-6885-502c-a95f-8e00b675a82c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_64","N/A","Ecoinvent  3.10, cut-off by allocation version","89a546df-22a4-5293-9058-5915230ea121_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_65","N/A","Ecoinvent  3.10, cut-off by allocation version","51653290-0910-5c53-9832-676388ad0e20_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_66","N/A","Ecoinvent  3.10, cut-off by allocation version","7334ae81-82a7-5423-9a8d-b9b8d0885347_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_67","N/A","Ecoinvent  3.10, cut-off by allocation version","053ce719-1cc3-5bca-8383-3e0c04f2556f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_68","N/A","Ecoinvent  3.10, cut-off by allocation version","c0e3d395-9bcf-542c-abbf-312ae80df261_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_69","N/A","Ecoinvent  3.10, cut-off by allocation version","e11f6315-cf7c-543e-93aa-42db02f156a6_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_70","N/A","Ecoinvent  3.10, cut-off by allocation version","f99a3a77-1a13-5e68-a657-e96e57e72b22_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_71","N/A","Ecoinvent  3.10, cut-off by allocation version","469cefbc-929d-51b7-906b-2642169b4075_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_72","N/A","Ecoinvent  3.10, cut-off by allocation version","6aa3a3ea-0ead-5cf7-8770-950aa5f64e10_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_73","N/A","Ecoinvent  3.10, cut-off by allocation version","f0613e44-8c68-5f7a-af9f-7f2fe2e48e84_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_74","N/A","Ecoinvent  3.10, cut-off by allocation version","3ec6e3fa-7524-5b00-a52b-968723e667ab_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_75","N/A","Ecoinvent  3.10, cut-off by allocation version","fb9c5497-a5ec-552c-b133-6b28af4ef7e1_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_76","N/A","Ecoinvent  3.10, cut-off by allocation version","9c0b45a9-4997-5953-b459-a1c89fbc44a0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_77","N/A","Ecoinvent  3.10, cut-off by allocation version","51fa6b66-b8f2-5475-9240-4ad88157d997_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_78","N/A","Ecoinvent  3.10, cut-off by allocation version","08883748-ffb3-537a-ad56-61c118aaf723_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_79","N/A","Ecoinvent  3.10, cut-off by allocation version","ea6ed979-2c3e-500a-9863-15c6f8eef81d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_80","N/A","Ecoinvent  3.10, cut-off by allocation version","5183e942-3664-5894-94d1-63bdf0b23daf_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_81","N/A","Ecoinvent  3.10, cut-off by allocation version","5b0b4c15-0aec-5772-b3b3-7d25bf723baf_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_82","N/A","Ecoinvent  3.10, cut-off by allocation version","4c19ac87-d1a1-5656-b1a9-05e5b3dd7ba5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_83","N/A","Ecoinvent  3.10, cut-off by allocation version","ea1a79e5-dfe9-5b67-89ac-0a2024ecec65_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_84","N/A","Ecoinvent  3.10, cut-off by allocation version","ca0533f7-60af-5e1f-b851-64033e9ca5cb_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_85","N/A","Ecoinvent  3.10, cut-off by allocation version","0ad7199c-7b0d-5b1f-9f40-bd0f41502a3a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_86","N/A","Ecoinvent  3.10, cut-off by allocation version","8662821a-12c7-558d-a8d8-6a5b0d7bfbbb_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_87","N/A","Ecoinvent  3.10, cut-off by allocation version","440eac7f-0117-52ac-af9e-d00defc3c285_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_88","N/A","Ecoinvent  3.10, cut-off by allocation version","81b7daa6-4845-5d63-8915-205a586fb550_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_89","N/A","Ecoinvent  3.10, cut-off by allocation version","e8577b3e-59c0-5c54-ad73-073efb411834_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_90","N/A","Ecoinvent  3.10, cut-off by allocation version","ebb7bff0-12e9-5c41-a1db-9e18e78c74be_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_91","N/A","Ecoinvent  3.10, cut-off by allocation version","64d81d22-4c9b-5bfa-8fbd-d775fac77972_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_92","N/A","Ecoinvent  3.10, cut-off by allocation version","e30a9776-31ac-5239-9d8c-45b8940fbbbd_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_93","N/A","Ecoinvent  3.10, cut-off by allocation version","ff2f2010-219e-583e-927b-a66deb7649e1_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_94","N/A","Ecoinvent  3.10, cut-off by allocation version","7ddf2644-bc3e-5f89-b4da-bb9b91963a10_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_95","N/A","Ecoinvent  3.10, cut-off by allocation version","b4cf8006-4329-5326-8790-0629582548df_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_96","N/A","Ecoinvent  3.10, cut-off by allocation version","cc87dc36-b51d-5609-8d8b-a31097103803_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_97","N/A","Ecoinvent  3.10, cut-off by allocation version","7d8b8318-9790-5dfb-a6ad-7238780a8f0a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_98","N/A","Ecoinvent  3.10, cut-off by allocation version","11a17d28-3a71-569f-b56c-12701fd7b094_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_99","N/A","Ecoinvent  3.10, cut-off by allocation version","d1cf7269-c305-5767-8006-10bda56df81e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_100","N/A","Ecoinvent  3.10, cut-off by allocation version","758d3d17-7a3e-5b30-961a-849a16d94cf3_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_101","N/A","Ecoinvent  3.10, cut-off by allocation version","5d8f39cc-fa03-5166-8ca3-98007070bf19_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_102","N/A","Ecoinvent  3.10, cut-off by allocation version","b6f7d61e-7614-5ccd-83b7-cc432475baac_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_103","N/A","Ecoinvent  3.10, cut-off by allocation version","8a5aaa7d-ccad-525a-be5f-5d7f1df898b9_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_104","N/A","Ecoinvent  3.10, cut-off by allocation version","311ac285-7ed6-50ea-a1dc-311c9a28c80a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_105","N/A","Ecoinvent  3.10, cut-off by allocation version","b0c4219b-7c45-5849-b7f4-630d19ed8eb6_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_106","N/A","Ecoinvent  3.10, cut-off by allocation version","3bb154e6-4405-5f8d-b1a0-b7b89a57705d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_107","N/A","Ecoinvent  3.10, cut-off by allocation version","9324bcd2-9447-561d-865e-02514dee0b5c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_108","N/A","Ecoinvent  3.10, cut-off by allocation version","01f66006-aa83-54ca-9330-78ee88f2b7c7_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_109","N/A","Ecoinvent  3.10, cut-off by allocation version","023804bb-ee14-58b0-abe1-41b1a28ff8ee_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_110","N/A","Ecoinvent  3.10, cut-off by allocation version","acab6c00-bdaf-5a67-a609-d8b28d149e4d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_111","N/A","Ecoinvent  3.10, cut-off by allocation version","5f03e37f-db10-5cf6-ac3c-2575b627c662_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_112","N/A","Ecoinvent  3.10, cut-off by allocation version","265ee001-ba3d-5379-82e0-a0c075b0ac02_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_113","N/A","Ecoinvent  3.10, cut-off by allocation version","fff7d27c-89c5-5282-b587-81ab232d7d6f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_114","N/A","Ecoinvent  3.10, cut-off by allocation version","0a765a9f-6d68-5a4c-8ba4-07a6b1508dc5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_115","N/A","Ecoinvent  3.10, cut-off by allocation version","39d45496-1958-5384-a553-9c7a73064866_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_116","N/A","Ecoinvent  3.10, cut-off by allocation version","07cac406-a071-5cd7-8c84-e8bcbe41b7ee_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_117","N/A","Ecoinvent  3.10, cut-off by allocation version","ee456a81-81aa-5e64-b607-ce14a8b24236_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_118","N/A","Ecoinvent  3.10, cut-off by allocation version","6ce260d8-04d7-5c41-8209-dc923db0928e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_119","N/A","Ecoinvent  3.10, cut-off by allocation version","8c4f006f-380c-538f-8a59-7df1d08c777d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_120","N/A","Ecoinvent  3.10, cut-off by allocation version","433b7238-0e9f-5343-a8eb-0e0a4c6c4eca_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_121","N/A","Ecoinvent  3.10, cut-off by allocation version","42407eff-aabe-566a-a151-3dc7c3d8dc3a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_122","N/A","Ecoinvent  3.10, cut-off by allocation version","257464d8-6250-5669-bb55-e256dcce29e0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_123","N/A","Ecoinvent  3.10, cut-off by allocation version","72f5c398-aadb-57dd-8b6a-e6571fbbb7c9_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_124","N/A","Ecoinvent  3.10, cut-off by allocation version","6c3b8106-17be-500e-a65a-3d12d07517a0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_125","N/A","Ecoinvent  3.10, cut-off by allocation version","81bdd3d2-a5b6-5fb4-b617-ebe79e02c050_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_126","N/A","Ecoinvent  3.10, cut-off by allocation version","8f486a15-4e49-5c00-9242-7e7ad70a3779_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_127","N/A","Ecoinvent  3.10, cut-off by allocation version","a8a31120-891f-595e-8162-bdc938a86343_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_128","N/A","Ecoinvent  3.10, cut-off by allocation version","96c5a4a4-5ec6-5d28-9ace-59c0414a631b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_129","N/A","Ecoinvent  3.10, cut-off by allocation version","72b26085-5a8b-58e2-ae83-abee9518abbe_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_130","N/A","Ecoinvent  3.10, cut-off by allocation version","995373ba-9aaf-51ee-a5a6-5a0679ca3131_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_131","N/A","Ecoinvent  3.10, cut-off by allocation version","9c1033e7-8db1-583f-b825-0d6e7ad28a72_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_132","N/A","Ecoinvent  3.10, cut-off by allocation version","6e7cdf4d-4e08-53be-b3e5-be169a30857e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_133","N/A","Ecoinvent  3.10, cut-off by allocation version","274e893c-d925-5d33-8b05-e4beea86eb1f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_134","N/A","Ecoinvent  3.10, cut-off by allocation version","62497925-a25b-5490-8d43-f626fab4dee3_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_135","N/A","Ecoinvent  3.10, cut-off by allocation version","9883579c-2621-58cf-bd7e-ad9cf3854264_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_136","N/A","Ecoinvent  3.10, cut-off by allocation version","04e14855-5bd0-58f2-9919-12352fbdf666_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_137","N/A","Ecoinvent  3.10, cut-off by allocation version","86ef6913-544e-5b9b-9b27-0731540b563e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_138","N/A","Ecoinvent  3.10, cut-off by allocation version","2fb93b9a-b882-5d99-a584-319fbc2d4888_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_139","N/A","Ecoinvent  3.10, cut-off by allocation version","3e74d4a1-652c-5cb3-af46-705998113b3b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_140","N/A","Ecoinvent  3.10, cut-off by allocation version","30cb3d2f-1967-5ab2-b024-ce57da0b3308_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_141","N/A","Ecoinvent  3.10, cut-off by allocation version","e77ffa79-0605-50fe-8c35-7695796966b9_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_142","N/A","Ecoinvent  3.10, cut-off by allocation version","e95b1799-89d8-5394-bed9-c9cc193221c0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_143","N/A","Ecoinvent  3.10, cut-off by allocation version","56e57368-1e71-5083-9cf2-7fbbd1bd4b97_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_144","N/A","Ecoinvent  3.10, cut-off by allocation version","55766f6a-4953-596b-9f4e-3e08873e8ec6_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_145","N/A","Ecoinvent  3.10, cut-off by allocation version","b32345b1-74dd-5002-b168-cdf1bf2ce085_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_146","N/A","Ecoinvent  3.10, cut-off by allocation version","045a8d09-9a26-55cd-ab83-152130df8104_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_147","N/A","Ecoinvent  3.10, cut-off by allocation version","aa7f6254-ce49-5cf4-9e1f-e19acbb335b7_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_148","N/A","Ecoinvent  3.10, cut-off by allocation version","dc35652a-6adf-5c96-9efb-070de65cce88_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_149","N/A","Ecoinvent  3.10, cut-off by allocation version","17bf22ac-3720-56ce-b678-1e896c81c5b0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_150","N/A","Ecoinvent  3.10, cut-off by allocation version","8c7e5ef5-8391-5cc1-a71d-3f1f74e4bf1a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_151","N/A","Ecoinvent  3.10, cut-off by allocation version","b1ab724c-ec07-5891-9fbe-9d56cdf16c7b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_152","N/A","Ecoinvent  3.10, cut-off by allocation version","d4976e17-addb-5f64-a762-90f89da7f05f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_153","N/A","Ecoinvent  3.10, cut-off by allocation version","0d78f095-f0be-541a-bd7f-1222879b8638_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_154","N/A","Ecoinvent  3.10, cut-off by allocation version","c12ee0e0-3cb6-5a2f-8c1d-94c62d324d4a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_155","N/A","Ecoinvent  3.10, cut-off by allocation version","ff8e6118-b4c0-58f1-a214-40b3dac03961_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_156","N/A","Ecoinvent  3.10, cut-off by allocation version","e187900c-4b7e-570c-8fb1-28f3cf860275_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_157","N/A","Ecoinvent  3.10, cut-off by allocation version","69556d8c-1c0e-59b1-90a9-5c05212972c4_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_158","N/A","Ecoinvent  3.10, cut-off by allocation version","375f2ed1-75d0-5065-aee9-45e53d048996_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_159","N/A","Ecoinvent  3.10, cut-off by allocation version","44eac5a7-f30b-5cff-99c6-b2a4208359da_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_160","N/A","Ecoinvent  3.10, cut-off by allocation version","7828dbba-e6f1-5e04-b6eb-dcd7af440a2d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_161","N/A","Ecoinvent  3.10, cut-off by allocation version","ba661998-a61a-5cdc-b7ce-302cbf7a9360_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_162","N/A","Ecoinvent  3.10, cut-off by allocation version","f67789ee-7aa3-58db-88c0-c232dc5f1f78_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_163","N/A","Ecoinvent  3.10, cut-off by allocation version","c6170cd7-00f8-5dfc-8bd4-1bcd1190857c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_164","N/A","Ecoinvent  3.10, cut-off by allocation version","bbb6924a-3ad6-56de-ae6e-050ead619bf2_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_165","N/A","Ecoinvent  3.10, cut-off by allocation version","048e3649-180b-5789-b12f-9223aa5b0e7f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_166","N/A","Ecoinvent  3.10, cut-off by allocation version","bc2de9e8-a936-5af2-a5df-f7d15df6ae7d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_167","N/A","Ecoinvent  3.10, cut-off by allocation version","46c2817e-317f-53b0-8cb5-85a1acbd6f7d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_168","N/A","Ecoinvent  3.10, cut-off by allocation version","e7469d76-1688-5c91-bce2-097bdd934b8b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_169","N/A","Ecoinvent  3.10, cut-off by allocation version","e2a3cf7a-33f6-596c-94c4-6794e8699854_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_170","N/A","Ecoinvent  3.10, cut-off by allocation version","d45fba3a-ded6-58d4-ae5f-1b64c53ba5cc_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_171","N/A","Ecoinvent  3.10, cut-off by allocation version","46e1ec5e-1be6-5fa5-aa4f-9a4897bc8a50_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_172","N/A","Ecoinvent  3.10, cut-off by allocation version","def10dfb-bfa2-5f37-ae70-5db9b840d93a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_173","N/A","Ecoinvent  3.10, cut-off by allocation version","29d264da-db2f-54d7-986a-ceaad846cdb4_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_174","N/A","Ecoinvent  3.10, cut-off by allocation version","faf37cde-4058-59f0-b67d-c26b9c054c34_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Electricity lifecycle"]
[null,"OSW_SE_175","N/A","Ecoinvent  3.10, cut-off by allocation version","eb0d1076-5276-5b7a-83bc-cce475127870_705f483c-0d06-4f1c-9be9-7d54b88c4015",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Gaseous fuels lifecycle"]
[null,"OSW_SE_176","N/A","Ecoinvent  3.10, cut-off by allocation version","f1b07269-1222-534b-b8a7-fa001e31dc17_b4e0b7c5-87b9-490e-971f-9ddc8c2b08d8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Liquid fuels lifecycle"]
[null,"OSW_SE_177","N/A","Ecoinvent  3.10, cut-off by allocation version","6e74a577-75d2-5023-941a-5007cde9c18a_fecdf330-8660-4362-adde-ab5ea197ab1d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Liquid fuels lifecycle"]
[null,"OSW_SE_178","N/A","Ecoinvent  3.10, cut-off by allocation version","e622ec20-8840-5a4c-90cc-9a073ee6e738_b0f4c2fb-5081-474a-8ffa-1457da8345db",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Liquid fuels lifecycle"]
[null,"OSW_SE_179","N/A","Ecoinvent  3.10, cut-off by allocation version","da0dbd21-a4fe-5ed0-98f3-8feb48d74787_1151abf1-5ac3-4518-bb20-60f003bb6a31",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Liquid fuels lifecycle"]
[null,"OSW_SE_180","N/A","Ecoinvent  3.10, cut-off by allocation version","e6576483-6c19-59fe-98b7-191f866a63df_533392d3-8fa6-44bb-9b79-b14c0a0e66e0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Liquid fuels lifecycle"]
[null,"OSW_SE_181","N/A","Ecoinvent  3.10, cut-off by allocation version","0cb8762f-ed6c-503d-bc05-3cf14601c72f_79838d89-26c0-4781-b17f-a0deb787d482",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Liquid fuels lifecycle"]
[null,"OSW_SE_182","N/A","Ecoinvent  3.10, cut-off by allocation version","f4aeaeba-ba0f-5236-845f-001a2d9a023b_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_183","N/A","Ecoinvent  3.10, cut-off by allocation version","988df15c-0222-5ba6-bbab-30e0695bf7eb_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_184","N/A","Ecoinvent  3.10, cut-off by allocation version","b564083a-0561-567b-9239-a82862ef7e6a_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_185","N/A","Ecoinvent  3.10, cut-off by allocation version","d747455f-a7c7-5798-85ba-a60e09d41b3d_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_186","N/A","Ecoinvent  3.10, cut-off by allocation version","1cb04872-15c3-54bc-ac35-1312b37eb8bf_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_187","N/A","Ecoinvent  3.10, cut-off by allocation version","6710b4ed-d4e1-527f-aa6c-670af3a595bb_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_188","N/A","Ecoinvent  3.10, cut-off by allocation version","7d456e1e-7622-5d1f-9292-402ee3cbdcc7_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_189","N/A","Ecoinvent  3.10, cut-off by allocation version","9c5a283f-37d0-5818-9e42-0484c5027ef6_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_190","N/A","Ecoinvent  3.10, cut-off by allocation version","b825409b-5694-5325-a11d-0fe92dd8a650_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilities","Water consumption"]
[null,"OSW_SE_191","N/A","Ecoinvent  3.10, cut-off by allocation version","278c318b-af70-5dc1-81ca-2079ef82d592_5bcb4640-2e25-4dc3-acc4-d89f308eb32c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_192","N/A","Ecoinvent  3.10, cut-off by allocation version","920bcef5-ca9c-5ae7-8d89-49be2287e530_4124c89b-fbf6-4320-a994-9f7d90447bd5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_193","N/A","Ecoinvent  3.10, cut-off by allocation version","2cc0d6c8-6b7e-5b2c-9596-1ca386c66a57_8795dc98-b6c7-4f09-be36-66739ea84900",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_194","N/A","Ecoinvent  3.10, cut-off by allocation version","f6314cea-f994-50f6-8fd4-60eb266e5969_3317126a-4dd7-4047-9ccf-163f94382c94",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_195","N/A","Ecoinvent  3.10, cut-off by allocation version","f96c0979-e6e6-54c9-8564-e0fab55df732_220fe333-5329-4a8d-b012-1db429f2383b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_196","N/A","Ecoinvent  3.10, cut-off by allocation version","b48b5a4d-54a0-59f7-8de2-913b5a4e24f9_07ad9bb5-f5d3-4e09-ac39-a6dcbb13a0ba",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_197","N/A","Ecoinvent  3.10, cut-off by allocation version","855fef94-252f-521e-b4d5-30e4bbf34926_02db23d4-0c70-4c90-98b6-2aa65ef4b268",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_198","N/A","Ecoinvent  3.10, cut-off by allocation version","dc851ae2-7510-5bd1-9787-2b006da03f35_3317126a-4dd7-4047-9ccf-163f94382c94",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_199","N/A","Ecoinvent  3.10, cut-off by allocation version","74220222-9c26-5611-8647-d8f035b32b5e_220fe333-5329-4a8d-b012-1db429f2383b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_200","N/A","Ecoinvent  3.10, cut-off by allocation version","df735d07-cc3c-56a9-b820-1308381c2c0c_07ad9bb5-f5d3-4e09-ac39-a6dcbb13a0ba",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_201","N/A","Ecoinvent  3.10, cut-off by allocation version","9578f022-c5f8-52a6-8179-a874e16c1323_02db23d4-0c70-4c90-98b6-2aa65ef4b268",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_202","N/A","Ecoinvent  3.10, cut-off by allocation version","1b6cdc0c-fdb0-56c9-b39f-9fe5b6b4b1a7_c784e421-2f79-47e4-8b6d-2c29fa41aad0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_203","N/A","Ecoinvent  3.10, cut-off by allocation version","c6e5ed96-f225-5ffd-974a-8efda70209d7_cc7e810b-79d2-4c9c-96e6-60a3c739952c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_204","N/A","Ecoinvent  3.10, cut-off by allocation version","0aefeb47-cf69-5ee0-8ac9-e3dfee68d5e8_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_205","N/A","Ecoinvent  3.10, cut-off by allocation version","394443c6-d2f4-5eba-9fb9-72e479cad99b_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_206","N/A","Ecoinvent  3.10, cut-off by allocation version","4f94bd0c-3028-57b7-93ba-127056601ac4_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_207","N/A","Ecoinvent  3.10, cut-off by allocation version","e6f415f7-267f-5a7a-a26e-38afcfb159a6_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_208","N/A","Ecoinvent  3.10, cut-off by allocation version","dcceff88-3edf-5291-ab2a-ae67b46bfb1b_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_209","N/A","Ecoinvent  3.10, cut-off by allocation version","245fe21a-bef8-5ed5-bc6b-799ab91cc4b3_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_210","N/A","Ecoinvent  3.10, cut-off by allocation version","e6581ba7-eba3-5cb5-a89e-41830e002068_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_211","N/A","Ecoinvent  3.10, cut-off by allocation version","0be94d2a-ebaf-5f72-9926-162c7edee0e1_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_212","N/A","Ecoinvent  3.10, cut-off by allocation version","a2b74eef-088d-528d-82fa-331855e70442_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_213","N/A","Ecoinvent  3.10, cut-off by allocation version","2e773d69-933e-57fa-a16a-3d505101ebc5_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_214","N/A","Ecoinvent  3.10, cut-off by allocation version","4a96b90f-d751-5ff9-b256-454971dc63a4_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_215","N/A","Ecoinvent  3.10, cut-off by allocation version","8fc6b375-653f-5dbf-856d-5196624c1dd4_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_216","N/A","Ecoinvent  3.10, cut-off by allocation version","96b8d86d-76bc-5500-b159-6ae084327b91_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_217","N/A","Ecoinvent  3.10, cut-off by allocation version","4e39d168-df1e-5c2d-b08a-bc8be50e131c_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_218","N/A","Ecoinvent  3.10, cut-off by allocation version","7eca3d84-04a7-5ead-a837-343689350ac2_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_219","N/A","Ecoinvent  3.10, cut-off by allocation version","57d005b5-1f11-5a27-ad75-249245cedd81_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_220","N/A","Ecoinvent  3.10, cut-off by allocation version","98467a29-aaf3-508f-ae4c-9a359ed1423c_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_221","N/A","Ecoinvent  3.10, cut-off by allocation version","ab481aec-f834-5863-b601-731be2115fcf_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_222","N/A","Ecoinvent  3.10, cut-off by allocation version","787fa53e-6b32-56d9-852c-5000fe4f7de4_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_223","N/A","Ecoinvent  3.10, cut-off by allocation version","3ed7f6bb-5b04-5b1d-a44f-6b2d1b0ba80f_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_224","N/A","Ecoinvent  3.10, cut-off by allocation version","4f675495-4f98-5f79-a371-c2c6058b9c44_090f56b8-6a83-48c1-ae26-234d04771e53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_225","N/A","Ecoinvent  3.10, cut-off by allocation version","148e286c-d4ec-5f5e-963f-4885b6a2b777_090f56b8-6a83-48c1-ae26-234d04771e53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_226","N/A","Ecoinvent  3.10, cut-off by allocation version","bf668603-c28d-5404-ad4f-e012820f39cd_090f56b8-6a83-48c1-ae26-234d04771e53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_227","N/A","Ecoinvent  3.10, cut-off by allocation version","eb228975-9d25-5925-b69a-c8e84902b62e_720d079e-242b-4d52-9268-bc9ffa6b5692",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_228","N/A","Ecoinvent  3.10, cut-off by allocation version","93891b3d-fc01-5844-bbb4-fe1557bc6341_173bc101-dadb-4bd8-952b-41b1b6fe2d90",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_229","N/A","Ecoinvent  3.10, cut-off by allocation version","efae5ae5-e980-579a-8ee7-28158db7f8f9_090f56b8-6a83-48c1-ae26-234d04771e53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_230","N/A","Ecoinvent  3.10, cut-off by allocation version","981623e0-8473-506b-b3af-fc89de20bcde_55b795a2-886f-419e-af38-fba1b83fa51b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_231","N/A","Ecoinvent  3.10, cut-off by allocation version","92c0f64c-87a6-59ea-b488-323144cc8c0e_4ecf1190-7028-4038-89b0-79adeb3e98cc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_232","N/A","Ecoinvent  3.10, cut-off by allocation version","00ebb760-a02e-515c-9dfe-b781d470118b_4ecf1190-7028-4038-89b0-79adeb3e98cc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_233","N/A","Ecoinvent  3.10, cut-off by allocation version","cf362a67-e18f-5a40-9fa0-e643a45e6a62_559d5695-102a-4beb-9f7f-3db334c9b51d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_234","N/A","Ecoinvent  3.10, cut-off by allocation version","d44d5da7-2c10-5f1f-9917-98c45ce08b3a_559d5695-102a-4beb-9f7f-3db334c9b51d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_235","N/A","Ecoinvent  3.10, cut-off by allocation version","59b4a49a-2816-5dd8-9b51-9924118f0365_f9895e44-5657-47fc-8eec-a4985e2bce2e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_236","N/A","Ecoinvent  3.10, cut-off by allocation version","ad0df3ef-6a94-59d1-af03-bc56e857e73e_f9895e44-5657-47fc-8eec-a4985e2bce2e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_237","N/A","Ecoinvent  3.10, cut-off by allocation version","340d0a19-f856-5f39-ac1c-524141fdb9e5_f9895e44-5657-47fc-8eec-a4985e2bce2e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_238","N/A","Ecoinvent  3.10, cut-off by allocation version","85add2fa-4e0b-5f63-9d39-1e5b06c32761_fb655769-10d8-446b-87f8-44ca60e20ed9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_239","N/A","Ecoinvent  3.10, cut-off by allocation version","404e4cd3-7e0e-548a-b5da-caa303df3a0a_fb655769-10d8-446b-87f8-44ca60e20ed9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_240","N/A","Ecoinvent  3.10, cut-off by allocation version","a3cc68f5-42cc-5be6-9a06-5a5017a6002e_f4e8b38b-d6c7-423b-bc9c-13b4a13d55f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_241","N/A","Ecoinvent  3.10, cut-off by allocation version","c7d08a8a-88f3-59ed-a131-307882e1536a_f4e8b38b-d6c7-423b-bc9c-13b4a13d55f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_242","N/A","Ecoinvent  3.10, cut-off by allocation version","23c14cca-52f9-5221-b5bc-559d5c88c2b8_f4e8b38b-d6c7-423b-bc9c-13b4a13d55f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_243","N/A","Ecoinvent  3.10, cut-off by allocation version","ce890a2c-afd2-51a4-b713-9fa9504776d3_c691b775-a65a-4b77-a588-c8c6cd01c725",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_244","N/A","Ecoinvent  3.10, cut-off by allocation version","985c231e-686d-5cf9-b282-b5a65b6d8804_c691b775-a65a-4b77-a588-c8c6cd01c725",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_245","N/A","Ecoinvent  3.10, cut-off by allocation version","e174683a-0200-5604-8344-50d8dc1cc5ce_653ca70d-49a6-4c62-ae9c-56b3c00b647c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_246","N/A","Ecoinvent  3.10, cut-off by allocation version","8ab97ce9-f88a-5fd5-a0ea-a87423d4e704_653ca70d-49a6-4c62-ae9c-56b3c00b647c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_247","N/A","Ecoinvent  3.10, cut-off by allocation version","fbddbcba-a9d3-58ac-bc2b-48ce2eb52299_2341598f-166d-4f0c-97d2-0077a191b11f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_248","N/A","Ecoinvent  3.10, cut-off by allocation version","828774ce-d14c-5fbb-bc4a-0def4669a08b_2341598f-166d-4f0c-97d2-0077a191b11f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_249","N/A","Ecoinvent  3.10, cut-off by allocation version","823929ce-afe1-5101-ac27-ce3ca72fdc4b_518404fc-5571-4fc8-80a0-67c099278772",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_250","N/A","Ecoinvent  3.10, cut-off by allocation version","173c274e-1f24-5a22-a7cf-c1e18494f8ec_518404fc-5571-4fc8-80a0-67c099278772",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_251","N/A","Ecoinvent  3.10, cut-off by allocation version","58cd4158-59d2-5c8c-88ae-beb86849b3d6_bd061b71-270b-4644-9e14-6c59b2e4090d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_252","N/A","Ecoinvent  3.10, cut-off by allocation version","252a8945-d0af-539f-ba04-8752ca19433f_bd061b71-270b-4644-9e14-6c59b2e4090d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_253","N/A","Ecoinvent  3.10, cut-off by allocation version","3092ea07-a68d-5bc3-8f99-f548d345908e_c0a7ba59-f9b5-45b5-8e1d-6e4e40ba86df",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_254","N/A","Ecoinvent  3.10, cut-off by allocation version","939b9ef2-7989-5365-9574-58e1227a293f_c0a7ba59-f9b5-45b5-8e1d-6e4e40ba86df",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_255","N/A","Ecoinvent  3.10, cut-off by allocation version","1a631c39-2fb7-53dc-b38e-81785eacf070_c0a7ba59-f9b5-45b5-8e1d-6e4e40ba86df",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_256","N/A","Ecoinvent  3.10, cut-off by allocation version","ba34f3de-8ef3-5d30-af2b-30a69caf0332_03bf1369-1eec-49d0-bc4b-8b29efa826b9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_257","N/A","Ecoinvent  3.10, cut-off by allocation version","e44f7efa-8844-5bbb-a986-03a77f19fd34_03bf1369-1eec-49d0-bc4b-8b29efa826b9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_258","N/A","Ecoinvent  3.10, cut-off by allocation version","1cf1f7c7-2ee9-5d0b-9dcd-436d3b5afcc5_99598921-d5df-489f-b96c-7dd4ba6b36a6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_259","N/A","Ecoinvent  3.10, cut-off by allocation version","b709b6c8-56a2-5da8-a729-2d99f44d03a5_99598921-d5df-489f-b96c-7dd4ba6b36a6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_260","N/A","Ecoinvent  3.10, cut-off by allocation version","95486215-9779-5cfc-8da4-359a8ad5fc9e_99598921-d5df-489f-b96c-7dd4ba6b36a6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_261","N/A","Ecoinvent  3.10, cut-off by allocation version","5e220af0-494e-518a-94ef-8fe400b79001_ccc1fbd3-3877-43b6-a845-0c2ed8359c29",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_262","N/A","Ecoinvent  3.10, cut-off by allocation version","20a2cec2-2498-5e43-bebc-385df005d06b_ccc1fbd3-3877-43b6-a845-0c2ed8359c29",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_263","N/A","Ecoinvent  3.10, cut-off by allocation version","a5756ad5-ffd8-59b3-be93-a54efdf31524_cf34bfa7-b49b-4ca1-a94d-0eff5dbd23d8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_264","N/A","Ecoinvent  3.10, cut-off by allocation version","fce59ef5-0422-5a7e-951a-6b838c2d3a4d_cf34bfa7-b49b-4ca1-a94d-0eff5dbd23d8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_265","N/A","Ecoinvent  3.10, cut-off by allocation version","62316927-dd5d-5472-bc65-f9dbdda06597_da85af95-9191-4be6-aa68-e0a980c28785",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_266","N/A","Ecoinvent  3.10, cut-off by allocation version","23d0098d-d329-56fa-9e07-7b3a7bb767c3_da85af95-9191-4be6-aa68-e0a980c28785",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_267","N/A","Ecoinvent  3.10, cut-off by allocation version","62d9f625-531c-564d-8ae1-b14bec334f08_999d5179-2235-493a-8bd8-d805bb71eee8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_268","N/A","Ecoinvent  3.10, cut-off by allocation version","b1fe1a60-0200-5faa-aedc-730732ba1b2d_999d5179-2235-493a-8bd8-d805bb71eee8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_269","N/A","Ecoinvent  3.10, cut-off by allocation version","58ab1e7f-e02e-540a-8291-9241313ad640_ae39ee61-d4d0-4cce-93b4-0745344da5fa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_270","N/A","Ecoinvent  3.10, cut-off by allocation version","43b7ccf2-4840-596e-91d0-8bb374e9d599_ae39ee61-d4d0-4cce-93b4-0745344da5fa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_271","N/A","Ecoinvent  3.10, cut-off by allocation version","fa4c1c14-af58-5faa-8fcb-0ac283c9854d_ae39ee61-d4d0-4cce-93b4-0745344da5fa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_272","N/A","Ecoinvent  3.10, cut-off by allocation version","179dae39-5e28-5dd5-a8fa-ab7336cadafa_639dba7b-1762-4e9a-a95c-f30380e65d53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_273","N/A","Ecoinvent  3.10, cut-off by allocation version","ac148ceb-591d-5d05-b80d-b2a420db10f9_639dba7b-1762-4e9a-a95c-f30380e65d53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_274","N/A","Ecoinvent  3.10, cut-off by allocation version","4a0ebfac-5c44-5475-86d6-e617d236b40e_24f5a760-85ea-4ed7-a4f2-cff90141671b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_275","N/A","Ecoinvent  3.10, cut-off by allocation version","6a52934c-e357-52ef-a33e-fa3420acc364_24f5a760-85ea-4ed7-a4f2-cff90141671b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_276","N/A","Ecoinvent  3.10, cut-off by allocation version","66352dc1-4469-5db8-b8c8-4111480f9766_24f5a760-85ea-4ed7-a4f2-cff90141671b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_277","N/A","Ecoinvent  3.10, cut-off by allocation version","975a8721-de91-5b10-b299-713b449be8d8_73585052-b3e9-4cde-832d-2db3272d2ae5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_278","N/A","Ecoinvent  3.10, cut-off by allocation version","14a7b03f-341f-5560-bb36-79a7de565718_73585052-b3e9-4cde-832d-2db3272d2ae5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_279","N/A","Ecoinvent  3.10, cut-off by allocation version","69b4fbb8-3991-575b-a26e-4eb864d7111b_a8523835-3905-4e3f-9e2f-ae1d8cad0317",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_280","N/A","Ecoinvent  3.10, cut-off by allocation version","e52061b7-a41f-500a-95b7-68e7977c04ef_a8523835-3905-4e3f-9e2f-ae1d8cad0317",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_281","N/A","Ecoinvent  3.10, cut-off by allocation version","81a1523d-cc38-58f7-8dc2-72f05aadcde7_8ddc8009-4733-49e9-8a4e-a1081d05eb8b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_282","N/A","Ecoinvent  3.10, cut-off by allocation version","7ecc69e1-15ca-5342-b246-ccc603b29c28_8ddc8009-4733-49e9-8a4e-a1081d05eb8b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_283","N/A","Ecoinvent  3.10, cut-off by allocation version","87653782-cc98-5a1b-8b4f-b7d1ca2c2941_3a40db23-1aed-4b82-8117-32251e039134",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_284","N/A","Ecoinvent  3.10, cut-off by allocation version","8f697305-28ed-55be-9512-b0456b77f4e2_3a40db23-1aed-4b82-8117-32251e039134",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_285","N/A","Ecoinvent  3.10, cut-off by allocation version","0f8768d4-90f1-55f3-a2d6-df33486935fe_b909dee2-76bd-4eae-87d5-fc831390f99b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_286","N/A","Ecoinvent  3.10, cut-off by allocation version","744b4753-4710-561f-96e9-5dd1152abb26_b909dee2-76bd-4eae-87d5-fc831390f99b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_287","N/A","Ecoinvent  3.10, cut-off by allocation version","e11cbcd9-a0ff-56a6-972c-4c686d948f56_b909dee2-76bd-4eae-87d5-fc831390f99b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_288","N/A","Ecoinvent  3.10, cut-off by allocation version","070a1713-7483-5465-b235-fea42f5d5de1_fea783cd-1b3e-47ed-a4a1-346094ebc39a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_289","N/A","Ecoinvent  3.10, cut-off by allocation version","b0856062-d28d-5019-bbad-03fa07c8f0f7_fea783cd-1b3e-47ed-a4a1-346094ebc39a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_290","N/A","Ecoinvent  3.10, cut-off by allocation version","fe02497f-fd5a-5c70-b6ca-480ea5776bda_93afc03f-5832-4ec0-8d76-cf6e62efff26",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_291","N/A","Ecoinvent  3.10, cut-off by allocation version","0edfde13-47ea-5462-964c-e1c8e21f72c3_93afc03f-5832-4ec0-8d76-cf6e62efff26",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_292","N/A","Ecoinvent  3.10, cut-off by allocation version","fd1b4b7c-49bc-584a-afb9-ff6395f4aec1_93afc03f-5832-4ec0-8d76-cf6e62efff26",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_293","N/A","Ecoinvent  3.10, cut-off by allocation version","378e389c-69c5-55fb-8d24-47ea16e992fb_52a8f3c4-df5d-4f18-830b-985bcd8ac830",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_294","N/A","Ecoinvent  3.10, cut-off by allocation version","904e0110-39da-5898-88a0-a706d3d2352e_52a8f3c4-df5d-4f18-830b-985bcd8ac830",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_295","N/A","Ecoinvent  3.10, cut-off by allocation version","222fe198-231d-5875-b2d7-e6fd6832e71d_eee5f6b0-7c73-473a-9e27-82d38ae3661b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_296","N/A","Ecoinvent  3.10, cut-off by allocation version","b25a4f38-1940-5159-97cc-e3870f94f8ed_eee5f6b0-7c73-473a-9e27-82d38ae3661b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_297","N/A","Ecoinvent  3.10, cut-off by allocation version","d0adf2c8-b203-5aee-aeff-205f93339c92_eeb68c18-502b-4117-a033-a5daf24322fc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_298","N/A","Ecoinvent  3.10, cut-off by allocation version","951bece1-40e9-52c6-886e-2a0beaab9959_2741cea8-327f-4e0f-9401-b10858dc68f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_299","N/A","Ecoinvent  3.10, cut-off by allocation version","1220dda3-c78a-55c1-97cf-d68700f14716_82befb8d-fc52-4942-b53f-67b526eb0c25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_300","N/A","Ecoinvent  3.10, cut-off by allocation version","28cc53c0-f97f-56f5-b52b-0f23316c21b5_b41ed270-f3f0-4126-b391-8c9ac9076d3b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_301","N/A","Ecoinvent  3.10, cut-off by allocation version","e348cde9-a345-5592-98ae-112c644b316b_6fcb39b4-3030-47b1-872e-a84c23dca79b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_302","N/A","Ecoinvent  3.10, cut-off by allocation version","34a9a389-ad3e-5265-b239-4504047d0cd5_a34be1fd-b392-4901-9602-f7d25e46426d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_303","N/A","Ecoinvent  3.10, cut-off by allocation version","e83a1735-5822-524c-ab09-921892bd1e11_a34be1fd-b392-4901-9602-f7d25e46426d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_304","N/A","Ecoinvent  3.10, cut-off by allocation version","739a1ba3-2a34-5792-b658-1abb326f8fa2_6bcb7d07-3c26-45c4-a87a-ead2ac75a66a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_305","N/A","Ecoinvent  3.10, cut-off by allocation version","f3aac569-4617-529d-93b8-9d8f643c4001_6bcb7d07-3c26-45c4-a87a-ead2ac75a66a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_306","N/A","Ecoinvent  3.10, cut-off by allocation version","6c31a4d3-a7f1-5ea8-9c0e-f556c4f46bc7_8d950031-fee3-4f3c-9bc1-889f6be31ea9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_307","N/A","Ecoinvent  3.10, cut-off by allocation version","30b6bcc3-ce9c-5307-912c-b1d117cc864a_8d950031-fee3-4f3c-9bc1-889f6be31ea9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_308","N/A","Ecoinvent  3.10, cut-off by allocation version","b9900f9a-5325-5bf1-ab5b-ee157c17cff6_1f4388f9-8a79-452d-8364-802a5bc5f548",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_309","N/A","Ecoinvent  3.10, cut-off by allocation version","f5f8b61f-76aa-5cf8-a5f5-3d7520953713_1f4388f9-8a79-452d-8364-802a5bc5f548",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_310","N/A","Ecoinvent  3.10, cut-off by allocation version","ead5f7a9-77c2-5c16-b304-5059c55254da_095528f2-b554-4cfb-9dc8-764b50bcbd7b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_311","N/A","Ecoinvent  3.10, cut-off by allocation version","99a9db3c-0727-5d27-a857-54eeb698e923_095528f2-b554-4cfb-9dc8-764b50bcbd7b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_312","N/A","Ecoinvent  3.10, cut-off by allocation version","c0bb7ead-2118-5870-930c-682920ed4d7b_7e02ffad-fa75-41ed-94f1-3d9c6f7e91bd",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_313","N/A","Ecoinvent  3.10, cut-off by allocation version","c3b92350-9ce1-5621-95f3-d3b04a1fff83_7e02ffad-fa75-41ed-94f1-3d9c6f7e91bd",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_314","N/A","Ecoinvent  3.10, cut-off by allocation version","9a5a217b-43ae-5c56-9969-bdffb869484a_4309fd1b-7875-491c-b158-65d8f5e2c663",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_315","N/A","Ecoinvent  3.10, cut-off by allocation version","13c79c73-181d-574f-a550-6cf13b119223_4309fd1b-7875-491c-b158-65d8f5e2c663",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_316","N/A","Ecoinvent  3.10, cut-off by allocation version","e2bc85d5-fa6a-5c4a-bfca-37883857bebd_3f225a75-4661-454e-9671-1b3e893ba72d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_317","N/A","Ecoinvent  3.10, cut-off by allocation version","d5d281ec-6086-5387-a7a8-966b07b38635_3f225a75-4661-454e-9671-1b3e893ba72d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_318","N/A","Ecoinvent  3.10, cut-off by allocation version","49e93c17-2909-57b9-bb74-1273959cab65_58f087c9-c348-4c55-bdc4-9805b5a0239a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_319","N/A","Ecoinvent  3.10, cut-off by allocation version","5c856191-f59f-5683-9563-6eaf5e4d1cf8_58f087c9-c348-4c55-bdc4-9805b5a0239a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_320","N/A","Ecoinvent  3.10, cut-off by allocation version","5072fda9-eb49-5be1-a6d6-d3aea58cdab4_ed65d3d9-349b-4e2c-870c-381209bc1484",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_321","N/A","Ecoinvent  3.10, cut-off by allocation version","2f7b2fcc-dbe0-5c51-9aab-38f05325d26e_ed65d3d9-349b-4e2c-870c-381209bc1484",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_322","N/A","Ecoinvent  3.10, cut-off by allocation version","fcf3ec5d-2c81-5d7d-bf1a-447474af504e_1305164c-678e-426b-95ff-b41e03e68aac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_323","N/A","Ecoinvent  3.10, cut-off by allocation version","718089a6-b151-5652-b61f-8ebdc1f8551e_1305164c-678e-426b-95ff-b41e03e68aac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_324","N/A","Ecoinvent  3.10, cut-off by allocation version","b06e2cba-f277-5e04-97cd-4987a78433a6_85a9dd8c-769e-4528-9a1a-105ab3269262",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_325","N/A","Ecoinvent  3.10, cut-off by allocation version","abba7741-1409-5783-96c4-343644af9a8b_85a9dd8c-769e-4528-9a1a-105ab3269262",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_326","N/A","Ecoinvent  3.10, cut-off by allocation version","4093ccfd-6e4a-55f9-ad27-b0b5e5b23b84_d710f3b0-f618-4627-83ed-bc53b82d26fc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_327","N/A","Ecoinvent  3.10, cut-off by allocation version","9b8bc605-7223-5622-bee0-6ab902651e24_ef9d859f-c740-4c1f-8f76-d4faddda1f9f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_328","N/A","Ecoinvent  3.10, cut-off by allocation version","edfa6868-06a1-515c-97dd-a2e7f2d0282c_ef9d859f-c740-4c1f-8f76-d4faddda1f9f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_329","N/A","Ecoinvent  3.10, cut-off by allocation version","59d894f1-3988-5e1f-996d-16eb40afb4be_692784c6-00e8-4309-971d-3fd8441120f1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_330","N/A","Ecoinvent  3.10, cut-off by allocation version","6b24f636-031b-5e7f-a376-34be6edb5ca7_692784c6-00e8-4309-971d-3fd8441120f1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_331","N/A","Ecoinvent  3.10, cut-off by allocation version","21870d94-54c0-5e13-aa4a-361023ef9097_9f2d5d73-1014-49ec-87ee-c6a6ed86b3d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_332","N/A","Ecoinvent  3.10, cut-off by allocation version","d2688e57-cf10-55a2-a64f-5e60fa5dcdf3_9f2d5d73-1014-49ec-87ee-c6a6ed86b3d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_333","N/A","Ecoinvent  3.10, cut-off by allocation version","cdf5199a-a55b-523e-8622-0e6a041880cb_3bf68190-17bd-4506-84da-3ef2bcb1b624",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_334","N/A","Ecoinvent  3.10, cut-off by allocation version","e0dbd35b-93b4-5dc1-ae1d-c62fee68ba4f_3bf68190-17bd-4506-84da-3ef2bcb1b624",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_335","N/A","Ecoinvent  3.10, cut-off by allocation version","8b93d34b-af3a-56cd-a6eb-dec7ac9b23e4_bf2ab99f-4704-4e62-958d-ec8efd2e1c1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_336","N/A","Ecoinvent  3.10, cut-off by allocation version","34f67d3e-c509-562a-9cc1-1f08e4ce9733_bf2ab99f-4704-4e62-958d-ec8efd2e1c1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_337","N/A","Ecoinvent  3.10, cut-off by allocation version","f736e877-5bc7-5ee3-ba36-1883aacb7597_e110266e-a20e-41ae-a5f6-7dbcf0935abd",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_338","N/A","Ecoinvent  3.10, cut-off by allocation version","be5aef40-bb22-51d6-80e4-dceaba4a11b9_e110266e-a20e-41ae-a5f6-7dbcf0935abd",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_339","N/A","Ecoinvent  3.10, cut-off by allocation version","9f41504d-db63-5ef6-a45c-596fe14f87e2_65e289a5-e378-41e7-9a41-bd51db029439",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_340","N/A","Ecoinvent  3.10, cut-off by allocation version","fe8577da-d422-555f-bb4b-16e6208c60fc_65e289a5-e378-41e7-9a41-bd51db029439",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_341","N/A","Ecoinvent  3.10, cut-off by allocation version","e3aa5b47-dee2-565e-b624-80b07286d7df_e095e692-5ebc-4bc5-89bc-8379bbc181f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_342","N/A","Ecoinvent  3.10, cut-off by allocation version","43d94a78-a534-52a7-90e9-8aa436f4b6fe_e095e692-5ebc-4bc5-89bc-8379bbc181f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_343","N/A","Ecoinvent  3.10, cut-off by allocation version","78f01775-083d-5885-af19-966c50e71295_e6f8dc95-a570-4a09-91cf-47c046e669e9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_344","N/A","Ecoinvent  3.10, cut-off by allocation version","c9697774-068e-5309-bee8-bfbe94956071_e6f8dc95-a570-4a09-91cf-47c046e669e9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_345","N/A","Ecoinvent  3.10, cut-off by allocation version","547a502a-d976-5861-bb6d-ec724fa18dbd_93d5bc32-a832-4ac1-960a-6705cdfaddc2",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_346","N/A","Ecoinvent  3.10, cut-off by allocation version","c0f8e8d3-371c-57e1-9226-022bb6157cc2_93d5bc32-a832-4ac1-960a-6705cdfaddc2",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_347","N/A","Ecoinvent  3.10, cut-off by allocation version","f988aa00-7f79-5161-bf6b-7b474acbda28_8f99cbf5-83d9-4989-aaa6-65bcedd82df1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_348","N/A","Ecoinvent  3.10, cut-off by allocation version","cedf4205-0da1-599e-8b44-20931c743d30_8f99cbf5-83d9-4989-aaa6-65bcedd82df1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_349","N/A","Ecoinvent  3.10, cut-off by allocation version","c6bad917-303f-568e-9187-6c293e03f3ed_c91eabe2-800b-48a3-9bc3-c46bbcfbdd5f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_350","N/A","Ecoinvent  3.10, cut-off by allocation version","f983eb56-1629-50b7-8dda-00c274159921_c91eabe2-800b-48a3-9bc3-c46bbcfbdd5f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_351","N/A","Ecoinvent  3.10, cut-off by allocation version","9f5ad98c-0c70-5727-8a5d-632b3100b85f_2496b794-9414-40bf-8545-5b84925b2f5f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_352","N/A","Ecoinvent  3.10, cut-off by allocation version","d1e2c45e-852b-5949-938f-e5681e00868c_2496b794-9414-40bf-8545-5b84925b2f5f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_353","N/A","Ecoinvent  3.10, cut-off by allocation version","d5e1f703-86be-5fae-ab89-694ad599f04c_54397bee-f5a8-4164-a43e-5dff00da3b10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_354","N/A","Ecoinvent  3.10, cut-off by allocation version","0495d309-6798-5ef4-8f3d-1460e1adb698_54397bee-f5a8-4164-a43e-5dff00da3b10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_355","N/A","Ecoinvent  3.10, cut-off by allocation version","50874e9f-6092-5b40-9e7c-07dd296f6dfe_ab08966c-085c-4cdf-9c2b-c137eee358c0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_356","N/A","Ecoinvent  3.10, cut-off by allocation version","bd00c8f2-5b6c-550c-8716-0cdc89aa7030_ab08966c-085c-4cdf-9c2b-c137eee358c0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_357","N/A","Ecoinvent  3.10, cut-off by allocation version","7b6abd95-be0e-5f44-8748-52a78a8e9083_068bf76a-bfaa-435c-85ed-3d2bb2c4bb4f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_358","N/A","Ecoinvent  3.10, cut-off by allocation version","2205ef31-4fe2-588f-95de-4fce4b2eb64f_068bf76a-bfaa-435c-85ed-3d2bb2c4bb4f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_359","N/A","Ecoinvent  3.10, cut-off by allocation version","49b22a98-176e-5b26-baa2-7d42532d9ad3_57143a43-20ab-44a5-a4a2-26effbdfafd1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_360","N/A","Ecoinvent  3.10, cut-off by allocation version","686983ca-8d05-563c-93f5-bbea3eb2bde9_57143a43-20ab-44a5-a4a2-26effbdfafd1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_361","N/A","Ecoinvent  3.10, cut-off by allocation version","4fb98a7a-b8c5-5b75-bc2b-dce7b0d49807_58b3db4e-19b8-43f2-8545-55229a5ee6e4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured assets","Cables"]
[null,"OSW_SE_362","N/A","Ecoinvent  3.10, cut-off by allocation version","8ec15097-54d0-592c-b814-ba9cf48cf9fc_8b988c18-f03b-46aa-83ae-d72d4639ff76",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured assets","Cables"]
[null,"OSW_SE_363","N/A","Ecoinvent  3.10, cut-off by allocation version","f82c7f4c-6690-514e-83af-7f79b5bee0dd_1692f537-b2ad-4143-bea3-226fc2fe9cf5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured assets","Wind turbine generators (WTG)"]
[null,"OSW_SE_364","N/A","Ecoinvent  3.10, cut-off by allocation version","ed7cf3b3-9b6d-5cd3-901f-2d36423c3a75_787cf1f4-ff36-4548-8a99-9adb6c4f8f23",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured components","Nacelle and internals"]
[null,"OSW_SE_365","N/A","Ecoinvent  3.10, cut-off by allocation version","2bf7943e-88ea-5a35-b5b2-6ee3d239bf07_9e2c266f-d04d-44bc-b277-b7f6a7e3dffa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured components","Transformer"]
[null,"OSW_SE_366","N/A","Ecoinvent  3.10, cut-off by allocation version","7ce3820e-523d-57fc-a959-328a99cabb00_0c7faf73-f5ea-4a3b-96ec-54d025cae6f4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured components","Transformer"]
[null,"OSW_SE_367","N/A","Ecoinvent  3.10, cut-off by allocation version","55945c81-d448-5182-9ef6-dd416454afca_d187adaf-a08d-4f75-a1ba-bb46c4597f45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Coating and galvanising processes"]
[null,"OSW_SE_368","N/A","Ecoinvent  3.10, cut-off by allocation version","c8f3325c-b8a7-50f8-a788-1e67e8fd1553_d187adaf-a08d-4f75-a1ba-bb46c4597f45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Coating and galvanising processes"]
[null,"OSW_SE_369","N/A","Ecoinvent  3.10, cut-off by allocation version","2a55050a-229b-5ed3-b17a-7133009d9a15_9087eb5f-4662-4cb1-a524-f5cb80b1238a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_370","N/A","Ecoinvent  3.10, cut-off by allocation version","d113489b-113e-5059-bc92-cd9f315a7e17_9087eb5f-4662-4cb1-a524-f5cb80b1238a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_371","N/A","Ecoinvent  3.10, cut-off by allocation version","001c496b-8ad1-5743-b901-836dfa6ff00a_06194d2b-4c2b-44de-9a29-1a364616a1d2",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_372","N/A","Ecoinvent  3.10, cut-off by allocation version","50ad4ffb-c431-5396-a1c8-956edcc22895_06194d2b-4c2b-44de-9a29-1a364616a1d2",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_373","N/A","Ecoinvent  3.10, cut-off by allocation version","4e273f0f-2246-5126-a337-1e06c7f7eb48_ee8d31fc-f67f-43b2-910d-172880730b28",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_374","N/A","Ecoinvent  3.10, cut-off by allocation version","8c498881-1eb5-56a6-90c9-70304184913f_ee8d31fc-f67f-43b2-910d-172880730b28",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_375","N/A","Ecoinvent  3.10, cut-off by allocation version","a8c9b91b-3788-582e-9dd3-b40f95af6453_cdb7b939-f508-49ed-80f3-b39f6137fe1c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_376","N/A","Ecoinvent  3.10, cut-off by allocation version","80ee09d6-809f-5ac9-80bf-64d001b28fab_444d81a0-13e0-41a4-8f63-e691b0133c04",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_377","N/A","Ecoinvent  3.10, cut-off by allocation version","f2511240-f350-53bf-b18f-7dc82d379af2_579049d0-3db8-4496-a234-2f61ed28a72b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_378","N/A","Ecoinvent  3.10, cut-off by allocation version","5bc75a9c-cb54-5327-8071-2f31486dbb90_579049d0-3db8-4496-a234-2f61ed28a72b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_379","N/A","Ecoinvent  3.10, cut-off by allocation version","49c0e19b-cdc5-52fc-888a-acc07c402d99_406ae9de-8894-4c8b-a601-40b7e849b66d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_380","N/A","Ecoinvent  3.10, cut-off by allocation version","07da644f-d126-5faf-82fd-056715b7e44c_406ae9de-8894-4c8b-a601-40b7e849b66d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_381","N/A","Ecoinvent  3.10, cut-off by allocation version","accecafc-3aea-5df7-ad09-de1949ddb26d_8ad0b079-38b6-4700-8462-74648a4edd7d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_382","N/A","Ecoinvent  3.10, cut-off by allocation version","3f7d1c92-5a70-5468-8ca0-b0da9b8af829_425089e2-ad80-414f-b6eb-67b32f5aa626",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_383","N/A","Ecoinvent  3.10, cut-off by allocation version","4ce56f07-081d-5ee4-b8aa-11448cdd7f5b_a5309c08-cc71-402e-b870-163a09ee0742",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_384","N/A","Ecoinvent  3.10, cut-off by allocation version","34d5c2a1-6eae-5bfe-a340-d1ec4298fb8d_a5309c08-cc71-402e-b870-163a09ee0742",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_385","N/A","Ecoinvent  3.10, cut-off by allocation version","eba86c08-c6ca-5ca0-a73c-55db44dee8bc_68b4fdd4-d341-4ac5-9dbc-59eb34653dab",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_386","N/A","Ecoinvent  3.10, cut-off by allocation version","56c28af4-c4e1-595b-bfcf-4cf98be56b0f_68b4fdd4-d341-4ac5-9dbc-59eb34653dab",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_387","N/A","Ecoinvent  3.10, cut-off by allocation version","beeba0ad-c2be-5ee3-b3dc-ef2f79aaf12a_dfbdd39b-2541-4069-9b87-ab61ef6fbc0c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_388","N/A","Ecoinvent  3.10, cut-off by allocation version","1e7cd149-2dd9-510a-a001-0fa9d5f40c7f_dfbdd39b-2541-4069-9b87-ab61ef6fbc0c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_389","N/A","Ecoinvent  3.10, cut-off by allocation version","1069c9d1-790a-5676-90ce-93ee690abf7c_e2f62697-57d4-42fe-95bf-c85fd32a9cf0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_390","N/A","Ecoinvent  3.10, cut-off by allocation version","87cc6df1-c49e-5fc0-b399-c2803ab13e0b_e2f62697-57d4-42fe-95bf-c85fd32a9cf0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_391","N/A","Ecoinvent  3.10, cut-off by allocation version","b180f717-b151-51e6-b27d-958075016be3_fef44ccb-917e-4c8d-bb35-a1898827b659",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Aluminium"]
[null,"OSW_SE_392","N/A","Ecoinvent  3.10, cut-off by allocation version","a1933dcd-abae-5bf4-bf34-f7b363be5b2e_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Aluminium"]
[null,"OSW_SE_393","N/A","Ecoinvent  3.10, cut-off by allocation version","d95292fe-49d6-5760-b82f-18ecc1136cd8_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Aluminium"]
[null,"OSW_SE_394","N/A","Ecoinvent  3.10, cut-off by allocation version","1e469dc6-d56a-57b5-87b3-df303bc1b2c9_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Aluminium"]
[null,"OSW_SE_395","N/A","Ecoinvent  3.10, cut-off by allocation version","caf41f87-e599-5995-b00c-46cbecc66aee_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_396","N/A","Ecoinvent  3.10, cut-off by allocation version","16aee8f7-1c95-5b49-82e8-94e23f073a3e_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_397","N/A","Ecoinvent  3.10, cut-off by allocation version","76941379-c364-501e-9008-a9c7e9fc78e0_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_398","N/A","Ecoinvent  3.10, cut-off by allocation version","d56f7390-6003-5462-b350-779a9faf202c_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_399","N/A","Ecoinvent  3.10, cut-off by allocation version","c625b7d3-07c9-5ac7-808b-95dc2e5befdf_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_400","N/A","Ecoinvent  3.10, cut-off by allocation version","f1865053-b23d-5d6b-b431-cde2ed998e08_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_401","N/A","Ecoinvent  3.10, cut-off by allocation version","fe92458a-3144-5b27-9cfa-0532321840ee_eee95138-58c8-4172-9b1f-754ba074325d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_402","N/A","Ecoinvent  3.10, cut-off by allocation version","f8566db2-34aa-52fc-8b62-b94bbeb5cfff_fbb039f7-f9cc-46d2-b631-313ddb125c1a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Copper"]
[null,"OSW_SE_403","N/A","Ecoinvent  3.10, cut-off by allocation version","58bc6741-6d78-5d59-b143-166b6e7f452d_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Copper"]
[null,"OSW_SE_404","N/A","Ecoinvent  3.10, cut-off by allocation version","ad21b0ab-468b-5685-b30e-750027985868_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Copper"]
[null,"OSW_SE_405","N/A","Ecoinvent  3.10, cut-off by allocation version","ecf8173e-692c-5c30-8bd3-f6eb005e72b7_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Copper"]
[null,"OSW_SE_406","N/A","Ecoinvent  3.10, cut-off by allocation version","dbb7dbf7-9d69-5a0e-b5ad-4e0f9b61154e_ea75b944-c676-4a13-85b8-2bea98f765a4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Oils and lubricants"]
[null,"OSW_SE_407","N/A","Ecoinvent  3.10, cut-off by allocation version","c17266f3-3f87-5ed7-ad2b-410db3d5ed1c_ea75b944-c676-4a13-85b8-2bea98f765a4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Oils and lubricants"]
[null,"OSW_SE_408","N/A","Ecoinvent  3.10, cut-off by allocation version","46b016c1-ff92-580f-93ee-562fc9b536f4_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_409","N/A","Ecoinvent  3.10, cut-off by allocation version","65839b8f-704e-57f2-a5eb-b9d982aab4f6_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_410","N/A","Ecoinvent  3.10, cut-off by allocation version","28e3e418-2bf5-58a9-a652-62cef90dced0_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_411","N/A","Ecoinvent  3.10, cut-off by allocation version","010faf91-efb8-5ecf-9e2c-1c20e866c179_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_412","N/A","Ecoinvent  3.10, cut-off by allocation version","fdb6a609-1928-55b4-b500-e433b8eaca01_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_413","N/A","Ecoinvent  3.10, cut-off by allocation version","c8ac0a8d-bc59-50ad-9e5e-e400d16040a4_237b35c6-69e1-49c4-8e99-0be6c1b1806e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_414","N/A","Ecoinvent  3.10, cut-off by allocation version","12a91e30-b1e5-501b-bf31-17e6ffc49ac6_71d0cff1-7f13-4476-94a9-4eaaec98d225",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_415","N/A","Ecoinvent  3.10, cut-off by allocation version","b8a94ec9-0189-5acc-b565-c7ae3e1f0f82_55cd1ee7-9869-4248-8800-1be2f66267aa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_416","N/A","Ecoinvent  3.10, cut-off by allocation version","87280257-a49a-500b-8b78-ef80cf493f4b_a95b9d49-4114-40c6-9929-0c6c79db22d1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_417","N/A","Ecoinvent  3.10, cut-off by allocation version","e7eb6c4f-f145-5417-9332-03c0300d774d_8be1b6bc-2fc3-5489-91dc-5861064039c6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_418","N/A","Ecoinvent  3.10, cut-off by allocation version","b87db45b-f2cc-5666-8024-0396e729420e_8be1b6bc-2fc3-5489-91dc-5861064039c6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_419","N/A","Ecoinvent  3.10, cut-off by allocation version","9b0f80c5-2042-5223-a7a6-81c33c25576a_d1c50e71-41bf-40ea-a259-0fc490c8e0c5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_420","N/A","Ecoinvent  3.10, cut-off by allocation version","a6acbf9f-8fe2-57bf-8fe2-641091c778cb_23fccced-e1e5-421d-9abe-5b59c51a862e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_421","N/A","Ecoinvent  3.10, cut-off by allocation version","238d13e8-d030-5a86-a33c-a72ed008ffa4_475e90d0-9d93-4baa-b5ac-c30966c74554",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_422","N/A","Ecoinvent  3.10, cut-off by allocation version","a1e2e13c-709c-5193-a0ae-7d254b5ff6a5_7fbe7184-9e9e-4a21-bd42-fa630266af1d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_423","N/A","Ecoinvent  3.10, cut-off by allocation version","f90ee562-ca1b-538e-b036-9d424d63f9ce_ab5dcfa8-e8f9-4923-84d4-51b25a898fa1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_424","N/A","Ecoinvent  3.10, cut-off by allocation version","841fac9a-07f7-5971-8850-db808d37ca79_ab5dcfa8-e8f9-4923-84d4-51b25a898fa1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_425","N/A","Ecoinvent  3.10, cut-off by allocation version","6bc62aa5-2761-5f69-8601-321a0f214789_a8f9b840-05ff-4dad-b11e-dd4b1342655d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_426","N/A","Ecoinvent  3.10, cut-off by allocation version","c0d35bc8-0bcc-5f87-82d1-4cd4255afc44_a8f9b840-05ff-4dad-b11e-dd4b1342655d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_427","N/A","Ecoinvent  3.10, cut-off by allocation version","6f3ee6e4-8734-5b2d-8648-603c46d2f48b_136f89b3-af52-4826-97f7-cc35f80f226f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_428","N/A","Ecoinvent  3.10, cut-off by allocation version","cb8e0506-9969-50a7-898e-8499d8475f84_0da5307e-df93-4bc2-b5bc-6cda3cb55e8c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_429","N/A","Ecoinvent  3.10, cut-off by allocation version","127e7bd3-8201-5e27-93dc-4a114e95717a_77ad34b3-7b53-412e-afbb-0536fb8d5c6a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_430","N/A","Ecoinvent  3.10, cut-off by allocation version","aa8c356a-ea38-54eb-ae06-c545162c5878_d2aea801-6631-4070-939b-7b6d6b73bee5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_431","N/A","Ecoinvent  3.10, cut-off by allocation version","872c4aa2-3aa5-5bf5-96ac-1771913ee4e5_b685192a-e033-421e-9074-8fe7cb176046",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_432","N/A","Ecoinvent  3.10, cut-off by allocation version","3165ffe2-7818-5bad-8259-cbc2733e7e54_947a85fa-114e-4d9e-b36c-3293e48ea5ae",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_433","N/A","Ecoinvent  3.10, cut-off by allocation version","b2f45e60-786c-5d39-a2ad-0c1c0aab6996_51c7e57a-00b7-4412-b56c-94c17b211ee7",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_434","N/A","Ecoinvent  3.10, cut-off by allocation version","ea39941b-639c-5c1a-ae80-ef0186a646c1_51c7e57a-00b7-4412-b56c-94c17b211ee7",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_435","N/A","Ecoinvent  3.10, cut-off by allocation version","4b0071c5-fc6d-5d56-9c17-da4c109ebe3e_102d2161-b570-42cd-b646-1c44e47d23c5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_436","N/A","Ecoinvent  3.10, cut-off by allocation version","ba14254b-6e7e-5786-aed1-73d5b4eece87_0798a5d1-6713-4c82-8ec9-c40ac2548279",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_437","N/A","Ecoinvent  3.10, cut-off by allocation version","7bdb6eec-ac75-503d-a68e-631d0c0857aa_f891d553-f8e5-4990-a56f-d032d9ec87f0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_438","N/A","Ecoinvent  3.10, cut-off by allocation version","e394b797-b3b8-5e9c-8a42-ebb2254156b7_f891d553-f8e5-4990-a56f-d032d9ec87f0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_439","N/A","Ecoinvent  3.10, cut-off by allocation version","90fee2a4-3631-51af-b81e-87a21a860ae6_fb4bb128-084e-4da3-8227-2ef8ad95da13",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_440","N/A","Ecoinvent  3.10, cut-off by allocation version","3e8c45cf-7645-531f-bbf9-da014e5d7324_fb4bb128-084e-4da3-8227-2ef8ad95da13",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_441","N/A","Ecoinvent  3.10, cut-off by allocation version","68720841-0b02-5bf0-82cd-d8c27385a316_d2aea801-6631-4070-939b-7b6d6b73bee5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_442","N/A","Ecoinvent  3.10, cut-off by allocation version","109a925c-18ef-57c3-bc0a-c8487f69b169_d16b5d3f-b5e4-45b6-9a04-23cde05220c0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_443","N/A","Ecoinvent  3.10, cut-off by allocation version","1489f27b-e471-59b4-9bd2-d1ec6b6680e0_d16b5d3f-b5e4-45b6-9a04-23cde05220c0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_444","N/A","Ecoinvent  3.10, cut-off by allocation version","8306ad5f-8079-5e87-aca6-edfdf0a9b7b6_6af79823-cba0-4b75-96eb-e7c161eed14e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_445","N/A","Ecoinvent  3.10, cut-off by allocation version","d97c9825-79d0-5013-a015-eecd61881f72_6af79823-cba0-4b75-96eb-e7c161eed14e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_446","N/A","Ecoinvent  3.10, cut-off by allocation version","16470154-dafe-59a0-9d4f-e31ec70fdac4_b167bcef-715e-4136-a743-2fae79a086d3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_447","N/A","Ecoinvent  3.10, cut-off by allocation version","e9a7f967-42c0-5621-ba80-8cdb0a11353a_b167bcef-715e-4136-a743-2fae79a086d3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_448","N/A","Ecoinvent  3.10, cut-off by allocation version","9874d54a-4279-53e9-bac1-2d6f9ba0d26f_6826a703-2476-42f3-bb7c-4f32594ab030",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_449","N/A","Ecoinvent  3.10, cut-off by allocation version","50dd7c19-06f3-584b-a483-84d0afcaea1a_6826a703-2476-42f3-bb7c-4f32594ab030",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_450","N/A","Ecoinvent  3.10, cut-off by allocation version","5e47916e-26cb-51fb-951f-2562a9f57009_e0d6f217-d1e3-4d5d-8b8a-b13c846d4ad6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_451","N/A","Ecoinvent  3.10, cut-off by allocation version","2faaa3fa-adb2-5438-9700-252557481563_e0d6f217-d1e3-4d5d-8b8a-b13c846d4ad6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_452","N/A","Ecoinvent  3.10, cut-off by allocation version","5e783490-2ff3-59a0-bbbc-b07693e18a4b_66ca2f38-5e51-4546-83c0-d7cef0c55c7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_453","N/A","Ecoinvent  3.10, cut-off by allocation version","40e32cec-0e36-5282-a540-9dc9fb4a7015_c33b5236-001e-49b5-aa3d-810c0214f9ce",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_454","N/A","Ecoinvent  3.10, cut-off by allocation version","1873afb0-8b20-580a-947e-63428cd2e791_c5246dbb-0abd-4bee-8dda-d52a1b202322",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_455","N/A","Ecoinvent  3.10, cut-off by allocation version","42eeb16c-7cb5-5cf4-9cba-1f537548f1af_817c3650-4fed-4ef2-b9b6-404a198834e6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_456","N/A","Ecoinvent  3.10, cut-off by allocation version","b72ee1aa-fc2e-51f8-9727-3ff33bdcea30_8cb650d5-8a48-4719-81b1-2080b3b4387f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_457","N/A","Ecoinvent  3.10, cut-off by allocation version","f3237d3d-1189-527c-a8b5-1b539c4ae4ef_a2fd8c95-f2db-436a-9f24-f33b17f7975b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_458","N/A","Ecoinvent  3.10, cut-off by allocation version","42de1cab-a735-530b-b4da-bc7eb1dbcc05_9ba48284-0f03-4fec-800d-de77833b12f6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_459","N/A","Ecoinvent  3.10, cut-off by allocation version","22decb26-3e6b-57a8-a27c-63edaf7fb880_4447af36-0897-4b00-8fd0-fd6a446dda6a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_460","N/A","Ecoinvent  3.10, cut-off by allocation version","7d8bfc44-ded8-5f97-b548-d3423b7f9ba9_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_461","N/A","Ecoinvent  3.10, cut-off by allocation version","2af26239-73ec-59ff-9821-1f4b86764c4e_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_462","N/A","Ecoinvent  3.10, cut-off by allocation version","8fc39dbb-3585-54e0-960e-35ca31de018a_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_463","N/A","Ecoinvent  3.10, cut-off by allocation version","29a5e34d-859e-5eb2-a295-2cb0f98877fd_3da25df2-438a-4e27-9141-4393f3b6f86f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_464","N/A","Ecoinvent  3.10, cut-off by allocation version","4febbf1f-bfd7-5868-9111-49708facb47f_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_465","N/A","Ecoinvent  3.10, cut-off by allocation version","cbed0288-184f-53df-84d4-c64c970f2fb7_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_466","N/A","Ecoinvent  3.10, cut-off by allocation version","cc57a51b-bf5a-53bb-9c7e-2b1d50f03f89_50306184-2a7e-4825-8e5d-fe8e674d1274",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_467","N/A","Ecoinvent  3.10, cut-off by allocation version","1f7b0c60-3b3a-5479-961c-fac0a5de20f5_50306184-2a7e-4825-8e5d-fe8e674d1274",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_468","N/A","Ecoinvent  3.10, cut-off by allocation version","60bc5c0f-653c-552b-8488-4f454cd31192_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_469","N/A","Ecoinvent  3.10, cut-off by allocation version","48e8b526-1176-5973-8caa-13e4c254793d_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_470","N/A","Ecoinvent  3.10, cut-off by allocation version","65790e01-0a67-514d-8a66-929bc0169fac_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_471","N/A","Ecoinvent  3.10, cut-off by allocation version","2b727e27-bfcb-5560-aab9-873ad69bcd73_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_472","N/A","Ecoinvent  3.10, cut-off by allocation version","0f8129e4-4840-513f-b53f-6a24089cbcd4_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_473","N/A","Ecoinvent  3.10, cut-off by allocation version","b277fbaf-6fed-59f1-9727-9f392ed9fa3d_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_474","N/A","Ecoinvent  3.10, cut-off by allocation version","0b8566a3-0d91-5e12-b71d-e3cc5ec4bc86_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_475","N/A","Ecoinvent  3.10, cut-off by allocation version","77bad89e-55c3-598b-89aa-dc7e9da86187_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_476","N/A","Ecoinvent  3.10, cut-off by allocation version","cfd17d33-ea32-59d0-a2f1-3f447e17c581_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_477","N/A","Ecoinvent  3.10, cut-off by allocation version","6617fee5-6572-5a93-9dc0-c0cb33e80ff2_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_478","N/A","Ecoinvent  3.10, cut-off by allocation version","c55c370c-7f1e-5077-889f-9f2c8863e285_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_479","N/A","Ecoinvent  3.10, cut-off by allocation version","b7a331c9-a2f1-5c1e-a685-7cee01b3cf69_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_480","N/A","Ecoinvent  3.10, cut-off by allocation version","28dfb649-5d63-5f8f-bf68-695772c18b82_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_481","N/A","Ecoinvent  3.10, cut-off by allocation version","6278c4cc-d909-5d0d-81c0-702ddc787d7f_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_482","N/A","Ecoinvent  3.10, cut-off by allocation version","063a18cf-2f17-5ba9-a1a3-15258dd85e47_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_483","N/A","Ecoinvent  3.10, cut-off by allocation version","103f42a6-58ba-586e-bd05-faf51396d873_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_484","N/A","Ecoinvent  3.10, cut-off by allocation version","fdce3b26-41dc-5819-ba07-c8b3f36b85fd_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_485","N/A","Ecoinvent  3.10, cut-off by allocation version","8b58a76a-e1d3-503e-a0de-35363c62bb38_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_486","N/A","Ecoinvent  3.10, cut-off by allocation version","7b5d5816-d30f-5049-9bb6-e81475155fcd_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_487","N/A","Ecoinvent  3.10, cut-off by allocation version","e5a5ad67-b5e9-57d3-95e5-f5d3ac3c6cd4_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_488","N/A","Ecoinvent  3.10, cut-off by allocation version","3511cbc7-9d84-5471-ad2d-dbefc862bbd3_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_489","N/A","Ecoinvent  3.10, cut-off by allocation version","9b874034-97f2-585a-8439-918eaf22b64f_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_490","N/A","Ecoinvent  3.10, cut-off by allocation version","77859587-bd7e-5112-a696-d9478c7667c3_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_491","N/A","Ecoinvent  3.10, cut-off by allocation version","72020167-a4de-537d-ab11-ec8ffd0e76c1_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_492","N/A","Ecoinvent  3.10, cut-off by allocation version","3024a276-42f5-59ae-a12d-fefee65e7c67_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_493","N/A","Ecoinvent  3.10, cut-off by allocation version","1386bf8f-7041-556c-a461-7ec1a9d07667_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_494","N/A","Ecoinvent  3.10, cut-off by allocation version","bc5124b5-80d4-5301-8091-49c4a9261a4d_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_495","N/A","Ecoinvent  3.10, cut-off by allocation version","e4afe892-c850-53be-a44a-9bf25eddf110_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_496","N/A","Ecoinvent  3.10, cut-off by allocation version","d20c579c-6e37-5c21-9201-39048a8222fb_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_497","N/A","Ecoinvent  3.10, cut-off by allocation version","ea9c0bd5-bd2c-5c0d-a643-28afeec6df10_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_498","N/A","Ecoinvent  3.10, cut-off by allocation version","b240d229-4331-514d-9237-f9af6fdfe3d8_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_499","N/A","Ecoinvent  3.10, cut-off by allocation version","f5b51cc5-f045-5d11-8ec2-456d5e4a6a36_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_500","N/A","Ecoinvent  3.10, cut-off by allocation version","2482bd47-8bae-5e00-a301-0eec09e93a57_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_501","N/A","Ecoinvent  3.10, cut-off by allocation version","9e403c61-2ef8-527d-9534-feb2de7f993a_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_502","N/A","Ecoinvent  3.10, cut-off by allocation version","86e28ed3-337b-5032-8d64-486fec7ff0f3_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_503","N/A","Ecoinvent  3.10, cut-off by allocation version","331f0c47-b561-526c-bc1a-be1caa864b38_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_504","N/A","Ecoinvent  3.10, cut-off by allocation version","13dfa6fe-be1d-5c36-9a74-a12d19bd166d_b7667b06-c667-481c-8718-bfbdfcd20d94",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_505","N/A","Ecoinvent  3.10, cut-off by allocation version","0e9bda8b-6bb8-55a2-9cb5-95fa8afc7a00_b7667b06-c667-481c-8718-bfbdfcd20d94",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_506","N/A","Ecoinvent  3.10, cut-off by allocation version","b5bb560e-fc33-56b1-8cb3-8124d8f6818d_d0125769-1059-41bb-8313-f4ef1cc1bd14",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_507","N/A","Ecoinvent  3.10, cut-off by allocation version","d514a5f9-ba78-5ce8-a6c4-c4bada59ff9b_d0125769-1059-41bb-8313-f4ef1cc1bd14",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_508","N/A","Ecoinvent  3.10, cut-off by allocation version","9b93855b-c3b1-57ac-ace2-96f086724628_d0125769-1059-41bb-8313-f4ef1cc1bd14",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_509","N/A","Ecoinvent  3.10, cut-off by allocation version","98c2609b-bf50-53ce-9a4b-5eb5877bd899_b28cfd95-443c-4abd-887d-8aec49e2b764",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_510","N/A","Ecoinvent  3.10, cut-off by allocation version","ecac82e4-4134-5e6e-b37c-29a6a8a0a87e_b28cfd95-443c-4abd-887d-8aec49e2b764",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_511","N/A","Ecoinvent  3.10, cut-off by allocation version","083a950a-a5e8-5888-a579-fd0db9768058_580b6c42-5004-49a0-b474-27dc65e0d47b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_512","N/A","Ecoinvent  3.10, cut-off by allocation version","2036f769-f714-5f9c-824a-ddecf243871f_580b6c42-5004-49a0-b474-27dc65e0d47b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_513","N/A","Ecoinvent  3.10, cut-off by allocation version","353bdd50-3cde-56c2-981f-de0ca15d192d_c2e3161e-4f3c-4f32-a3bb-4459d50b430a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_514","N/A","Ecoinvent  3.10, cut-off by allocation version","0fce7403-5366-5169-a405-a8395c11c7d6_c2e3161e-4f3c-4f32-a3bb-4459d50b430a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_515","N/A","Ecoinvent  3.10, cut-off by allocation version","6f38c539-07be-5bc8-a99a-7526da07d377_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_516","N/A","Ecoinvent  3.10, cut-off by allocation version","f2c2fe4e-caff-5bfb-aeaa-a206ac1a60cf_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_517","N/A","Ecoinvent  3.10, cut-off by allocation version","ec1dceda-86aa-5f48-97b2-6052d44fd8a5_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_518","N/A","Ecoinvent  3.10, cut-off by allocation version","717d603b-893c-5481-a67e-d0e39d208239_9090888c-6089-4d65-9317-7695e029e25f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_519","N/A","Ecoinvent  3.10, cut-off by allocation version","14d47dfc-7097-5e42-b686-24cbb33e9d7e_9090888c-6089-4d65-9317-7695e029e25f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_520","N/A","Ecoinvent  3.10, cut-off by allocation version","f9eb1b96-c895-5cb2-bef8-a48bde7c3d6e_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_521","N/A","Ecoinvent  3.10, cut-off by allocation version","f48039fb-26fe-5d8a-bd6c-6c3ffdfa5ca9_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_522","N/A","Ecoinvent  3.10, cut-off by allocation version","7aa825d2-bd38-5a01-92c7-a50c03fd0060_d51e5a32-c20a-4da6-8d58-31f344b50c00",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_523","N/A","Ecoinvent  3.10, cut-off by allocation version","3bdaa769-5f20-5be7-89c3-ac30583c7a2c_d51e5a32-c20a-4da6-8d58-31f344b50c00",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_524","N/A","Ecoinvent  3.10, cut-off by allocation version","331c3985-e999-5b8c-ba46-9939cc83a79c_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_525","N/A","Ecoinvent  3.10, cut-off by allocation version","90710843-6406-5807-bd83-c6e0a10e04d2_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_526","N/A","Ecoinvent  3.10, cut-off by allocation version","36d35b21-da69-562d-83ce-4ee715e6d890_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_527","N/A","Ecoinvent  3.10, cut-off by allocation version","6fdeeada-48c4-55f3-8426-08cd1a0720bd_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_528","N/A","Ecoinvent  3.10, cut-off by allocation version","c2ed2a6f-4557-5b2f-8de6-2c5d5c3fac01_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_529","N/A","Ecoinvent  3.10, cut-off by allocation version","8b80cedb-462a-5916-bed7-6f490b08e8f3_80761dd3-0a68-4821-aa1c-088faeac8386",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_530","N/A","Ecoinvent  3.10, cut-off by allocation version","805dd5e5-4515-5c6f-927c-8636c3b8671c_80761dd3-0a68-4821-aa1c-088faeac8386",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_531","N/A","Ecoinvent  3.10, cut-off by allocation version","4062a9ca-0059-56b0-bd5f-13965f89199e_db3559ad-a065-425f-9d03-551068d5548e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_532","N/A","Ecoinvent  3.10, cut-off by allocation version","d5cb5f84-d241-5289-b5f1-dd5049f36cab_db3559ad-a065-425f-9d03-551068d5548e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_533","N/A","Ecoinvent  3.10, cut-off by allocation version","771b2b9d-f985-5004-b20f-313259aab523_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_534","N/A","Ecoinvent  3.10, cut-off by allocation version","4f728108-ef18-5a00-b206-7460665c074d_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_535","N/A","Ecoinvent  3.10, cut-off by allocation version","400cb029-6e10-5e9d-832b-b25bffc1fe68_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_536","N/A","Ecoinvent  3.10, cut-off by allocation version","c4dd0d51-e6e5-5e1d-b416-98f354484dd6_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_537","N/A","Ecoinvent  3.10, cut-off by allocation version","875a1016-e31c-5e21-97bc-90c5b74b48e8_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_538","N/A","Ecoinvent  3.10, cut-off by allocation version","9bc1d45d-f598-51d9-b9ea-bc32719b7720_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_539","N/A","Ecoinvent  3.10, cut-off by allocation version","102b15f6-f788-5019-9b16-24f55b6fc5b5_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_540","N/A","Ecoinvent  3.10, cut-off by allocation version","3b8b16ae-91a5-547d-baa0-ec6ab44ab5a8_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_541","N/A","Ecoinvent  3.10, cut-off by allocation version","048e0209-8804-5ca1-9832-8284b254d3f2_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_542","N/A","Ecoinvent  3.10, cut-off by allocation version","56047049-8a95-5c5f-9687-f628c6f45467_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_543","N/A","Ecoinvent  3.10, cut-off by allocation version","7fe4c4c7-91e4-5f21-b2f8-c25eaee5e3a1_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_544","N/A","Ecoinvent  3.10, cut-off by allocation version","943b263d-92b3-584d-9a3b-16b8fab1686d_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_545","N/A","Ecoinvent  3.10, cut-off by allocation version","a09150c3-22b4-5032-9694-82401fe65d66_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_546","N/A","Ecoinvent  3.10, cut-off by allocation version","23cc6b1d-c3f7-50b7-8678-ca2964db64b7_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_547","N/A","Ecoinvent  3.10, cut-off by allocation version","42fd398a-05b7-5727-b197-c844f207c143_b6abeedb-cebf-4b0d-943a-2980192bfc07",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_548","N/A","Ecoinvent  3.10, cut-off by allocation version","46a1caee-31fb-5573-bf83-f1612b16ae98_b6abeedb-cebf-4b0d-943a-2980192bfc07",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_549","N/A","Ecoinvent  3.10, cut-off by allocation version","95d4646e-6f37-5764-a73e-92fb3ab5fe34_7513d2f5-d7ee-497b-971b-a5ad34ab5c83",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_550","N/A","Ecoinvent  3.10, cut-off by allocation version","ad8c1de4-97d0-59e6-bb91-1d583d0b3f96_7513d2f5-d7ee-497b-971b-a5ad34ab5c83",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_551","N/A","Ecoinvent  3.10, cut-off by allocation version","7b353053-d8c7-5bde-ad5c-49fc7efbd6ed_7513d2f5-d7ee-497b-971b-a5ad34ab5c83",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_552","N/A","Ecoinvent  3.10, cut-off by allocation version","4481c64f-c092-5db8-8fd1-3e9057360f4a_171e53d3-3f3a-45a1-99f6-fad22caf1cd6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_553","N/A","Ecoinvent  3.10, cut-off by allocation version","0d7ce2a5-da4e-585f-b965-e68f89fb8dac_171e53d3-3f3a-45a1-99f6-fad22caf1cd6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_554","N/A","Ecoinvent  3.10, cut-off by allocation version","8d870d1f-ab11-5a5b-9c04-27a28688c01e_aa78f007-28b9-473d-af21-fe233c21f7d3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_555","N/A","Ecoinvent  3.10, cut-off by allocation version","752400a7-9e94-5a83-b1c6-8100a0cd5c19_aa78f007-28b9-473d-af21-fe233c21f7d3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_556","N/A","Ecoinvent  3.10, cut-off by allocation version","cb280103-a085-5d9c-8fc0-77b59774361c_11b71553-cc51-438e-8cb5-0337836737ae",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_557","N/A","Ecoinvent  3.10, cut-off by allocation version","85ddd581-cd8c-5238-9a3f-807d4b56b871_11b71553-cc51-438e-8cb5-0337836737ae",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_558","N/A","Ecoinvent  3.10, cut-off by allocation version","6e3106f8-7418-55b0-93eb-8a6bd4c389b4_9ccedb7d-205a-4729-90aa-17809aa1f511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_559","N/A","Ecoinvent  3.10, cut-off by allocation version","62dec963-b6bb-5a64-a1db-ac31cab60ee3_9ccedb7d-205a-4729-90aa-17809aa1f511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_560","N/A","Ecoinvent  3.10, cut-off by allocation version","f47411b1-eb72-59af-b66c-de3ef7b98143_5fb6a985-faa0-44cc-b183-f0b549833357",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_561","N/A","Ecoinvent  3.10, cut-off by allocation version","efb68dc4-32a5-5b96-bfb2-6cc7567e581f_5fb6a985-faa0-44cc-b183-f0b549833357",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_562","N/A","Ecoinvent  3.10, cut-off by allocation version","ee133340-f5ad-532f-a0a3-63dd7592010e_7ef961a9-b8c2-425f-8b79-9ad184c86c00",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_563","N/A","Ecoinvent  3.10, cut-off by allocation version","a1b26b8b-4135-53be-a72d-776a377a7f0e_7ef961a9-b8c2-425f-8b79-9ad184c86c00",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_564","N/A","Ecoinvent  3.10, cut-off by allocation version","0a708089-d92a-53b3-9c26-ab1334a624dd_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_565","N/A","Ecoinvent  3.10, cut-off by allocation version","5ed2b92d-e34b-54c1-b65c-ca806824d07a_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_566","N/A","Ecoinvent  3.10, cut-off by allocation version","8591bc73-5739-51b8-82ea-719125195cb2_a7abd72a-4d9c-4f99-abfc-3de79d425a96",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_567","N/A","Ecoinvent  3.10, cut-off by allocation version","73501e63-dd94-52f5-a349-5ee55ddf5a2b_a7abd72a-4d9c-4f99-abfc-3de79d425a96",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_568","N/A","Ecoinvent  3.10, cut-off by allocation version","59e5c64e-638f-5739-9ccf-944987c39aa1_a7abd72a-4d9c-4f99-abfc-3de79d425a96",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_569","N/A","Ecoinvent  3.10, cut-off by allocation version","34e2b77a-7207-5f62-98bf-5b5ca75c2af7_240c1a3c-1aba-4528-afc3-3f27f56583be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_570","N/A","Ecoinvent  3.10, cut-off by allocation version","b471c925-cc2f-5b7f-b1c1-cb56c0edff13_240c1a3c-1aba-4528-afc3-3f27f56583be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_571","N/A","Ecoinvent  3.10, cut-off by allocation version","46bb4963-1aff-55c1-b9d3-3a2a05791438_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_572","N/A","Ecoinvent  3.10, cut-off by allocation version","56d4476d-e4d5-50c5-9e15-67a5d98c4a11_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_573","N/A","Ecoinvent  3.10, cut-off by allocation version","5ae48163-32be-5510-a709-006bd09d096b_3a91cb7d-843b-495d-9973-33ba5efee877",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_574","N/A","Ecoinvent  3.10, cut-off by allocation version","f246e4f5-9501-5521-8601-3f752da59480_3a91cb7d-843b-495d-9973-33ba5efee877",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_575","N/A","Ecoinvent  3.10, cut-off by allocation version","ae05a346-96bc-5cae-bd16-17e1721b4a2b_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_576","N/A","Ecoinvent  3.10, cut-off by allocation version","071d52ef-12c5-57e4-9b13-918a3141ac87_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_577","N/A","Ecoinvent  3.10, cut-off by allocation version","e9502c59-061a-55b7-b841-2fca78477a55_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_578","N/A","Ecoinvent  3.10, cut-off by allocation version","1e20ad36-8b8c-5828-90ef-c648fefb25ab_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_579","N/A","Ecoinvent  3.10, cut-off by allocation version","6b69de33-8f3c-5483-bfe0-a67c3cb2a004_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_580","N/A","Ecoinvent  3.10, cut-off by allocation version","9040f7ae-34b8-5aa1-9051-994d48073738_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_581","N/A","Ecoinvent  3.10, cut-off by allocation version","6fa37465-d31d-5dba-94a9-423c81751eb6_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_582","N/A","Ecoinvent  3.10, cut-off by allocation version","4b625f6b-f869-51b4-9b1e-97dfc63b39da_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_583","N/A","Ecoinvent  3.10, cut-off by allocation version","8b636500-5512-5f5a-8a68-e5d8baf9d876_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_584","N/A","Ecoinvent  3.10, cut-off by allocation version","6b67e8b2-ab23-5bfe-9489-d11589caf3bb_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_585","N/A","Ecoinvent  3.10, cut-off by allocation version","12bf0ada-8a6f-5df1-9a6a-d533fdf23ee4_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_586","N/A","Ecoinvent  3.10, cut-off by allocation version","ef99265a-753d-579d-a3db-5415d851d04b_7df87cd6-22cd-4010-ab95-b1a02917bbfe",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_587","N/A","Ecoinvent  3.10, cut-off by allocation version","668786c6-a0f3-57fa-9d81-64ac449d766f_7df87cd6-22cd-4010-ab95-b1a02917bbfe",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_588","N/A","Ecoinvent  3.10, cut-off by allocation version","77e4a728-d495-5edf-a2dd-3a3d97e97167_22e27360-4621-4591-8412-a4f2045ac1a0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_589","N/A","Ecoinvent  3.10, cut-off by allocation version","ce6fd926-f7ad-5332-b31a-05462495483a_22e27360-4621-4591-8412-a4f2045ac1a0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_590","N/A","Ecoinvent  3.10, cut-off by allocation version","d73f6f02-9176-5bce-aab6-13d01a5fae4c_d3fe6705-5f5c-4961-b14d-0f9dd0e90e34",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_591","N/A","Ecoinvent  3.10, cut-off by allocation version","d5a0305a-274b-59b9-97b9-712e8f755172_d3fe6705-5f5c-4961-b14d-0f9dd0e90e34",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_592","N/A","Ecoinvent  3.10, cut-off by allocation version","703544c9-2d32-5b4b-9a1a-c50e4c823d3d_d3fe6705-5f5c-4961-b14d-0f9dd0e90e34",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_593","N/A","Ecoinvent  3.10, cut-off by allocation version","39e5dd99-3d50-519a-9bc4-7132cbec9af0_7f6bb533-2d3c-43a6-ac60-6eef299d7c52",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_594","N/A","Ecoinvent  3.10, cut-off by allocation version","b838b2a9-a327-59de-96de-7419e943378b_7f6bb533-2d3c-43a6-ac60-6eef299d7c52",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_595","N/A","Ecoinvent  3.10, cut-off by allocation version","26f97507-24ae-5ca4-b83f-fed9bfb27234_7f6bb533-2d3c-43a6-ac60-6eef299d7c52",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_596","N/A","Ecoinvent  3.10, cut-off by allocation version","3034047a-ab5e-523f-82b8-bdadd4ce3a63_e9f6d312-001c-435a-a668-82239a3b7511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_597","N/A","Ecoinvent  3.10, cut-off by allocation version","1071ae53-b776-513d-b10a-b6af35c34e07_e9f6d312-001c-435a-a668-82239a3b7511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_598","N/A","Ecoinvent  3.10, cut-off by allocation version","34f1837d-d0c4-52e8-a8b1-091acde2f585_e9f6d312-001c-435a-a668-82239a3b7511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_599","N/A","Ecoinvent  3.10, cut-off by allocation version","cdbe9ad5-e843-5426-878c-870b7cd2ef1e_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_600","N/A","Ecoinvent  3.10, cut-off by allocation version","8e4fb6a0-7c6b-57d3-a2d2-7501f4b08779_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_601","N/A","Ecoinvent  3.10, cut-off by allocation version","93b802a6-416a-5620-bcc6-9007fd112b1b_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_602","N/A","Ecoinvent  3.10, cut-off by allocation version","f8031ae7-cf6c-5966-8854-c8e57aa09d90_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_603","N/A","Ecoinvent  3.10, cut-off by allocation version","119278e3-228c-5abd-b6f4-544b0cd492ce_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_604","N/A","Ecoinvent  3.10, cut-off by allocation version","f9659364-8048-515c-8463-4f81f8e9d02c_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_605","N/A","Ecoinvent  3.10, cut-off by allocation version","cf756897-6af0-5718-ac4f-7473ed707602_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_606","N/A","Ecoinvent  3.10, cut-off by allocation version","6483793c-2d77-5fcf-8c76-532de84acd66_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_607","N/A","Ecoinvent  3.10, cut-off by allocation version","7dc42d63-01da-5c13-99c9-d66d23450772_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_608","N/A","Ecoinvent  3.10, cut-off by allocation version","d91ef8a4-8106-53d5-87ae-e30a3ac28568_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_609","N/A","Ecoinvent  3.10, cut-off by allocation version","10c1da51-1e0b-5606-a848-6a26c1f75455_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_610","N/A","Ecoinvent  3.10, cut-off by allocation version","b0d8e38e-a2e5-5c66-b877-0f36d101c6c1_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_611","N/A","Ecoinvent  3.10, cut-off by allocation version","10ab4600-daef-535f-afa6-64a2aeb64b89_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_612","N/A","Ecoinvent  3.10, cut-off by allocation version","b6478d29-95dd-53bc-b5a7-bf58806cc736_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_613","N/A","Ecoinvent  3.10, cut-off by allocation version","efd2fd19-3fa9-542f-875c-0e0b6dcf6295_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_614","N/A","Ecoinvent  3.10, cut-off by allocation version","02823727-5016-5a14-a821-5176ab9922dd_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_615","N/A","Ecoinvent  3.10, cut-off by allocation version","e880edeb-bc06-56de-9b22-396896ec350e_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_616","N/A","Ecoinvent  3.10, cut-off by allocation version","a786664b-f7fc-5402-8227-0394ab1d238e_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_617","N/A","Ecoinvent  3.10, cut-off by allocation version","bd8fd478-fc3f-587a-8c4f-9ac192cf3aa7_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_618","N/A","Ecoinvent  3.10, cut-off by allocation version","b936d081-b249-52c8-b45f-4499d00b490e_759b89bd-3aa6-42ad-b767-5bb9ef5d331d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_619","N/A","Ecoinvent  3.10, cut-off by allocation version","b936d081-b249-52c8-b45f-4499d00b490e_71e2f1db-a2c5-44d0-8337-dfff15be974d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_620","N/A","Ecoinvent  3.10, cut-off by allocation version","76cf2cb2-0204-579e-9030-b7d4c248acac_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_621","N/A","Ecoinvent  3.10, cut-off by allocation version","3f55efb4-3510-5281-a17a-96433c64134a_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_622","N/A","Ecoinvent  3.10, cut-off by allocation version","fde5d4cb-6004-501f-8428-784c4769da83_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_623","N/A","Ecoinvent  3.10, cut-off by allocation version","346f28e8-a832-5309-82a2-0cb7e970920e_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_624","N/A","Ecoinvent  3.10, cut-off by allocation version","4f134710-fa4c-57d0-8b40-2a808f5a13fe_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_625","N/A","Ecoinvent  3.10, cut-off by allocation version","197a78a5-1111-5b38-9e5f-8f459e4809f6_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_626","N/A","Ecoinvent  3.10, cut-off by allocation version","738bb629-f281-58d6-b1c6-488afe6c4a0f_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_627","N/A","Ecoinvent  3.10, cut-off by allocation version","9b821100-47d9-5424-b251-c963504382aa_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_628","N/A","Ecoinvent  3.10, cut-off by allocation version","b8793adf-9b78-58c6-b580-8609389763ad_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_629","N/A","Ecoinvent  3.10, cut-off by allocation version","f67f96ef-19a4-54f5-9c15-e0e1ef39512f_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_630","N/A","Ecoinvent  3.10, cut-off by allocation version","a6f99432-7aa4-53bd-a30f-849934877b68_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_631","N/A","Ecoinvent  3.10, cut-off by allocation version","444e455a-035b-5fc4-82d5-884e4fbb3681_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_632","N/A","Ecoinvent  3.10, cut-off by allocation version","0ad2369a-3c41-511c-bae7-8ebefad4c88d_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_633","N/A","Ecoinvent  3.10, cut-off by allocation version","76b43621-ac11-57d1-8bc7-8ac76edbc03d_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_634","N/A","Ecoinvent  3.10, cut-off by allocation version","b67a14e1-b8e0-531a-bde5-985cb8ba92f7_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_635","N/A","Ecoinvent  3.10, cut-off by allocation version","a64619db-578c-5468-84bd-29bd897ecd1d_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_636","N/A","Ecoinvent  3.10, cut-off by allocation version","6188687a-e150-5e2d-93c5-cbb9d5bd0c6d_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_637","N/A","Ecoinvent  3.10, cut-off by allocation version","32065dc5-09ff-5225-a4b0-2421056c5aa8_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_638","N/A","Ecoinvent  3.10, cut-off by allocation version","0db9c4ae-185c-50b9-8894-842d2636bda7_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_639","N/A","Ecoinvent  3.10, cut-off by allocation version","abe228a4-6b01-5f48-88c6-86a823e4829d_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_640","N/A","Ecoinvent  3.10, cut-off by allocation version","a1009b4b-d792-545b-9822-3f3b4186b165_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_641","N/A","Ecoinvent  3.10, cut-off by allocation version","411a91ca-c1fa-5b99-8092-905f1fdc0e80_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_642","N/A","Ecoinvent  3.10, cut-off by allocation version","69f85ea2-7d20-5753-b636-df7beed7db53_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_643","N/A","Ecoinvent  3.10, cut-off by allocation version","d36d4b82-c612-5393-9fdf-edbc0b1d464e_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_644","N/A","Ecoinvent  3.10, cut-off by allocation version","b6241c46-4c1a-5364-8a6b-e14de75672fc_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_645","N/A","Ecoinvent  3.10, cut-off by allocation version","69b191f5-7439-5e62-8bbd-e742a68ee2a1_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_646","N/A","Ecoinvent  3.10, cut-off by allocation version","dd1f4d8e-beff-594e-b84f-9bde4c2000fc_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_647","N/A","Ecoinvent  3.10, cut-off by allocation version","d927a87b-dd71-504b-9126-ce86890a07c2_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_648","N/A","Ecoinvent  3.10, cut-off by allocation version","64a5834f-df1a-5b90-9308-224c60d3a493_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_649","N/A","Ecoinvent  3.10, cut-off by allocation version","b80c3d97-be06-52e2-819b-444da06b8f03_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_650","N/A","Ecoinvent  3.10, cut-off by allocation version","bc41350d-f328-5464-8342-6b037bbb0027_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_651","N/A","Ecoinvent  3.10, cut-off by allocation version","4bd907e5-1e93-5b73-bcb7-7746b0ad25cf_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_652","N/A","Ecoinvent  3.10, cut-off by allocation version","440f9524-2c05-547f-b018-cb14cd887381_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_653","N/A","Ecoinvent  3.10, cut-off by allocation version","f409a032-0953-5c55-b6ce-aaf7dd4e07bc_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_654","N/A","Ecoinvent  3.10, cut-off by allocation version","ccab8588-d306-5fb1-9d58-99a22774e70c_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_655","N/A","Ecoinvent  3.10, cut-off by allocation version","d9561a2f-7645-5932-9e63-b69ce46120af_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_656","N/A","Ecoinvent  3.10, cut-off by allocation version","9124231e-9484-542c-8e65-c84a0421b65c_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_657","N/A","Ecoinvent  3.10, cut-off by allocation version","86a38984-6490-5884-9bfe-e5bf9bf5021b_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_658","N/A","Ecoinvent  3.10, cut-off by allocation version","fafcc8ba-03da-54f5-8b25-1bbdad4ffbe4_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_659","N/A","Ecoinvent  3.10, cut-off by allocation version","b272d3c1-fbd9-5a7f-95ee-ce78f6381a30_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_660","N/A","Ecoinvent  3.10, cut-off by allocation version","fb93faf4-8d93-5a8e-9225-d109e7c0c3b8_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_661","N/A","Ecoinvent  3.10, cut-off by allocation version","a211099d-cf81-5df3-9243-408ff8798c0c_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_662","N/A","Ecoinvent  3.10, cut-off by allocation version","205613c6-76db-51c8-8be3-ee531d5f05e6_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_663","N/A","Ecoinvent  3.10, cut-off by allocation version","d72a465b-79ff-585e-ace9-dd6f71df10b1_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_664","N/A","Ecoinvent  3.10, cut-off by allocation version","5254d128-7917-5937-87e3-8c4c441b0009_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_665","N/A","Ecoinvent  3.10, cut-off by allocation version","9a354579-0358-5792-88cd-1d13b1c608f6_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_666","N/A","Ecoinvent  3.10, cut-off by allocation version","ca653034-a623-5646-996e-d17dbdedfe22_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_667","N/A","Ecoinvent  3.10, cut-off by allocation version","48e8c46b-22ca-5f90-b08b-29649020cfb1_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_668","N/A","Ecoinvent  3.10, cut-off by allocation version","e86f9c7f-a45a-5991-b546-3f370fde332d_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_669","N/A","Ecoinvent  3.10, cut-off by allocation version","8c4d300c-4330-5302-bb2c-65e47ee655e3_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_670","N/A","Ecoinvent  3.10, cut-off by allocation version","296615ca-ff07-5bcd-96f4-683fa553b20c_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_671","N/A","Ecoinvent  3.10, cut-off by allocation version","e52b75a0-60ec-580b-9fa1-5a139b9f0d6d_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_672","N/A","Ecoinvent  3.10, cut-off by allocation version","e8fb465f-f4a6-5e13-afc3-8d15fd6d8804_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_673","N/A","Ecoinvent  3.10, cut-off by allocation version","345f63b7-4215-5444-a9ca-f166703f0d10_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_674","N/A","Ecoinvent  3.10, cut-off by allocation version","af4dae40-fc48-567c-bada-4a48cc72f75a_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_675","N/A","Ecoinvent  3.10, cut-off by allocation version","83008680-f1f5-5ec5-8b31-d6c90bf88f4b_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_676","N/A","Ecoinvent  3.10, cut-off by allocation version","5046b742-d327-5808-a22f-0a1839d7d481_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_677","N/A","Ecoinvent  3.10, cut-off by allocation version","9b4b0c61-7de3-5a4d-a3e8-59c0083f39b9_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_678","N/A","Ecoinvent  3.10, cut-off by allocation version","e3170900-8b44-59a6-be94-0fa96279c5f4_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_679","N/A","Ecoinvent  3.10, cut-off by allocation version","1326a00a-c4a9-550f-8cc0-20082053e07f_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_680","N/A","Ecoinvent  3.10, cut-off by allocation version","efb2f643-2e04-580d-97e4-e7d9f11b56f1_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_681","N/A","Ecoinvent  3.10, cut-off by allocation version","b234cac6-4a28-5e6a-be03-722d9106e3a6_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_682","N/A","Ecoinvent  3.10, cut-off by allocation version","1d3962b2-ccc6-5997-a930-096d68cac33e_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_683","N/A","Ecoinvent  3.10, cut-off by allocation version","222e716a-e0e5-59e4-9e39-450e83114603_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_684","N/A","Ecoinvent  3.10, cut-off by allocation version","c3fdb1d1-5b5b-566b-addb-0695c945e935_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_685","N/A","Ecoinvent  3.10, cut-off by allocation version","6265767f-83f3-5b25-8431-261de92489eb_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_686","N/A","Ecoinvent  3.10, cut-off by allocation version","35ed35a7-0ccd-504c-bfe8-bea0547bc437_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_687","N/A","Ecoinvent  3.10, cut-off by allocation version","39483239-2dbb-57b3-a040-cd2c5fe08c49_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_688","N/A","Ecoinvent  3.10, cut-off by allocation version","9397b852-28fc-54eb-8009-8248a42d309e_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_689","N/A","Ecoinvent  3.10, cut-off by allocation version","59667853-6eeb-5180-86fc-34ce0704f742_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_690","N/A","Ecoinvent  3.10, cut-off by allocation version","1ab2fc12-b156-58a2-b7fd-d950d8b72f14_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_691","N/A","Ecoinvent  3.10, cut-off by allocation version","4ffc91cd-cb9b-5d15-9f26-35f4046e8476_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_692","N/A","Ecoinvent  3.10, cut-off by allocation version","4ffc91cd-cb9b-5d15-9f26-35f4046e8476_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_693","N/A","Ecoinvent  3.10, cut-off by allocation version","4ffc91cd-cb9b-5d15-9f26-35f4046e8476_60fa2c28-1f8f-5486-aab5-da2e493250d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_694","N/A","Ecoinvent  3.10, cut-off by allocation version","4e3e256b-ebff-5d2f-9e2d-5c11f55c5754_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_695","N/A","Ecoinvent  3.10, cut-off by allocation version","4e3e256b-ebff-5d2f-9e2d-5c11f55c5754_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_696","N/A","Ecoinvent  3.10, cut-off by allocation version","4e3e256b-ebff-5d2f-9e2d-5c11f55c5754_60fa2c28-1f8f-5486-aab5-da2e493250d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_697","N/A","Ecoinvent  3.10, cut-off by allocation version","7ff71172-d0dc-52ec-9279-96b9d76dce8a_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_698","N/A","Ecoinvent  3.10, cut-off by allocation version","7ff71172-d0dc-52ec-9279-96b9d76dce8a_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_699","N/A","Ecoinvent  3.10, cut-off by allocation version","7ff71172-d0dc-52ec-9279-96b9d76dce8a_60fa2c28-1f8f-5486-aab5-da2e493250d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_700","N/A","Ecoinvent  3.10, cut-off by allocation version","c1a287e7-b2f5-59a9-9050-c0d3926ddd2d_bd4b5819-02c6-41c3-97ea-a91f14b3e0bc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_701","N/A","Ecoinvent  3.10, cut-off by allocation version","185e71dc-422a-5d66-9b09-9bf51ab066ad_bd4b5819-02c6-41c3-97ea-a91f14b3e0bc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_702","N/A","Ecoinvent  3.10, cut-off by allocation version","0a3f4352-f586-5547-bc95-1009fb4cc9ba_eb211196-8882-4baf-9113-31229f23e6aa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_703","N/A","Ecoinvent  3.10, cut-off by allocation version","36d59a17-1805-563a-9231-9bc8f4f555cb_eb211196-8882-4baf-9113-31229f23e6aa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_704","N/A","Ecoinvent  3.10, cut-off by allocation version","204e11be-4628-504f-80bb-27033b0b4c73_b2011f87-e037-4f68-8dec-6d8e6de4ae25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_705","N/A","Ecoinvent  3.10, cut-off by allocation version","bcbdf779-d61b-5ed5-b715-26efff19eb06_b2011f87-e037-4f68-8dec-6d8e6de4ae25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_706","N/A","Ecoinvent  3.10, cut-off by allocation version","4fef1ea8-3a7f-5b2c-8f6c-713c43806d51_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_707","N/A","Ecoinvent  3.10, cut-off by allocation version","5c48a01a-4ebf-54d0-8bdf-d0515bfa3049_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_708","N/A","Ecoinvent  3.10, cut-off by allocation version","d66a0e7e-5301-543d-91f8-6aff435d5759_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_709","N/A","Ecoinvent  3.10, cut-off by allocation version","67ed5154-8998-56ea-bb54-34e5a058190e_4058ca6d-92c0-4ce5-bdc9-a3a96eeade93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_710","N/A","Ecoinvent  3.10, cut-off by allocation version","6a192587-f929-5ede-8d07-cb8aeaff9c6f_4058ca6d-92c0-4ce5-bdc9-a3a96eeade93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_711","N/A","Ecoinvent  3.10, cut-off by allocation version","adfad858-4132-5cc7-87d3-7cb08fde8981_818559f3-b129-4e35-9b12-b5ab589c178a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_712","N/A","Ecoinvent  3.10, cut-off by allocation version","106fc593-24d1-5f70-84ec-e15b2fe8c8ae_818559f3-b129-4e35-9b12-b5ab589c178a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_713","N/A","Ecoinvent  3.10, cut-off by allocation version","66c9e605-cdb4-5e9f-99fc-53cf65958109_b3184435-d00c-5713-823d-5ff6741bfbbc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_714","N/A","Ecoinvent  3.10, cut-off by allocation version","f5828d5c-8f41-5653-a295-1b9d66eb95ef_b3184435-d00c-5713-823d-5ff6741bfbbc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_715","N/A","Ecoinvent  3.10, cut-off by allocation version","82f87e19-06e9-5d4f-ad66-2f8fae15a849_b3184435-d00c-5713-823d-5ff6741bfbbc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_716","N/A","Ecoinvent  3.10, cut-off by allocation version","34597a01-f156-5ba0-b5d6-0ba2bf2df2cf_b3184435-d00c-5713-823d-5ff6741bfbbc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_717","N/A","Ecoinvent  3.10, cut-off by allocation version","2b541ada-3444-5c9f-922c-b92b965aeeb1_ed25f589-c6c8-56a7-a518-b01dd3e8a453",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_718","N/A","Ecoinvent  3.10, cut-off by allocation version","6c8e7ad0-4022-5f26-a3c1-92ef1ab575c5_ed25f589-c6c8-56a7-a518-b01dd3e8a453",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_719","N/A","Ecoinvent  3.10, cut-off by allocation version","e47ba1b6-97dd-5ca9-9f6a-3f2251cbf0dd_ed25f589-c6c8-56a7-a518-b01dd3e8a453",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_720","N/A","Ecoinvent  3.10, cut-off by allocation version","961e30aa-8a68-5868-b8fe-2bd7a55675de_ed25f589-c6c8-56a7-a518-b01dd3e8a453",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_721","N/A","Ecoinvent  3.10, cut-off by allocation version","50989dbf-2baf-5c8d-b017-5a03421b2f74_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_722","N/A","Ecoinvent  3.10, cut-off by allocation version","a05e9c42-49ae-5c40-9801-d76ea9343d3d_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_723","N/A","Ecoinvent  3.10, cut-off by allocation version","e0be6f23-9f12-5c72-bd66-3dfd2eb76a8c_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_724","N/A","Ecoinvent  3.10, cut-off by allocation version","c28cc60c-fbf7-52f5-8301-252b1ce140ed_f3b9ab33-932a-4908-8e6b-5709f9bd6e0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_725","N/A","Ecoinvent  3.10, cut-off by allocation version","70aba8d6-2164-50d4-9ffc-b3fa1e5ea114_f3b9ab33-932a-4908-8e6b-5709f9bd6e0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_726","N/A","Ecoinvent  3.10, cut-off by allocation version","b265dcfc-b7ed-595e-84fc-3c8a6e19245f_9a8c2994-7cbb-4d86-a1b7-27fc0c4e49e3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_727","N/A","Ecoinvent  3.10, cut-off by allocation version","98e99ba7-aa39-5123-b7c5-630bfa552cef_9a8c2994-7cbb-4d86-a1b7-27fc0c4e49e3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_728","N/A","Ecoinvent  3.10, cut-off by allocation version","7c8d95d9-f22e-5552-a12f-8c32ea1799fa_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_729","N/A","Ecoinvent  3.10, cut-off by allocation version","8453a785-ece3-5db5-9128-9cee7b8c2e93_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_730","N/A","Ecoinvent  3.10, cut-off by allocation version","95138ef3-5c2a-5abe-976b-26f4821d20fd_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_731","N/A","Ecoinvent  3.10, cut-off by allocation version","f7d88982-8723-5f62-a473-da170b8aefd1_1c17413f-82b0-4ddb-beef-63854b1a8e1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_732","N/A","Ecoinvent  3.10, cut-off by allocation version","802900c1-a6b6-5b7b-ae71-20c92c1984dd_1c17413f-82b0-4ddb-beef-63854b1a8e1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_733","N/A","Ecoinvent  3.10, cut-off by allocation version","ab316fdf-3e2d-5657-9afc-1199de07976d_1c17413f-82b0-4ddb-beef-63854b1a8e1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_734","N/A","Ecoinvent  3.10, cut-off by allocation version","80bb9c3a-b776-5001-95f9-0c92e65c1257_3728ce01-009e-4b64-94d4-3c3e9fabf888",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_735","N/A","Ecoinvent  3.10, cut-off by allocation version","7b741193-47bd-5785-be6f-5c3abd1ea8d1_3728ce01-009e-4b64-94d4-3c3e9fabf888",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_736","N/A","Ecoinvent  3.10, cut-off by allocation version","3be54b0f-bfcc-504a-bb03-39d183658e9d_3728ce01-009e-4b64-94d4-3c3e9fabf888",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_737","N/A","Ecoinvent  3.10, cut-off by allocation version","86372858-2a46-515c-996a-c24137d726af_b2011f87-e037-4f68-8dec-6d8e6de4ae25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_738","N/A","Ecoinvent  3.10, cut-off by allocation version","8d46f893-30d7-5514-8c9a-f9c0f01b0064_b2011f87-e037-4f68-8dec-6d8e6de4ae25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_739","N/A","Ecoinvent  3.10, cut-off by allocation version","61e2b2aa-7c51-5ba1-b2e2-eb3c0ca22d4c_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_740","N/A","Ecoinvent  3.10, cut-off by allocation version","450f0376-73bb-5edf-b0ff-df2cc7f47538_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_741","N/A","Ecoinvent  3.10, cut-off by allocation version","1ff6ae54-ded8-593f-9f95-c4fcd5e64492_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_742","N/A","Ecoinvent  3.10, cut-off by allocation version","6419cc2f-f9d8-5215-9b53-a960775292c5_bc7c3720-dcba-41b4-9d96-380b55275e57",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_743","N/A","Ecoinvent  3.10, cut-off by allocation version","6ea294ed-cd88-54d2-aeea-b2a7edfb45ee_bc7c3720-dcba-41b4-9d96-380b55275e57",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_744","N/A","Ecoinvent  3.10, cut-off by allocation version","f396d9d5-6487-50f1-80ce-5c513be70321_0a6c7524-9e23-41b8-ac7b-b0489ed4681c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_745","N/A","Ecoinvent  3.10, cut-off by allocation version","dd918b0e-d736-5668-828e-c7297335097c_0a6c7524-9e23-41b8-ac7b-b0489ed4681c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_746","N/A","Ecoinvent  3.10, cut-off by allocation version","f9ff01bd-5b9d-5036-a032-d1abf5186fea_93bd3d97-0440-4e9f-8f69-6324fe28c4b6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_747","N/A","Ecoinvent  3.10, cut-off by allocation version","ccf2bcd0-c939-53f4-bda4-3c55e5213d5e_93bd3d97-0440-4e9f-8f69-6324fe28c4b6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_748","N/A","Ecoinvent  3.10, cut-off by allocation version","19a6527c-66e1-5c3b-818f-76441fb2f751_42b1c202-8308-422e-bfb7-3efe54dfcef6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_749","N/A","Ecoinvent  3.10, cut-off by allocation version","6a7d0a4c-7725-5606-9d43-b360d28123ad_42b1c202-8308-422e-bfb7-3efe54dfcef6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_750","N/A","Ecoinvent  3.10, cut-off by allocation version","47112c66-3ab9-5bea-9e66-d24c47dec7d0_42b1c202-8308-422e-bfb7-3efe54dfcef6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_751","N/A","Ecoinvent  3.10, cut-off by allocation version","4ab7e916-ebf4-52d1-9802-f8058ff3bb83_4058ca6d-92c0-4ce5-bdc9-a3a96eeade93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_752","N/A","Ecoinvent  3.10, cut-off by allocation version","b8868c2c-e7ce-563b-881c-669f76c9dc1b_4058ca6d-92c0-4ce5-bdc9-a3a96eeade93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_753","N/A","Ecoinvent  3.10, cut-off by allocation version","65d24a7f-b4f8-562e-8821-ed740d0f6f20_e88c3a19-945a-4396-a107-37e3876b2f0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_754","N/A","Ecoinvent  3.10, cut-off by allocation version","207b787b-00f6-53f7-af2b-9d666fe93d17_e88c3a19-945a-4396-a107-37e3876b2f0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_755","N/A","Ecoinvent  3.10, cut-off by allocation version","5b02d68e-19b3-56a1-be3b-930e4b72e767_bfd577e2-82b4-4166-af2b-3bda540931f6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_756","N/A","Ecoinvent  3.10, cut-off by allocation version","4e983651-673f-5cf8-bc0f-bfa5139f1b71_bfd577e2-82b4-4166-af2b-3bda540931f6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_757","N/A","Ecoinvent  3.10, cut-off by allocation version","a5ed667d-bf8f-52b4-bfdb-fa44acf90127_bfd577e2-82b4-4166-af2b-3bda540931f6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_758","N/A","Ecoinvent  3.10, cut-off by allocation version","75057433-27e9-56b1-aef0-45c0164a0546_4e758deb-57bd-45c6-96f6-9b4d25ba7a60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_759","N/A","Ecoinvent  3.10, cut-off by allocation version","7ca945d1-cebc-5019-b592-0074494f9992_4e758deb-57bd-45c6-96f6-9b4d25ba7a60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_760","N/A","Ecoinvent  3.10, cut-off by allocation version","d1933cff-f101-54cc-ac84-495b3fdf82b9_2a1db579-5d40-4d28-9b5a-c8ce7525b62d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_761","N/A","Ecoinvent  3.10, cut-off by allocation version","c1a692f8-6b85-50f0-a1d0-f51872190b3b_2a1db579-5d40-4d28-9b5a-c8ce7525b62d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_762","N/A","Ecoinvent  3.10, cut-off by allocation version","da5567af-ae9b-5011-8124-e916e0837602_0baac448-32a1-4b9f-afec-69a9b9b203ac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_763","N/A","Ecoinvent  3.10, cut-off by allocation version","bb5512e1-f8da-5b1b-b490-6ee06fc19d63_0baac448-32a1-4b9f-afec-69a9b9b203ac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_764","N/A","Ecoinvent  3.10, cut-off by allocation version","75c7eaab-e510-5a1f-81ff-d3bd09404f6e_0baac448-32a1-4b9f-afec-69a9b9b203ac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_765","N/A","Ecoinvent  3.10, cut-off by allocation version","8f77df58-fa32-5c8f-974f-9599f7695356_fd27af60-7b68-4549-bf35-022eacd74f93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_766","N/A","Ecoinvent  3.10, cut-off by allocation version","36788bb1-5454-537a-adc5-06f33d3ba9e2_fd27af60-7b68-4549-bf35-022eacd74f93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_767","N/A","Ecoinvent  3.10, cut-off by allocation version","ce19058b-3f99-54e8-bf85-2e9468748588_fd27af60-7b68-4549-bf35-022eacd74f93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_768","N/A","Ecoinvent  3.10, cut-off by allocation version","83af1209-44ae-58d3-8837-cf4a412c8889_818559f3-b129-4e35-9b12-b5ab589c178a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_769","N/A","Ecoinvent  3.10, cut-off by allocation version","56d1cea5-8bdb-5798-a367-ace2f4c020e2_818559f3-b129-4e35-9b12-b5ab589c178a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_770","N/A","Ecoinvent  3.10, cut-off by allocation version","4743fafb-0071-59d0-8231-e95a24bfb1c8_10d4f2e3-6343-4ea1-a721-86c89858e646",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_771","N/A","Ecoinvent  3.10, cut-off by allocation version","062cb1dd-7420-528b-9a80-4c892872d074_10d4f2e3-6343-4ea1-a721-86c89858e646",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_772","N/A","Ecoinvent  3.10, cut-off by allocation version","94f43c81-ecba-5fe8-8f18-393d60150656_2cb0d6c6-349c-46fc-b31f-a036c847a267",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_773","N/A","Ecoinvent  3.10, cut-off by allocation version","533c63fd-eb6f-59be-a7e2-4b9a471e381c_2cb0d6c6-349c-46fc-b31f-a036c847a267",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_774","N/A","Ecoinvent  3.10, cut-off by allocation version","e1762e44-2065-5139-8922-7089420bf115_19c15d45-57de-43b4-9772-4ef06ec9971a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_775","N/A","Ecoinvent  3.10, cut-off by allocation version","014ba1fb-1eb3-5578-8e62-e4639d41d04a_19c15d45-57de-43b4-9772-4ef06ec9971a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_776","N/A","Ecoinvent  3.10, cut-off by allocation version","39671b5a-63cf-581f-809a-98707500006d_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_777","N/A","Ecoinvent  3.10, cut-off by allocation version","745e6615-2ba9-5503-af7e-9450be3b9c6f_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_778","N/A","Ecoinvent  3.10, cut-off by allocation version","e887158d-1c78-5757-9e16-01930ed65bae_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_779","N/A","Ecoinvent  3.10, cut-off by allocation version","b8190844-9f7a-5a14-aa5b-1225639509a0_f3b9ab33-932a-4908-8e6b-5709f9bd6e0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_780","N/A","Ecoinvent  3.10, cut-off by allocation version","95afbb1d-55cd-54f7-b883-91ba8ff562a9_f3b9ab33-932a-4908-8e6b-5709f9bd6e0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_781","N/A","Ecoinvent  3.10, cut-off by allocation version","97446480-5c1e-5396-8ea5-c63947da70f3_9a8c2994-7cbb-4d86-a1b7-27fc0c4e49e3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_782","N/A","Ecoinvent  3.10, cut-off by allocation version","4a7cfad2-6f3d-5418-8234-f1642619f62b_9a8c2994-7cbb-4d86-a1b7-27fc0c4e49e3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_783","N/A","Ecoinvent  3.10, cut-off by allocation version","ea9184a1-2e8c-5f2d-b382-6a0f6d63ba49_bbae1509-eb89-42e9-81d8-70e5cae46488",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_784","N/A","Ecoinvent  3.10, cut-off by allocation version","9498aee7-192d-5796-9ec3-061b48f4e791_bbae1509-eb89-42e9-81d8-70e5cae46488",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]

{"sheet":"Proxy EF Database","index":9,"n_rows":227,"n_cols":26,"rows_kept":227,"cut":false,"hidden":false,"merged":[[18,1,18,15],[7,1,7,14],[18,16,18,25]]}
["OSW_SP_51",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Secondary: Proxy"]
[null,"SUS-JIP  |  Offshore Wind Footprinting Tool"]
[null,"SECONDARY: PROXY EF DATABASE"]
[]
[]
[null," Secondary: Proxy Emission Factor Database Guidance"]
[]
[null,"The Proxy Emission Factor Database contains a prepopulated set of proxy EFs. Proxy EFs are a subcategory of secondary EFs which typically consist of data taken from PCF or LCA assessment produced by suppliers or manufacturers (similar to Primary EFs). Proxy EFs are data to describe similar activities which are deemed to be reasonable representations of the actual activities taking place in the system boundary. For example, in the foundations, the manufacturer uses a heavy plate steel which was produced by supplier X. Supplier X does not yet produce PCF or LCA assessments for their steel, but their steel is of the same specification as that produced by Supplier Y, who has published an EPD online. Therefore, the EPD from Supplier Y may be considered to be a reasonable proxy for the Steel supplied by supplier X.\n\nProxy EFs may be found from online publications by suppliers, manufacturers and OEMs, and are typically found on online repositories of environmental data (PCF, LCA, EPD), such as:\n1. The Build Environment Carbon Database (BECD)\n2. The Embodied Carbon in Construction Calculator (EC3) \n3. EPD International\n4. Product Environmental Profile Eco passport (PEP)\n5. ICE Database\n5. Government National Inventories\n\nThe Proxy EF database has been prepopulated with a number of relevant datasets which describe activities that are relevant to OSW development, primarily sourced from the databases stated above. The Proxy EF database will continue to grow as the SUS-JIP Consortium engages their suppliers. A periodic review of the Primary Data collected by different organisations and assessors will enable Primary datasets to be transitioned into the Proxy EF database for use by other assessors.\n\nThis worksheet and table cannot be directly manipulated by the users outside of using the user controls below, which allows the user to enter a Proxy EF into the database through a user form, which will request a data from the user. A separate button is available to delete the previous row of the table in the event that the user makes a mistake in data entry.\n\nAfter adding data to this database please go to the EF library and click 'compile EF library' to make EFs available for use in the calculation sheets."]
[]
[null,"User Controls"]
[]
[]
[]
[]
[]
[null,"Data input column guidance"]
[null,"Emission Factor ID is automatically populated","For first version of a factor please enter \"V1\". If you update the study and provide a new values, please up the version number.","The name of the EF source. This may be a supplier or other entity who conducted the study and produced the data.","Native database identifier (e.g. ID in EPD database). If not available please state \"NA\".","The type of assessment that factor is derived from (PCF, LCA, EPD, OCF allocation)","A short description of the activity/process the factor represents. E.g. \"This factor represents the production of cables\"","UN classification code for the activity. If not available please state \"NA\"","Boundary of the factor, e.g. cradle-to-gate, A1-A3.","Background LCI dataset and version used for assessment, if unknown please state \"NA\" (Ecoinvent, GaBi, US EPA, etc.)","Impact methodology used for assessment (e.g. IPCC 2021, CML, EF, ReCiPi)","Impact indicator. This must be GWP100.","Reporting standard for the underlying assessment (ISO 14067, ISO 14040/44, GHGP). If unknown please state \"NA","Product Category Rules (PCR) used for the assessment. If none used please state \"NA\"","Has the assessment been verified by a 3rd party (Yes or No)","When is the assessment valid until (MM-YY), if unknown please state \"NA\" ","OSW EF Factor Category is autopopulated","OSW Activity Taxonomy L1 (please select from  the dropdown)","OSW Activity Taxonomy L2 (please select from dropdown)","Name of Emission Factor process. E.g. \"Steel production, heavy-plate, produced via BOF\"","The geographical location of the activity","The Unit of Measure for the factor (the reference unit for the assessment)","Greenhouse gas emissions for factor from fossil origin. If split is not available, leave blank.","Greenhouse gas emissions for factor from biogenic origin. If split is not available, leave blank.","Greenhouse gas emissions for factor from land use change. If split is not available, leave blank.","Total greenhouse gas emissions for the activity. If split is not available, populate the total, or net, in this column."]
[]
[null,"EMISSION FACTOR METADATA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Emissions Factor"]
[null,"Emission Factor ID","Emission Factor version number","EF source name","Native database ID (optional)","Assessment Type","Activity Description","UN CPC 2.1 Code (optional)","Emission Factor Boundary","Background Dataset Used","Impact Methodology Used","Impact Indicator","Reporting Standard used ","PCR used (optional)","Verified","Valid until","OSW EF Category","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Geography","Emissions Factor Unit","climate change: fossil (kgCO2e/unit)","climate change: biogenic (kgCO2e/unit)","climate change: land use (kgCO2e/unit)","Emissions Factor Net (kgCO2e/unit)"]
[null,"OSW_SP_1",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bio Petrol","GB","GJ",null,null,null,8.2692300000000003]
[null,"OSW_SP_2",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bio Petrol","GB","kg",null,null,null,0.36924000000000001]
[null,"OSW_SP_3",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bio Petrol","GB","litres",null,null,null,0.27392]
[null,"OSW_SP_4",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel HVO","GB","GJ",null,null,null,10.25]
[null,"OSW_SP_5",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel HVO","GB","kg",null,null,null,0.45100000000000001]
[null,"OSW_SP_6",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel HVO","GB","litres",null,null,null,0.35177999999999998]
[null,"OSW_SP_7",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME","GB","GJ",null,null,null,10.97411]
[null,"OSW_SP_8",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME","GB","kg",null,null,null,0.40823999999999999]
[null,"OSW_SP_9",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME","GB","litres",null,null,null,0.36332999999999999]
[null,"OSW_SP_10",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from tallow)","GB","GJ",null,null,null,14]
[null,"OSW_SP_11",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from tallow)","GB","kg",null,null,null,0.52080000000000004]
[null,"OSW_SP_12",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from tallow)","GB","litres",null,null,null,0.46350999999999998]
[null,"OSW_SP_13",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from used cooking oil)","GB","GJ",null,null,null,10.34563]
[null,"OSW_SP_14",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from used cooking oil)","GB","kg",null,null,null,0.38485999999999998]
[null,"OSW_SP_15",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from used cooking oil)","GB","litres",null,null,null,0.34251999999999999]
[null,"OSW_SP_16",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bioethanol","GB","GJ",null,null,null,19.542120000000001]
[null,"OSW_SP_17",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bioethanol","GB","kg",null,null,null,0.52373000000000003]
[null,"OSW_SP_18",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bioethanol","GB","litres",null,null,null,0.41583999999999999]
[null,"OSW_SP_19",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (compressed)","GB","GJ",null,null,null,11.367470000000001]
[null,"OSW_SP_20",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (compressed)","GB","kg",null,null,null,0.55701000000000001]
[null,"OSW_SP_21",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (compressed)","GB","litres"]
[null,"OSW_SP_22",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (liquified)","GB","GJ",null,null,null,11.367470000000001]
[null,"OSW_SP_23",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (liquified)","GB","kg",null,null,null,0.55701000000000001]
[null,"OSW_SP_24",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (liquified)","GB","litres"]
[null,"OSW_SP_25",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biopropane","GB","GJ",null,null,null,10.28659]
[null,"OSW_SP_26",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biopropane","GB","kg",null,null,null,0.4773]
[null,"OSW_SP_27",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biopropane","GB","litres",null,null,null,0.24578]
[null,"OSW_SP_28",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Methanol (bio)","GB","GJ",null,null,null,19.542120000000001]
[null,"OSW_SP_29",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Methanol (bio)","GB","kg",null,null,null,0.52373000000000003]
[null,"OSW_SP_30",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Methanol (bio)","GB","litres",null,null,null,0.41583999999999999]
[null,"OSW_SP_31",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Off road biodiesel","GB","GJ",null,null,null,10.97411]
[null,"OSW_SP_32",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Off road biodiesel","GB","kg",null,null,null,0.40823999999999999]
[null,"OSW_SP_33",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Off road biodiesel","GB","litres",null,null,null,0.36332999999999999]
[null,"OSW_SP_34",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Renewable petrol","GB","GJ",null,null,null,18.27807]
[null,"OSW_SP_35",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Renewable petrol","GB","kg",null,null,null,0.51283999999999996]
[null,"OSW_SP_36",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Renewable petrol","GB","litres",null,null,null,0.45724999999999999]
[null,"OSW_SP_37",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biogas","GB","kWh",null,null,null,2.8410000000000001E-2]
[null,"OSW_SP_38",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biogas","GB","tonnes",null,null,null,157.82597000000001]
[null,"OSW_SP_39",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Landfill gas","GB","kWh",null,null,null,2.0000000000000001E-4]
[null,"OSW_SP_40",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Landfill gas","GB","tonnes",null,null,null,0.68844000000000005]
[null,"OSW_SP_41",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Grass/straw","GB","kWh",null,null,null,1.6039999999999999E-2]
[null,"OSW_SP_42",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Grass/straw","GB","tonnes",null,null,null,68.650000000000006]
[null,"OSW_SP_43",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood chips","GB","kWh",null,null,null,1.0529999999999999E-2]
[null,"OSW_SP_44",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood chips","GB","tonnes",null,null,null,39.788330000000002]
[null,"OSW_SP_45",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood logs","GB","kWh",null,null,null,1.277E-2]
[null,"OSW_SP_46",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood logs","GB","tonnes",null,null,null,52.14]
[null,"OSW_SP_47",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood pellets","GB","kWh",null,null,null,3.7440000000000001E-2]
[null,"OSW_SP_48",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood pellets","GB","tonnes",null,null,null,177]
[null,"OSW_SP_49",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Butane","GB","kWh (Gross CV)",null,null,null,0.22239999999999999]
[null,"OSW_SP_50",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Butane","GB","kWh (Net CV)",null,null,null,0.24106]
[null,"OSW_SP_51",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Butane","GB","litres",null,null,null,1.74529]
[null,"OSW_SP_52",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Butane","GB","tonnes",null,null,null,3033.32]
[null,"OSW_SP_53",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","CNG","GB","kWh (Gross CV)",null,null,null,0.18253999999999998]
[null,"OSW_SP_54",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","CNG","GB","kWh (Net CV)",null,null,null,0.20227000000000001]
[null,"OSW_SP_55",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","CNG","GB","litres",null,null,null,0.44435999999999998]
[null,"OSW_SP_56",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","CNG","GB","tonnes",null,null,null,2539.25]
[null,"OSW_SP_57",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LNG","GB","kWh (Gross CV)",null,null,null,0.18396999999999999]
[null,"OSW_SP_58",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LNG","GB","kWh (Net CV)",null,null,null,0.20386000000000001]
[null,"OSW_SP_59",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LNG","GB","litres",null,null,null,1.1579999999999999]
[null,"OSW_SP_60",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LNG","GB","tonnes",null,null,null,2559.17]
[null,"OSW_SP_61",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LPG","GB","kWh (Gross CV)",null,null,null,0.21448999999999999]
[null,"OSW_SP_62",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LPG","GB","kWh (Net CV)",null,null,null,0.23030999999999999]
[null,"OSW_SP_63",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LPG","GB","litres",null,null,null,1.5570900000000001]
[null,"OSW_SP_64",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LPG","GB","tonnes",null,null,null,2939.29]
[null,"OSW_SP_65",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas","GB","cubic metres",null,null,null,2.0157400000000001]
[null,"OSW_SP_66",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas","GB","kWh (Gross CV)",null,null,null,0.18253999999999998]
[null,"OSW_SP_67",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas","GB","kWh (Net CV)",null,null,null,0.20227000000000001]
[null,"OSW_SP_68",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas","GB","tonnes",null,null,null,2539.25]
[null,"OSW_SP_69",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas (100% mineral blend)","GB","cubic metres",null,null,null,2.0315500000000002]
[null,"OSW_SP_70",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas (100% mineral blend)","GB","kWh (Gross CV)",null,null,null,0.18396999999999999]
[null,"OSW_SP_71",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas (100% mineral blend)","GB","kWh (Net CV)",null,null,null,0.20386000000000001]
[null,"OSW_SP_72",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas (100% mineral blend)","GB","tonnes",null,null,null,2559.17]
[null,"OSW_SP_73",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Other petroleum gas","GB","kWh (Gross CV)",null,null,null,0.18323999999999999]
[null,"OSW_SP_74",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Other petroleum gas","GB","kWh (Net CV)",null,null,null,0.19917000000000001]
[null,"OSW_SP_75",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Other petroleum gas","GB","litres",null,null,null,0.94440999999999997]
[null,"OSW_SP_76",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Other petroleum gas","GB","tonnes",null,null,null,2578.25]
[null,"OSW_SP_77",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Propane","GB","kWh (Gross CV)",null,null,null,0.21410999999999999]
[null,"OSW_SP_78",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Propane","GB","kWh (Net CV)",null,null,null,0.23257]
[null,"OSW_SP_79",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Propane","GB","litres",null,null,null,1.5435399999999999]
[null,"OSW_SP_80",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Propane","GB","tonnes",null,null,null,2997.55]
[null,"OSW_SP_81",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation spirit","GB","kWh (Gross CV)",null,null,null,0.24374999999999999]
[null,"OSW_SP_82",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation spirit","GB","kWh (Net CV)",null,null,null,0.25658000000000003]
[null,"OSW_SP_83",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation spirit","GB","litres",null,null,null,2.3304800000000001]
[null,"OSW_SP_84",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation spirit","GB","tonnes",null,null,null,3192.76]
[null,"OSW_SP_85",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation turbine fuel","GB","kWh (Gross CV)",null,null,null,0.24782000000000001]
[null,"OSW_SP_86",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation turbine fuel","GB","kWh (Net CV)",null,null,null,0.26085999999999998]
[null,"OSW_SP_87",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation turbine fuel","GB","litres",null,null,null,2.54514]
[null,"OSW_SP_88",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation turbine fuel","GB","tonnes",null,null,null,3181.4300000000003]
[null,"OSW_SP_89",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Burning oil","GB","kWh (Gross CV)",null,null,null,0.24677000000000002]
[null,"OSW_SP_90",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Burning oil","GB","kWh (Net CV)",null,null,null,0.25974999999999998]
[null,"OSW_SP_91",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Burning oil","GB","litres",null,null,null,2.54013]
[null,"OSW_SP_92",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Burning oil","GB","tonnes",null,null,null,3165.01]
[null,"OSW_SP_93",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (100% mineral diesel)","GB","kWh (Gross CV)",null,null,null,0.25320999999999999]
[null,"OSW_SP_94",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (100% mineral diesel)","GB","kWh (Net CV)",null,null,null,0.26938999999999996]
[null,"OSW_SP_95",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (100% mineral diesel)","GB","litres",null,null,null,2.6987999999999999]
[null,"OSW_SP_96",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (100% mineral diesel)","GB","tonnes",null,null,null,3208.7599999999998]
[null,"OSW_SP_97",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (average biofuel blend)","GB","kWh (Gross CV)",null,null,null,0.24114999999999998]
[null,"OSW_SP_98",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (average biofuel blend)","GB","kWh (Net CV)",null,null,null,0.25630999999999998]
[null,"OSW_SP_99",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (average biofuel blend)","GB","litres",null,null,null,2.5578399999999997]
[null,"OSW_SP_100",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (average biofuel blend)","GB","tonnes",null,null,null,3032.89]
[null,"OSW_SP_101",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Fuel oil","GB","kWh (Gross CV)",null,null,null,0.26816000000000001]
[null,"OSW_SP_102",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Fuel oil","GB","kWh (Net CV)",null,null,null,0.28525999999999996]
[null,"OSW_SP_103",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Fuel oil","GB","litres",null,null,null,3.17523]
[null,"OSW_SP_104",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Fuel oil","GB","tonnes",null,null,null,3229.2000000000003]
[null,"OSW_SP_105",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Gas oil","GB","kWh (Gross CV)",null,null,null,0.25678999999999996]
[null,"OSW_SP_106",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Gas oil","GB","kWh (Net CV)",null,null,null,0.27319000000000004]
[null,"OSW_SP_107",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Gas oil","GB","litres",null,null,null,2.7585700000000002]
[null,"OSW_SP_108",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Gas oil","GB","tonnes",null,null,null,3230.2799999999997]
[null,"OSW_SP_109",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Lubricants","GB","kWh (Gross CV)",null,null,null,0.26417999999999997]
[null,"OSW_SP_110",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Lubricants","GB","kWh (Net CV)",null,null,null,0.28103999999999996]
[null,"OSW_SP_111",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Lubricants","GB","litres",null,null,null,2.7497199999999999]
[null,"OSW_SP_112",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Lubricants","GB","tonnes",null,null,null,3181.44]
[null,"OSW_SP_113",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine fuel oil","GB","kWh (Gross CV)",null,null,null,0.26235999999999998]
[null,"OSW_SP_114",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine fuel oil","GB","kWh (Net CV)",null,null,null,0.27911000000000002]
[null,"OSW_SP_115",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine fuel oil","GB","litres",null,null,null,3.10669]
[null,"OSW_SP_116",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine fuel oil","GB","tonnes",null,null,null,3159.4999999999995]
[null,"OSW_SP_117",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine gas oil","GB","kWh (Gross CV)",null,null,null,0.25834999999999997]
[null,"OSW_SP_118",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine gas oil","GB","kWh (Net CV)",null,null,null,0.27484999999999998]
[null,"OSW_SP_119",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine gas oil","GB","litres",null,null,null,2.7753900000000002]
[null,"OSW_SP_120",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine gas oil","GB","tonnes",null,null,null,3249.99]
[null,"OSW_SP_121",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Naphtha","GB","kWh (Gross CV)",null,null,null,0.23651]
[null,"OSW_SP_122",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Naphtha","GB","kWh (Net CV)",null,null,null,0.24895]
[null,"OSW_SP_123",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Naphtha","GB","litres",null,null,null,2.1192699999999998]
[null,"OSW_SP_124",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Naphtha","GB","tonnes",null,null,null,3142.87]
[null,"OSW_SP_125",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (100% mineral petrol)","GB","kWh (Gross CV)",null,null,null,0.24156]
[null,"OSW_SP_126",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (100% mineral petrol)","GB","kWh (Net CV)",null,null,null,0.25428000000000001]
[null,"OSW_SP_127",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (100% mineral petrol)","GB","litres",null,null,null,2.3397000000000001]
[null,"OSW_SP_128",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (100% mineral petrol)","GB","tonnes",null,null,null,3153.9]
[null,"OSW_SP_129",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (average biofuel blend)","GB","kWh (Gross CV)",null,null,null,0.22719]
[null,"OSW_SP_130",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (average biofuel blend)","GB","kWh (Net CV)",null,null,null,0.23961000000000002]
[null,"OSW_SP_131",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (average biofuel blend)","GB","litres",null,null,null,2.1618500000000003]
[null,"OSW_SP_132",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (average biofuel blend)","GB","tonnes",null,null,null,2903.08]
[null,"OSW_SP_133",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - distillate oil","GB","kWh (Gross CV)",null,null,null,0.25678999999999996]
[null,"OSW_SP_134",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - distillate oil","GB","kWh (Net CV)",null,null,null,0.27319000000000004]
[null,"OSW_SP_135",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - distillate oil","GB","litres",null,null,null,2.7585700000000002]
[null,"OSW_SP_136",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - distillate oil","GB","tonnes",null,null,null,3230.2799999999997]
[null,"OSW_SP_137",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - residual oil","GB","kWh (Gross CV)",null,null,null,0.26816000000000001]
[null,"OSW_SP_138",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - residual oil","GB","kWh (Net CV)",null,null,null,0.28525999999999996]
[null,"OSW_SP_139",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - residual oil","GB","litres",null,null,null,3.17523]
[null,"OSW_SP_140",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - residual oil","GB","tonnes",null,null,null,3229.2000000000003]
[null,"OSW_SP_141",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Refinery miscellaneous","GB","kWh (Gross CV)",null,null,null,0.24667]
[null,"OSW_SP_142",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Refinery miscellaneous","GB","kWh (Net CV)",null,null,null,0.25964999999999999]
[null,"OSW_SP_143",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Refinery miscellaneous","GB","litres"]
[null,"OSW_SP_144",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Refinery miscellaneous","GB","tonnes",null,null,null,2944.81]
[null,"OSW_SP_145",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Waste oils","GB","kWh (Gross CV)",null,null,null,0.25681999999999999]
[null,"OSW_SP_146",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Waste oils","GB","kWh (Net CV)",null,null,null,0.27503]
[null,"OSW_SP_147",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Waste oils","GB","litres",null,null,null,2.7536699999999996]
[null,"OSW_SP_148",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Waste oils","GB","tonnes",null,null,null,3224.57]
[null,"OSW_SP_149",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (domestic)","GB","kWh (Gross CV)",null,null,null,0.34461999999999998]
[null,"OSW_SP_150",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (domestic)","GB","kWh (Net CV)",null,null,null,0.36276000000000003]
[null,"OSW_SP_151",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (domestic)","GB","tonnes",null,null,null,2883.2599999999998]
[null,"OSW_SP_152",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation - home produced coal only)","GB","kWh (Gross CV)",null,null,null,0.32133]
[null,"OSW_SP_153",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation - home produced coal only)","GB","kWh (Net CV)",null,null,null,0.33823999999999999]
[null,"OSW_SP_154",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation - home produced coal only)","GB","tonnes",null,null,null,2266.8999999999996]
[null,"OSW_SP_155",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation)","GB","kWh (Gross CV)",null,null,null,0.32133]
[null,"OSW_SP_156",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation)","GB","kWh (Net CV)",null,null,null,0.33823999999999999]
[null,"OSW_SP_157",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation)","GB","tonnes",null,null,null,2270.4499999999998]
[null,"OSW_SP_158",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (industrial)","GB","kWh (Gross CV)",null,null,null,0.32462999999999997]
[null,"OSW_SP_159",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (industrial)","GB","kWh (Net CV)",null,null,null,0.34172000000000002]
[null,"OSW_SP_160",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (industrial)","GB","tonnes",null,null,null,2411.4300000000003]
[null,"OSW_SP_161",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coking coal","GB","kWh (Gross CV)",null,null,null,0.35797000000000001]
[null,"OSW_SP_162",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coking coal","GB","kWh (Net CV)",null,null,null,0.37681999999999999]
[null,"OSW_SP_163",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coking coal","GB","tonnes",null,null,null,3165.24]
[null,"OSW_SP_164",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Petroleum coke","GB","kWh (Gross CV)",null,null,null,0.34094999999999998]
[null,"OSW_SP_165",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Petroleum coke","GB","kWh (Net CV)",null,null,null,0.35890000000000005]
[null,"OSW_SP_166",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Petroleum coke","GB","tonnes",null,null,null,3386.8700000000003]
[null,"OSW_SP_167",1,"Elcowire AB","S-P-07031","LCA","Copper wire rod",415,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","2019:14 Construction products, version 1.11","Yes","2027-12-01","Secondary: Proxy","Materials","Copper","Copper wire rod","EUR","kg",4.32,1.3599999999999999E-2,1.5800000000000002E-2,4.3490000000000002]
[null,"OSW_SP_168",1,"LaFarga SA","S-P-02032","LCA","Copper wire rod",415,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","PCR 2012:01","Yes","2025-08-01","Secondary: Proxy","Materials","Copper","Copper wire rod","GLO","kg",null,null,null,1.24]
[null,"OSW_SP_169",1,"Union Copper Rod","S-P-10570","LCA","Copper wire rod",415,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","2019:14 Construction products, version 1.11","Yes","2028-09-01","Secondary: Proxy","Materials","Copper","Copper wire rod","GLO","kg",null,null,null,6.76]
[null,"OSW_SP_170",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220174-IBF1-EN","LCA","Products based on epoxy-resin, group 1",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2027-08-01","Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 1","EUR","kg",3.95,-0.23799999999999999,8.8400000000000006E-2,3.8004000000000002]
[null,"OSW_SP_171",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220175-IBF1-EN","LCA","Products based on epoxy-resin, group 2",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2027-08-01","Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 2","EUR","kg",10.6,-3.3399999999999999E-2,5.0699999999999999E-3,10.571669999999999]
[null,"OSW_SP_172",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220176-IBF1-EN","LCA","Products based on epoxy-resin, group 3",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2027-08-01","Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 3","EUR","kg",5.26,-6.4100000000000004E-2,1.9300000000000001E-3,5.1978299999999997]
[null,"OSW_SP_173",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220177-IBF1-EN","LCA","Products based on epoxy-resin, group 4",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2027-08-01","Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 4","EUR","kg",4.26,-0.23100000000000001,9.1600000000000001E-2,4.1205999999999996]
[null,"OSW_SP_174",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220178-IBF1-EN","LCA","Products based on epoxy-resin, group 5",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2027-08-01","Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 5","EUR","kg",3.56,-5.2400000000000002E-2,9.6400000000000001E-4,3.5085640000000002]
[null,"OSW_SP_175",1,"Sistemas Técnicos del Accesorio y Componentes S. L. (STAC)","NA","LCA","Fibreglass",369,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2027-08-01","Secondary: Proxy","Materials","Fibreglass","Polyamide profiles reinforced with 25% fibreglass","GLO","kg",6.69,-1.26E-2,1.8600000000000001E-3,6.6792600000000002]
[null,"OSW_SP_176",1,"VALMIERAS STIKLA ŠĶIEDRA , AS","NA","LCA","Glass fibre mesh",26890,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2027-11-01","Secondary: Proxy","Materials","Fibreglass","Mesh","GLO","kg",1.718,-4.8000000000000001E-2,7.1199999999999996E-3,1.6771199999999999]
[null,"OSW_SP_177",1,"ArcelorMittal Europe – Flat Products","ECO-00001206","LCA","Heavy steel plates production",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","Structural steels, 07.2014","Yes","2025-04-01","Secondary: Proxy","Materials","Steel","Heavy steel plates","RER","kg",null,null,null,2.6]
[null,"OSW_SP_178",1,"SSAB EMEA AB","S-P-01918","LCA","Hot rolled steel plates production",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","PCR 2012:01. Construction Products and Construction Services.","Yes","2025-03-30","Secondary: Proxy","Materials","Steel","Hot rolled steel plates","GLO","kg",2.78,1.9900000000000001E-4,6.38E-4,2.7808369999999996]
[null,"OSW_SP_179",1,"Spartan UK LTD","S-P-03571","LCA","Hot rolled steel plates production",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2026-06-12","Secondary: Proxy","Materials","Steel","Hot rolled steel plates","Unreported","kg",2.1,-8.1899999999999994E-3,5.9099999999999995E-4,2.0924010000000002]
[null,"OSW_SP_180",1,"BE Group","S-P-04888","LCA","Hot rolled steel plates production",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2026-10-28","Secondary: Proxy","Materials","Steel","Hot rolled steel plates","Unreported","kg",2.02,-4.47E-3,7.1199999999999996E-4,2.0162420000000001]
[null,"OSW_SP_181",1,"Marcegaglia Plates S.p.A.","S-P-07882","LCA","Hot rolled steel plate",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2027-12-23","Secondary: Proxy","Materials","Steel","Hot rolled steel plates","GLO","kg",2.0470000000000002,1.1850000000000001E-3,1.1609999999999999E-3,2.0493460000000003]
[null,"OSW_SP_182",1,"Ferriera Valsider Spa","S-P-08032","LCA","Hot rolled steel plate",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-03-01","Secondary: Proxy","Materials","Steel","Hot rolled steel plates","EUR","kg",2.5099999999999998,2.8999999999999998E-3,1E-3,2.5138999999999996]
[null,"OSW_SP_183",1,"Metinvest Trametal SpA","S-P-08033","LCA","Hot rolled steel plate",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-03-01","Secondary: Proxy","Materials","Steel","Hot rolled steel plates","EUR","kg",2.81,2.3400000000000001E-3,1.1299999999999999E-3,2.8134699999999997]
[null,"OSW_SP_184",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator full asset production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured assets","Wind turbine generators (WTG)","WTG (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,5535730]
[null,"OSW_SP_185",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,525500]
[null,"OSW_SP_186",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Generator (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,664190]
[null,"OSW_SP_187",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Hub (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,424590]
[null,"OSW_SP_188",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend assembly (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,25440]
[null,"OSW_SP_189",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Electric components (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,2085120]
[null,"OSW_SP_190",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Blades (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,470910]
[null,"OSW_SP_191",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Tower","Tower (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,1339980]
[null,"OSW_SP_192",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator full asset production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured assets","Wind turbine generators (WTG)","WTG (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,7272570]
[null,"OSW_SP_193",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,638990]
[null,"OSW_SP_194",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Generator (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,887040]
[null,"OSW_SP_195",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Hub (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,537810]
[null,"OSW_SP_196",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend assembly (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,32369.999999999996]
[null,"OSW_SP_197",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Electric components (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,2653830]
[null,"OSW_SP_198",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Blades (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,579790]
[null,"OSW_SP_199",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Tower","Tower (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,1942740]
[null,"OSW_SP_200",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator full asset production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured assets","Wind turbine generators (WTG)","WTG (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,7272570]
[null,"OSW_SP_201",1,"Siemens Gamesa","S-P-09792","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,638990]
[null,"OSW_SP_202",1,"Siemens Gamesa","S-P-09793","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Generator (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,887040]
[null,"OSW_SP_203",1,"Siemens Gamesa","S-P-09794","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Hub (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,537810]
[null,"OSW_SP_204",1,"Siemens Gamesa","S-P-09795","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend assembly (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,32369.999999999996]
[null,"OSW_SP_205",1,"Siemens Gamesa","S-P-09796","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Nacelle and internals","Electric components (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,2653830]
[null,"OSW_SP_206",1,"Siemens Gamesa","S-P-09797","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Blades (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,579790]
[null,"OSW_SP_207",1,"Siemens Gamesa","S-P-09798","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes","2028-09-01","Secondary: Proxy","Fully manufactured components","Tower","Tower (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,1942740]

{"sheet":"IPCC Characterisation Factors","index":10,"n_rows":62,"n_cols":26,"rows_kept":62,"cut":false,"hidden":false,"merged":[[7,1,8,14],[13,1,13,15],[13,16,13,25]]}
[]
[null,"SUS-JIP  |  Offshore Wind Footprinting Tool"]
[null,"IPCC CHARACTERISATION FACTOR DATABASE"]
[]
[]
[null,"Secondary EF Database Guidance"]
[]
[null,"The IPCC 2021 Characterisation Factor database contains the GWP100 values for greenhouse gasses as defined by the IPCC. These form the basis of the other emission factors in the database, and may also be used directly as emission factors where there was direct emissions of removals of greenhouse gasses in the boundary of the OSW development system."]
[]
[]
[null,"User Controls"]
[]
[]
[null,"EMISSION FACTOR METADATA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EMISSION FACTOR"]
[null,"Emission Factor ID","Emission Factor version number","EF source name","Native database ID (optional)","Assessment Type","Activity Description","UN CPC 2.1 Code (optional)","Emission Factor Boundary","Background Dataset Used","Impact Methodology Used","Impact Indicator","Reporting Standard used ","PCR used (optional)","Verified","Valid until","OSW EF Category","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Geography","Emissions Factor Unit","climate change: fossil (kgCO2e/unit)","climate change: biogenic (kgCO2e/unit)","climate change: land use (kgCO2e/unit)","Emissions Factor Net (kgCO2e/unit)"]
[null,"OSW_CF_1","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Bromopropane","GLO","kg",null,null,null,5.1999999999999998E-2]
[null,"OSW_CF_2","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Butane","GLO","kg",null,null,null,6.0000000000000001E-3]
[null,"OSW_CF_3","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Carbon dioxide, fossil","GLO","kg",null,null,null,1]
[null,"OSW_CF_4","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Carbon dioxide, from soil or biomass stock","GLO","kg",null,null,1,1]
[null,"OSW_CF_5","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Removals","Carbon dioxide, removal from atmosphere","GLO","kg",null,null,null,-1]
[null,"OSW_CF_6","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Chloroform","GLO","kg",null,null,null,20.6]
[null,"OSW_CF_7","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Dinitrogen monoxide","GLO","kg",null,null,null,273]
[null,"OSW_CF_8","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane","GLO","kg",null,null,null,0.437]
[null,"OSW_CF_9","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1,1,2-tetrafluoro-, HFC-134a","GLO","kg",null,null,null,1530]
[null,"OSW_CF_10","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1,1-trichloro-, HCFC-140","GLO","kg",null,null,null,161]
[null,"OSW_CF_11","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1,1-trifluoro-, HFC-143a","GLO","kg",null,null,null,5810]
[null,"OSW_CF_12","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1,2-trichloro-1,2,2-trifluoro-, CFC-113","GLO","kg",null,null,null,6520]
[null,"OSW_CF_13","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1-dichloro-1-fluoro-, HCFC-141b","GLO","kg",null,null,null,860]
[null,"OSW_CF_14","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1-difluoro-, HFC-152a","GLO","kg",null,null,null,164]
[null,"OSW_CF_15","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,2-dichloro-","GLO","kg",null,null,null,1.3]
[null,"OSW_CF_16","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,2-dichloro-1,1,2,2-tetrafluoro-, CFC-114","GLO","kg",null,null,null,9430]
[null,"OSW_CF_17","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1-chloro-1,1-difluoro-, HCFC-142b","GLO","kg",null,null,null,2300]
[null,"OSW_CF_18","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 2,2-dichloro-1,1,1-trifluoro-, HCFC-123","GLO","kg",null,null,null,90.4]
[null,"OSW_CF_19","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 2-chloro-1,1,1,2-tetrafluoro-, HCFC-124","GLO","kg",null,null,null,597]
[null,"OSW_CF_20","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, chloropentafluoro-, CFC-115","GLO","kg",null,null,null,9600]
[null,"OSW_CF_21","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, hexafluoro-, HFC-116","GLO","kg",null,null,null,12400]
[null,"OSW_CF_22","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, pentafluoro-, HFC-125","GLO","kg",null,null,null,3740]
[null,"OSW_CF_23","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, bromo-, Halon 1001","GLO","kg",null,null,null,2.4300000000000002]
[null,"OSW_CF_24","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, bromochlorodifluoro-, Halon 1211","GLO","kg",null,null,null,1930]
[null,"OSW_CF_25","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, bromotrifluoro-, Halon 1301","GLO","kg",null,null,null,7200]
[null,"OSW_CF_26","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, chlorodifluoro-, HCFC-22","GLO","kg",null,null,null,1960]
[null,"OSW_CF_27","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, chloro-fluoro-, HCFC-31","GLO","kg",null,null,null,79.400000000000006]
[null,"OSW_CF_28","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, chlorotrifluoro-, CFC-13","GLO","kg",null,null,null,16200]
[null,"OSW_CF_29","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, dichloro-, HCC-30","GLO","kg",null,null,null,11.2]
[null,"OSW_CF_30","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, dichlorodifluoro-, CFC-12","GLO","kg",null,null,null,12500]
[null,"OSW_CF_31","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, dichlorofluoro-, HCFC-21","GLO","kg",null,null,null,160]
[null,"OSW_CF_32","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, difluoro-, HFC-32","GLO","kg",null,null,null,771]
[null,"OSW_CF_33","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, fossil","GLO","kg",null,null,null,29.8]
[null,"OSW_CF_34","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, from soil or biomass stock","GLO","kg",null,null,29.8,29.8]
[null,"OSW_CF_35","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, monochloro-, R-40","GLO","kg",5.54,null,null,5.54]
[null,"OSW_CF_36","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, non-fossil","GLO","kg",null,27,0,27]
[null,"OSW_CF_37","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, tetrachloro-, R-10","GLO","kg",null,null,null,2200]
[null,"OSW_CF_38","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, tetrafluoro-, R-14","GLO","kg",null,null,null,7380]
[null,"OSW_CF_39","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, trichlorofluoro-, CFC-11","GLO","kg",null,null,null,6230]
[null,"OSW_CF_40","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, trifluoro-, HFC-23","GLO","kg",null,null,null,14600]
[null,"OSW_CF_41","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Monochloroethane","GLO","kg",null,null,null,0.48099999999999998]
[null,"OSW_CF_42","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Nitrogen fluoride","GLO","kg",null,null,null,17400]
[null,"OSW_CF_43","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Perfluoropentane","GLO","kg",null,null,null,9220]
[null,"OSW_CF_44","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Propane","GLO","kg",null,null,null,0.02]
[null,"OSW_CF_45","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Sulfur hexafluoride","GLO","kg",null,null,null,25200]
[null,"OSW_CF_46","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Tetrachloroethylene","GLO","kg",null,null,null,6.34]
[null,"OSW_CF_47","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Trichloroethylene","GLO","kg",null,null,null,4.3999999999999997E-2]

{"sheet":"EF Library","index":11,"n_rows":1057,"n_cols":26,"rows_kept":1057,"cut":false,"hidden":false,"merged":[[17,1,17,15],[17,16,17,25],[7,1,8,14]]}
[]
[null,"SUS-JIP  |  Offshore Wind Footprinting Tool"]
[null,"EMISSIONS FACTOR LIBRARY"]
[]
[]
[null,"Emission Factor Library Guidance"]
[]
[null,"The Emission Factor Library is the central database of Emission Factors that may be pulled through by the assessor to the calculation tabs and used in the PCF calculation. The EF Library combines data from the other tabs that constitute the SUS-JIP Emission Factor Database:\n\n1. Primary EF Database\n2. Secondary EF Database\n3. Proxy EF Database\n4. IPCC Characterisation Factors (GWP of greenhouse gasses)\n\nThis worksheet and table cannot be directly manipulated by the users outside of using the user controls below, which allows the user to combine all of the Emissions Factor data, clear the data table. You may also use the filters to search for Emission Factors in the table. First, before clicking the \"Compile EF Library\" button, the user should make sure that all of the required emission factor datasets have been added to the EF tabs listed above. When the user clicks the \"Compile EF Library\" button, the table below will automatically update to include all of the relevant EF datasets, which may subsequently be used in your PCF calculations. A separate button is included to clear the table, which may be used before repeating the compilation of data in the event that there was a mistake on one of the other tabs."]
[]
[]
[null,"User Controls"]
[]
[]
[]
[]
[]
[]
[null,"EMISSION FACTOR METADATA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EMISSION FACTOR"]
[null,"Emission Factor ID","Emission Factor version number","EF source name","Native database ID (optional)","Assessment Type","Activity Description","UN CPC 2.1 Code (optional)","Emission Factor Boundary","Background Dataset Used","Impact Methodology Used","Impact Indicator","Reporting Standard used ","PCR used (optional)","Verified","Valid until","OSW EF Category","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Geography","Emissions Factor Unit","climate change: fossil (kgCO2e/unit)","climate change: biogenic (kgCO2e/unit)","climate change: land use (kgCO2e/unit)","Emissions Factor Net (kgCO2e/unit)"]
[null,"OSW_SE_1","N/A","Ecoinvent  3.10, cut-off by allocation version","0d88960c-7038-525c-8d90-194b3ba5d604_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_2","N/A","Ecoinvent  3.10, cut-off by allocation version","4e959cbd-4b18-5f8d-9eb6-1c347ea2c2ff_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_3","N/A","Ecoinvent  3.10, cut-off by allocation version","d7bb4e4f-49d6-5054-aff8-6290f98f8205_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_4","N/A","Ecoinvent  3.10, cut-off by allocation version","efe8be91-2ffc-533f-bcd6-22e70a11d008_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_5","N/A","Ecoinvent  3.10, cut-off by allocation version","bd1a994e-9b13-5afb-9b86-9880dc35a62a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_6","N/A","Ecoinvent  3.10, cut-off by allocation version","a6f17f0f-8b94-5475-9f13-1a6f4e54218f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_7","N/A","Ecoinvent  3.10, cut-off by allocation version","bc019df7-0f00-59c7-9538-67ce8a4b0081_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_8","N/A","Ecoinvent  3.10, cut-off by allocation version","bcf870ca-7662-5fab-88e1-05f0fae4f45e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_9","N/A","Ecoinvent  3.10, cut-off by allocation version","867301f4-8db2-5bd4-95d5-52404f98c69f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_10","N/A","Ecoinvent  3.10, cut-off by allocation version","c5362e7d-fc80-5c74-a13d-1cc248ea169f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_11","N/A","Ecoinvent  3.10, cut-off by allocation version","d2ad7d45-9fab-59eb-ae32-e34aba958ba6_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_12","N/A","Ecoinvent  3.10, cut-off by allocation version","e305c073-d9bd-5bb9-89ea-6987758a00d7_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_13","N/A","Ecoinvent  3.10, cut-off by allocation version","5c309945-5358-5228-bfbe-9edd9e3f5e20_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_14","N/A","Ecoinvent  3.10, cut-off by allocation version","4b5ababf-cb44-59ed-9f92-bb4492ec52b5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_15","N/A","Ecoinvent  3.10, cut-off by allocation version","c6931985-d821-5ad0-bb60-b08fa52f62d9_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_16","N/A","Ecoinvent  3.10, cut-off by allocation version","1e48c229-e40a-5bb9-9509-e5513c1437dd_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_17","N/A","Ecoinvent  3.10, cut-off by allocation version","eebad817-5f9a-5572-b361-8009c47698db_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_18","N/A","Ecoinvent  3.10, cut-off by allocation version","c9a2346c-4228-574d-a767-fd01a981bb80_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_19","N/A","Ecoinvent  3.10, cut-off by allocation version","2f1625c1-a80d-5264-96b1-929f3d5d513c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_20","N/A","Ecoinvent  3.10, cut-off by allocation version","920c3004-54f6-5f18-9d9b-3d6c4f9bcd6d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_21","N/A","Ecoinvent  3.10, cut-off by allocation version","e53e0491-6ca1-5901-8674-cb18ad0287e8_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_22","N/A","Ecoinvent  3.10, cut-off by allocation version","8814190a-62d5-5294-a961-ebc78ccdfc5c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_23","N/A","Ecoinvent  3.10, cut-off by allocation version","fbe35edd-e62e-525a-8cb8-fca983b2019b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_24","N/A","Ecoinvent  3.10, cut-off by allocation version","f490b95e-5a62-5064-9c34-7c77c1805c76_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_25","N/A","Ecoinvent  3.10, cut-off by allocation version","ee1bb605-5372-5e41-a497-fcbaf6d2e9d5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_26","N/A","Ecoinvent  3.10, cut-off by allocation version","bf8effe2-d954-51ae-ad2e-b0115b455211_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_27","N/A","Ecoinvent  3.10, cut-off by allocation version","bb151bdb-a8a1-554b-922e-625822c50dce_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_28","N/A","Ecoinvent  3.10, cut-off by allocation version","275f5839-90f3-50ab-8971-89cbd9fc793d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_29","N/A","Ecoinvent  3.10, cut-off by allocation version","11c0049d-e481-52b2-bd7b-72a491ad7ed3_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_30","N/A","Ecoinvent  3.10, cut-off by allocation version","91d8acb4-e0a7-51a8-85b8-0792e4e2c492_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_31","N/A","Ecoinvent  3.10, cut-off by allocation version","80e62ca3-236c-5e43-b007-942e61757853_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_32","N/A","Ecoinvent  3.10, cut-off by allocation version","b5cf1a85-ab39-5145-9544-155be6ca6d43_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_33","N/A","Ecoinvent  3.10, cut-off by allocation version","a8df3de1-1915-54cc-85aa-451e018d8332_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_34","N/A","Ecoinvent  3.10, cut-off by allocation version","581af806-d4f7-532f-99f5-46b495724400_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_35","N/A","Ecoinvent  3.10, cut-off by allocation version","dd9c8cc4-f857-51a9-a4ac-62b4b96f3bdf_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_36","N/A","Ecoinvent  3.10, cut-off by allocation version","9996f97c-69b6-5e77-a2b6-20d2253e137d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_37","N/A","Ecoinvent  3.10, cut-off by allocation version","a2b3c97a-e5f8-596d-adbe-b53627f210c3_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_38","N/A","Ecoinvent  3.10, cut-off by allocation version","c518da90-0362-54fe-913d-57118042bb09_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_39","N/A","Ecoinvent  3.10, cut-off by allocation version","2484baaa-e415-5fbc-9c33-c6a2ccd2e6ce_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_40","N/A","Ecoinvent  3.10, cut-off by allocation version","4d9f590b-bf4c-510b-b899-a83f138d78ea_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_41","N/A","Ecoinvent  3.10, cut-off by allocation version","da8aa9b5-cf46-5519-9159-0468958cae27_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_42","N/A","Ecoinvent  3.10, cut-off by allocation version","3e3d2f61-6803-57be-b6cd-73cd8a888f8e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_43","N/A","Ecoinvent  3.10, cut-off by allocation version","a228a463-f671-5180-af65-d2afe362f0fa_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_44","N/A","Ecoinvent  3.10, cut-off by allocation version","1bba7748-a22d-5ef3-ac7b-9f84e6376db2_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_45","N/A","Ecoinvent  3.10, cut-off by allocation version","75a39532-1863-5b57-bdfa-1d767b4ccf78_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_46","N/A","Ecoinvent  3.10, cut-off by allocation version","6c3d75b9-34ab-5e29-bcd1-e87b11908d96_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_47","N/A","Ecoinvent  3.10, cut-off by allocation version","9baa4e58-25c6-558f-abf1-9f796c57ab81_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_48","N/A","Ecoinvent  3.10, cut-off by allocation version","68f01316-97bb-5702-aa86-bbdd8414e490_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_49","N/A","Ecoinvent  3.10, cut-off by allocation version","7537f6a4-8e59-5766-bbb3-50e404fcca23_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_50","N/A","Ecoinvent  3.10, cut-off by allocation version","f0596e75-2d5f-5910-a974-af2f0267df23_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_51","N/A","Ecoinvent  3.10, cut-off by allocation version","4e32e3bd-b3a8-5d45-89b4-4f62c6c8c139_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_52","N/A","Ecoinvent  3.10, cut-off by allocation version","4b751597-0cf6-5cbc-af97-6068af6f1c09_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_53","N/A","Ecoinvent  3.10, cut-off by allocation version","1a8d13b2-87ac-5c43-aa62-4f1ceb9c9b54_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_54","N/A","Ecoinvent  3.10, cut-off by allocation version","a044fcb0-673d-54d9-a33a-fa8751352510_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_55","N/A","Ecoinvent  3.10, cut-off by allocation version","02f0edec-9d38-563d-bbfb-17d34b844ae1_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_56","N/A","Ecoinvent  3.10, cut-off by allocation version","2ad5c0a5-7831-5f5c-9b65-ed34e996d85a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_57","N/A","Ecoinvent  3.10, cut-off by allocation version","3eb03656-f9be-55f3-94cb-f421abfc38f5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","N/A","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_58","N/A","Ecoinvent  3.10, cut-off by allocation version","beef6691-f62f-5282-b8fe-c5d3f67fc624_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_59","N/A","Ecoinvent  3.10, cut-off by allocation version","8fae52c3-23ea-5d05-9aef-207d988fa26f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_60","N/A","Ecoinvent  3.10, cut-off by allocation version","2efd189f-472d-5931-89c0-57799674b9bf_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_61","N/A","Ecoinvent  3.10, cut-off by allocation version","2d5fbeac-02e0-5777-bb55-de3ab2d769ce_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_62","N/A","Ecoinvent  3.10, cut-off by allocation version","fc09fb1b-5219-5605-9f56-07f491033a59_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_63","N/A","Ecoinvent  3.10, cut-off by allocation version","ac460e8b-6885-502c-a95f-8e00b675a82c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_64","N/A","Ecoinvent  3.10, cut-off by allocation version","89a546df-22a4-5293-9058-5915230ea121_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_65","N/A","Ecoinvent  3.10, cut-off by allocation version","51653290-0910-5c53-9832-676388ad0e20_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_66","N/A","Ecoinvent  3.10, cut-off by allocation version","7334ae81-82a7-5423-9a8d-b9b8d0885347_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_67","N/A","Ecoinvent  3.10, cut-off by allocation version","053ce719-1cc3-5bca-8383-3e0c04f2556f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_68","N/A","Ecoinvent  3.10, cut-off by allocation version","c0e3d395-9bcf-542c-abbf-312ae80df261_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_69","N/A","Ecoinvent  3.10, cut-off by allocation version","e11f6315-cf7c-543e-93aa-42db02f156a6_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_70","N/A","Ecoinvent  3.10, cut-off by allocation version","f99a3a77-1a13-5e68-a657-e96e57e72b22_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_71","N/A","Ecoinvent  3.10, cut-off by allocation version","469cefbc-929d-51b7-906b-2642169b4075_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_72","N/A","Ecoinvent  3.10, cut-off by allocation version","6aa3a3ea-0ead-5cf7-8770-950aa5f64e10_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_73","N/A","Ecoinvent  3.10, cut-off by allocation version","f0613e44-8c68-5f7a-af9f-7f2fe2e48e84_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_74","N/A","Ecoinvent  3.10, cut-off by allocation version","3ec6e3fa-7524-5b00-a52b-968723e667ab_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_75","N/A","Ecoinvent  3.10, cut-off by allocation version","fb9c5497-a5ec-552c-b133-6b28af4ef7e1_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_76","N/A","Ecoinvent  3.10, cut-off by allocation version","9c0b45a9-4997-5953-b459-a1c89fbc44a0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_77","N/A","Ecoinvent  3.10, cut-off by allocation version","51fa6b66-b8f2-5475-9240-4ad88157d997_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_78","N/A","Ecoinvent  3.10, cut-off by allocation version","08883748-ffb3-537a-ad56-61c118aaf723_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_79","N/A","Ecoinvent  3.10, cut-off by allocation version","ea6ed979-2c3e-500a-9863-15c6f8eef81d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_80","N/A","Ecoinvent  3.10, cut-off by allocation version","5183e942-3664-5894-94d1-63bdf0b23daf_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_81","N/A","Ecoinvent  3.10, cut-off by allocation version","5b0b4c15-0aec-5772-b3b3-7d25bf723baf_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_82","N/A","Ecoinvent  3.10, cut-off by allocation version","4c19ac87-d1a1-5656-b1a9-05e5b3dd7ba5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_83","N/A","Ecoinvent  3.10, cut-off by allocation version","ea1a79e5-dfe9-5b67-89ac-0a2024ecec65_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_84","N/A","Ecoinvent  3.10, cut-off by allocation version","ca0533f7-60af-5e1f-b851-64033e9ca5cb_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_85","N/A","Ecoinvent  3.10, cut-off by allocation version","0ad7199c-7b0d-5b1f-9f40-bd0f41502a3a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_86","N/A","Ecoinvent  3.10, cut-off by allocation version","8662821a-12c7-558d-a8d8-6a5b0d7bfbbb_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_87","N/A","Ecoinvent  3.10, cut-off by allocation version","440eac7f-0117-52ac-af9e-d00defc3c285_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_88","N/A","Ecoinvent  3.10, cut-off by allocation version","81b7daa6-4845-5d63-8915-205a586fb550_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_89","N/A","Ecoinvent  3.10, cut-off by allocation version","e8577b3e-59c0-5c54-ad73-073efb411834_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_90","N/A","Ecoinvent  3.10, cut-off by allocation version","ebb7bff0-12e9-5c41-a1db-9e18e78c74be_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_91","N/A","Ecoinvent  3.10, cut-off by allocation version","64d81d22-4c9b-5bfa-8fbd-d775fac77972_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_92","N/A","Ecoinvent  3.10, cut-off by allocation version","e30a9776-31ac-5239-9d8c-45b8940fbbbd_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_93","N/A","Ecoinvent  3.10, cut-off by allocation version","ff2f2010-219e-583e-927b-a66deb7649e1_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_94","N/A","Ecoinvent  3.10, cut-off by allocation version","7ddf2644-bc3e-5f89-b4da-bb9b91963a10_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_95","N/A","Ecoinvent  3.10, cut-off by allocation version","b4cf8006-4329-5326-8790-0629582548df_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_96","N/A","Ecoinvent  3.10, cut-off by allocation version","cc87dc36-b51d-5609-8d8b-a31097103803_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_97","N/A","Ecoinvent  3.10, cut-off by allocation version","7d8b8318-9790-5dfb-a6ad-7238780a8f0a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_98","N/A","Ecoinvent  3.10, cut-off by allocation version","11a17d28-3a71-569f-b56c-12701fd7b094_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_99","N/A","Ecoinvent  3.10, cut-off by allocation version","d1cf7269-c305-5767-8006-10bda56df81e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_100","N/A","Ecoinvent  3.10, cut-off by allocation version","758d3d17-7a3e-5b30-961a-849a16d94cf3_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_101","N/A","Ecoinvent  3.10, cut-off by allocation version","5d8f39cc-fa03-5166-8ca3-98007070bf19_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_102","N/A","Ecoinvent  3.10, cut-off by allocation version","b6f7d61e-7614-5ccd-83b7-cc432475baac_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_103","N/A","Ecoinvent  3.10, cut-off by allocation version","8a5aaa7d-ccad-525a-be5f-5d7f1df898b9_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_104","N/A","Ecoinvent  3.10, cut-off by allocation version","311ac285-7ed6-50ea-a1dc-311c9a28c80a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_105","N/A","Ecoinvent  3.10, cut-off by allocation version","b0c4219b-7c45-5849-b7f4-630d19ed8eb6_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_106","N/A","Ecoinvent  3.10, cut-off by allocation version","3bb154e6-4405-5f8d-b1a0-b7b89a57705d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_107","N/A","Ecoinvent  3.10, cut-off by allocation version","9324bcd2-9447-561d-865e-02514dee0b5c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_108","N/A","Ecoinvent  3.10, cut-off by allocation version","01f66006-aa83-54ca-9330-78ee88f2b7c7_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_109","N/A","Ecoinvent  3.10, cut-off by allocation version","023804bb-ee14-58b0-abe1-41b1a28ff8ee_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_110","N/A","Ecoinvent  3.10, cut-off by allocation version","acab6c00-bdaf-5a67-a609-d8b28d149e4d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_111","N/A","Ecoinvent  3.10, cut-off by allocation version","5f03e37f-db10-5cf6-ac3c-2575b627c662_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_112","N/A","Ecoinvent  3.10, cut-off by allocation version","265ee001-ba3d-5379-82e0-a0c075b0ac02_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_113","N/A","Ecoinvent  3.10, cut-off by allocation version","fff7d27c-89c5-5282-b587-81ab232d7d6f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_114","N/A","Ecoinvent  3.10, cut-off by allocation version","0a765a9f-6d68-5a4c-8ba4-07a6b1508dc5_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_115","N/A","Ecoinvent  3.10, cut-off by allocation version","39d45496-1958-5384-a553-9c7a73064866_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_116","N/A","Ecoinvent  3.10, cut-off by allocation version","07cac406-a071-5cd7-8c84-e8bcbe41b7ee_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_117","N/A","Ecoinvent  3.10, cut-off by allocation version","ee456a81-81aa-5e64-b607-ce14a8b24236_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_118","N/A","Ecoinvent  3.10, cut-off by allocation version","6ce260d8-04d7-5c41-8209-dc923db0928e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_119","N/A","Ecoinvent  3.10, cut-off by allocation version","8c4f006f-380c-538f-8a59-7df1d08c777d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_120","N/A","Ecoinvent  3.10, cut-off by allocation version","433b7238-0e9f-5343-a8eb-0e0a4c6c4eca_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_121","N/A","Ecoinvent  3.10, cut-off by allocation version","42407eff-aabe-566a-a151-3dc7c3d8dc3a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_122","N/A","Ecoinvent  3.10, cut-off by allocation version","257464d8-6250-5669-bb55-e256dcce29e0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_123","N/A","Ecoinvent  3.10, cut-off by allocation version","72f5c398-aadb-57dd-8b6a-e6571fbbb7c9_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_124","N/A","Ecoinvent  3.10, cut-off by allocation version","6c3b8106-17be-500e-a65a-3d12d07517a0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_125","N/A","Ecoinvent  3.10, cut-off by allocation version","81bdd3d2-a5b6-5fb4-b617-ebe79e02c050_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_126","N/A","Ecoinvent  3.10, cut-off by allocation version","8f486a15-4e49-5c00-9242-7e7ad70a3779_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_127","N/A","Ecoinvent  3.10, cut-off by allocation version","a8a31120-891f-595e-8162-bdc938a86343_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_128","N/A","Ecoinvent  3.10, cut-off by allocation version","96c5a4a4-5ec6-5d28-9ace-59c0414a631b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_129","N/A","Ecoinvent  3.10, cut-off by allocation version","72b26085-5a8b-58e2-ae83-abee9518abbe_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_130","N/A","Ecoinvent  3.10, cut-off by allocation version","995373ba-9aaf-51ee-a5a6-5a0679ca3131_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_131","N/A","Ecoinvent  3.10, cut-off by allocation version","9c1033e7-8db1-583f-b825-0d6e7ad28a72_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_132","N/A","Ecoinvent  3.10, cut-off by allocation version","6e7cdf4d-4e08-53be-b3e5-be169a30857e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_133","N/A","Ecoinvent  3.10, cut-off by allocation version","274e893c-d925-5d33-8b05-e4beea86eb1f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_134","N/A","Ecoinvent  3.10, cut-off by allocation version","62497925-a25b-5490-8d43-f626fab4dee3_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_135","N/A","Ecoinvent  3.10, cut-off by allocation version","9883579c-2621-58cf-bd7e-ad9cf3854264_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_136","N/A","Ecoinvent  3.10, cut-off by allocation version","04e14855-5bd0-58f2-9919-12352fbdf666_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_137","N/A","Ecoinvent  3.10, cut-off by allocation version","86ef6913-544e-5b9b-9b27-0731540b563e_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_138","N/A","Ecoinvent  3.10, cut-off by allocation version","2fb93b9a-b882-5d99-a584-319fbc2d4888_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_139","N/A","Ecoinvent  3.10, cut-off by allocation version","3e74d4a1-652c-5cb3-af46-705998113b3b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_140","N/A","Ecoinvent  3.10, cut-off by allocation version","30cb3d2f-1967-5ab2-b024-ce57da0b3308_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_141","N/A","Ecoinvent  3.10, cut-off by allocation version","e77ffa79-0605-50fe-8c35-7695796966b9_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_142","N/A","Ecoinvent  3.10, cut-off by allocation version","e95b1799-89d8-5394-bed9-c9cc193221c0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_143","N/A","Ecoinvent  3.10, cut-off by allocation version","56e57368-1e71-5083-9cf2-7fbbd1bd4b97_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_144","N/A","Ecoinvent  3.10, cut-off by allocation version","55766f6a-4953-596b-9f4e-3e08873e8ec6_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_145","N/A","Ecoinvent  3.10, cut-off by allocation version","b32345b1-74dd-5002-b168-cdf1bf2ce085_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_146","N/A","Ecoinvent  3.10, cut-off by allocation version","045a8d09-9a26-55cd-ab83-152130df8104_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_147","N/A","Ecoinvent  3.10, cut-off by allocation version","aa7f6254-ce49-5cf4-9e1f-e19acbb335b7_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_148","N/A","Ecoinvent  3.10, cut-off by allocation version","dc35652a-6adf-5c96-9efb-070de65cce88_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_149","N/A","Ecoinvent  3.10, cut-off by allocation version","17bf22ac-3720-56ce-b678-1e896c81c5b0_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_150","N/A","Ecoinvent  3.10, cut-off by allocation version","8c7e5ef5-8391-5cc1-a71d-3f1f74e4bf1a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_151","N/A","Ecoinvent  3.10, cut-off by allocation version","b1ab724c-ec07-5891-9fbe-9d56cdf16c7b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_152","N/A","Ecoinvent  3.10, cut-off by allocation version","d4976e17-addb-5f64-a762-90f89da7f05f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_153","N/A","Ecoinvent  3.10, cut-off by allocation version","0d78f095-f0be-541a-bd7f-1222879b8638_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_154","N/A","Ecoinvent  3.10, cut-off by allocation version","c12ee0e0-3cb6-5a2f-8c1d-94c62d324d4a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_155","N/A","Ecoinvent  3.10, cut-off by allocation version","ff8e6118-b4c0-58f1-a214-40b3dac03961_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_156","N/A","Ecoinvent  3.10, cut-off by allocation version","e187900c-4b7e-570c-8fb1-28f3cf860275_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_157","N/A","Ecoinvent  3.10, cut-off by allocation version","69556d8c-1c0e-59b1-90a9-5c05212972c4_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_158","N/A","Ecoinvent  3.10, cut-off by allocation version","375f2ed1-75d0-5065-aee9-45e53d048996_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_159","N/A","Ecoinvent  3.10, cut-off by allocation version","44eac5a7-f30b-5cff-99c6-b2a4208359da_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_160","N/A","Ecoinvent  3.10, cut-off by allocation version","7828dbba-e6f1-5e04-b6eb-dcd7af440a2d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_161","N/A","Ecoinvent  3.10, cut-off by allocation version","ba661998-a61a-5cdc-b7ce-302cbf7a9360_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_162","N/A","Ecoinvent  3.10, cut-off by allocation version","f67789ee-7aa3-58db-88c0-c232dc5f1f78_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_163","N/A","Ecoinvent  3.10, cut-off by allocation version","c6170cd7-00f8-5dfc-8bd4-1bcd1190857c_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_164","N/A","Ecoinvent  3.10, cut-off by allocation version","bbb6924a-3ad6-56de-ae6e-050ead619bf2_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_165","N/A","Ecoinvent  3.10, cut-off by allocation version","048e3649-180b-5789-b12f-9223aa5b0e7f_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_166","N/A","Ecoinvent  3.10, cut-off by allocation version","bc2de9e8-a936-5af2-a5df-f7d15df6ae7d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_167","N/A","Ecoinvent  3.10, cut-off by allocation version","46c2817e-317f-53b0-8cb5-85a1acbd6f7d_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_168","N/A","Ecoinvent  3.10, cut-off by allocation version","e7469d76-1688-5c91-bce2-097bdd934b8b_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_169","N/A","Ecoinvent  3.10, cut-off by allocation version","e2a3cf7a-33f6-596c-94c4-6794e8699854_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_170","N/A","Ecoinvent  3.10, cut-off by allocation version","d45fba3a-ded6-58d4-ae5f-1b64c53ba5cc_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_171","N/A","Ecoinvent  3.10, cut-off by allocation version","46e1ec5e-1be6-5fa5-aa4f-9a4897bc8a50_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_172","N/A","Ecoinvent  3.10, cut-off by allocation version","def10dfb-bfa2-5f37-ae70-5db9b840d93a_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_173","N/A","Ecoinvent  3.10, cut-off by allocation version","29d264da-db2f-54d7-986a-ceaad846cdb4_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_174","N/A","Ecoinvent  3.10, cut-off by allocation version","faf37cde-4058-59f0-b67d-c26b9c054c34_66c93e71-f32b-4591-901c-55395db5c132",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Electricity lifecycle"]
[null,"OSW_SE_175","N/A","Ecoinvent  3.10, cut-off by allocation version","eb0d1076-5276-5b7a-83bc-cce475127870_705f483c-0d06-4f1c-9be9-7d54b88c4015",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Gaseous fuels lifecycle"]
[null,"OSW_SE_176","N/A","Ecoinvent  3.10, cut-off by allocation version","f1b07269-1222-534b-b8a7-fa001e31dc17_b4e0b7c5-87b9-490e-971f-9ddc8c2b08d8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Liquid fuels lifecycle"]
[null,"OSW_SE_177","N/A","Ecoinvent  3.10, cut-off by allocation version","6e74a577-75d2-5023-941a-5007cde9c18a_fecdf330-8660-4362-adde-ab5ea197ab1d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Liquid fuels lifecycle"]
[null,"OSW_SE_178","N/A","Ecoinvent  3.10, cut-off by allocation version","e622ec20-8840-5a4c-90cc-9a073ee6e738_b0f4c2fb-5081-474a-8ffa-1457da8345db",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Liquid fuels lifecycle"]
[null,"OSW_SE_179","N/A","Ecoinvent  3.10, cut-off by allocation version","da0dbd21-a4fe-5ed0-98f3-8feb48d74787_1151abf1-5ac3-4518-bb20-60f003bb6a31",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Liquid fuels lifecycle"]
[null,"OSW_SE_180","N/A","Ecoinvent  3.10, cut-off by allocation version","e6576483-6c19-59fe-98b7-191f866a63df_533392d3-8fa6-44bb-9b79-b14c0a0e66e0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Liquid fuels lifecycle"]
[null,"OSW_SE_181","N/A","Ecoinvent  3.10, cut-off by allocation version","0cb8762f-ed6c-503d-bc05-3cf14601c72f_79838d89-26c0-4781-b17f-a0deb787d482",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Liquid fuels lifecycle"]
[null,"OSW_SE_182","N/A","Ecoinvent  3.10, cut-off by allocation version","f4aeaeba-ba0f-5236-845f-001a2d9a023b_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_183","N/A","Ecoinvent  3.10, cut-off by allocation version","988df15c-0222-5ba6-bbab-30e0695bf7eb_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_184","N/A","Ecoinvent  3.10, cut-off by allocation version","b564083a-0561-567b-9239-a82862ef7e6a_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_185","N/A","Ecoinvent  3.10, cut-off by allocation version","d747455f-a7c7-5798-85ba-a60e09d41b3d_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_186","N/A","Ecoinvent  3.10, cut-off by allocation version","1cb04872-15c3-54bc-ac35-1312b37eb8bf_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_187","N/A","Ecoinvent  3.10, cut-off by allocation version","6710b4ed-d4e1-527f-aa6c-670af3a595bb_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_188","N/A","Ecoinvent  3.10, cut-off by allocation version","7d456e1e-7622-5d1f-9292-402ee3cbdcc7_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_189","N/A","Ecoinvent  3.10, cut-off by allocation version","9c5a283f-37d0-5818-9e42-0484c5027ef6_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_190","N/A","Ecoinvent  3.10, cut-off by allocation version","b825409b-5694-5325-a11d-0fe92dd8a650_c5adb1fb-872e-4446-a3bb-c4b61aa4bd45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Electricity, fuels and other utilitites","Water consumption"]
[null,"OSW_SE_191","N/A","Ecoinvent  3.10, cut-off by allocation version","278c318b-af70-5dc1-81ca-2079ef82d592_5bcb4640-2e25-4dc3-acc4-d89f308eb32c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_192","N/A","Ecoinvent  3.10, cut-off by allocation version","920bcef5-ca9c-5ae7-8d89-49be2287e530_4124c89b-fbf6-4320-a994-9f7d90447bd5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_193","N/A","Ecoinvent  3.10, cut-off by allocation version","2cc0d6c8-6b7e-5b2c-9596-1ca386c66a57_8795dc98-b6c7-4f09-be36-66739ea84900",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_194","N/A","Ecoinvent  3.10, cut-off by allocation version","f6314cea-f994-50f6-8fd4-60eb266e5969_3317126a-4dd7-4047-9ccf-163f94382c94",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_195","N/A","Ecoinvent  3.10, cut-off by allocation version","f96c0979-e6e6-54c9-8564-e0fab55df732_220fe333-5329-4a8d-b012-1db429f2383b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_196","N/A","Ecoinvent  3.10, cut-off by allocation version","b48b5a4d-54a0-59f7-8de2-913b5a4e24f9_07ad9bb5-f5d3-4e09-ac39-a6dcbb13a0ba",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_197","N/A","Ecoinvent  3.10, cut-off by allocation version","855fef94-252f-521e-b4d5-30e4bbf34926_02db23d4-0c70-4c90-98b6-2aa65ef4b268",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_198","N/A","Ecoinvent  3.10, cut-off by allocation version","dc851ae2-7510-5bd1-9787-2b006da03f35_3317126a-4dd7-4047-9ccf-163f94382c94",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_199","N/A","Ecoinvent  3.10, cut-off by allocation version","74220222-9c26-5611-8647-d8f035b32b5e_220fe333-5329-4a8d-b012-1db429f2383b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_200","N/A","Ecoinvent  3.10, cut-off by allocation version","df735d07-cc3c-56a9-b820-1308381c2c0c_07ad9bb5-f5d3-4e09-ac39-a6dcbb13a0ba",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_201","N/A","Ecoinvent  3.10, cut-off by allocation version","9578f022-c5f8-52a6-8179-a874e16c1323_02db23d4-0c70-4c90-98b6-2aa65ef4b268",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_202","N/A","Ecoinvent  3.10, cut-off by allocation version","1b6cdc0c-fdb0-56c9-b39f-9fe5b6b4b1a7_c784e421-2f79-47e4-8b6d-2c29fa41aad0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_203","N/A","Ecoinvent  3.10, cut-off by allocation version","c6e5ed96-f225-5ffd-974a-8efda70209d7_cc7e810b-79d2-4c9c-96e6-60a3c739952c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Air freight and transportation"]
[null,"OSW_SE_204","N/A","Ecoinvent  3.10, cut-off by allocation version","0aefeb47-cf69-5ee0-8ac9-e3dfee68d5e8_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_205","N/A","Ecoinvent  3.10, cut-off by allocation version","394443c6-d2f4-5eba-9fb9-72e479cad99b_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_206","N/A","Ecoinvent  3.10, cut-off by allocation version","4f94bd0c-3028-57b7-93ba-127056601ac4_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_207","N/A","Ecoinvent  3.10, cut-off by allocation version","e6f415f7-267f-5a7a-a26e-38afcfb159a6_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_208","N/A","Ecoinvent  3.10, cut-off by allocation version","dcceff88-3edf-5291-ab2a-ae67b46bfb1b_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_209","N/A","Ecoinvent  3.10, cut-off by allocation version","245fe21a-bef8-5ed5-bc6b-799ab91cc4b3_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_210","N/A","Ecoinvent  3.10, cut-off by allocation version","e6581ba7-eba3-5cb5-a89e-41830e002068_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_211","N/A","Ecoinvent  3.10, cut-off by allocation version","0be94d2a-ebaf-5f72-9926-162c7edee0e1_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_212","N/A","Ecoinvent  3.10, cut-off by allocation version","a2b74eef-088d-528d-82fa-331855e70442_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_213","N/A","Ecoinvent  3.10, cut-off by allocation version","2e773d69-933e-57fa-a16a-3d505101ebc5_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_214","N/A","Ecoinvent  3.10, cut-off by allocation version","4a96b90f-d751-5ff9-b256-454971dc63a4_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_215","N/A","Ecoinvent  3.10, cut-off by allocation version","8fc6b375-653f-5dbf-856d-5196624c1dd4_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_216","N/A","Ecoinvent  3.10, cut-off by allocation version","96b8d86d-76bc-5500-b159-6ae084327b91_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_217","N/A","Ecoinvent  3.10, cut-off by allocation version","4e39d168-df1e-5c2d-b08a-bc8be50e131c_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_218","N/A","Ecoinvent  3.10, cut-off by allocation version","7eca3d84-04a7-5ead-a837-343689350ac2_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_219","N/A","Ecoinvent  3.10, cut-off by allocation version","57d005b5-1f11-5a27-ad75-249245cedd81_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_220","N/A","Ecoinvent  3.10, cut-off by allocation version","98467a29-aaf3-508f-ae4c-9a359ed1423c_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_221","N/A","Ecoinvent  3.10, cut-off by allocation version","ab481aec-f834-5863-b601-731be2115fcf_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_222","N/A","Ecoinvent  3.10, cut-off by allocation version","787fa53e-6b32-56d9-852c-5000fe4f7de4_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_223","N/A","Ecoinvent  3.10, cut-off by allocation version","3ed7f6bb-5b04-5b1d-a44f-6b2d1b0ba80f_0ace02fa-eca5-482d-a829-c18e46a52db4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Rail freight and transportation"]
[null,"OSW_SE_224","N/A","Ecoinvent  3.10, cut-off by allocation version","4f675495-4f98-5f79-a371-c2c6058b9c44_090f56b8-6a83-48c1-ae26-234d04771e53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_225","N/A","Ecoinvent  3.10, cut-off by allocation version","148e286c-d4ec-5f5e-963f-4885b6a2b777_090f56b8-6a83-48c1-ae26-234d04771e53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_226","N/A","Ecoinvent  3.10, cut-off by allocation version","bf668603-c28d-5404-ad4f-e012820f39cd_090f56b8-6a83-48c1-ae26-234d04771e53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_227","N/A","Ecoinvent  3.10, cut-off by allocation version","eb228975-9d25-5925-b69a-c8e84902b62e_720d079e-242b-4d52-9268-bc9ffa6b5692",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_228","N/A","Ecoinvent  3.10, cut-off by allocation version","93891b3d-fc01-5844-bbb4-fe1557bc6341_173bc101-dadb-4bd8-952b-41b1b6fe2d90",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_229","N/A","Ecoinvent  3.10, cut-off by allocation version","efae5ae5-e980-579a-8ee7-28158db7f8f9_090f56b8-6a83-48c1-ae26-234d04771e53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_230","N/A","Ecoinvent  3.10, cut-off by allocation version","981623e0-8473-506b-b3af-fc89de20bcde_55b795a2-886f-419e-af38-fba1b83fa51b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_231","N/A","Ecoinvent  3.10, cut-off by allocation version","92c0f64c-87a6-59ea-b488-323144cc8c0e_4ecf1190-7028-4038-89b0-79adeb3e98cc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_232","N/A","Ecoinvent  3.10, cut-off by allocation version","00ebb760-a02e-515c-9dfe-b781d470118b_4ecf1190-7028-4038-89b0-79adeb3e98cc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_233","N/A","Ecoinvent  3.10, cut-off by allocation version","cf362a67-e18f-5a40-9fa0-e643a45e6a62_559d5695-102a-4beb-9f7f-3db334c9b51d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_234","N/A","Ecoinvent  3.10, cut-off by allocation version","d44d5da7-2c10-5f1f-9917-98c45ce08b3a_559d5695-102a-4beb-9f7f-3db334c9b51d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_235","N/A","Ecoinvent  3.10, cut-off by allocation version","59b4a49a-2816-5dd8-9b51-9924118f0365_f9895e44-5657-47fc-8eec-a4985e2bce2e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_236","N/A","Ecoinvent  3.10, cut-off by allocation version","ad0df3ef-6a94-59d1-af03-bc56e857e73e_f9895e44-5657-47fc-8eec-a4985e2bce2e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_237","N/A","Ecoinvent  3.10, cut-off by allocation version","340d0a19-f856-5f39-ac1c-524141fdb9e5_f9895e44-5657-47fc-8eec-a4985e2bce2e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_238","N/A","Ecoinvent  3.10, cut-off by allocation version","85add2fa-4e0b-5f63-9d39-1e5b06c32761_fb655769-10d8-446b-87f8-44ca60e20ed9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_239","N/A","Ecoinvent  3.10, cut-off by allocation version","404e4cd3-7e0e-548a-b5da-caa303df3a0a_fb655769-10d8-446b-87f8-44ca60e20ed9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_240","N/A","Ecoinvent  3.10, cut-off by allocation version","a3cc68f5-42cc-5be6-9a06-5a5017a6002e_f4e8b38b-d6c7-423b-bc9c-13b4a13d55f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_241","N/A","Ecoinvent  3.10, cut-off by allocation version","c7d08a8a-88f3-59ed-a131-307882e1536a_f4e8b38b-d6c7-423b-bc9c-13b4a13d55f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_242","N/A","Ecoinvent  3.10, cut-off by allocation version","23c14cca-52f9-5221-b5bc-559d5c88c2b8_f4e8b38b-d6c7-423b-bc9c-13b4a13d55f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_243","N/A","Ecoinvent  3.10, cut-off by allocation version","ce890a2c-afd2-51a4-b713-9fa9504776d3_c691b775-a65a-4b77-a588-c8c6cd01c725",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_244","N/A","Ecoinvent  3.10, cut-off by allocation version","985c231e-686d-5cf9-b282-b5a65b6d8804_c691b775-a65a-4b77-a588-c8c6cd01c725",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_245","N/A","Ecoinvent  3.10, cut-off by allocation version","e174683a-0200-5604-8344-50d8dc1cc5ce_653ca70d-49a6-4c62-ae9c-56b3c00b647c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_246","N/A","Ecoinvent  3.10, cut-off by allocation version","8ab97ce9-f88a-5fd5-a0ea-a87423d4e704_653ca70d-49a6-4c62-ae9c-56b3c00b647c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_247","N/A","Ecoinvent  3.10, cut-off by allocation version","fbddbcba-a9d3-58ac-bc2b-48ce2eb52299_2341598f-166d-4f0c-97d2-0077a191b11f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_248","N/A","Ecoinvent  3.10, cut-off by allocation version","828774ce-d14c-5fbb-bc4a-0def4669a08b_2341598f-166d-4f0c-97d2-0077a191b11f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_249","N/A","Ecoinvent  3.10, cut-off by allocation version","823929ce-afe1-5101-ac27-ce3ca72fdc4b_518404fc-5571-4fc8-80a0-67c099278772",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_250","N/A","Ecoinvent  3.10, cut-off by allocation version","173c274e-1f24-5a22-a7cf-c1e18494f8ec_518404fc-5571-4fc8-80a0-67c099278772",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_251","N/A","Ecoinvent  3.10, cut-off by allocation version","58cd4158-59d2-5c8c-88ae-beb86849b3d6_bd061b71-270b-4644-9e14-6c59b2e4090d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_252","N/A","Ecoinvent  3.10, cut-off by allocation version","252a8945-d0af-539f-ba04-8752ca19433f_bd061b71-270b-4644-9e14-6c59b2e4090d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_253","N/A","Ecoinvent  3.10, cut-off by allocation version","3092ea07-a68d-5bc3-8f99-f548d345908e_c0a7ba59-f9b5-45b5-8e1d-6e4e40ba86df",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_254","N/A","Ecoinvent  3.10, cut-off by allocation version","939b9ef2-7989-5365-9574-58e1227a293f_c0a7ba59-f9b5-45b5-8e1d-6e4e40ba86df",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_255","N/A","Ecoinvent  3.10, cut-off by allocation version","1a631c39-2fb7-53dc-b38e-81785eacf070_c0a7ba59-f9b5-45b5-8e1d-6e4e40ba86df",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_256","N/A","Ecoinvent  3.10, cut-off by allocation version","ba34f3de-8ef3-5d30-af2b-30a69caf0332_03bf1369-1eec-49d0-bc4b-8b29efa826b9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_257","N/A","Ecoinvent  3.10, cut-off by allocation version","e44f7efa-8844-5bbb-a986-03a77f19fd34_03bf1369-1eec-49d0-bc4b-8b29efa826b9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_258","N/A","Ecoinvent  3.10, cut-off by allocation version","1cf1f7c7-2ee9-5d0b-9dcd-436d3b5afcc5_99598921-d5df-489f-b96c-7dd4ba6b36a6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_259","N/A","Ecoinvent  3.10, cut-off by allocation version","b709b6c8-56a2-5da8-a729-2d99f44d03a5_99598921-d5df-489f-b96c-7dd4ba6b36a6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_260","N/A","Ecoinvent  3.10, cut-off by allocation version","95486215-9779-5cfc-8da4-359a8ad5fc9e_99598921-d5df-489f-b96c-7dd4ba6b36a6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_261","N/A","Ecoinvent  3.10, cut-off by allocation version","5e220af0-494e-518a-94ef-8fe400b79001_ccc1fbd3-3877-43b6-a845-0c2ed8359c29",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_262","N/A","Ecoinvent  3.10, cut-off by allocation version","20a2cec2-2498-5e43-bebc-385df005d06b_ccc1fbd3-3877-43b6-a845-0c2ed8359c29",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_263","N/A","Ecoinvent  3.10, cut-off by allocation version","a5756ad5-ffd8-59b3-be93-a54efdf31524_cf34bfa7-b49b-4ca1-a94d-0eff5dbd23d8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_264","N/A","Ecoinvent  3.10, cut-off by allocation version","fce59ef5-0422-5a7e-951a-6b838c2d3a4d_cf34bfa7-b49b-4ca1-a94d-0eff5dbd23d8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_265","N/A","Ecoinvent  3.10, cut-off by allocation version","62316927-dd5d-5472-bc65-f9dbdda06597_da85af95-9191-4be6-aa68-e0a980c28785",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_266","N/A","Ecoinvent  3.10, cut-off by allocation version","23d0098d-d329-56fa-9e07-7b3a7bb767c3_da85af95-9191-4be6-aa68-e0a980c28785",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_267","N/A","Ecoinvent  3.10, cut-off by allocation version","62d9f625-531c-564d-8ae1-b14bec334f08_999d5179-2235-493a-8bd8-d805bb71eee8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_268","N/A","Ecoinvent  3.10, cut-off by allocation version","b1fe1a60-0200-5faa-aedc-730732ba1b2d_999d5179-2235-493a-8bd8-d805bb71eee8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_269","N/A","Ecoinvent  3.10, cut-off by allocation version","58ab1e7f-e02e-540a-8291-9241313ad640_ae39ee61-d4d0-4cce-93b4-0745344da5fa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_270","N/A","Ecoinvent  3.10, cut-off by allocation version","43b7ccf2-4840-596e-91d0-8bb374e9d599_ae39ee61-d4d0-4cce-93b4-0745344da5fa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_271","N/A","Ecoinvent  3.10, cut-off by allocation version","fa4c1c14-af58-5faa-8fcb-0ac283c9854d_ae39ee61-d4d0-4cce-93b4-0745344da5fa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_272","N/A","Ecoinvent  3.10, cut-off by allocation version","179dae39-5e28-5dd5-a8fa-ab7336cadafa_639dba7b-1762-4e9a-a95c-f30380e65d53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_273","N/A","Ecoinvent  3.10, cut-off by allocation version","ac148ceb-591d-5d05-b80d-b2a420db10f9_639dba7b-1762-4e9a-a95c-f30380e65d53",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_274","N/A","Ecoinvent  3.10, cut-off by allocation version","4a0ebfac-5c44-5475-86d6-e617d236b40e_24f5a760-85ea-4ed7-a4f2-cff90141671b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_275","N/A","Ecoinvent  3.10, cut-off by allocation version","6a52934c-e357-52ef-a33e-fa3420acc364_24f5a760-85ea-4ed7-a4f2-cff90141671b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_276","N/A","Ecoinvent  3.10, cut-off by allocation version","66352dc1-4469-5db8-b8c8-4111480f9766_24f5a760-85ea-4ed7-a4f2-cff90141671b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_277","N/A","Ecoinvent  3.10, cut-off by allocation version","975a8721-de91-5b10-b299-713b449be8d8_73585052-b3e9-4cde-832d-2db3272d2ae5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_278","N/A","Ecoinvent  3.10, cut-off by allocation version","14a7b03f-341f-5560-bb36-79a7de565718_73585052-b3e9-4cde-832d-2db3272d2ae5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_279","N/A","Ecoinvent  3.10, cut-off by allocation version","69b4fbb8-3991-575b-a26e-4eb864d7111b_a8523835-3905-4e3f-9e2f-ae1d8cad0317",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_280","N/A","Ecoinvent  3.10, cut-off by allocation version","e52061b7-a41f-500a-95b7-68e7977c04ef_a8523835-3905-4e3f-9e2f-ae1d8cad0317",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_281","N/A","Ecoinvent  3.10, cut-off by allocation version","81a1523d-cc38-58f7-8dc2-72f05aadcde7_8ddc8009-4733-49e9-8a4e-a1081d05eb8b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_282","N/A","Ecoinvent  3.10, cut-off by allocation version","7ecc69e1-15ca-5342-b246-ccc603b29c28_8ddc8009-4733-49e9-8a4e-a1081d05eb8b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_283","N/A","Ecoinvent  3.10, cut-off by allocation version","87653782-cc98-5a1b-8b4f-b7d1ca2c2941_3a40db23-1aed-4b82-8117-32251e039134",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_284","N/A","Ecoinvent  3.10, cut-off by allocation version","8f697305-28ed-55be-9512-b0456b77f4e2_3a40db23-1aed-4b82-8117-32251e039134",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_285","N/A","Ecoinvent  3.10, cut-off by allocation version","0f8768d4-90f1-55f3-a2d6-df33486935fe_b909dee2-76bd-4eae-87d5-fc831390f99b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_286","N/A","Ecoinvent  3.10, cut-off by allocation version","744b4753-4710-561f-96e9-5dd1152abb26_b909dee2-76bd-4eae-87d5-fc831390f99b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_287","N/A","Ecoinvent  3.10, cut-off by allocation version","e11cbcd9-a0ff-56a6-972c-4c686d948f56_b909dee2-76bd-4eae-87d5-fc831390f99b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_288","N/A","Ecoinvent  3.10, cut-off by allocation version","070a1713-7483-5465-b235-fea42f5d5de1_fea783cd-1b3e-47ed-a4a1-346094ebc39a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_289","N/A","Ecoinvent  3.10, cut-off by allocation version","b0856062-d28d-5019-bbad-03fa07c8f0f7_fea783cd-1b3e-47ed-a4a1-346094ebc39a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_290","N/A","Ecoinvent  3.10, cut-off by allocation version","fe02497f-fd5a-5c70-b6ca-480ea5776bda_93afc03f-5832-4ec0-8d76-cf6e62efff26",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_291","N/A","Ecoinvent  3.10, cut-off by allocation version","0edfde13-47ea-5462-964c-e1c8e21f72c3_93afc03f-5832-4ec0-8d76-cf6e62efff26",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_292","N/A","Ecoinvent  3.10, cut-off by allocation version","fd1b4b7c-49bc-584a-afb9-ff6395f4aec1_93afc03f-5832-4ec0-8d76-cf6e62efff26",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_293","N/A","Ecoinvent  3.10, cut-off by allocation version","378e389c-69c5-55fb-8d24-47ea16e992fb_52a8f3c4-df5d-4f18-830b-985bcd8ac830",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_294","N/A","Ecoinvent  3.10, cut-off by allocation version","904e0110-39da-5898-88a0-a706d3d2352e_52a8f3c4-df5d-4f18-830b-985bcd8ac830",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_295","N/A","Ecoinvent  3.10, cut-off by allocation version","222fe198-231d-5875-b2d7-e6fd6832e71d_eee5f6b0-7c73-473a-9e27-82d38ae3661b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_296","N/A","Ecoinvent  3.10, cut-off by allocation version","b25a4f38-1940-5159-97cc-e3870f94f8ed_eee5f6b0-7c73-473a-9e27-82d38ae3661b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_297","N/A","Ecoinvent  3.10, cut-off by allocation version","d0adf2c8-b203-5aee-aeff-205f93339c92_eeb68c18-502b-4117-a033-a5daf24322fc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_298","N/A","Ecoinvent  3.10, cut-off by allocation version","951bece1-40e9-52c6-886e-2a0beaab9959_2741cea8-327f-4e0f-9401-b10858dc68f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_299","N/A","Ecoinvent  3.10, cut-off by allocation version","1220dda3-c78a-55c1-97cf-d68700f14716_82befb8d-fc52-4942-b53f-67b526eb0c25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_300","N/A","Ecoinvent  3.10, cut-off by allocation version","28cc53c0-f97f-56f5-b52b-0f23316c21b5_b41ed270-f3f0-4126-b391-8c9ac9076d3b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_301","N/A","Ecoinvent  3.10, cut-off by allocation version","e348cde9-a345-5592-98ae-112c644b316b_6fcb39b4-3030-47b1-872e-a84c23dca79b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_302","N/A","Ecoinvent  3.10, cut-off by allocation version","34a9a389-ad3e-5265-b239-4504047d0cd5_a34be1fd-b392-4901-9602-f7d25e46426d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_303","N/A","Ecoinvent  3.10, cut-off by allocation version","e83a1735-5822-524c-ab09-921892bd1e11_a34be1fd-b392-4901-9602-f7d25e46426d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_304","N/A","Ecoinvent  3.10, cut-off by allocation version","739a1ba3-2a34-5792-b658-1abb326f8fa2_6bcb7d07-3c26-45c4-a87a-ead2ac75a66a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_305","N/A","Ecoinvent  3.10, cut-off by allocation version","f3aac569-4617-529d-93b8-9d8f643c4001_6bcb7d07-3c26-45c4-a87a-ead2ac75a66a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_306","N/A","Ecoinvent  3.10, cut-off by allocation version","6c31a4d3-a7f1-5ea8-9c0e-f556c4f46bc7_8d950031-fee3-4f3c-9bc1-889f6be31ea9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_307","N/A","Ecoinvent  3.10, cut-off by allocation version","30b6bcc3-ce9c-5307-912c-b1d117cc864a_8d950031-fee3-4f3c-9bc1-889f6be31ea9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_308","N/A","Ecoinvent  3.10, cut-off by allocation version","b9900f9a-5325-5bf1-ab5b-ee157c17cff6_1f4388f9-8a79-452d-8364-802a5bc5f548",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_309","N/A","Ecoinvent  3.10, cut-off by allocation version","f5f8b61f-76aa-5cf8-a5f5-3d7520953713_1f4388f9-8a79-452d-8364-802a5bc5f548",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_310","N/A","Ecoinvent  3.10, cut-off by allocation version","ead5f7a9-77c2-5c16-b304-5059c55254da_095528f2-b554-4cfb-9dc8-764b50bcbd7b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_311","N/A","Ecoinvent  3.10, cut-off by allocation version","99a9db3c-0727-5d27-a857-54eeb698e923_095528f2-b554-4cfb-9dc8-764b50bcbd7b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_312","N/A","Ecoinvent  3.10, cut-off by allocation version","c0bb7ead-2118-5870-930c-682920ed4d7b_7e02ffad-fa75-41ed-94f1-3d9c6f7e91bd",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_313","N/A","Ecoinvent  3.10, cut-off by allocation version","c3b92350-9ce1-5621-95f3-d3b04a1fff83_7e02ffad-fa75-41ed-94f1-3d9c6f7e91bd",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_314","N/A","Ecoinvent  3.10, cut-off by allocation version","9a5a217b-43ae-5c56-9969-bdffb869484a_4309fd1b-7875-491c-b158-65d8f5e2c663",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_315","N/A","Ecoinvent  3.10, cut-off by allocation version","13c79c73-181d-574f-a550-6cf13b119223_4309fd1b-7875-491c-b158-65d8f5e2c663",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_316","N/A","Ecoinvent  3.10, cut-off by allocation version","e2bc85d5-fa6a-5c4a-bfca-37883857bebd_3f225a75-4661-454e-9671-1b3e893ba72d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_317","N/A","Ecoinvent  3.10, cut-off by allocation version","d5d281ec-6086-5387-a7a8-966b07b38635_3f225a75-4661-454e-9671-1b3e893ba72d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_318","N/A","Ecoinvent  3.10, cut-off by allocation version","49e93c17-2909-57b9-bb74-1273959cab65_58f087c9-c348-4c55-bdc4-9805b5a0239a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_319","N/A","Ecoinvent  3.10, cut-off by allocation version","5c856191-f59f-5683-9563-6eaf5e4d1cf8_58f087c9-c348-4c55-bdc4-9805b5a0239a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_320","N/A","Ecoinvent  3.10, cut-off by allocation version","5072fda9-eb49-5be1-a6d6-d3aea58cdab4_ed65d3d9-349b-4e2c-870c-381209bc1484",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_321","N/A","Ecoinvent  3.10, cut-off by allocation version","2f7b2fcc-dbe0-5c51-9aab-38f05325d26e_ed65d3d9-349b-4e2c-870c-381209bc1484",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_322","N/A","Ecoinvent  3.10, cut-off by allocation version","fcf3ec5d-2c81-5d7d-bf1a-447474af504e_1305164c-678e-426b-95ff-b41e03e68aac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_323","N/A","Ecoinvent  3.10, cut-off by allocation version","718089a6-b151-5652-b61f-8ebdc1f8551e_1305164c-678e-426b-95ff-b41e03e68aac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_324","N/A","Ecoinvent  3.10, cut-off by allocation version","b06e2cba-f277-5e04-97cd-4987a78433a6_85a9dd8c-769e-4528-9a1a-105ab3269262",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_325","N/A","Ecoinvent  3.10, cut-off by allocation version","abba7741-1409-5783-96c4-343644af9a8b_85a9dd8c-769e-4528-9a1a-105ab3269262",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_326","N/A","Ecoinvent  3.10, cut-off by allocation version","4093ccfd-6e4a-55f9-ad27-b0b5e5b23b84_d710f3b0-f618-4627-83ed-bc53b82d26fc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_327","N/A","Ecoinvent  3.10, cut-off by allocation version","9b8bc605-7223-5622-bee0-6ab902651e24_ef9d859f-c740-4c1f-8f76-d4faddda1f9f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_328","N/A","Ecoinvent  3.10, cut-off by allocation version","edfa6868-06a1-515c-97dd-a2e7f2d0282c_ef9d859f-c740-4c1f-8f76-d4faddda1f9f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_329","N/A","Ecoinvent  3.10, cut-off by allocation version","59d894f1-3988-5e1f-996d-16eb40afb4be_692784c6-00e8-4309-971d-3fd8441120f1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_330","N/A","Ecoinvent  3.10, cut-off by allocation version","6b24f636-031b-5e7f-a376-34be6edb5ca7_692784c6-00e8-4309-971d-3fd8441120f1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_331","N/A","Ecoinvent  3.10, cut-off by allocation version","21870d94-54c0-5e13-aa4a-361023ef9097_9f2d5d73-1014-49ec-87ee-c6a6ed86b3d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_332","N/A","Ecoinvent  3.10, cut-off by allocation version","d2688e57-cf10-55a2-a64f-5e60fa5dcdf3_9f2d5d73-1014-49ec-87ee-c6a6ed86b3d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_333","N/A","Ecoinvent  3.10, cut-off by allocation version","cdf5199a-a55b-523e-8622-0e6a041880cb_3bf68190-17bd-4506-84da-3ef2bcb1b624",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_334","N/A","Ecoinvent  3.10, cut-off by allocation version","e0dbd35b-93b4-5dc1-ae1d-c62fee68ba4f_3bf68190-17bd-4506-84da-3ef2bcb1b624",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_335","N/A","Ecoinvent  3.10, cut-off by allocation version","8b93d34b-af3a-56cd-a6eb-dec7ac9b23e4_bf2ab99f-4704-4e62-958d-ec8efd2e1c1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_336","N/A","Ecoinvent  3.10, cut-off by allocation version","34f67d3e-c509-562a-9cc1-1f08e4ce9733_bf2ab99f-4704-4e62-958d-ec8efd2e1c1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_337","N/A","Ecoinvent  3.10, cut-off by allocation version","f736e877-5bc7-5ee3-ba36-1883aacb7597_e110266e-a20e-41ae-a5f6-7dbcf0935abd",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_338","N/A","Ecoinvent  3.10, cut-off by allocation version","be5aef40-bb22-51d6-80e4-dceaba4a11b9_e110266e-a20e-41ae-a5f6-7dbcf0935abd",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_339","N/A","Ecoinvent  3.10, cut-off by allocation version","9f41504d-db63-5ef6-a45c-596fe14f87e2_65e289a5-e378-41e7-9a41-bd51db029439",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_340","N/A","Ecoinvent  3.10, cut-off by allocation version","fe8577da-d422-555f-bb4b-16e6208c60fc_65e289a5-e378-41e7-9a41-bd51db029439",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_341","N/A","Ecoinvent  3.10, cut-off by allocation version","e3aa5b47-dee2-565e-b624-80b07286d7df_e095e692-5ebc-4bc5-89bc-8379bbc181f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_342","N/A","Ecoinvent  3.10, cut-off by allocation version","43d94a78-a534-52a7-90e9-8aa436f4b6fe_e095e692-5ebc-4bc5-89bc-8379bbc181f8",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_343","N/A","Ecoinvent  3.10, cut-off by allocation version","78f01775-083d-5885-af19-966c50e71295_e6f8dc95-a570-4a09-91cf-47c046e669e9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_344","N/A","Ecoinvent  3.10, cut-off by allocation version","c9697774-068e-5309-bee8-bfbe94956071_e6f8dc95-a570-4a09-91cf-47c046e669e9",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_345","N/A","Ecoinvent  3.10, cut-off by allocation version","547a502a-d976-5861-bb6d-ec724fa18dbd_93d5bc32-a832-4ac1-960a-6705cdfaddc2",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_346","N/A","Ecoinvent  3.10, cut-off by allocation version","c0f8e8d3-371c-57e1-9226-022bb6157cc2_93d5bc32-a832-4ac1-960a-6705cdfaddc2",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_347","N/A","Ecoinvent  3.10, cut-off by allocation version","f988aa00-7f79-5161-bf6b-7b474acbda28_8f99cbf5-83d9-4989-aaa6-65bcedd82df1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_348","N/A","Ecoinvent  3.10, cut-off by allocation version","cedf4205-0da1-599e-8b44-20931c743d30_8f99cbf5-83d9-4989-aaa6-65bcedd82df1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_349","N/A","Ecoinvent  3.10, cut-off by allocation version","c6bad917-303f-568e-9187-6c293e03f3ed_c91eabe2-800b-48a3-9bc3-c46bbcfbdd5f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_350","N/A","Ecoinvent  3.10, cut-off by allocation version","f983eb56-1629-50b7-8dda-00c274159921_c91eabe2-800b-48a3-9bc3-c46bbcfbdd5f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_351","N/A","Ecoinvent  3.10, cut-off by allocation version","9f5ad98c-0c70-5727-8a5d-632b3100b85f_2496b794-9414-40bf-8545-5b84925b2f5f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_352","N/A","Ecoinvent  3.10, cut-off by allocation version","d1e2c45e-852b-5949-938f-e5681e00868c_2496b794-9414-40bf-8545-5b84925b2f5f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_353","N/A","Ecoinvent  3.10, cut-off by allocation version","d5e1f703-86be-5fae-ab89-694ad599f04c_54397bee-f5a8-4164-a43e-5dff00da3b10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_354","N/A","Ecoinvent  3.10, cut-off by allocation version","0495d309-6798-5ef4-8f3d-1460e1adb698_54397bee-f5a8-4164-a43e-5dff00da3b10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_355","N/A","Ecoinvent  3.10, cut-off by allocation version","50874e9f-6092-5b40-9e7c-07dd296f6dfe_ab08966c-085c-4cdf-9c2b-c137eee358c0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_356","N/A","Ecoinvent  3.10, cut-off by allocation version","bd00c8f2-5b6c-550c-8716-0cdc89aa7030_ab08966c-085c-4cdf-9c2b-c137eee358c0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Road freight and transportation"]
[null,"OSW_SE_357","N/A","Ecoinvent  3.10, cut-off by allocation version","7b6abd95-be0e-5f44-8748-52a78a8e9083_068bf76a-bfaa-435c-85ed-3d2bb2c4bb4f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_358","N/A","Ecoinvent  3.10, cut-off by allocation version","2205ef31-4fe2-588f-95de-4fce4b2eb64f_068bf76a-bfaa-435c-85ed-3d2bb2c4bb4f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_359","N/A","Ecoinvent  3.10, cut-off by allocation version","49b22a98-176e-5b26-baa2-7d42532d9ad3_57143a43-20ab-44a5-a4a2-26effbdfafd1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_360","N/A","Ecoinvent  3.10, cut-off by allocation version","686983ca-8d05-563c-93f5-bbea3eb2bde9_57143a43-20ab-44a5-a4a2-26effbdfafd1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Freight and transportation","Sea freight and transportation"]
[null,"OSW_SE_361","N/A","Ecoinvent  3.10, cut-off by allocation version","4fb98a7a-b8c5-5b75-bc2b-dce7b0d49807_58b3db4e-19b8-43f2-8545-55229a5ee6e4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured assets","Cables"]
[null,"OSW_SE_362","N/A","Ecoinvent  3.10, cut-off by allocation version","8ec15097-54d0-592c-b814-ba9cf48cf9fc_8b988c18-f03b-46aa-83ae-d72d4639ff76",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured assets","Cables"]
[null,"OSW_SE_363","N/A","Ecoinvent  3.10, cut-off by allocation version","f82c7f4c-6690-514e-83af-7f79b5bee0dd_1692f537-b2ad-4143-bea3-226fc2fe9cf5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured assets","Wind turbine generators (WTG)"]
[null,"OSW_SE_364","N/A","Ecoinvent  3.10, cut-off by allocation version","ed7cf3b3-9b6d-5cd3-901f-2d36423c3a75_787cf1f4-ff36-4548-8a99-9adb6c4f8f23",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured components","Nacelle and internals"]
[null,"OSW_SE_365","N/A","Ecoinvent  3.10, cut-off by allocation version","2bf7943e-88ea-5a35-b5b2-6ee3d239bf07_9e2c266f-d04d-44bc-b277-b7f6a7e3dffa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured components","Transformer"]
[null,"OSW_SE_366","N/A","Ecoinvent  3.10, cut-off by allocation version","7ce3820e-523d-57fc-a959-328a99cabb00_0c7faf73-f5ea-4a3b-96ec-54d025cae6f4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Fully manufactured components","Transformer"]
[null,"OSW_SE_367","N/A","Ecoinvent  3.10, cut-off by allocation version","55945c81-d448-5182-9ef6-dd416454afca_d187adaf-a08d-4f75-a1ba-bb46c4597f45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Coating and galvanising processes"]
[null,"OSW_SE_368","N/A","Ecoinvent  3.10, cut-off by allocation version","c8f3325c-b8a7-50f8-a788-1e67e8fd1553_d187adaf-a08d-4f75-a1ba-bb46c4597f45",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Coating and galvanising processes"]
[null,"OSW_SE_369","N/A","Ecoinvent  3.10, cut-off by allocation version","2a55050a-229b-5ed3-b17a-7133009d9a15_9087eb5f-4662-4cb1-a524-f5cb80b1238a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_370","N/A","Ecoinvent  3.10, cut-off by allocation version","d113489b-113e-5059-bc92-cd9f315a7e17_9087eb5f-4662-4cb1-a524-f5cb80b1238a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_371","N/A","Ecoinvent  3.10, cut-off by allocation version","001c496b-8ad1-5743-b901-836dfa6ff00a_06194d2b-4c2b-44de-9a29-1a364616a1d2",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_372","N/A","Ecoinvent  3.10, cut-off by allocation version","50ad4ffb-c431-5396-a1c8-956edcc22895_06194d2b-4c2b-44de-9a29-1a364616a1d2",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_373","N/A","Ecoinvent  3.10, cut-off by allocation version","4e273f0f-2246-5126-a337-1e06c7f7eb48_ee8d31fc-f67f-43b2-910d-172880730b28",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_374","N/A","Ecoinvent  3.10, cut-off by allocation version","8c498881-1eb5-56a6-90c9-70304184913f_ee8d31fc-f67f-43b2-910d-172880730b28",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Joining and welding processes"]
[null,"OSW_SE_375","N/A","Ecoinvent  3.10, cut-off by allocation version","a8c9b91b-3788-582e-9dd3-b40f95af6453_cdb7b939-f508-49ed-80f3-b39f6137fe1c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_376","N/A","Ecoinvent  3.10, cut-off by allocation version","80ee09d6-809f-5ac9-80bf-64d001b28fab_444d81a0-13e0-41a4-8f63-e691b0133c04",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_377","N/A","Ecoinvent  3.10, cut-off by allocation version","f2511240-f350-53bf-b18f-7dc82d379af2_579049d0-3db8-4496-a234-2f61ed28a72b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_378","N/A","Ecoinvent  3.10, cut-off by allocation version","5bc75a9c-cb54-5327-8071-2f31486dbb90_579049d0-3db8-4496-a234-2f61ed28a72b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_379","N/A","Ecoinvent  3.10, cut-off by allocation version","49c0e19b-cdc5-52fc-888a-acc07c402d99_406ae9de-8894-4c8b-a601-40b7e849b66d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_380","N/A","Ecoinvent  3.10, cut-off by allocation version","07da644f-d126-5faf-82fd-056715b7e44c_406ae9de-8894-4c8b-a601-40b7e849b66d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_381","N/A","Ecoinvent  3.10, cut-off by allocation version","accecafc-3aea-5df7-ad09-de1949ddb26d_8ad0b079-38b6-4700-8462-74648a4edd7d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_382","N/A","Ecoinvent  3.10, cut-off by allocation version","3f7d1c92-5a70-5468-8ca0-b0da9b8af829_425089e2-ad80-414f-b6eb-67b32f5aa626",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_383","N/A","Ecoinvent  3.10, cut-off by allocation version","4ce56f07-081d-5ee4-b8aa-11448cdd7f5b_a5309c08-cc71-402e-b870-163a09ee0742",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_384","N/A","Ecoinvent  3.10, cut-off by allocation version","34d5c2a1-6eae-5bfe-a340-d1ec4298fb8d_a5309c08-cc71-402e-b870-163a09ee0742",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_385","N/A","Ecoinvent  3.10, cut-off by allocation version","eba86c08-c6ca-5ca0-a73c-55db44dee8bc_68b4fdd4-d341-4ac5-9dbc-59eb34653dab",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_386","N/A","Ecoinvent  3.10, cut-off by allocation version","56c28af4-c4e1-595b-bfcf-4cf98be56b0f_68b4fdd4-d341-4ac5-9dbc-59eb34653dab",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_387","N/A","Ecoinvent  3.10, cut-off by allocation version","beeba0ad-c2be-5ee3-b3dc-ef2f79aaf12a_dfbdd39b-2541-4069-9b87-ab61ef6fbc0c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_388","N/A","Ecoinvent  3.10, cut-off by allocation version","1e7cd149-2dd9-510a-a001-0fa9d5f40c7f_dfbdd39b-2541-4069-9b87-ab61ef6fbc0c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_389","N/A","Ecoinvent  3.10, cut-off by allocation version","1069c9d1-790a-5676-90ce-93ee690abf7c_e2f62697-57d4-42fe-95bf-c85fd32a9cf0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_390","N/A","Ecoinvent  3.10, cut-off by allocation version","87cc6df1-c49e-5fc0-b399-c2803ab13e0b_e2f62697-57d4-42fe-95bf-c85fd32a9cf0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Manufacturing processes","Material processing"]
[null,"OSW_SE_391","N/A","Ecoinvent  3.10, cut-off by allocation version","b180f717-b151-51e6-b27d-958075016be3_fef44ccb-917e-4c8d-bb35-a1898827b659",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Aluminium"]
[null,"OSW_SE_392","N/A","Ecoinvent  3.10, cut-off by allocation version","a1933dcd-abae-5bf4-bf34-f7b363be5b2e_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Aluminium"]
[null,"OSW_SE_393","N/A","Ecoinvent  3.10, cut-off by allocation version","d95292fe-49d6-5760-b82f-18ecc1136cd8_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Aluminium"]
[null,"OSW_SE_394","N/A","Ecoinvent  3.10, cut-off by allocation version","1e469dc6-d56a-57b5-87b3-df303bc1b2c9_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Aluminium"]
[null,"OSW_SE_395","N/A","Ecoinvent  3.10, cut-off by allocation version","caf41f87-e599-5995-b00c-46cbecc66aee_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_396","N/A","Ecoinvent  3.10, cut-off by allocation version","16aee8f7-1c95-5b49-82e8-94e23f073a3e_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_397","N/A","Ecoinvent  3.10, cut-off by allocation version","76941379-c364-501e-9008-a9c7e9fc78e0_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_398","N/A","Ecoinvent  3.10, cut-off by allocation version","d56f7390-6003-5462-b350-779a9faf202c_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_399","N/A","Ecoinvent  3.10, cut-off by allocation version","c625b7d3-07c9-5ac7-808b-95dc2e5befdf_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_400","N/A","Ecoinvent  3.10, cut-off by allocation version","f1865053-b23d-5d6b-b431-cde2ed998e08_eb266390-532c-4f14-ba91-a1e1b688cf5c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_401","N/A","Ecoinvent  3.10, cut-off by allocation version","fe92458a-3144-5b27-9cfa-0532321840ee_eee95138-58c8-4172-9b1f-754ba074325d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Concrete"]
[null,"OSW_SE_402","N/A","Ecoinvent  3.10, cut-off by allocation version","f8566db2-34aa-52fc-8b62-b94bbeb5cfff_fbb039f7-f9cc-46d2-b631-313ddb125c1a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Copper"]
[null,"OSW_SE_403","N/A","Ecoinvent  3.10, cut-off by allocation version","58bc6741-6d78-5d59-b143-166b6e7f452d_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Copper"]
[null,"OSW_SE_404","N/A","Ecoinvent  3.10, cut-off by allocation version","ad21b0ab-468b-5685-b30e-750027985868_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Copper"]
[null,"OSW_SE_405","N/A","Ecoinvent  3.10, cut-off by allocation version","ecf8173e-692c-5c30-8bd3-f6eb005e72b7_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Copper"]
[null,"OSW_SE_406","N/A","Ecoinvent  3.10, cut-off by allocation version","dbb7dbf7-9d69-5a0e-b5ad-4e0f9b61154e_ea75b944-c676-4a13-85b8-2bea98f765a4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Oils and lubricants"]
[null,"OSW_SE_407","N/A","Ecoinvent  3.10, cut-off by allocation version","c17266f3-3f87-5ed7-ad2b-410db3d5ed1c_ea75b944-c676-4a13-85b8-2bea98f765a4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Oils and lubricants"]
[null,"OSW_SE_408","N/A","Ecoinvent  3.10, cut-off by allocation version","46b016c1-ff92-580f-93ee-562fc9b536f4_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_409","N/A","Ecoinvent  3.10, cut-off by allocation version","65839b8f-704e-57f2-a5eb-b9d982aab4f6_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_410","N/A","Ecoinvent  3.10, cut-off by allocation version","28e3e418-2bf5-58a9-a652-62cef90dced0_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_411","N/A","Ecoinvent  3.10, cut-off by allocation version","010faf91-efb8-5ecf-9e2c-1c20e866c179_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_412","N/A","Ecoinvent  3.10, cut-off by allocation version","fdb6a609-1928-55b4-b500-e433b8eaca01_37eceabd-b33f-4757-a4b9-5c51dee1710d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_413","N/A","Ecoinvent  3.10, cut-off by allocation version","c8ac0a8d-bc59-50ad-9e5e-e400d16040a4_237b35c6-69e1-49c4-8e99-0be6c1b1806e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_414","N/A","Ecoinvent  3.10, cut-off by allocation version","12a91e30-b1e5-501b-bf31-17e6ffc49ac6_71d0cff1-7f13-4476-94a9-4eaaec98d225",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_415","N/A","Ecoinvent  3.10, cut-off by allocation version","b8a94ec9-0189-5acc-b565-c7ae3e1f0f82_55cd1ee7-9869-4248-8800-1be2f66267aa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_416","N/A","Ecoinvent  3.10, cut-off by allocation version","87280257-a49a-500b-8b78-ef80cf493f4b_a95b9d49-4114-40c6-9929-0c6c79db22d1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_417","N/A","Ecoinvent  3.10, cut-off by allocation version","e7eb6c4f-f145-5417-9332-03c0300d774d_8be1b6bc-2fc3-5489-91dc-5861064039c6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_418","N/A","Ecoinvent  3.10, cut-off by allocation version","b87db45b-f2cc-5666-8024-0396e729420e_8be1b6bc-2fc3-5489-91dc-5861064039c6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_419","N/A","Ecoinvent  3.10, cut-off by allocation version","9b0f80c5-2042-5223-a7a6-81c33c25576a_d1c50e71-41bf-40ea-a259-0fc490c8e0c5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_420","N/A","Ecoinvent  3.10, cut-off by allocation version","a6acbf9f-8fe2-57bf-8fe2-641091c778cb_23fccced-e1e5-421d-9abe-5b59c51a862e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_421","N/A","Ecoinvent  3.10, cut-off by allocation version","238d13e8-d030-5a86-a33c-a72ed008ffa4_475e90d0-9d93-4baa-b5ac-c30966c74554",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_422","N/A","Ecoinvent  3.10, cut-off by allocation version","a1e2e13c-709c-5193-a0ae-7d254b5ff6a5_7fbe7184-9e9e-4a21-bd42-fa630266af1d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_423","N/A","Ecoinvent  3.10, cut-off by allocation version","f90ee562-ca1b-538e-b036-9d424d63f9ce_ab5dcfa8-e8f9-4923-84d4-51b25a898fa1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_424","N/A","Ecoinvent  3.10, cut-off by allocation version","841fac9a-07f7-5971-8850-db808d37ca79_ab5dcfa8-e8f9-4923-84d4-51b25a898fa1",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_425","N/A","Ecoinvent  3.10, cut-off by allocation version","6bc62aa5-2761-5f69-8601-321a0f214789_a8f9b840-05ff-4dad-b11e-dd4b1342655d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_426","N/A","Ecoinvent  3.10, cut-off by allocation version","c0d35bc8-0bcc-5f87-82d1-4cd4255afc44_a8f9b840-05ff-4dad-b11e-dd4b1342655d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_427","N/A","Ecoinvent  3.10, cut-off by allocation version","6f3ee6e4-8734-5b2d-8648-603c46d2f48b_136f89b3-af52-4826-97f7-cc35f80f226f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_428","N/A","Ecoinvent  3.10, cut-off by allocation version","cb8e0506-9969-50a7-898e-8499d8475f84_0da5307e-df93-4bc2-b5bc-6cda3cb55e8c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_429","N/A","Ecoinvent  3.10, cut-off by allocation version","127e7bd3-8201-5e27-93dc-4a114e95717a_77ad34b3-7b53-412e-afbb-0536fb8d5c6a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_430","N/A","Ecoinvent  3.10, cut-off by allocation version","aa8c356a-ea38-54eb-ae06-c545162c5878_d2aea801-6631-4070-939b-7b6d6b73bee5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Other materials"]
[null,"OSW_SE_431","N/A","Ecoinvent  3.10, cut-off by allocation version","872c4aa2-3aa5-5bf5-96ac-1771913ee4e5_b685192a-e033-421e-9074-8fe7cb176046",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_432","N/A","Ecoinvent  3.10, cut-off by allocation version","3165ffe2-7818-5bad-8259-cbc2733e7e54_947a85fa-114e-4d9e-b36c-3293e48ea5ae",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_433","N/A","Ecoinvent  3.10, cut-off by allocation version","b2f45e60-786c-5d39-a2ad-0c1c0aab6996_51c7e57a-00b7-4412-b56c-94c17b211ee7",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_434","N/A","Ecoinvent  3.10, cut-off by allocation version","ea39941b-639c-5c1a-ae80-ef0186a646c1_51c7e57a-00b7-4412-b56c-94c17b211ee7",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_435","N/A","Ecoinvent  3.10, cut-off by allocation version","4b0071c5-fc6d-5d56-9c17-da4c109ebe3e_102d2161-b570-42cd-b646-1c44e47d23c5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_436","N/A","Ecoinvent  3.10, cut-off by allocation version","ba14254b-6e7e-5786-aed1-73d5b4eece87_0798a5d1-6713-4c82-8ec9-c40ac2548279",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_437","N/A","Ecoinvent  3.10, cut-off by allocation version","7bdb6eec-ac75-503d-a68e-631d0c0857aa_f891d553-f8e5-4990-a56f-d032d9ec87f0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_438","N/A","Ecoinvent  3.10, cut-off by allocation version","e394b797-b3b8-5e9c-8a42-ebb2254156b7_f891d553-f8e5-4990-a56f-d032d9ec87f0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_439","N/A","Ecoinvent  3.10, cut-off by allocation version","90fee2a4-3631-51af-b81e-87a21a860ae6_fb4bb128-084e-4da3-8227-2ef8ad95da13",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_440","N/A","Ecoinvent  3.10, cut-off by allocation version","3e8c45cf-7645-531f-bbf9-da014e5d7324_fb4bb128-084e-4da3-8227-2ef8ad95da13",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_441","N/A","Ecoinvent  3.10, cut-off by allocation version","68720841-0b02-5bf0-82cd-d8c27385a316_d2aea801-6631-4070-939b-7b6d6b73bee5",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_442","N/A","Ecoinvent  3.10, cut-off by allocation version","109a925c-18ef-57c3-bc0a-c8487f69b169_d16b5d3f-b5e4-45b6-9a04-23cde05220c0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_443","N/A","Ecoinvent  3.10, cut-off by allocation version","1489f27b-e471-59b4-9bd2-d1ec6b6680e0_d16b5d3f-b5e4-45b6-9a04-23cde05220c0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_444","N/A","Ecoinvent  3.10, cut-off by allocation version","8306ad5f-8079-5e87-aca6-edfdf0a9b7b6_6af79823-cba0-4b75-96eb-e7c161eed14e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_445","N/A","Ecoinvent  3.10, cut-off by allocation version","d97c9825-79d0-5013-a015-eecd61881f72_6af79823-cba0-4b75-96eb-e7c161eed14e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_446","N/A","Ecoinvent  3.10, cut-off by allocation version","16470154-dafe-59a0-9d4f-e31ec70fdac4_b167bcef-715e-4136-a743-2fae79a086d3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_447","N/A","Ecoinvent  3.10, cut-off by allocation version","e9a7f967-42c0-5621-ba80-8cdb0a11353a_b167bcef-715e-4136-a743-2fae79a086d3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_448","N/A","Ecoinvent  3.10, cut-off by allocation version","9874d54a-4279-53e9-bac1-2d6f9ba0d26f_6826a703-2476-42f3-bb7c-4f32594ab030",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_449","N/A","Ecoinvent  3.10, cut-off by allocation version","50dd7c19-06f3-584b-a483-84d0afcaea1a_6826a703-2476-42f3-bb7c-4f32594ab030",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_450","N/A","Ecoinvent  3.10, cut-off by allocation version","5e47916e-26cb-51fb-951f-2562a9f57009_e0d6f217-d1e3-4d5d-8b8a-b13c846d4ad6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_451","N/A","Ecoinvent  3.10, cut-off by allocation version","2faaa3fa-adb2-5438-9700-252557481563_e0d6f217-d1e3-4d5d-8b8a-b13c846d4ad6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_452","N/A","Ecoinvent  3.10, cut-off by allocation version","5e783490-2ff3-59a0-bbbc-b07693e18a4b_66ca2f38-5e51-4546-83c0-d7cef0c55c7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Polymers"]
[null,"OSW_SE_453","N/A","Ecoinvent  3.10, cut-off by allocation version","40e32cec-0e36-5282-a540-9dc9fb4a7015_c33b5236-001e-49b5-aa3d-810c0214f9ce",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_454","N/A","Ecoinvent  3.10, cut-off by allocation version","1873afb0-8b20-580a-947e-63428cd2e791_c5246dbb-0abd-4bee-8dda-d52a1b202322",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_455","N/A","Ecoinvent  3.10, cut-off by allocation version","42eeb16c-7cb5-5cf4-9cba-1f537548f1af_817c3650-4fed-4ef2-b9b6-404a198834e6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_456","N/A","Ecoinvent  3.10, cut-off by allocation version","b72ee1aa-fc2e-51f8-9727-3ff33bdcea30_8cb650d5-8a48-4719-81b1-2080b3b4387f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_457","N/A","Ecoinvent  3.10, cut-off by allocation version","f3237d3d-1189-527c-a8b5-1b539c4ae4ef_a2fd8c95-f2db-436a-9f24-f33b17f7975b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_458","N/A","Ecoinvent  3.10, cut-off by allocation version","42de1cab-a735-530b-b4da-bc7eb1dbcc05_9ba48284-0f03-4fec-800d-de77833b12f6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_459","N/A","Ecoinvent  3.10, cut-off by allocation version","22decb26-3e6b-57a8-a27c-63edaf7fb880_4447af36-0897-4b00-8fd0-fd6a446dda6a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_460","N/A","Ecoinvent  3.10, cut-off by allocation version","7d8bfc44-ded8-5f97-b548-d3423b7f9ba9_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_461","N/A","Ecoinvent  3.10, cut-off by allocation version","2af26239-73ec-59ff-9821-1f4b86764c4e_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_462","N/A","Ecoinvent  3.10, cut-off by allocation version","8fc39dbb-3585-54e0-960e-35ca31de018a_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_463","N/A","Ecoinvent  3.10, cut-off by allocation version","29a5e34d-859e-5eb2-a295-2cb0f98877fd_3da25df2-438a-4e27-9141-4393f3b6f86f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_464","N/A","Ecoinvent  3.10, cut-off by allocation version","4febbf1f-bfd7-5868-9111-49708facb47f_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_465","N/A","Ecoinvent  3.10, cut-off by allocation version","cbed0288-184f-53df-84d4-c64c970f2fb7_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Materials","Steel"]
[null,"OSW_SE_466","N/A","Ecoinvent  3.10, cut-off by allocation version","cc57a51b-bf5a-53bb-9c7e-2b1d50f03f89_50306184-2a7e-4825-8e5d-fe8e674d1274",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_467","N/A","Ecoinvent  3.10, cut-off by allocation version","1f7b0c60-3b3a-5479-961c-fac0a5de20f5_50306184-2a7e-4825-8e5d-fe8e674d1274",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_468","N/A","Ecoinvent  3.10, cut-off by allocation version","60bc5c0f-653c-552b-8488-4f454cd31192_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_469","N/A","Ecoinvent  3.10, cut-off by allocation version","48e8b526-1176-5973-8caa-13e4c254793d_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_470","N/A","Ecoinvent  3.10, cut-off by allocation version","65790e01-0a67-514d-8a66-929bc0169fac_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_471","N/A","Ecoinvent  3.10, cut-off by allocation version","2b727e27-bfcb-5560-aab9-873ad69bcd73_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_472","N/A","Ecoinvent  3.10, cut-off by allocation version","0f8129e4-4840-513f-b53f-6a24089cbcd4_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_473","N/A","Ecoinvent  3.10, cut-off by allocation version","b277fbaf-6fed-59f1-9727-9f392ed9fa3d_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_474","N/A","Ecoinvent  3.10, cut-off by allocation version","0b8566a3-0d91-5e12-b71d-e3cc5ec4bc86_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_475","N/A","Ecoinvent  3.10, cut-off by allocation version","77bad89e-55c3-598b-89aa-dc7e9da86187_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_476","N/A","Ecoinvent  3.10, cut-off by allocation version","cfd17d33-ea32-59d0-a2f1-3f447e17c581_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_477","N/A","Ecoinvent  3.10, cut-off by allocation version","6617fee5-6572-5a93-9dc0-c0cb33e80ff2_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_478","N/A","Ecoinvent  3.10, cut-off by allocation version","c55c370c-7f1e-5077-889f-9f2c8863e285_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_479","N/A","Ecoinvent  3.10, cut-off by allocation version","b7a331c9-a2f1-5c1e-a685-7cee01b3cf69_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_480","N/A","Ecoinvent  3.10, cut-off by allocation version","28dfb649-5d63-5f8f-bf68-695772c18b82_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_481","N/A","Ecoinvent  3.10, cut-off by allocation version","6278c4cc-d909-5d0d-81c0-702ddc787d7f_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_482","N/A","Ecoinvent  3.10, cut-off by allocation version","063a18cf-2f17-5ba9-a1a3-15258dd85e47_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_483","N/A","Ecoinvent  3.10, cut-off by allocation version","103f42a6-58ba-586e-bd05-faf51396d873_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_484","N/A","Ecoinvent  3.10, cut-off by allocation version","fdce3b26-41dc-5819-ba07-c8b3f36b85fd_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_485","N/A","Ecoinvent  3.10, cut-off by allocation version","8b58a76a-e1d3-503e-a0de-35363c62bb38_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_486","N/A","Ecoinvent  3.10, cut-off by allocation version","7b5d5816-d30f-5049-9bb6-e81475155fcd_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_487","N/A","Ecoinvent  3.10, cut-off by allocation version","e5a5ad67-b5e9-57d3-95e5-f5d3ac3c6cd4_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_488","N/A","Ecoinvent  3.10, cut-off by allocation version","3511cbc7-9d84-5471-ad2d-dbefc862bbd3_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_489","N/A","Ecoinvent  3.10, cut-off by allocation version","9b874034-97f2-585a-8439-918eaf22b64f_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_490","N/A","Ecoinvent  3.10, cut-off by allocation version","77859587-bd7e-5112-a696-d9478c7667c3_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_491","N/A","Ecoinvent  3.10, cut-off by allocation version","72020167-a4de-537d-ab11-ec8ffd0e76c1_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_492","N/A","Ecoinvent  3.10, cut-off by allocation version","3024a276-42f5-59ae-a12d-fefee65e7c67_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_493","N/A","Ecoinvent  3.10, cut-off by allocation version","1386bf8f-7041-556c-a461-7ec1a9d07667_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_494","N/A","Ecoinvent  3.10, cut-off by allocation version","bc5124b5-80d4-5301-8091-49c4a9261a4d_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_495","N/A","Ecoinvent  3.10, cut-off by allocation version","e4afe892-c850-53be-a44a-9bf25eddf110_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_496","N/A","Ecoinvent  3.10, cut-off by allocation version","d20c579c-6e37-5c21-9201-39048a8222fb_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_497","N/A","Ecoinvent  3.10, cut-off by allocation version","ea9c0bd5-bd2c-5c0d-a643-28afeec6df10_618bf4eb-bee5-4d38-8e4f-78cfebf779be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_498","N/A","Ecoinvent  3.10, cut-off by allocation version","b240d229-4331-514d-9237-f9af6fdfe3d8_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_499","N/A","Ecoinvent  3.10, cut-off by allocation version","f5b51cc5-f045-5d11-8ec2-456d5e4a6a36_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_500","N/A","Ecoinvent  3.10, cut-off by allocation version","2482bd47-8bae-5e00-a301-0eec09e93a57_adb8247d-8bbd-45aa-b111-289d0e5e2307",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_501","N/A","Ecoinvent  3.10, cut-off by allocation version","9e403c61-2ef8-527d-9534-feb2de7f993a_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_502","N/A","Ecoinvent  3.10, cut-off by allocation version","86e28ed3-337b-5032-8d64-486fec7ff0f3_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_503","N/A","Ecoinvent  3.10, cut-off by allocation version","331f0c47-b561-526c-bc1a-be1caa864b38_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_504","N/A","Ecoinvent  3.10, cut-off by allocation version","13dfa6fe-be1d-5c36-9a74-a12d19bd166d_b7667b06-c667-481c-8718-bfbdfcd20d94",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_505","N/A","Ecoinvent  3.10, cut-off by allocation version","0e9bda8b-6bb8-55a2-9cb5-95fa8afc7a00_b7667b06-c667-481c-8718-bfbdfcd20d94",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_506","N/A","Ecoinvent  3.10, cut-off by allocation version","b5bb560e-fc33-56b1-8cb3-8124d8f6818d_d0125769-1059-41bb-8313-f4ef1cc1bd14",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_507","N/A","Ecoinvent  3.10, cut-off by allocation version","d514a5f9-ba78-5ce8-a6c4-c4bada59ff9b_d0125769-1059-41bb-8313-f4ef1cc1bd14",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_508","N/A","Ecoinvent  3.10, cut-off by allocation version","9b93855b-c3b1-57ac-ace2-96f086724628_d0125769-1059-41bb-8313-f4ef1cc1bd14",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_509","N/A","Ecoinvent  3.10, cut-off by allocation version","98c2609b-bf50-53ce-9a4b-5eb5877bd899_b28cfd95-443c-4abd-887d-8aec49e2b764",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_510","N/A","Ecoinvent  3.10, cut-off by allocation version","ecac82e4-4134-5e6e-b37c-29a6a8a0a87e_b28cfd95-443c-4abd-887d-8aec49e2b764",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_511","N/A","Ecoinvent  3.10, cut-off by allocation version","083a950a-a5e8-5888-a579-fd0db9768058_580b6c42-5004-49a0-b474-27dc65e0d47b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_512","N/A","Ecoinvent  3.10, cut-off by allocation version","2036f769-f714-5f9c-824a-ddecf243871f_580b6c42-5004-49a0-b474-27dc65e0d47b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_513","N/A","Ecoinvent  3.10, cut-off by allocation version","353bdd50-3cde-56c2-981f-de0ca15d192d_c2e3161e-4f3c-4f32-a3bb-4459d50b430a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_514","N/A","Ecoinvent  3.10, cut-off by allocation version","0fce7403-5366-5169-a405-a8395c11c7d6_c2e3161e-4f3c-4f32-a3bb-4459d50b430a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_515","N/A","Ecoinvent  3.10, cut-off by allocation version","6f38c539-07be-5bc8-a99a-7526da07d377_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_516","N/A","Ecoinvent  3.10, cut-off by allocation version","f2c2fe4e-caff-5bfb-aeaa-a206ac1a60cf_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_517","N/A","Ecoinvent  3.10, cut-off by allocation version","ec1dceda-86aa-5f48-97b2-6052d44fd8a5_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_518","N/A","Ecoinvent  3.10, cut-off by allocation version","717d603b-893c-5481-a67e-d0e39d208239_9090888c-6089-4d65-9317-7695e029e25f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_519","N/A","Ecoinvent  3.10, cut-off by allocation version","14d47dfc-7097-5e42-b686-24cbb33e9d7e_9090888c-6089-4d65-9317-7695e029e25f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_520","N/A","Ecoinvent  3.10, cut-off by allocation version","f9eb1b96-c895-5cb2-bef8-a48bde7c3d6e_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_521","N/A","Ecoinvent  3.10, cut-off by allocation version","f48039fb-26fe-5d8a-bd6c-6c3ffdfa5ca9_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_522","N/A","Ecoinvent  3.10, cut-off by allocation version","7aa825d2-bd38-5a01-92c7-a50c03fd0060_d51e5a32-c20a-4da6-8d58-31f344b50c00",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_523","N/A","Ecoinvent  3.10, cut-off by allocation version","3bdaa769-5f20-5be7-89c3-ac30583c7a2c_d51e5a32-c20a-4da6-8d58-31f344b50c00",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_524","N/A","Ecoinvent  3.10, cut-off by allocation version","331c3985-e999-5b8c-ba46-9939cc83a79c_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_525","N/A","Ecoinvent  3.10, cut-off by allocation version","90710843-6406-5807-bd83-c6e0a10e04d2_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_526","N/A","Ecoinvent  3.10, cut-off by allocation version","36d35b21-da69-562d-83ce-4ee715e6d890_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_527","N/A","Ecoinvent  3.10, cut-off by allocation version","6fdeeada-48c4-55f3-8426-08cd1a0720bd_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_528","N/A","Ecoinvent  3.10, cut-off by allocation version","c2ed2a6f-4557-5b2f-8de6-2c5d5c3fac01_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_529","N/A","Ecoinvent  3.10, cut-off by allocation version","8b80cedb-462a-5916-bed7-6f490b08e8f3_80761dd3-0a68-4821-aa1c-088faeac8386",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_530","N/A","Ecoinvent  3.10, cut-off by allocation version","805dd5e5-4515-5c6f-927c-8636c3b8671c_80761dd3-0a68-4821-aa1c-088faeac8386",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_531","N/A","Ecoinvent  3.10, cut-off by allocation version","4062a9ca-0059-56b0-bd5f-13965f89199e_db3559ad-a065-425f-9d03-551068d5548e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_532","N/A","Ecoinvent  3.10, cut-off by allocation version","d5cb5f84-d241-5289-b5f1-dd5049f36cab_db3559ad-a065-425f-9d03-551068d5548e",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_533","N/A","Ecoinvent  3.10, cut-off by allocation version","771b2b9d-f985-5004-b20f-313259aab523_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_534","N/A","Ecoinvent  3.10, cut-off by allocation version","4f728108-ef18-5a00-b206-7460665c074d_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_535","N/A","Ecoinvent  3.10, cut-off by allocation version","400cb029-6e10-5e9d-832b-b25bffc1fe68_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_536","N/A","Ecoinvent  3.10, cut-off by allocation version","c4dd0d51-e6e5-5e1d-b416-98f354484dd6_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_537","N/A","Ecoinvent  3.10, cut-off by allocation version","875a1016-e31c-5e21-97bc-90c5b74b48e8_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_538","N/A","Ecoinvent  3.10, cut-off by allocation version","9bc1d45d-f598-51d9-b9ea-bc32719b7720_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_539","N/A","Ecoinvent  3.10, cut-off by allocation version","102b15f6-f788-5019-9b16-24f55b6fc5b5_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_540","N/A","Ecoinvent  3.10, cut-off by allocation version","3b8b16ae-91a5-547d-baa0-ec6ab44ab5a8_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_541","N/A","Ecoinvent  3.10, cut-off by allocation version","048e0209-8804-5ca1-9832-8284b254d3f2_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_542","N/A","Ecoinvent  3.10, cut-off by allocation version","56047049-8a95-5c5f-9687-f628c6f45467_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_543","N/A","Ecoinvent  3.10, cut-off by allocation version","7fe4c4c7-91e4-5f21-b2f8-c25eaee5e3a1_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_544","N/A","Ecoinvent  3.10, cut-off by allocation version","943b263d-92b3-584d-9a3b-16b8fab1686d_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_545","N/A","Ecoinvent  3.10, cut-off by allocation version","a09150c3-22b4-5032-9694-82401fe65d66_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_546","N/A","Ecoinvent  3.10, cut-off by allocation version","23cc6b1d-c3f7-50b7-8678-ca2964db64b7_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_547","N/A","Ecoinvent  3.10, cut-off by allocation version","42fd398a-05b7-5727-b197-c844f207c143_b6abeedb-cebf-4b0d-943a-2980192bfc07",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_548","N/A","Ecoinvent  3.10, cut-off by allocation version","46a1caee-31fb-5573-bf83-f1612b16ae98_b6abeedb-cebf-4b0d-943a-2980192bfc07",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_549","N/A","Ecoinvent  3.10, cut-off by allocation version","95d4646e-6f37-5764-a73e-92fb3ab5fe34_7513d2f5-d7ee-497b-971b-a5ad34ab5c83",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_550","N/A","Ecoinvent  3.10, cut-off by allocation version","ad8c1de4-97d0-59e6-bb91-1d583d0b3f96_7513d2f5-d7ee-497b-971b-a5ad34ab5c83",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_551","N/A","Ecoinvent  3.10, cut-off by allocation version","7b353053-d8c7-5bde-ad5c-49fc7efbd6ed_7513d2f5-d7ee-497b-971b-a5ad34ab5c83",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_552","N/A","Ecoinvent  3.10, cut-off by allocation version","4481c64f-c092-5db8-8fd1-3e9057360f4a_171e53d3-3f3a-45a1-99f6-fad22caf1cd6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_553","N/A","Ecoinvent  3.10, cut-off by allocation version","0d7ce2a5-da4e-585f-b965-e68f89fb8dac_171e53d3-3f3a-45a1-99f6-fad22caf1cd6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_554","N/A","Ecoinvent  3.10, cut-off by allocation version","8d870d1f-ab11-5a5b-9c04-27a28688c01e_aa78f007-28b9-473d-af21-fe233c21f7d3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_555","N/A","Ecoinvent  3.10, cut-off by allocation version","752400a7-9e94-5a83-b1c6-8100a0cd5c19_aa78f007-28b9-473d-af21-fe233c21f7d3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_556","N/A","Ecoinvent  3.10, cut-off by allocation version","cb280103-a085-5d9c-8fc0-77b59774361c_11b71553-cc51-438e-8cb5-0337836737ae",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_557","N/A","Ecoinvent  3.10, cut-off by allocation version","85ddd581-cd8c-5238-9a3f-807d4b56b871_11b71553-cc51-438e-8cb5-0337836737ae",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_558","N/A","Ecoinvent  3.10, cut-off by allocation version","6e3106f8-7418-55b0-93eb-8a6bd4c389b4_9ccedb7d-205a-4729-90aa-17809aa1f511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_559","N/A","Ecoinvent  3.10, cut-off by allocation version","62dec963-b6bb-5a64-a1db-ac31cab60ee3_9ccedb7d-205a-4729-90aa-17809aa1f511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_560","N/A","Ecoinvent  3.10, cut-off by allocation version","f47411b1-eb72-59af-b66c-de3ef7b98143_5fb6a985-faa0-44cc-b183-f0b549833357",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_561","N/A","Ecoinvent  3.10, cut-off by allocation version","efb68dc4-32a5-5b96-bfb2-6cc7567e581f_5fb6a985-faa0-44cc-b183-f0b549833357",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_562","N/A","Ecoinvent  3.10, cut-off by allocation version","ee133340-f5ad-532f-a0a3-63dd7592010e_7ef961a9-b8c2-425f-8b79-9ad184c86c00",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_563","N/A","Ecoinvent  3.10, cut-off by allocation version","a1b26b8b-4135-53be-a72d-776a377a7f0e_7ef961a9-b8c2-425f-8b79-9ad184c86c00",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_564","N/A","Ecoinvent  3.10, cut-off by allocation version","0a708089-d92a-53b3-9c26-ab1334a624dd_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_565","N/A","Ecoinvent  3.10, cut-off by allocation version","5ed2b92d-e34b-54c1-b65c-ca806824d07a_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_566","N/A","Ecoinvent  3.10, cut-off by allocation version","8591bc73-5739-51b8-82ea-719125195cb2_a7abd72a-4d9c-4f99-abfc-3de79d425a96",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_567","N/A","Ecoinvent  3.10, cut-off by allocation version","73501e63-dd94-52f5-a349-5ee55ddf5a2b_a7abd72a-4d9c-4f99-abfc-3de79d425a96",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_568","N/A","Ecoinvent  3.10, cut-off by allocation version","59e5c64e-638f-5739-9ccf-944987c39aa1_a7abd72a-4d9c-4f99-abfc-3de79d425a96",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Incineration"]
[null,"OSW_SE_569","N/A","Ecoinvent  3.10, cut-off by allocation version","34e2b77a-7207-5f62-98bf-5b5ca75c2af7_240c1a3c-1aba-4528-afc3-3f27f56583be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_570","N/A","Ecoinvent  3.10, cut-off by allocation version","b471c925-cc2f-5b7f-b1c1-cb56c0edff13_240c1a3c-1aba-4528-afc3-3f27f56583be",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_571","N/A","Ecoinvent  3.10, cut-off by allocation version","46bb4963-1aff-55c1-b9d3-3a2a05791438_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_572","N/A","Ecoinvent  3.10, cut-off by allocation version","56d4476d-e4d5-50c5-9e15-67a5d98c4a11_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_573","N/A","Ecoinvent  3.10, cut-off by allocation version","5ae48163-32be-5510-a709-006bd09d096b_3a91cb7d-843b-495d-9973-33ba5efee877",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_574","N/A","Ecoinvent  3.10, cut-off by allocation version","f246e4f5-9501-5521-8601-3f752da59480_3a91cb7d-843b-495d-9973-33ba5efee877",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_575","N/A","Ecoinvent  3.10, cut-off by allocation version","ae05a346-96bc-5cae-bd16-17e1721b4a2b_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_576","N/A","Ecoinvent  3.10, cut-off by allocation version","071d52ef-12c5-57e4-9b13-918a3141ac87_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_577","N/A","Ecoinvent  3.10, cut-off by allocation version","e9502c59-061a-55b7-b841-2fca78477a55_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_578","N/A","Ecoinvent  3.10, cut-off by allocation version","1e20ad36-8b8c-5828-90ef-c648fefb25ab_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_579","N/A","Ecoinvent  3.10, cut-off by allocation version","6b69de33-8f3c-5483-bfe0-a67c3cb2a004_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_580","N/A","Ecoinvent  3.10, cut-off by allocation version","9040f7ae-34b8-5aa1-9051-994d48073738_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_581","N/A","Ecoinvent  3.10, cut-off by allocation version","6fa37465-d31d-5dba-94a9-423c81751eb6_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_582","N/A","Ecoinvent  3.10, cut-off by allocation version","4b625f6b-f869-51b4-9b1e-97dfc63b39da_27da8130-82ba-485c-a800-b89efdcb0491",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_583","N/A","Ecoinvent  3.10, cut-off by allocation version","8b636500-5512-5f5a-8a68-e5d8baf9d876_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_584","N/A","Ecoinvent  3.10, cut-off by allocation version","6b67e8b2-ab23-5bfe-9489-d11589caf3bb_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_585","N/A","Ecoinvent  3.10, cut-off by allocation version","12bf0ada-8a6f-5df1-9a6a-d533fdf23ee4_d1a4a803-c563-4740-84cf-3c21a488bd74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_586","N/A","Ecoinvent  3.10, cut-off by allocation version","ef99265a-753d-579d-a3db-5415d851d04b_7df87cd6-22cd-4010-ab95-b1a02917bbfe",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_587","N/A","Ecoinvent  3.10, cut-off by allocation version","668786c6-a0f3-57fa-9d81-64ac449d766f_7df87cd6-22cd-4010-ab95-b1a02917bbfe",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_588","N/A","Ecoinvent  3.10, cut-off by allocation version","77e4a728-d495-5edf-a2dd-3a3d97e97167_22e27360-4621-4591-8412-a4f2045ac1a0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_589","N/A","Ecoinvent  3.10, cut-off by allocation version","ce6fd926-f7ad-5332-b31a-05462495483a_22e27360-4621-4591-8412-a4f2045ac1a0",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_590","N/A","Ecoinvent  3.10, cut-off by allocation version","d73f6f02-9176-5bce-aab6-13d01a5fae4c_d3fe6705-5f5c-4961-b14d-0f9dd0e90e34",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_591","N/A","Ecoinvent  3.10, cut-off by allocation version","d5a0305a-274b-59b9-97b9-712e8f755172_d3fe6705-5f5c-4961-b14d-0f9dd0e90e34",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_592","N/A","Ecoinvent  3.10, cut-off by allocation version","703544c9-2d32-5b4b-9a1a-c50e4c823d3d_d3fe6705-5f5c-4961-b14d-0f9dd0e90e34",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_593","N/A","Ecoinvent  3.10, cut-off by allocation version","39e5dd99-3d50-519a-9bc4-7132cbec9af0_7f6bb533-2d3c-43a6-ac60-6eef299d7c52",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_594","N/A","Ecoinvent  3.10, cut-off by allocation version","b838b2a9-a327-59de-96de-7419e943378b_7f6bb533-2d3c-43a6-ac60-6eef299d7c52",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_595","N/A","Ecoinvent  3.10, cut-off by allocation version","26f97507-24ae-5ca4-b83f-fed9bfb27234_7f6bb533-2d3c-43a6-ac60-6eef299d7c52",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_596","N/A","Ecoinvent  3.10, cut-off by allocation version","3034047a-ab5e-523f-82b8-bdadd4ce3a63_e9f6d312-001c-435a-a668-82239a3b7511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_597","N/A","Ecoinvent  3.10, cut-off by allocation version","1071ae53-b776-513d-b10a-b6af35c34e07_e9f6d312-001c-435a-a668-82239a3b7511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_598","N/A","Ecoinvent  3.10, cut-off by allocation version","34f1837d-d0c4-52e8-a8b1-091acde2f585_e9f6d312-001c-435a-a668-82239a3b7511",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_599","N/A","Ecoinvent  3.10, cut-off by allocation version","cdbe9ad5-e843-5426-878c-870b7cd2ef1e_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_600","N/A","Ecoinvent  3.10, cut-off by allocation version","8e4fb6a0-7c6b-57d3-a2d2-7501f4b08779_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_601","N/A","Ecoinvent  3.10, cut-off by allocation version","93b802a6-416a-5620-bcc6-9007fd112b1b_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_602","N/A","Ecoinvent  3.10, cut-off by allocation version","f8031ae7-cf6c-5966-8854-c8e57aa09d90_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_603","N/A","Ecoinvent  3.10, cut-off by allocation version","119278e3-228c-5abd-b6f4-544b0cd492ce_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_604","N/A","Ecoinvent  3.10, cut-off by allocation version","f9659364-8048-515c-8463-4f81f8e9d02c_777bc26c-02e7-441e-a487-e4d4a87dae49",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_605","N/A","Ecoinvent  3.10, cut-off by allocation version","cf756897-6af0-5718-ac4f-7473ed707602_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_606","N/A","Ecoinvent  3.10, cut-off by allocation version","6483793c-2d77-5fcf-8c76-532de84acd66_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_607","N/A","Ecoinvent  3.10, cut-off by allocation version","7dc42d63-01da-5c13-99c9-d66d23450772_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_608","N/A","Ecoinvent  3.10, cut-off by allocation version","d91ef8a4-8106-53d5-87ae-e30a3ac28568_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_609","N/A","Ecoinvent  3.10, cut-off by allocation version","10c1da51-1e0b-5606-a848-6a26c1f75455_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_610","N/A","Ecoinvent  3.10, cut-off by allocation version","b0d8e38e-a2e5-5c66-b877-0f36d101c6c1_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_611","N/A","Ecoinvent  3.10, cut-off by allocation version","10ab4600-daef-535f-afa6-64a2aeb64b89_dae141a8-7daa-4f03-a649-b85b718ac65b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_612","N/A","Ecoinvent  3.10, cut-off by allocation version","b6478d29-95dd-53bc-b5a7-bf58806cc736_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_613","N/A","Ecoinvent  3.10, cut-off by allocation version","efd2fd19-3fa9-542f-875c-0e0b6dcf6295_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_614","N/A","Ecoinvent  3.10, cut-off by allocation version","02823727-5016-5a14-a821-5176ab9922dd_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_615","N/A","Ecoinvent  3.10, cut-off by allocation version","e880edeb-bc06-56de-9b22-396896ec350e_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_616","N/A","Ecoinvent  3.10, cut-off by allocation version","a786664b-f7fc-5402-8227-0394ab1d238e_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_617","N/A","Ecoinvent  3.10, cut-off by allocation version","bd8fd478-fc3f-587a-8c4f-9ac192cf3aa7_27a9b2b8-30cd-45a6-bf1a-9c1f7afde003",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_618","N/A","Ecoinvent  3.10, cut-off by allocation version","b936d081-b249-52c8-b45f-4499d00b490e_759b89bd-3aa6-42ad-b767-5bb9ef5d331d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_619","N/A","Ecoinvent  3.10, cut-off by allocation version","b936d081-b249-52c8-b45f-4499d00b490e_71e2f1db-a2c5-44d0-8337-dfff15be974d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_620","N/A","Ecoinvent  3.10, cut-off by allocation version","76cf2cb2-0204-579e-9030-b7d4c248acac_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_621","N/A","Ecoinvent  3.10, cut-off by allocation version","3f55efb4-3510-5281-a17a-96433c64134a_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_622","N/A","Ecoinvent  3.10, cut-off by allocation version","fde5d4cb-6004-501f-8428-784c4769da83_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_623","N/A","Ecoinvent  3.10, cut-off by allocation version","346f28e8-a832-5309-82a2-0cb7e970920e_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_624","N/A","Ecoinvent  3.10, cut-off by allocation version","4f134710-fa4c-57d0-8b40-2a808f5a13fe_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_625","N/A","Ecoinvent  3.10, cut-off by allocation version","197a78a5-1111-5b38-9e5f-8f459e4809f6_cee6769c-ac58-45d5-9597-de2569031d74",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_626","N/A","Ecoinvent  3.10, cut-off by allocation version","738bb629-f281-58d6-b1c6-488afe6c4a0f_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_627","N/A","Ecoinvent  3.10, cut-off by allocation version","9b821100-47d9-5424-b251-c963504382aa_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_628","N/A","Ecoinvent  3.10, cut-off by allocation version","b8793adf-9b78-58c6-b580-8609389763ad_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_629","N/A","Ecoinvent  3.10, cut-off by allocation version","f67f96ef-19a4-54f5-9c15-e0e1ef39512f_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_630","N/A","Ecoinvent  3.10, cut-off by allocation version","a6f99432-7aa4-53bd-a30f-849934877b68_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_631","N/A","Ecoinvent  3.10, cut-off by allocation version","444e455a-035b-5fc4-82d5-884e4fbb3681_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_632","N/A","Ecoinvent  3.10, cut-off by allocation version","0ad2369a-3c41-511c-bae7-8ebefad4c88d_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_633","N/A","Ecoinvent  3.10, cut-off by allocation version","76b43621-ac11-57d1-8bc7-8ac76edbc03d_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_634","N/A","Ecoinvent  3.10, cut-off by allocation version","b67a14e1-b8e0-531a-bde5-985cb8ba92f7_42baed81-24d1-4aed-a120-cc7d35ddac10",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_635","N/A","Ecoinvent  3.10, cut-off by allocation version","a64619db-578c-5468-84bd-29bd897ecd1d_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_636","N/A","Ecoinvent  3.10, cut-off by allocation version","6188687a-e150-5e2d-93c5-cbb9d5bd0c6d_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_637","N/A","Ecoinvent  3.10, cut-off by allocation version","32065dc5-09ff-5225-a4b0-2421056c5aa8_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_638","N/A","Ecoinvent  3.10, cut-off by allocation version","0db9c4ae-185c-50b9-8894-842d2636bda7_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_639","N/A","Ecoinvent  3.10, cut-off by allocation version","abe228a4-6b01-5f48-88c6-86a823e4829d_88afd721-07ec-4910-a004-fa3fecb6bf70",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_640","N/A","Ecoinvent  3.10, cut-off by allocation version","a1009b4b-d792-545b-9822-3f3b4186b165_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_641","N/A","Ecoinvent  3.10, cut-off by allocation version","411a91ca-c1fa-5b99-8092-905f1fdc0e80_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_642","N/A","Ecoinvent  3.10, cut-off by allocation version","69f85ea2-7d20-5753-b636-df7beed7db53_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_643","N/A","Ecoinvent  3.10, cut-off by allocation version","d36d4b82-c612-5393-9fdf-edbc0b1d464e_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_644","N/A","Ecoinvent  3.10, cut-off by allocation version","b6241c46-4c1a-5364-8a6b-e14de75672fc_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_645","N/A","Ecoinvent  3.10, cut-off by allocation version","69b191f5-7439-5e62-8bbd-e742a68ee2a1_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_646","N/A","Ecoinvent  3.10, cut-off by allocation version","dd1f4d8e-beff-594e-b84f-9bde4c2000fc_dcb70fd5-e305-4920-b68b-40697cc6a206",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_647","N/A","Ecoinvent  3.10, cut-off by allocation version","d927a87b-dd71-504b-9126-ce86890a07c2_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_648","N/A","Ecoinvent  3.10, cut-off by allocation version","64a5834f-df1a-5b90-9308-224c60d3a493_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_649","N/A","Ecoinvent  3.10, cut-off by allocation version","b80c3d97-be06-52e2-819b-444da06b8f03_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_650","N/A","Ecoinvent  3.10, cut-off by allocation version","bc41350d-f328-5464-8342-6b037bbb0027_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_651","N/A","Ecoinvent  3.10, cut-off by allocation version","4bd907e5-1e93-5b73-bcb7-7746b0ad25cf_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_652","N/A","Ecoinvent  3.10, cut-off by allocation version","440f9524-2c05-547f-b018-cb14cd887381_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_653","N/A","Ecoinvent  3.10, cut-off by allocation version","f409a032-0953-5c55-b6ce-aaf7dd4e07bc_7ee0ddc3-924d-4339-b9bf-7856af6a698f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_654","N/A","Ecoinvent  3.10, cut-off by allocation version","ccab8588-d306-5fb1-9d58-99a22774e70c_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_655","N/A","Ecoinvent  3.10, cut-off by allocation version","d9561a2f-7645-5932-9e63-b69ce46120af_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_656","N/A","Ecoinvent  3.10, cut-off by allocation version","9124231e-9484-542c-8e65-c84a0421b65c_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_657","N/A","Ecoinvent  3.10, cut-off by allocation version","86a38984-6490-5884-9bfe-e5bf9bf5021b_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_658","N/A","Ecoinvent  3.10, cut-off by allocation version","fafcc8ba-03da-54f5-8b25-1bbdad4ffbe4_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_659","N/A","Ecoinvent  3.10, cut-off by allocation version","b272d3c1-fbd9-5a7f-95ee-ce78f6381a30_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_660","N/A","Ecoinvent  3.10, cut-off by allocation version","fb93faf4-8d93-5a8e-9225-d109e7c0c3b8_00478901-732f-4bf4-81cc-2255f9874512",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_661","N/A","Ecoinvent  3.10, cut-off by allocation version","a211099d-cf81-5df3-9243-408ff8798c0c_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_662","N/A","Ecoinvent  3.10, cut-off by allocation version","205613c6-76db-51c8-8be3-ee531d5f05e6_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_663","N/A","Ecoinvent  3.10, cut-off by allocation version","d72a465b-79ff-585e-ace9-dd6f71df10b1_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_664","N/A","Ecoinvent  3.10, cut-off by allocation version","5254d128-7917-5937-87e3-8c4c441b0009_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_665","N/A","Ecoinvent  3.10, cut-off by allocation version","9a354579-0358-5792-88cd-1d13b1c608f6_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_666","N/A","Ecoinvent  3.10, cut-off by allocation version","ca653034-a623-5646-996e-d17dbdedfe22_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_667","N/A","Ecoinvent  3.10, cut-off by allocation version","48e8c46b-22ca-5f90-b08b-29649020cfb1_b0176c67-5bc0-462a-8466-4f372f446f7c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_668","N/A","Ecoinvent  3.10, cut-off by allocation version","e86f9c7f-a45a-5991-b546-3f370fde332d_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_669","N/A","Ecoinvent  3.10, cut-off by allocation version","8c4d300c-4330-5302-bb2c-65e47ee655e3_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_670","N/A","Ecoinvent  3.10, cut-off by allocation version","296615ca-ff07-5bcd-96f4-683fa553b20c_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_671","N/A","Ecoinvent  3.10, cut-off by allocation version","e52b75a0-60ec-580b-9fa1-5a139b9f0d6d_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_672","N/A","Ecoinvent  3.10, cut-off by allocation version","e8fb465f-f4a6-5e13-afc3-8d15fd6d8804_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_673","N/A","Ecoinvent  3.10, cut-off by allocation version","345f63b7-4215-5444-a9ca-f166703f0d10_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_674","N/A","Ecoinvent  3.10, cut-off by allocation version","af4dae40-fc48-567c-bada-4a48cc72f75a_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_675","N/A","Ecoinvent  3.10, cut-off by allocation version","83008680-f1f5-5ec5-8b31-d6c90bf88f4b_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_676","N/A","Ecoinvent  3.10, cut-off by allocation version","5046b742-d327-5808-a22f-0a1839d7d481_9cdb112b-0d90-4d76-9cec-412b0c67d8bb",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_677","N/A","Ecoinvent  3.10, cut-off by allocation version","9b4b0c61-7de3-5a4d-a3e8-59c0083f39b9_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_678","N/A","Ecoinvent  3.10, cut-off by allocation version","e3170900-8b44-59a6-be94-0fa96279c5f4_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_679","N/A","Ecoinvent  3.10, cut-off by allocation version","1326a00a-c4a9-550f-8cc0-20082053e07f_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_680","N/A","Ecoinvent  3.10, cut-off by allocation version","efb2f643-2e04-580d-97e4-e7d9f11b56f1_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_681","N/A","Ecoinvent  3.10, cut-off by allocation version","b234cac6-4a28-5e6a-be03-722d9106e3a6_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_682","N/A","Ecoinvent  3.10, cut-off by allocation version","1d3962b2-ccc6-5997-a930-096d68cac33e_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_683","N/A","Ecoinvent  3.10, cut-off by allocation version","222e716a-e0e5-59e4-9e39-450e83114603_9219c94a-7a25-4a4c-b25d-c096fdd50d47",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_684","N/A","Ecoinvent  3.10, cut-off by allocation version","c3fdb1d1-5b5b-566b-addb-0695c945e935_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_685","N/A","Ecoinvent  3.10, cut-off by allocation version","6265767f-83f3-5b25-8431-261de92489eb_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_686","N/A","Ecoinvent  3.10, cut-off by allocation version","35ed35a7-0ccd-504c-bfe8-bea0547bc437_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_687","N/A","Ecoinvent  3.10, cut-off by allocation version","39483239-2dbb-57b3-a040-cd2c5fe08c49_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_688","N/A","Ecoinvent  3.10, cut-off by allocation version","9397b852-28fc-54eb-8009-8248a42d309e_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_689","N/A","Ecoinvent  3.10, cut-off by allocation version","59667853-6eeb-5180-86fc-34ce0704f742_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_690","N/A","Ecoinvent  3.10, cut-off by allocation version","1ab2fc12-b156-58a2-b7fd-d950d8b72f14_6f2eb438-cde2-4d07-a770-d023a988a9c4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Landfill"]
[null,"OSW_SE_691","N/A","Ecoinvent  3.10, cut-off by allocation version","4ffc91cd-cb9b-5d15-9f26-35f4046e8476_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_692","N/A","Ecoinvent  3.10, cut-off by allocation version","4ffc91cd-cb9b-5d15-9f26-35f4046e8476_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_693","N/A","Ecoinvent  3.10, cut-off by allocation version","4ffc91cd-cb9b-5d15-9f26-35f4046e8476_60fa2c28-1f8f-5486-aab5-da2e493250d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_694","N/A","Ecoinvent  3.10, cut-off by allocation version","4e3e256b-ebff-5d2f-9e2d-5c11f55c5754_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_695","N/A","Ecoinvent  3.10, cut-off by allocation version","4e3e256b-ebff-5d2f-9e2d-5c11f55c5754_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_696","N/A","Ecoinvent  3.10, cut-off by allocation version","4e3e256b-ebff-5d2f-9e2d-5c11f55c5754_60fa2c28-1f8f-5486-aab5-da2e493250d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_697","N/A","Ecoinvent  3.10, cut-off by allocation version","7ff71172-d0dc-52ec-9279-96b9d76dce8a_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_698","N/A","Ecoinvent  3.10, cut-off by allocation version","7ff71172-d0dc-52ec-9279-96b9d76dce8a_4f312355-ac65-4635-8fb2-006dba64ce60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_699","N/A","Ecoinvent  3.10, cut-off by allocation version","7ff71172-d0dc-52ec-9279-96b9d76dce8a_60fa2c28-1f8f-5486-aab5-da2e493250d4",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_700","N/A","Ecoinvent  3.10, cut-off by allocation version","c1a287e7-b2f5-59a9-9050-c0d3926ddd2d_bd4b5819-02c6-41c3-97ea-a91f14b3e0bc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_701","N/A","Ecoinvent  3.10, cut-off by allocation version","185e71dc-422a-5d66-9b09-9bf51ab066ad_bd4b5819-02c6-41c3-97ea-a91f14b3e0bc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_702","N/A","Ecoinvent  3.10, cut-off by allocation version","0a3f4352-f586-5547-bc95-1009fb4cc9ba_eb211196-8882-4baf-9113-31229f23e6aa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_703","N/A","Ecoinvent  3.10, cut-off by allocation version","36d59a17-1805-563a-9231-9bc8f4f555cb_eb211196-8882-4baf-9113-31229f23e6aa",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_704","N/A","Ecoinvent  3.10, cut-off by allocation version","204e11be-4628-504f-80bb-27033b0b4c73_b2011f87-e037-4f68-8dec-6d8e6de4ae25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_705","N/A","Ecoinvent  3.10, cut-off by allocation version","bcbdf779-d61b-5ed5-b715-26efff19eb06_b2011f87-e037-4f68-8dec-6d8e6de4ae25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_706","N/A","Ecoinvent  3.10, cut-off by allocation version","4fef1ea8-3a7f-5b2c-8f6c-713c43806d51_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_707","N/A","Ecoinvent  3.10, cut-off by allocation version","5c48a01a-4ebf-54d0-8bdf-d0515bfa3049_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_708","N/A","Ecoinvent  3.10, cut-off by allocation version","d66a0e7e-5301-543d-91f8-6aff435d5759_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_709","N/A","Ecoinvent  3.10, cut-off by allocation version","67ed5154-8998-56ea-bb54-34e5a058190e_4058ca6d-92c0-4ce5-bdc9-a3a96eeade93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_710","N/A","Ecoinvent  3.10, cut-off by allocation version","6a192587-f929-5ede-8d07-cb8aeaff9c6f_4058ca6d-92c0-4ce5-bdc9-a3a96eeade93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_711","N/A","Ecoinvent  3.10, cut-off by allocation version","adfad858-4132-5cc7-87d3-7cb08fde8981_818559f3-b129-4e35-9b12-b5ab589c178a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_712","N/A","Ecoinvent  3.10, cut-off by allocation version","106fc593-24d1-5f70-84ec-e15b2fe8c8ae_818559f3-b129-4e35-9b12-b5ab589c178a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_713","N/A","Ecoinvent  3.10, cut-off by allocation version","66c9e605-cdb4-5e9f-99fc-53cf65958109_b3184435-d00c-5713-823d-5ff6741bfbbc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_714","N/A","Ecoinvent  3.10, cut-off by allocation version","f5828d5c-8f41-5653-a295-1b9d66eb95ef_b3184435-d00c-5713-823d-5ff6741bfbbc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_715","N/A","Ecoinvent  3.10, cut-off by allocation version","82f87e19-06e9-5d4f-ad66-2f8fae15a849_b3184435-d00c-5713-823d-5ff6741bfbbc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_716","N/A","Ecoinvent  3.10, cut-off by allocation version","34597a01-f156-5ba0-b5d6-0ba2bf2df2cf_b3184435-d00c-5713-823d-5ff6741bfbbc",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_717","N/A","Ecoinvent  3.10, cut-off by allocation version","2b541ada-3444-5c9f-922c-b92b965aeeb1_ed25f589-c6c8-56a7-a518-b01dd3e8a453",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_718","N/A","Ecoinvent  3.10, cut-off by allocation version","6c8e7ad0-4022-5f26-a3c1-92ef1ab575c5_ed25f589-c6c8-56a7-a518-b01dd3e8a453",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_719","N/A","Ecoinvent  3.10, cut-off by allocation version","e47ba1b6-97dd-5ca9-9f6a-3f2251cbf0dd_ed25f589-c6c8-56a7-a518-b01dd3e8a453",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_720","N/A","Ecoinvent  3.10, cut-off by allocation version","961e30aa-8a68-5868-b8fe-2bd7a55675de_ed25f589-c6c8-56a7-a518-b01dd3e8a453",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_721","N/A","Ecoinvent  3.10, cut-off by allocation version","50989dbf-2baf-5c8d-b017-5a03421b2f74_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_722","N/A","Ecoinvent  3.10, cut-off by allocation version","a05e9c42-49ae-5c40-9801-d76ea9343d3d_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_723","N/A","Ecoinvent  3.10, cut-off by allocation version","e0be6f23-9f12-5c72-bd66-3dfd2eb76a8c_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_724","N/A","Ecoinvent  3.10, cut-off by allocation version","c28cc60c-fbf7-52f5-8301-252b1ce140ed_f3b9ab33-932a-4908-8e6b-5709f9bd6e0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_725","N/A","Ecoinvent  3.10, cut-off by allocation version","70aba8d6-2164-50d4-9ffc-b3fa1e5ea114_f3b9ab33-932a-4908-8e6b-5709f9bd6e0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_726","N/A","Ecoinvent  3.10, cut-off by allocation version","b265dcfc-b7ed-595e-84fc-3c8a6e19245f_9a8c2994-7cbb-4d86-a1b7-27fc0c4e49e3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_727","N/A","Ecoinvent  3.10, cut-off by allocation version","98e99ba7-aa39-5123-b7c5-630bfa552cef_9a8c2994-7cbb-4d86-a1b7-27fc0c4e49e3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_728","N/A","Ecoinvent  3.10, cut-off by allocation version","7c8d95d9-f22e-5552-a12f-8c32ea1799fa_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_729","N/A","Ecoinvent  3.10, cut-off by allocation version","8453a785-ece3-5db5-9128-9cee7b8c2e93_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_730","N/A","Ecoinvent  3.10, cut-off by allocation version","95138ef3-5c2a-5abe-976b-26f4821d20fd_858164b0-44f1-4118-b6cb-47054faa21ef",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_731","N/A","Ecoinvent  3.10, cut-off by allocation version","f7d88982-8723-5f62-a473-da170b8aefd1_1c17413f-82b0-4ddb-beef-63854b1a8e1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_732","N/A","Ecoinvent  3.10, cut-off by allocation version","802900c1-a6b6-5b7b-ae71-20c92c1984dd_1c17413f-82b0-4ddb-beef-63854b1a8e1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_733","N/A","Ecoinvent  3.10, cut-off by allocation version","ab316fdf-3e2d-5657-9afc-1199de07976d_1c17413f-82b0-4ddb-beef-63854b1a8e1f",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_734","N/A","Ecoinvent  3.10, cut-off by allocation version","80bb9c3a-b776-5001-95f9-0c92e65c1257_3728ce01-009e-4b64-94d4-3c3e9fabf888",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_735","N/A","Ecoinvent  3.10, cut-off by allocation version","7b741193-47bd-5785-be6f-5c3abd1ea8d1_3728ce01-009e-4b64-94d4-3c3e9fabf888",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_736","N/A","Ecoinvent  3.10, cut-off by allocation version","3be54b0f-bfcc-504a-bb03-39d183658e9d_3728ce01-009e-4b64-94d4-3c3e9fabf888",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_737","N/A","Ecoinvent  3.10, cut-off by allocation version","86372858-2a46-515c-996a-c24137d726af_b2011f87-e037-4f68-8dec-6d8e6de4ae25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_738","N/A","Ecoinvent  3.10, cut-off by allocation version","8d46f893-30d7-5514-8c9a-f9c0f01b0064_b2011f87-e037-4f68-8dec-6d8e6de4ae25",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_739","N/A","Ecoinvent  3.10, cut-off by allocation version","61e2b2aa-7c51-5ba1-b2e2-eb3c0ca22d4c_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_740","N/A","Ecoinvent  3.10, cut-off by allocation version","450f0376-73bb-5edf-b0ff-df2cc7f47538_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_741","N/A","Ecoinvent  3.10, cut-off by allocation version","1ff6ae54-ded8-593f-9f95-c4fcd5e64492_48f6b7c9-093b-4dd0-bf0d-9ba54b4c2d22",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_742","N/A","Ecoinvent  3.10, cut-off by allocation version","6419cc2f-f9d8-5215-9b53-a960775292c5_bc7c3720-dcba-41b4-9d96-380b55275e57",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_743","N/A","Ecoinvent  3.10, cut-off by allocation version","6ea294ed-cd88-54d2-aeea-b2a7edfb45ee_bc7c3720-dcba-41b4-9d96-380b55275e57",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_744","N/A","Ecoinvent  3.10, cut-off by allocation version","f396d9d5-6487-50f1-80ce-5c513be70321_0a6c7524-9e23-41b8-ac7b-b0489ed4681c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_745","N/A","Ecoinvent  3.10, cut-off by allocation version","dd918b0e-d736-5668-828e-c7297335097c_0a6c7524-9e23-41b8-ac7b-b0489ed4681c",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_746","N/A","Ecoinvent  3.10, cut-off by allocation version","f9ff01bd-5b9d-5036-a032-d1abf5186fea_93bd3d97-0440-4e9f-8f69-6324fe28c4b6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_747","N/A","Ecoinvent  3.10, cut-off by allocation version","ccf2bcd0-c939-53f4-bda4-3c55e5213d5e_93bd3d97-0440-4e9f-8f69-6324fe28c4b6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_748","N/A","Ecoinvent  3.10, cut-off by allocation version","19a6527c-66e1-5c3b-818f-76441fb2f751_42b1c202-8308-422e-bfb7-3efe54dfcef6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_749","N/A","Ecoinvent  3.10, cut-off by allocation version","6a7d0a4c-7725-5606-9d43-b360d28123ad_42b1c202-8308-422e-bfb7-3efe54dfcef6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_750","N/A","Ecoinvent  3.10, cut-off by allocation version","47112c66-3ab9-5bea-9e66-d24c47dec7d0_42b1c202-8308-422e-bfb7-3efe54dfcef6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_751","N/A","Ecoinvent  3.10, cut-off by allocation version","4ab7e916-ebf4-52d1-9802-f8058ff3bb83_4058ca6d-92c0-4ce5-bdc9-a3a96eeade93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_752","N/A","Ecoinvent  3.10, cut-off by allocation version","b8868c2c-e7ce-563b-881c-669f76c9dc1b_4058ca6d-92c0-4ce5-bdc9-a3a96eeade93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_753","N/A","Ecoinvent  3.10, cut-off by allocation version","65d24a7f-b4f8-562e-8821-ed740d0f6f20_e88c3a19-945a-4396-a107-37e3876b2f0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_754","N/A","Ecoinvent  3.10, cut-off by allocation version","207b787b-00f6-53f7-af2b-9d666fe93d17_e88c3a19-945a-4396-a107-37e3876b2f0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_755","N/A","Ecoinvent  3.10, cut-off by allocation version","5b02d68e-19b3-56a1-be3b-930e4b72e767_bfd577e2-82b4-4166-af2b-3bda540931f6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_756","N/A","Ecoinvent  3.10, cut-off by allocation version","4e983651-673f-5cf8-bc0f-bfa5139f1b71_bfd577e2-82b4-4166-af2b-3bda540931f6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_757","N/A","Ecoinvent  3.10, cut-off by allocation version","a5ed667d-bf8f-52b4-bfdb-fa44acf90127_bfd577e2-82b4-4166-af2b-3bda540931f6",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_758","N/A","Ecoinvent  3.10, cut-off by allocation version","75057433-27e9-56b1-aef0-45c0164a0546_4e758deb-57bd-45c6-96f6-9b4d25ba7a60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_759","N/A","Ecoinvent  3.10, cut-off by allocation version","7ca945d1-cebc-5019-b592-0074494f9992_4e758deb-57bd-45c6-96f6-9b4d25ba7a60",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_760","N/A","Ecoinvent  3.10, cut-off by allocation version","d1933cff-f101-54cc-ac84-495b3fdf82b9_2a1db579-5d40-4d28-9b5a-c8ce7525b62d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_761","N/A","Ecoinvent  3.10, cut-off by allocation version","c1a692f8-6b85-50f0-a1d0-f51872190b3b_2a1db579-5d40-4d28-9b5a-c8ce7525b62d",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_762","N/A","Ecoinvent  3.10, cut-off by allocation version","da5567af-ae9b-5011-8124-e916e0837602_0baac448-32a1-4b9f-afec-69a9b9b203ac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_763","N/A","Ecoinvent  3.10, cut-off by allocation version","bb5512e1-f8da-5b1b-b490-6ee06fc19d63_0baac448-32a1-4b9f-afec-69a9b9b203ac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_764","N/A","Ecoinvent  3.10, cut-off by allocation version","75c7eaab-e510-5a1f-81ff-d3bd09404f6e_0baac448-32a1-4b9f-afec-69a9b9b203ac",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_765","N/A","Ecoinvent  3.10, cut-off by allocation version","8f77df58-fa32-5c8f-974f-9599f7695356_fd27af60-7b68-4549-bf35-022eacd74f93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_766","N/A","Ecoinvent  3.10, cut-off by allocation version","36788bb1-5454-537a-adc5-06f33d3ba9e2_fd27af60-7b68-4549-bf35-022eacd74f93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_767","N/A","Ecoinvent  3.10, cut-off by allocation version","ce19058b-3f99-54e8-bf85-2e9468748588_fd27af60-7b68-4549-bf35-022eacd74f93",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_768","N/A","Ecoinvent  3.10, cut-off by allocation version","83af1209-44ae-58d3-8837-cf4a412c8889_818559f3-b129-4e35-9b12-b5ab589c178a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_769","N/A","Ecoinvent  3.10, cut-off by allocation version","56d1cea5-8bdb-5798-a367-ace2f4c020e2_818559f3-b129-4e35-9b12-b5ab589c178a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_770","N/A","Ecoinvent  3.10, cut-off by allocation version","4743fafb-0071-59d0-8231-e95a24bfb1c8_10d4f2e3-6343-4ea1-a721-86c89858e646",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_771","N/A","Ecoinvent  3.10, cut-off by allocation version","062cb1dd-7420-528b-9a80-4c892872d074_10d4f2e3-6343-4ea1-a721-86c89858e646",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_772","N/A","Ecoinvent  3.10, cut-off by allocation version","94f43c81-ecba-5fe8-8f18-393d60150656_2cb0d6c6-349c-46fc-b31f-a036c847a267",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_773","N/A","Ecoinvent  3.10, cut-off by allocation version","533c63fd-eb6f-59be-a7e2-4b9a471e381c_2cb0d6c6-349c-46fc-b31f-a036c847a267",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_774","N/A","Ecoinvent  3.10, cut-off by allocation version","e1762e44-2065-5139-8922-7089420bf115_19c15d45-57de-43b4-9772-4ef06ec9971a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_775","N/A","Ecoinvent  3.10, cut-off by allocation version","014ba1fb-1eb3-5578-8e62-e4639d41d04a_19c15d45-57de-43b4-9772-4ef06ec9971a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_776","N/A","Ecoinvent  3.10, cut-off by allocation version","39671b5a-63cf-581f-809a-98707500006d_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_777","N/A","Ecoinvent  3.10, cut-off by allocation version","745e6615-2ba9-5503-af7e-9450be3b9c6f_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_778","N/A","Ecoinvent  3.10, cut-off by allocation version","e887158d-1c78-5757-9e16-01930ed65bae_5357a067-f798-46fb-97b0-fa18f723341b",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_779","N/A","Ecoinvent  3.10, cut-off by allocation version","b8190844-9f7a-5a14-aa5b-1225639509a0_f3b9ab33-932a-4908-8e6b-5709f9bd6e0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_780","N/A","Ecoinvent  3.10, cut-off by allocation version","95afbb1d-55cd-54f7-b883-91ba8ff562a9_f3b9ab33-932a-4908-8e6b-5709f9bd6e0a",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_781","N/A","Ecoinvent  3.10, cut-off by allocation version","97446480-5c1e-5396-8ea5-c63947da70f3_9a8c2994-7cbb-4d86-a1b7-27fc0c4e49e3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_782","N/A","Ecoinvent  3.10, cut-off by allocation version","4a7cfad2-6f3d-5418-8234-f1642619f62b_9a8c2994-7cbb-4d86-a1b7-27fc0c4e49e3",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_783","N/A","Ecoinvent  3.10, cut-off by allocation version","ea9184a1-2e8c-5f2d-b382-6a0f6d63ba49_bbae1509-eb89-42e9-81d8-70e5cae46488",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SE_784","N/A","Ecoinvent  3.10, cut-off by allocation version","9498aee7-192d-5796-9ec3-061b48f4e791_bbae1509-eb89-42e9-81d8-70e5cae46488",null,null,null,"Cradle-to-gate (A1-A3)","Ecoinvent","IPCC 2021","GWP100","ISO 14044","N/A","N/A","No","Secondary: Ecoinvent","Waste treatment","Processing, sorting for recycling and reuse"]
[null,"OSW_SP_1",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bio Petrol","GB","GJ",null,null,null,8.2692300000000003]
[null,"OSW_SP_2",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bio Petrol","GB","kg",null,null,null,0.36924000000000001]
[null,"OSW_SP_3",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bio Petrol","GB","litres",null,null,null,0.27392]
[null,"OSW_SP_4",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel HVO","GB","GJ",null,null,null,10.25]
[null,"OSW_SP_5",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel HVO","GB","kg",null,null,null,0.45100000000000001]
[null,"OSW_SP_6",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel HVO","GB","litres",null,null,null,0.35177999999999998]
[null,"OSW_SP_7",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME","GB","GJ",null,null,null,10.97411]
[null,"OSW_SP_8",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME","GB","kg",null,null,null,0.40823999999999999]
[null,"OSW_SP_9",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME","GB","litres",null,null,null,0.36332999999999999]
[null,"OSW_SP_10",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from tallow)","GB","GJ",null,null,null,14]
[null,"OSW_SP_11",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from tallow)","GB","kg",null,null,null,0.52080000000000004]
[null,"OSW_SP_12",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from tallow)","GB","litres",null,null,null,0.46350999999999998]
[null,"OSW_SP_13",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from used cooking oil)","GB","GJ",null,null,null,10.34563]
[null,"OSW_SP_14",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from used cooking oil)","GB","kg",null,null,null,0.38485999999999998]
[null,"OSW_SP_15",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biodiesel ME (from used cooking oil)","GB","litres",null,null,null,0.34251999999999999]
[null,"OSW_SP_16",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bioethanol","GB","GJ",null,null,null,19.542120000000001]
[null,"OSW_SP_17",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bioethanol","GB","kg",null,null,null,0.52373000000000003]
[null,"OSW_SP_18",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Bioethanol","GB","litres",null,null,null,0.41583999999999999]
[null,"OSW_SP_19",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (compressed)","GB","GJ",null,null,null,11.367470000000001]
[null,"OSW_SP_20",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (compressed)","GB","kg",null,null,null,0.55701000000000001]
[null,"OSW_SP_21",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (compressed)","GB","litres"]
[null,"OSW_SP_22",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (liquified)","GB","GJ",null,null,null,11.367470000000001]
[null,"OSW_SP_23",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (liquified)","GB","kg",null,null,null,0.55701000000000001]
[null,"OSW_SP_24",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biomethane (liquified)","GB","litres"]
[null,"OSW_SP_25",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biopropane","GB","GJ",null,null,null,10.28659]
[null,"OSW_SP_26",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biopropane","GB","kg",null,null,null,0.4773]
[null,"OSW_SP_27",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biopropane","GB","litres",null,null,null,0.24578]
[null,"OSW_SP_28",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Methanol (bio)","GB","GJ",null,null,null,19.542120000000001]
[null,"OSW_SP_29",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Methanol (bio)","GB","kg",null,null,null,0.52373000000000003]
[null,"OSW_SP_30",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Methanol (bio)","GB","litres",null,null,null,0.41583999999999999]
[null,"OSW_SP_31",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Off road biodiesel","GB","GJ",null,null,null,10.97411]
[null,"OSW_SP_32",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Off road biodiesel","GB","kg",null,null,null,0.40823999999999999]
[null,"OSW_SP_33",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Off road biodiesel","GB","litres",null,null,null,0.36332999999999999]
[null,"OSW_SP_34",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Renewable petrol","GB","GJ",null,null,null,18.27807]
[null,"OSW_SP_35",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Renewable petrol","GB","kg",null,null,null,0.51283999999999996]
[null,"OSW_SP_36",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Renewable petrol","GB","litres",null,null,null,0.45724999999999999]
[null,"OSW_SP_37",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biogas","GB","kWh",null,null,null,2.8410000000000001E-2]
[null,"OSW_SP_38",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Biogas","GB","tonnes",null,null,null,157.82597000000001]
[null,"OSW_SP_39",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Landfill gas","GB","kWh",null,null,null,2.0000000000000001E-4]
[null,"OSW_SP_40",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Landfill gas","GB","tonnes",null,null,null,0.68844000000000005]
[null,"OSW_SP_41",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Grass/straw","GB","kWh",null,null,null,1.6039999999999999E-2]
[null,"OSW_SP_42",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Grass/straw","GB","tonnes",null,null,null,68.650000000000006]
[null,"OSW_SP_43",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood chips","GB","kWh",null,null,null,1.0529999999999999E-2]
[null,"OSW_SP_44",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood chips","GB","tonnes",null,null,null,39.788330000000002]
[null,"OSW_SP_45",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood logs","GB","kWh",null,null,null,1.277E-2]
[null,"OSW_SP_46",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood logs","GB","tonnes",null,null,null,52.14]
[null,"OSW_SP_47",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood pellets","GB","kWh",null,null,null,3.7440000000000001E-2]
[null,"OSW_SP_48",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",35491,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Biofuels lifecycle","Wood pellets","GB","tonnes",null,null,null,177]
[null,"OSW_SP_49",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Butane","GB","kWh (Gross CV)",null,null,null,0.22239999999999999]
[null,"OSW_SP_50",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Butane","GB","kWh (Net CV)",null,null,null,0.24106]
[null,"OSW_SP_51",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Butane","GB","litres",null,null,null,1.74529]
[null,"OSW_SP_52",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Butane","GB","tonnes",null,null,null,3033.32]
[null,"OSW_SP_53",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","CNG","GB","kWh (Gross CV)",null,null,null,0.18253999999999998]
[null,"OSW_SP_54",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","CNG","GB","kWh (Net CV)",null,null,null,0.20227000000000001]
[null,"OSW_SP_55",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","CNG","GB","litres",null,null,null,0.44435999999999998]
[null,"OSW_SP_56",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","CNG","GB","tonnes",null,null,null,2539.25]
[null,"OSW_SP_57",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LNG","GB","kWh (Gross CV)",null,null,null,0.18396999999999999]
[null,"OSW_SP_58",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LNG","GB","kWh (Net CV)",null,null,null,0.20386000000000001]
[null,"OSW_SP_59",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LNG","GB","litres",null,null,null,1.1579999999999999]
[null,"OSW_SP_60",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LNG","GB","tonnes",null,null,null,2559.17]
[null,"OSW_SP_61",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LPG","GB","kWh (Gross CV)",null,null,null,0.21448999999999999]
[null,"OSW_SP_62",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LPG","GB","kWh (Net CV)",null,null,null,0.23030999999999999]
[null,"OSW_SP_63",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LPG","GB","litres",null,null,null,1.5570900000000001]
[null,"OSW_SP_64",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","LPG","GB","tonnes",null,null,null,2939.29]
[null,"OSW_SP_65",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas","GB","cubic metres",null,null,null,2.0157400000000001]
[null,"OSW_SP_66",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas","GB","kWh (Gross CV)",null,null,null,0.18253999999999998]
[null,"OSW_SP_67",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas","GB","kWh (Net CV)",null,null,null,0.20227000000000001]
[null,"OSW_SP_68",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas","GB","tonnes",null,null,null,2539.25]
[null,"OSW_SP_69",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas (100% mineral blend)","GB","cubic metres",null,null,null,2.0315500000000002]
[null,"OSW_SP_70",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas (100% mineral blend)","GB","kWh (Gross CV)",null,null,null,0.18396999999999999]
[null,"OSW_SP_71",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas (100% mineral blend)","GB","kWh (Net CV)",null,null,null,0.20386000000000001]
[null,"OSW_SP_72",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",12020,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Natural gas (100% mineral blend)","GB","tonnes",null,null,null,2559.17]
[null,"OSW_SP_73",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Other petroleum gas","GB","kWh (Gross CV)",null,null,null,0.18323999999999999]
[null,"OSW_SP_74",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Other petroleum gas","GB","kWh (Net CV)",null,null,null,0.19917000000000001]
[null,"OSW_SP_75",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Other petroleum gas","GB","litres",null,null,null,0.94440999999999997]
[null,"OSW_SP_76",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Other petroleum gas","GB","tonnes",null,null,null,2578.25]
[null,"OSW_SP_77",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Propane","GB","kWh (Gross CV)",null,null,null,0.21410999999999999]
[null,"OSW_SP_78",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Propane","GB","kWh (Net CV)",null,null,null,0.23257]
[null,"OSW_SP_79",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Propane","GB","litres",null,null,null,1.5435399999999999]
[null,"OSW_SP_80",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Gaseous fuels lifecycle","Propane","GB","tonnes",null,null,null,2997.55]
[null,"OSW_SP_81",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation spirit","GB","kWh (Gross CV)",null,null,null,0.24374999999999999]
[null,"OSW_SP_82",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation spirit","GB","kWh (Net CV)",null,null,null,0.25658000000000003]
[null,"OSW_SP_83",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation spirit","GB","litres",null,null,null,2.3304800000000001]
[null,"OSW_SP_84",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation spirit","GB","tonnes",null,null,null,3192.76]
[null,"OSW_SP_85",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation turbine fuel","GB","kWh (Gross CV)",null,null,null,0.24782000000000001]
[null,"OSW_SP_86",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation turbine fuel","GB","kWh (Net CV)",null,null,null,0.26085999999999998]
[null,"OSW_SP_87",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation turbine fuel","GB","litres",null,null,null,2.54514]
[null,"OSW_SP_88",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Aviation turbine fuel","GB","tonnes",null,null,null,3181.4300000000003]
[null,"OSW_SP_89",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Burning oil","GB","kWh (Gross CV)",null,null,null,0.24677000000000002]
[null,"OSW_SP_90",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Burning oil","GB","kWh (Net CV)",null,null,null,0.25974999999999998]
[null,"OSW_SP_91",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Burning oil","GB","litres",null,null,null,2.54013]
[null,"OSW_SP_92",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",334,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Burning oil","GB","tonnes",null,null,null,3165.01]
[null,"OSW_SP_93",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (100% mineral diesel)","GB","kWh (Gross CV)",null,null,null,0.25320999999999999]
[null,"OSW_SP_94",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (100% mineral diesel)","GB","kWh (Net CV)",null,null,null,0.26938999999999996]
[null,"OSW_SP_95",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (100% mineral diesel)","GB","litres",null,null,null,2.6987999999999999]
[null,"OSW_SP_96",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (100% mineral diesel)","GB","tonnes",null,null,null,3208.7599999999998]
[null,"OSW_SP_97",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (average biofuel blend)","GB","kWh (Gross CV)",null,null,null,0.24114999999999998]
[null,"OSW_SP_98",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (average biofuel blend)","GB","kWh (Net CV)",null,null,null,0.25630999999999998]
[null,"OSW_SP_99",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (average biofuel blend)","GB","litres",null,null,null,2.5578399999999997]
[null,"OSW_SP_100",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Diesel (average biofuel blend)","GB","tonnes",null,null,null,3032.89]
[null,"OSW_SP_101",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Fuel oil","GB","kWh (Gross CV)",null,null,null,0.26816000000000001]
[null,"OSW_SP_102",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Fuel oil","GB","kWh (Net CV)",null,null,null,0.28525999999999996]
[null,"OSW_SP_103",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Fuel oil","GB","litres",null,null,null,3.17523]
[null,"OSW_SP_104",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Fuel oil","GB","tonnes",null,null,null,3229.2000000000003]
[null,"OSW_SP_105",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Gas oil","GB","kWh (Gross CV)",null,null,null,0.25678999999999996]
[null,"OSW_SP_106",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Gas oil","GB","kWh (Net CV)",null,null,null,0.27319000000000004]
[null,"OSW_SP_107",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Gas oil","GB","litres",null,null,null,2.7585700000000002]
[null,"OSW_SP_108",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Gas oil","GB","tonnes",null,null,null,3230.2799999999997]
[null,"OSW_SP_109",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Lubricants","GB","kWh (Gross CV)",null,null,null,0.26417999999999997]
[null,"OSW_SP_110",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Lubricants","GB","kWh (Net CV)",null,null,null,0.28103999999999996]
[null,"OSW_SP_111",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Lubricants","GB","litres",null,null,null,2.7497199999999999]
[null,"OSW_SP_112",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Lubricants","GB","tonnes",null,null,null,3181.44]
[null,"OSW_SP_113",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine fuel oil","GB","kWh (Gross CV)",null,null,null,0.26235999999999998]
[null,"OSW_SP_114",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine fuel oil","GB","kWh (Net CV)",null,null,null,0.27911000000000002]
[null,"OSW_SP_115",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine fuel oil","GB","litres",null,null,null,3.10669]
[null,"OSW_SP_116",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3337,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine fuel oil","GB","tonnes",null,null,null,3159.4999999999995]
[null,"OSW_SP_117",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine gas oil","GB","kWh (Gross CV)",null,null,null,0.25834999999999997]
[null,"OSW_SP_118",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine gas oil","GB","kWh (Net CV)",null,null,null,0.27484999999999998]
[null,"OSW_SP_119",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine gas oil","GB","litres",null,null,null,2.7753900000000002]
[null,"OSW_SP_120",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Marine gas oil","GB","tonnes",null,null,null,3249.99]
[null,"OSW_SP_121",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Naphtha","GB","kWh (Gross CV)",null,null,null,0.23651]
[null,"OSW_SP_122",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Naphtha","GB","kWh (Net CV)",null,null,null,0.24895]
[null,"OSW_SP_123",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Naphtha","GB","litres",null,null,null,2.1192699999999998]
[null,"OSW_SP_124",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Naphtha","GB","tonnes",null,null,null,3142.87]
[null,"OSW_SP_125",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (100% mineral petrol)","GB","kWh (Gross CV)",null,null,null,0.24156]
[null,"OSW_SP_126",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (100% mineral petrol)","GB","kWh (Net CV)",null,null,null,0.25428000000000001]
[null,"OSW_SP_127",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (100% mineral petrol)","GB","litres",null,null,null,2.3397000000000001]
[null,"OSW_SP_128",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (100% mineral petrol)","GB","tonnes",null,null,null,3153.9]
[null,"OSW_SP_129",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (average biofuel blend)","GB","kWh (Gross CV)",null,null,null,0.22719]
[null,"OSW_SP_130",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (average biofuel blend)","GB","kWh (Net CV)",null,null,null,0.23961000000000002]
[null,"OSW_SP_131",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (average biofuel blend)","GB","litres",null,null,null,2.1618500000000003]
[null,"OSW_SP_132",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Petrol (average biofuel blend)","GB","tonnes",null,null,null,2903.08]
[null,"OSW_SP_133",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - distillate oil","GB","kWh (Gross CV)",null,null,null,0.25678999999999996]
[null,"OSW_SP_134",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - distillate oil","GB","kWh (Net CV)",null,null,null,0.27319000000000004]
[null,"OSW_SP_135",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - distillate oil","GB","litres",null,null,null,2.7585700000000002]
[null,"OSW_SP_136",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - distillate oil","GB","tonnes",null,null,null,3230.2799999999997]
[null,"OSW_SP_137",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - residual oil","GB","kWh (Gross CV)",null,null,null,0.26816000000000001]
[null,"OSW_SP_138",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - residual oil","GB","kWh (Net CV)",null,null,null,0.28525999999999996]
[null,"OSW_SP_139",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - residual oil","GB","litres",null,null,null,3.17523]
[null,"OSW_SP_140",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Processed fuel oils - residual oil","GB","tonnes",null,null,null,3229.2000000000003]
[null,"OSW_SP_141",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Refinery miscellaneous","GB","kWh (Gross CV)",null,null,null,0.24667]
[null,"OSW_SP_142",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Refinery miscellaneous","GB","kWh (Net CV)",null,null,null,0.25964999999999999]
[null,"OSW_SP_143",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Refinery miscellaneous","GB","litres"]
[null,"OSW_SP_144",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Refinery miscellaneous","GB","tonnes",null,null,null,2944.81]
[null,"OSW_SP_145",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Waste oils","GB","kWh (Gross CV)",null,null,null,0.25681999999999999]
[null,"OSW_SP_146",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Waste oils","GB","kWh (Net CV)",null,null,null,0.27503]
[null,"OSW_SP_147",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Waste oils","GB","litres",null,null,null,2.7536699999999996]
[null,"OSW_SP_148",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Liquid fuels lifecycle","Waste oils","GB","tonnes",null,null,null,3224.57]
[null,"OSW_SP_149",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (domestic)","GB","kWh (Gross CV)",null,null,null,0.34461999999999998]
[null,"OSW_SP_150",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (domestic)","GB","kWh (Net CV)",null,null,null,0.36276000000000003]
[null,"OSW_SP_151",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (domestic)","GB","tonnes",null,null,null,2883.2599999999998]
[null,"OSW_SP_152",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation - home produced coal only)","GB","kWh (Gross CV)",null,null,null,0.32133]
[null,"OSW_SP_153",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation - home produced coal only)","GB","kWh (Net CV)",null,null,null,0.33823999999999999]
[null,"OSW_SP_154",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation - home produced coal only)","GB","tonnes",null,null,null,2266.8999999999996]
[null,"OSW_SP_155",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation)","GB","kWh (Gross CV)",null,null,null,0.32133]
[null,"OSW_SP_156",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation)","GB","kWh (Net CV)",null,null,null,0.33823999999999999]
[null,"OSW_SP_157",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (electricity generation)","GB","tonnes",null,null,null,2270.4499999999998]
[null,"OSW_SP_158",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (industrial)","GB","kWh (Gross CV)",null,null,null,0.32462999999999997]
[null,"OSW_SP_159",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (industrial)","GB","kWh (Net CV)",null,null,null,0.34172000000000002]
[null,"OSW_SP_160",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coal (industrial)","GB","tonnes",null,null,null,2411.4300000000003]
[null,"OSW_SP_161",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coking coal","GB","kWh (Gross CV)",null,null,null,0.35797000000000001]
[null,"OSW_SP_162",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coking coal","GB","kWh (Net CV)",null,null,null,0.37681999999999999]
[null,"OSW_SP_163",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Coking coal","GB","tonnes",null,null,null,3165.24]
[null,"OSW_SP_164",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Petroleum coke","GB","kWh (Gross CV)",null,null,null,0.34094999999999998]
[null,"OSW_SP_165",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Petroleum coke","GB","kWh (Net CV)",null,null,null,0.35890000000000005]
[null,"OSW_SP_166",1,"UK Gov GHG Conversion Factors","NA","LCA","Lifecycle emissions from production and combustion of fuels",3336,"Cradle-to-grave","NA","IPCC","GWP100","ISO 14040/ISO 14044","Unknown","No","N/A","Secondary: Proxy","Electricity, fuels and other utilitites","Solid fuels lifecycle","Petroleum coke","GB","tonnes",null,null,null,3386.8700000000003]
[null,"OSW_SP_167",1,"Elcowire AB","S-P-07031","LCA","Copper wire rod",415,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","2019:14 Construction products, version 1.11","Yes",46722,"Secondary: Proxy","Materials","Copper","Copper wire rod","EUR","kg",4.32,1.3599999999999999E-2,1.5800000000000002E-2,4.3490000000000002]
[null,"OSW_SP_168",1,"LaFarga SA","S-P-02032","LCA","Copper wire rod",415,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","PCR 2012:01","Yes",45870,"Secondary: Proxy","Materials","Copper","Copper wire rod","GLO","kg",null,null,null,1.24]
[null,"OSW_SP_169",1,"Union Copper Rod","S-P-10570","LCA","Copper wire rod",415,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","2019:14 Construction products, version 1.11","Yes",46997,"Secondary: Proxy","Materials","Copper","Copper wire rod","GLO","kg",null,null,null,6.76]
[null,"OSW_SP_170",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220174-IBF1-EN","LCA","Products based on epoxy-resin, group 1",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46600,"Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 1","EUR","kg",3.95,-0.23799999999999999,8.8400000000000006E-2,3.8004000000000002]
[null,"OSW_SP_171",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220175-IBF1-EN","LCA","Products based on epoxy-resin, group 2",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46600,"Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 2","EUR","kg",10.6,-3.3399999999999999E-2,5.0699999999999999E-3,10.571669999999999]
[null,"OSW_SP_172",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220176-IBF1-EN","LCA","Products based on epoxy-resin, group 3",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46600,"Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 3","EUR","kg",5.26,-6.4100000000000004E-2,1.9300000000000001E-3,5.1978299999999997]
[null,"OSW_SP_173",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220177-IBF1-EN","LCA","Products based on epoxy-resin, group 4",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46600,"Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 4","EUR","kg",4.26,-0.23100000000000001,9.1600000000000001E-2,4.1205999999999996]
[null,"OSW_SP_174",1,"FEICA - Association of the European Adhesive and Sealant Industry","EPD-DBC-20220178-IBF1-EN","LCA","Products based on epoxy-resin, group 5",341,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46600,"Secondary: Proxy","Materials","Epoxy resin","Products based on epoxy-resin, group 5","EUR","kg",3.56,-5.2400000000000002E-2,9.6400000000000001E-4,3.5085640000000002]
[null,"OSW_SP_175",1,"Sistemas Técnicos del Accesorio y Componentes S. L. (STAC)","NA","LCA","Fibreglass",369,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46600,"Secondary: Proxy","Materials","Fibreglass","Polyamide profiles reinforced with 25% fibreglass","GLO","kg",6.69,-1.26E-2,1.8600000000000001E-3,6.6792600000000002]
[null,"OSW_SP_176",1,"VALMIERAS STIKLA ŠĶIEDRA , AS","NA","LCA","Glass fibre mesh",26890,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46692,"Secondary: Proxy","Materials","Fibreglass","Mesh","GLO","kg",1.718,-4.8000000000000001E-2,7.1199999999999996E-3,1.6771199999999999]
[null,"OSW_SP_177",1,"ArcelorMittal Europe – Flat Products","ECO-00001206","LCA","Heavy steel plates production",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","Structural steels, 07.2014","Yes",45748,"Secondary: Proxy","Materials","Steel","Heavy steel plates","RER","kg",null,null,null,2.6]
[null,"OSW_SP_178",1,"SSAB EMEA AB","S-P-01918","LCA","Hot rolled steel plates production",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","PCR 2012:01. Construction Products and Construction Services.","Yes",45746,"Secondary: Proxy","Materials","Steel","Hot rolled steel plates","GLO","kg",2.78,1.9900000000000001E-4,6.38E-4,2.7808369999999996]
[null,"OSW_SP_179",1,"Spartan UK LTD","S-P-03571","LCA","Hot rolled steel plates production",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46185,"Secondary: Proxy","Materials","Steel","Hot rolled steel plates","Unreported","kg",2.1,-8.1899999999999994E-3,5.9099999999999995E-4,2.0924010000000002]
[null,"OSW_SP_180",1,"BE Group","S-P-04888","LCA","Hot rolled steel plates production",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46323,"Secondary: Proxy","Materials","Steel","Hot rolled steel plates","Unreported","kg",2.02,-4.47E-3,7.1199999999999996E-4,2.0162420000000001]
[null,"OSW_SP_181",1,"Marcegaglia Plates S.p.A.","S-P-07882","LCA","Hot rolled steel plate",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46744,"Secondary: Proxy","Materials","Steel","Hot rolled steel plates","GLO","kg",2.0470000000000002,1.1850000000000001E-3,1.1609999999999999E-3,2.0493460000000003]
[null,"OSW_SP_182",1,"Ferriera Valsider Spa","S-P-08032","LCA","Hot rolled steel plate",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46813,"Secondary: Proxy","Materials","Steel","Hot rolled steel plates","EUR","kg",2.5099999999999998,2.8999999999999998E-3,1E-3,2.5138999999999996]
[null,"OSW_SP_183",1,"Metinvest Trametal SpA","S-P-08033","LCA","Hot rolled steel plate",412,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46813,"Secondary: Proxy","Materials","Steel","Hot rolled steel plates","EUR","kg",2.81,2.3400000000000001E-3,1.1299999999999999E-3,2.8134699999999997]
[null,"OSW_SP_184",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator full asset production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured assets","Wind turbine generators (WTG)","WTG (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,5535730]
[null,"OSW_SP_185",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,525500]
[null,"OSW_SP_186",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Generator (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,664190]
[null,"OSW_SP_187",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Hub (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,424590]
[null,"OSW_SP_188",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend assembly (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,25440]
[null,"OSW_SP_189",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Electric components (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,2085120]
[null,"OSW_SP_190",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Blades (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,470910]
[null,"OSW_SP_191",1,"Siemens Gamesa","S-P-09790","LCA","SG 11 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Tower","Tower (Siemens Gamesa 11-200 (11 MW))","GLO","Unit",null,null,null,1339980]
[null,"OSW_SP_192",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator full asset production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured assets","Wind turbine generators (WTG)","WTG (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,7272570]
[null,"OSW_SP_193",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,638990]
[null,"OSW_SP_194",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Generator (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,887040]
[null,"OSW_SP_195",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Hub (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,537810]
[null,"OSW_SP_196",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend assembly (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,32369.999999999996]
[null,"OSW_SP_197",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Electric components (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,2653830]
[null,"OSW_SP_198",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Blades (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,579790]
[null,"OSW_SP_199",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Tower","Tower (Siemens Gamesa 14-222 (14 MW))","GLO","Unit",null,null,null,1942740]
[null,"OSW_SP_200",1,"Siemens Gamesa","S-P-09791","LCA","SG 14 MW Wind Turbine Generator full asset production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured assets","Wind turbine generators (WTG)","WTG (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,7272570]
[null,"OSW_SP_201",1,"Siemens Gamesa","S-P-09792","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,638990]
[null,"OSW_SP_202",1,"Siemens Gamesa","S-P-09793","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Generator (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,887040]
[null,"OSW_SP_203",1,"Siemens Gamesa","S-P-09794","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Hub (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,537810]
[null,"OSW_SP_204",1,"Siemens Gamesa","S-P-09795","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Backend assembly (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,32369.999999999996]
[null,"OSW_SP_205",1,"Siemens Gamesa","S-P-09796","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Nacelle and internals","Electric components (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,2653830]
[null,"OSW_SP_206",1,"Siemens Gamesa","S-P-09797","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Blades, hub, and rotor system","Blades (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,579790]
[null,"OSW_SP_207",1,"Siemens Gamesa","S-P-09798","LCA","SG 14 MW Wind Turbine Generator components production",null,"Cradle-to-gate","NA","IPCC","GWP100","ISO 14040/ISO 14044","NA","Yes",46997,"Secondary: Proxy","Fully manufactured components","Tower","Tower (Siemens Gamesa 14-236 (14 MW))","GLO","Unit",null,null,null,1942740]
[null,"OSW_CF_1","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Bromopropane","GLO","kg",null,null,null,5.1999999999999998E-2]
[null,"OSW_CF_2","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Butane","GLO","kg",null,null,null,6.0000000000000001E-3]
[null,"OSW_CF_3","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Carbon dioxide, fossil","GLO","kg",null,null,null,1]
[null,"OSW_CF_4","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Carbon dioxide, from soil or biomass stock","GLO","kg",null,null,1,1]
[null,"OSW_CF_5","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Removals","Carbon dioxide, removal from atmosphere","GLO","kg",null,null,null,-1]
[null,"OSW_CF_6","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Chloroform","GLO","kg",null,null,null,20.6]
[null,"OSW_CF_7","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Dinitrogen monoxide","GLO","kg",null,null,null,273]
[null,"OSW_CF_8","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane","GLO","kg",null,null,null,0.437]
[null,"OSW_CF_9","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1,1,2-tetrafluoro-, HFC-134a","GLO","kg",null,null,null,1530]
[null,"OSW_CF_10","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1,1-trichloro-, HCFC-140","GLO","kg",null,null,null,161]
[null,"OSW_CF_11","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1,1-trifluoro-, HFC-143a","GLO","kg",null,null,null,5810]
[null,"OSW_CF_12","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1,2-trichloro-1,2,2-trifluoro-, CFC-113","GLO","kg",null,null,null,6520]
[null,"OSW_CF_13","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1-dichloro-1-fluoro-, HCFC-141b","GLO","kg",null,null,null,860]
[null,"OSW_CF_14","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,1-difluoro-, HFC-152a","GLO","kg",null,null,null,164]
[null,"OSW_CF_15","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,2-dichloro-","GLO","kg",null,null,null,1.3]
[null,"OSW_CF_16","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1,2-dichloro-1,1,2,2-tetrafluoro-, CFC-114","GLO","kg",null,null,null,9430]
[null,"OSW_CF_17","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 1-chloro-1,1-difluoro-, HCFC-142b","GLO","kg",null,null,null,2300]
[null,"OSW_CF_18","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 2,2-dichloro-1,1,1-trifluoro-, HCFC-123","GLO","kg",null,null,null,90.4]
[null,"OSW_CF_19","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, 2-chloro-1,1,1,2-tetrafluoro-, HCFC-124","GLO","kg",null,null,null,597]
[null,"OSW_CF_20","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, chloropentafluoro-, CFC-115","GLO","kg",null,null,null,9600]
[null,"OSW_CF_21","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, hexafluoro-, HFC-116","GLO","kg",null,null,null,12400]
[null,"OSW_CF_22","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Ethane, pentafluoro-, HFC-125","GLO","kg",null,null,null,3740]
[null,"OSW_CF_23","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, bromo-, Halon 1001","GLO","kg",null,null,null,2.4300000000000002]
[null,"OSW_CF_24","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, bromochlorodifluoro-, Halon 1211","GLO","kg",null,null,null,1930]
[null,"OSW_CF_25","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, bromotrifluoro-, Halon 1301","GLO","kg",null,null,null,7200]
[null,"OSW_CF_26","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, chlorodifluoro-, HCFC-22","GLO","kg",null,null,null,1960]
[null,"OSW_CF_27","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, chloro-fluoro-, HCFC-31","GLO","kg",null,null,null,79.400000000000006]
[null,"OSW_CF_28","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, chlorotrifluoro-, CFC-13","GLO","kg",null,null,null,16200]
[null,"OSW_CF_29","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, dichloro-, HCC-30","GLO","kg",null,null,null,11.2]
[null,"OSW_CF_30","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, dichlorodifluoro-, CFC-12","GLO","kg",null,null,null,12500]
[null,"OSW_CF_31","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, dichlorofluoro-, HCFC-21","GLO","kg",null,null,null,160]
[null,"OSW_CF_32","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, difluoro-, HFC-32","GLO","kg",null,null,null,771]
[null,"OSW_CF_33","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, fossil","GLO","kg",null,null,null,29.8]
[null,"OSW_CF_34","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, from soil or biomass stock","GLO","kg",null,null,29.8,29.8]
[null,"OSW_CF_35","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, monochloro-, R-40","GLO","kg",5.54,null,null,5.54]
[null,"OSW_CF_36","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, non-fossil","GLO","kg",null,27,0,27]
[null,"OSW_CF_37","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, tetrachloro-, R-10","GLO","kg",null,null,null,2200]
[null,"OSW_CF_38","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, tetrafluoro-, R-14","GLO","kg",null,null,null,7380]
[null,"OSW_CF_39","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, trichlorofluoro-, CFC-11","GLO","kg",null,null,null,6230]
[null,"OSW_CF_40","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Methane, trifluoro-, HFC-23","GLO","kg",null,null,null,14600]
[null,"OSW_CF_41","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Monochloroethane","GLO","kg",null,null,null,0.48099999999999998]
[null,"OSW_CF_42","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Nitrogen fluoride","GLO","kg",null,null,null,17400]
[null,"OSW_CF_43","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Perfluoropentane","GLO","kg",null,null,null,9220]
[null,"OSW_CF_44","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Propane","GLO","kg",null,null,null,0.02]
[null,"OSW_CF_45","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Sulfur hexafluoride","GLO","kg",null,null,null,25200]
[null,"OSW_CF_46","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Tetrachloroethylene","GLO","kg",null,null,null,6.34]
[null,"OSW_CF_47","N/A","IPCC 2021","N/A","N/A","N/A","N/A","N/A","N/A","IPCC 2021","GWP100","N/A","N/A","N/A","N/A","Characterisation Factors","Direct emissions and removals","Emissions","Trichloroethylene","GLO","kg",null,null,null,4.3999999999999997E-2]

{"sheet":"A0 - Preconstruction","index":12,"n_rows":53,"n_cols":26,"rows_kept":53,"cut":false,"hidden":false,"merged":[[23,4,23,7],[34,3,34,9],[8,3,8,11]]}
[]
[null,null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,null,"Offshore Wind Footprinting Tool"]
[null,null,null,"DATA INPUTS - A0 - Preconstruction"]
[]
[]
[null,null,null,"Lifecycle Stage & Module Description"]
[]
[null,null,null,"Module A0: The Preconstruction lifecycle stage estimates the emissions associated with all preconstruction activities occurring due to the OSW development. The emissions sources in module A0 primarily relate to energy and fuel consumption in vessels and equipment used to conduct preconstruction surveys, but may also include emissions related to material use from sensors and equipment used for surveys. Relevant activities for module A0, including but not limited to:\n  - Development & consenting services\n  - Environmental Surveys\n  - Metocean assessment\n  - Geological & hydrological surveys\n\nFor energy & fuels used in preconstruction surveys, the activity data may be in the form of quantity of energy consumed (kg, l, MJ), where the data is available or else in weight and distance data (e.g. ton.km)."]
[]
[null,null,null,"READ ME"]
[]
[null,null,null,"This tab calculates the expected emissions associated with preconstruction activities for the OSW development, including surveys and equipment"]
[]
[null,null,null,"Description cell"]
[null,null,null,"Guidance"]
[null,null,null,"Input cell"]
[null,null,null,"Calculation Cell"]
[null,null,null,"Preset Cell"]
[]
[null,1,null,"Results"]
[]
[null,1.1000000000000001,null,"Footprinting results "]
[null,null,null,"Error check:",{"$f":"IF(COUNTIF(Table_A0[Unit Match?],\"No\"),\"A unit matching error has been detected - please check the quantities and units input into this sheet\",\"No issues with unit matching\")","v":"No issues with unit matching"}]
[]
[null,null,null,"Module A0 Results"]
[null,null,null,"Lifecycle Stage","Total Fossil Emissions by lifecycle stage","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Emissions by lifecycle stage ","Total Fossil Emissions by lifecycle stage ","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Project Emissions "]
[null,null,null,"Units"," kgCO2e"," kgCO2e"," kgCO2e"," kgCO2e","tCO2e","tCO2e","tCO2e","tCO2e"]
[null,null,null,"A0 - Preconstruction Total",{"$f":"SUM(Table_A0[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_A0[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_A0[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_A0[Total Emissions (kgCO2e)])","v":0},{"$f":"E29/1000","v":0},{"$f":"F29/1000","v":0},{"$f":"G29/1000","v":0},{"$f":"IFERROR(H29/1000,0)","v":0}]
[]
[null,2,null,"Footprinting Information"]
[]
[null,2.1,null,"Module A0","Emissions due to vehicle, vessel, and aircraft use and emissions from materials and equipment used in preconstruction activities for the OSW development"]
[]
[null,null,null,"Please provide the electricity or fuel consumption or distance travelled in vehicles, vessels and aircraft during preconstruction.\nPlease provide the material and equipment used during preconstruction if the materials and equipment are solely to be used on the development under calculation."]
[null,null,null,null,null,null,null,null,null,null,"`",null,null,null,"Note: All Activity Data quantities should be input as a value rather than a formula or calculation"]
[null,null,null,"GHG Module","Preconstruction Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A0 - Preconstruction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A0[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A0[[#This Row],[Activity Data: Unit]]=Table_A0[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A0[[#This Row],[Emissions Factor: Unit]]<>Table_A0[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A0[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A0[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A0[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A0[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A0[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A0[[#This Row],[Activity Data: Quantity]]*Table_A0[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A0[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A0[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A0[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A0[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]

{"sheet":"A1-A3 - Production","index":13,"n_rows":212,"n_cols":26,"rows_kept":212,"cut":false,"hidden":false,"merged":[[39,3,39,9],[23,4,23,7],[7,3,7,9],[198,3,198,9],[43,3,43,9],[175,3,175,9],[176,12,176,21],[153,3,153,9]]}
[]
[null,null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,null,"DATA INPUTS -  A1-A3 - Production"]
[]
[]
[null,null,null,"Lifecycle Stage Description"]
[]
[null,null,null,"Module A1-A2: calculates the emissions associated with the extraction, processing and transportation to the manufacturing site of material inputs for the manufacturing process (e.g. Steel, Copper, Aluminium, etc.). \n\nModule A3: calculates emissions from the energy input for the manufacturing process for the production of the assets and components (e.g. joining, welding, extrusion, etc. ). If the manufacturing process emissions can not be easily allocated to individual assets (for example, a factory produces different components, including electrical components for the WTG) you need to calculate using an allocation approach."]
[]
[null,null,null,"READ ME"]
[]
[null,null,null,"This tab calculates the expected emissions associated with procurement of key assets for the OSW development."]
[]
[null,null,null,"Description cell"]
[null,null,null,"Guidance"]
[null,null,null,"Input cell"]
[null,null,null,"Calculation Cell"]
[null,null,null,"Preset Cell"]
[]
[null,1,null,"Results"]
[]
[null,1.1000000000000001,null,"Footprinting results "]
[]
[null,null,null,"Error check:",{"$f":"IF(COUNTIF(P:P,\"No\"),\"A unit matching error has been detected - please check the quantities and units input into this sheet\",\"No issues with unit matching\")","v":"No issues with unit matching"}]
[]
[null,null,null,"Module A1-A3 Results"]
[null,null,null,"Lifecycle Stage","Total Fossil Emissions by lifecycle stage","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Emissions by lifecycle stage ","Total Fossil Emissions by lifecycle stage ","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Project Emissions "]
[null,null,null,"Units"," kgCO2e"," kgCO2e"," kgCO2e"," kgCO2e","tCO2e","tCO2e","tCO2e","tCO2e"]
[null,null,null,"A1-A2 - Raw Material and Transport",{"$f":"SUM(Table_A1_Module_A1A2[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A1A2[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A1A2[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A1A2[Total Emissions (kgCO2e)])","v":0},{"$f":"E29/1000","v":0},0,0,0]
[null,null,null,"A3 - Manufacturing",{"$f":"SUM(Table_A1_Module_A3[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A3[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A3[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A3[Total Emissions (kgCO2e)])","v":0},0,0,0,0]
[null,null,null,"A1-A3 - Production and Manufacturing of finished assets & sub-components",{"$f":"SUM(Table_A1_Module_A1A3[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A1A3[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A1A3[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_A1_Module_A1A3[Total Emissions (kgCO2e)])","v":0},0,0,0,0]
[null,null,null,"A1-A3 - Production and Manufacturing Total",{"$f":"SUM(E29:E31)","v":0},0,0,0,0,0,0,0]
[]
[null,null,null,"Total material quantities used in development (table 2.1.4)"]
[null,null,null,"Total tonnage of materials used in OSW development",{"$f":"Material_Inventory[[#Totals],[Total material quantities for OSW development in terms of OSW Activity Taxonomy]]/1000","v":0},"tonnes"]
[]
[]
[null,2,null,"Footprinting Information"]
[]
[null,null,null,"You may calculate A1-A2 and A3 separately or combined as A1-A3 in tables 2.1.1, 2.1.2 and 2.1.3 respectively. EPDs, PCFs and LCAs will often cover A1-A3 combined. If you have input an emission factor that covers a fully manufactured asset or sub-component's A1-A3 into the primary or proxy database, you may use it in this calculation. This approach should involve significantly less data input from the user, as you can capture the full emissions of specific assets or subcomponents (e.g. a WTG, export cable, foundation) in one row, rather than splitting it into the constituent materials.\n\nMaterial composition approach (A1-A2, and A3 separately) \nYou should include the full bill of materials for all of the assets and sub-components (WTG, foundation, cables etc), including any material waste. Please provide the most accurate description of the materials you can, including material grade, recycled content, etc. The user should select the relevant emissions factor from the emissions factor database, or add a supplier-specific factor if available. \n\nAsset and component approach (A1-A3 combined)\nWhere you have emission factors from an LCA or EPD for fully manufactured assets or sub-components covering A1-A3 (cradle-to-gate) these should be used. Waste material should already be captured in the Emission Factor.\n\nYou may use a combination of approaches if, for example, you have an EPD for some of the core assets (WTG, Cables, etc) but need to take the material composition approach for other assets (Foundations, Offshore substation etc.).\n"]
[null,2.1]
[]
[null,"2.1.1",null,"Module A1-A2","Raw material supply and upstream transport"]
[null,null,null,"Material composition approach\nTo calculate A1-A2 emissions must consider the breakdown of materials used in assets and sub-components. Please individually input quantities of each material into the following table. For each material, you are also required to input transportation associated with transporting the material to the manufacturing site. Waste incurred through the production process must be included in the quantities. \n\nWhen using the material composition approach, the chosen emissions factors should be \"market\" factors for raw materials, rather than production factors, to include upstream transportation emissions from raw material manufacturers to tier 1 suppliers.\n\nA3 will be calculated in the following table using manufacturing process emission factors. "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Material Production Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1-A2 Raw Material and Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A2[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A2[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A2[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A2[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A2[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A2[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[]
[null,"2.1.2",null,"Module A3","Manufacturing of assets and components from raw materials"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Manufacturing Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A3 Manufacturing",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A3[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A1_Module_A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,"2.1.3",null,"Module A1-A3","Full production (e.g. a finished WTG, Cable, Foundation, etc.)"]
[]
[null,null,null,"Asset and component approach\nThis table should be used where you have populated the Primary or Proxy EF database with an emission factor for a full asset or subcomponent instead of using the material composition approach. \nFor example, supplier X provides you with an EPD for a full WTG, which shows the total emissions per turbine and does not require disaggregation into materials. \n\nWhen using proxy emission factor to represent the asset, the activity data quantity should be scaled accordingly. \nFor example, a proxy EF for a 10MW turbine is being used to represent a 12MW turbine. The activity data quantity shall be scaled linearly by multiplying by 1.2."]
[]
[null,null,null,"GHG Module","Finished Goods Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/UOM)","Emissions Factor: Biogenic (kgCO2e/UOM)","Emissions Factor: Land Use (kgCO2e/UOM)","Emissions Factor: Total (kgCO2e/UOM)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A1 - A3 Production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]]=Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]<>Table_A1_Module_A1A3[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"check entries\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A1_Module_A1A3[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A1_Module_A1A3[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]*Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A1_Module_A1A3[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A1_Module_A1A3[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A1_Module_A1A3[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,null,null,"Material composition of finished assets and components"]
[]
[null,null,null,"The following section is used to understand accurately understand the material composition of the OSW development, and should be completed where the assessor has used the asset and component approach. Understanding material composition is important for modelling the EoL pathways for these materials in modules C1-C5. Additionally, the following table allows further interpretation of material hotspots in your in your results. You may calculate the total emissions (A1-A3) for assets or subcomponents without detailing the material composition, but you will not be able to accurately model the EoL.\n\nIf you want to calculate the EoL section and see material hotspots in results, please populate the green cells in the material composition table. To do this you will need to describe the key manufacturing materials and contribution by mass (% of total) for each asset or sub-component."]
[null,null,null,null,null,null,null,null,null,null,null,null,"Bill of Material per unit of Finished Asset or Sub-component (required for Material inventory and End-of-Life)"]
[null,null,null,"GHG Module","Finished Goods Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Activity Data: Quantity","Units","Aluminium (kg)","Biogenic materials(kg) ","Carbon fibre (kg)","Concrete (kg)","Copper (kg)","Fibreglass (kg)","Oils & Lubricants (kg)","Other (kg)","Polymers (kg)","Steel (kg)","Total mass of unit asset or subcomponent (kg)","Total mass for full OSW development (kg)"]
[null,null,null,{"$f":"D157","v":"A1 - A3 Production"},0,0,0,0,{"$f":"I157","v":0},{"$f":"J157","v":0},{"$f":"N157","v":0},{"$f":"O157","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D158","v":"A1 - A3 Production"},0,0,0,0,{"$f":"I158","v":0},0,{"$f":"N158","v":0},{"$f":"O158","v":0},null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D159","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D160","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D161","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D162","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D163","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D164","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D165","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D166","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D167","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D168","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D169","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D170","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D171","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[null,null,null,{"$f":"D172","v":"A1 - A3 Production"},0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(SUM(Finished_Goods_Material_Composition[[#This Row],[Aluminium (kg)]:[Steel (kg)]]), \"Please polpulate material quantity sheets\")","v":0},{"$f":"IFERROR(Finished_Goods_Material_Composition[[#This Row],[Activity Data: Quantity]]*Finished_Goods_Material_Composition[[#This Row],[Total mass of unit asset or subcomponent (kg)]],\"CHECK ENTRIES\")","v":0}]
[]
[]
[null,"2.1.4",null,"Combined material inventory for the OSW development"]
[]
[null,null,null,"This table calculates  the total material inventory for the OSW development under study. This combines the quantities of materials from the separate tables 2.1.1 and 2.1.3. Units are expressed in kg rather than tonnes to match the standard waste treatment emission factor unit. The material inventory is important for ensuring mass balance across the lifecycle of the OSW development."]
[]
[null,null,null,"Material Type","Material inventory UoM","Total material quantities - Material approach","Total material quantities - Asset & sub-component approach","Total material quantities for OSW development in terms of OSW Activity Taxonomy"]
[null,null,null,"Aluminium","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D202,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Aluminium (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Biogenic materials","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D203,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Biogenic materials(kg) ]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Carbon fibre","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D204,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Carbon fibre (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Concrete","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D205,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Concrete (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Copper","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D206,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Copper (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Fibreglass","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D207,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Fibreglass (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Oils and Lubricants","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D208,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Oils & Lubricants (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Other materials","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D209,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Other (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Polymers","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D210,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Polymers (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Steel","kg",{"$f":"IFERROR(SUMIF(Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$D211,Table_A1_Module_A1A2[Activity Data: Quantity]),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(SUMPRODUCT(Finished_Goods_Material_Composition[Activity Data: Quantity],Finished_Goods_Material_Composition[Steel (kg)]),\"Complete material composition table\")","v":0},{"$f":"SUM(Material_Inventory[[#This Row],[Total material quantities - Material approach]:[Total material quantities - Asset & sub-component approach]])","v":0}]
[null,null,null,"Total","kg",{"$f":"SUBTOTAL(109,Material_Inventory[Total material quantities - Material approach])","v":0},{"$f":"SUBTOTAL(109,Material_Inventory[Total material quantities - Asset & sub-component approach])","v":0},{"$f":"SUBTOTAL(109,Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy])","v":0}]

{"sheet":"A4-A5 -Transport & Construction","index":14,"n_rows":102,"n_cols":27,"rows_kept":102,"cut":false,"hidden":false,"merged":[[24,4,24,7],[41,3,41,9],[8,3,8,12],[62,3,62,9],[83,3,83,9]]}
[]
[]
[null,null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,null,"DATA INPUTS - A4-A5 - Transportation and Construction & Installation"]
[]
[]
[null,null,null,"Lifecycle Stage Description"]
[]
[null,null,null,"Module A4 calculates the emissions associated with material and product transportation, including transportation of manufactured assets and construction materials from factory gate to the infrastructure construction site. It should also include the transportation of construction equipment to the infrastructure site. If known, please assign an Asset ID to the transportation, so the transportation emissions can be allocated to specific asset categories.\n\nModule A5: calculates the emissions associated with construction and installation activities from the development. \nThis also includes:\n  - Enabling works\n  - Temporary works\n  - Site compound works\n  - Construction installation of primary infrastructure assets (foundation laying, turbine installation, cable laying, and offshore & onshore substation construction for connecting the infrastructure to the grid) \nA5 should capture all fuel and energy-related emissions sources (scope 1&2, if conducted by the developer, scope 3 if outsourced) for the site during the entire construction and installation phase.  If known, please assign an Asset ID to the transportation, so the transportation emissions can be allocated to specific asset categories.\n\nFor some of the assets, transportation and installation may be carried out by the same asset (e.g. a Turbine Installation Vessel), in which case, it may be difficult to disaggregate the total amount of activity attributable to each module. In this case, please ensure that the full activity is included and clearly describe in your assumptions where the emissions have been accounted for\n"]
[]
[null,null,null,"READ ME"]
[]
[null,null,null,"This tab calculates the expected emissions associated with the transportation of assets to the development site."]
[]
[null,null,null,"Description cell"]
[null,null,null,"Guidance"]
[null,null,null,"Input cell"]
[null,null,null,"Calculation Cell"]
[null,null,null,"Preset Cell"]
[]
[null,1,null,"Results"]
[]
[null,1.1000000000000001,null,"Footprinting results "]
[]
[null,null,null,"Error check:",{"$f":"IF(COUNTIF(P:P,\"No\"),\"A unit matching error has been detected - please check the quantities and units input into this sheet\",\"No issues with unit matching\")","v":"No issues with unit matching"}]
[]
[null,null,null,"Module A4 Results"]
[null,null,null,"Lifecycle Stage","Total Fossil Emissions by lifecycle stage","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Emissions by lifecycle stage ","Total Fossil Emissions by lifecycle stage ","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Project Emissions "]
[null,null,null,"Units"," kgCO2e"," kgCO2e"," kgCO2e"," kgCO2e","tCO2e","tCO2e","tCO2e","tCO2e"]
[null,null,null,"A4 - Transport",{"$f":"SUM(Table_A4[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_A4[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_A4[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_A4[Total Emissions (kgCO2e)])","v":0},{"$f":"E30/1000","v":0},0,0,{"$f":"IFERROR(H30/1000,0)","v":0}]
[null,null,null,"A5 - Construction",{"$f":"SUM(Table_A5_Fuel[Calculated Emissions: Fossil (kgCO2e)],Table_A5_Waste[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_A5_Fuel[Calculated Emissions: Biogenic (kgCO2e)],Table_A5_Waste[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_A5_Fuel[Calculated Emissions: Land Use (kgCO2e)],Table_A5_Waste[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Waste[Total Emissions (kgCO2e)])","v":0},0,0,0,{"$f":"H31/1000","v":0}]
[null,null,null,"A4-A5 - Total emissions",{"$f":"SUM(E30:E31)","v":0},{"$f":"SUM(F30:F31)","v":0},0,0,0,0,0,{"$f":"SUM(L30:L31)","v":0}]
[]
[null,null,null,null,"Tonnes","Mass balance check (A1-A3)"]
[null,null,null,"Total tonnage of materials transported to site",{"$f":"SUM(Table_A4[Mass of assets and materials transported (tonnes)])","v":0},{"$f":"IFERROR(IF(('A1-A3 - Production'!E35-E35)/'A1-A3 - Production'!E35<0.001,\"OK\", \"Check material quantities and units (>1% difference)\"),\"Check inputs\")","v":"Check inputs"}]
[]
[]
[null,2,null,"Footprinting Information"]
[]
[null,2.1,null,"Module A4","Emissions due to vehicle, vessel, and aircraft use"]
[]
[null,null,null,"Please provide the electricity consumption, fuel consumption or distance travelled in vehicles, vessels and aircraft to transport equipment, assets, materials and staff to site.\nThis transportation represents transportation from factory gate to the OSW development. \nPlease note that marine gas oil is a liquid fuel and can be selected under the activity taxonomy L2 \"Liquid fuels lifecycle\"."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Mass of assets and materials transported (tonnes)","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A4 - Transportation",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A4[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A4[[#This Row],[Activity Data: Unit]]=Table_A4[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A4[[#This Row],[Emissions Factor: Unit]]<>Table_A4[[#This Row],[Activity Data: Unit]],\"No\")","v":""},null,{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A4[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A4[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A4[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A4[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A4[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A4[[#This Row],[Activity Data: Quantity]]*Table_A4[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A4[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A4[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A4[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A4[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,2.2000000000000002,null,"Module A5","Construction installation at site"]
[null,null,null,"Please provide the fuel and energy consumption or distance travelled in vehicles and equipment used in the construction and installation phase of the OSW development. This will typically include the fuel consumed by construction vessels offshore."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Construction Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Fuel[[#This Row],[Activity Data: Unit]]=Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Fuel[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Fuel[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Fuel[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Fuel[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]*Table_A5_Fuel[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Fuel[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Fuel[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_A5_Fuel[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Fuel[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,2.2000000000000002,null,"Module A5","Construction waste - Processing, sorting for reuse and recycling and final disposal for non-recyclable waste"]
[null,null,null,"Please provide waste type and fate for all waste created during construction.\n\nWhen calculating emissions from recycling, emissions must be allocated to either the initial product that gets recycled or the resultant recycled product. The OSW footprinting guidance uses the \"recycled content method - cut-off (100/0)\". The cut-off criteria 100/0 allocates all recycling emissions to the resultant recycled product. Waste is delivered to a recycling facility, sorted and then recycled. Under our cut-off criteria, emissions from transport and sorting must be accounted for but no emissions from recycling processes should be included under the end-of-life emissions calculation. Instead, all emissions are allocated to the resultant recycled product that leaves the processing facility and is used in a different system. Recycling totals will be carried forward for use in the calculation of Module D: Benefits & Loads beyond the system boundary. This means these tables provide no option for recycling. For any products that are expect to be recycled the sorting emission factor should be used."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Construction Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/UOM)","Emissions Factor: Biogenic (kgCO2e/UOM)","Emissions Factor: Land Use (kgCO2e/UOM)","Emissions Factor: Total (kgCO2e/UOM)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"A5 - Construction",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_A5_Waste[[#This Row],[Activity Data: Unit]]=Table_A5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_A5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_A5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_A5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_A5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_A5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]*Table_A5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_A5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_A5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_A5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_A5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]

{"sheet":"B1-B8 - Use","index":15,"n_rows":190,"n_cols":26,"rows_kept":190,"cut":false,"hidden":false,"merged":[[8,3,8,11],[9,3,9,11],[10,3,10,11],[11,3,11,11],[12,3,12,11],[150,3,150,9],[170,6,170,12],[171,3,171,9],[149,6,149,12],[67,6,67,12],[27,4,27,7],[47,3,47,9],[68,3,68,9],[88,3,88,9],[129,3,129,9],[108,3,108,9]]}
[]
[]
[null,null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,null,"DATA INPUTS - B1-B7 - Use of infrastructure"]
[]
[]
[null,null,null,"Lifecycle Stage Description"]
[]
[null,null,null,"Module B1 estimates the lifetime direct emissions associated with the use of the product. This module is related to any expected direct release or absorption of GHGs directly from the OSW development infrastructure itself. For emissions, this module may include the leakage of refrigerant gasses such as SF6 from the electrical infrastructure. Sometimes, this module can result in removals, for example, concrete will gradually absorb CO2 from the atmosphere over the course of its lifecycle due to the carbonation process in the material. "]
[null,null,null,"Modules B2-B5 calculates the lifetime emissions associated with ongoing upkeep of the assets that make up the OSW Development. B2-B5 can include ongoing general maintenance, significant and structural repair or planned replacement of assets during the development lifecycle (e.g. replacement of blades, coating or painting of blades). The calculation is split into material inputs in the upkeep processes. Material inputs cover all materials used in asset repair or replacement and energy inputs cover upkeep processes."]
[null,null,null,"Module B6 estimates the lifetime operational emissions associated with energy consumption or other use of the product. This module is related to any expected use of energy or fuels in the running of the development itself, for example, consumption of electricity & fuels during the operation of the OSW development."]
[null,null,null,"Module B7 estimates the lifetime operational emissions associated with water consumption in the asset. This module is related to any expected use of fresh water in the running of the development itself."]
[null,null,null,"Module B8 estimates the lifetime operational emissions associated with any use phase activities not otherwise captured in modules B1-B7."]
[]
[null,null,null,"READ ME"]
[]
[null,null,null,"This tab calculates the expected emissions from use of the infrastructure."]
[]
[null,null,null,"Description cell"]
[null,null,null,"Guidance"]
[null,null,null,"Input cell"]
[null,null,null,"Calculation Cell"]
[null,null,null,"Preset Cell"]
[]
[null,1,null,"Results"]
[]
[null,1.1000000000000001,null,"Footprinting results "]
[null,null,null,"Error check:",{"$f":"IF(COUNTIF(P:P,\"No\"),\"A unit matching error has been detected - please check the quantities and units input into this sheet\",\"No issues with unit matching\")","v":"No issues with unit matching"}]
[]
[null,null,null,"Modules B1-B8 Results"]
[null,null,null,"Lifecycle Stage","Total Fossil Emissions by lifecycle stage","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Emissions by lifecycle stage ","Total Fossil Emissions by lifecycle stage ","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Emissions by lifecycle stage "]
[null,null,null,"Units"," kgCO2e"," kgCO2e"," kgCO2e"," kgCO2e","tCO2e","tCO2e","tCO2e","tCO2e"]
[null,null,null,"B1 - Use",{"$f":"SUM(Table_B1_Refrigerants[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_B1_Refrigerants[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_B1_Refrigerants[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_B1_Refrigerants[Calculated Emissions: Total (kgCO2e)])","v":0},{"$f":"E33/1000","v":0},{"$f":"F33/1000","v":0},{"$f":"G33/1000","v":0},{"$f":"H33/1000","v":0}]
[null,null,null,"B2 - Maintenance",{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Materials[Calculated Emissions: Fossil (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Energy[Calculated Emissions: Fossil (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Waste[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Materials[Calculated Emissions: Biogenic (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Energy[Calculated Emissions: Biogenic (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Waste[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Materials[Calculated Emissions: Land Use (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Energy[Calculated Emissions: Land Use (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Waste[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Materials[Calculated Emissions: Total (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Energy[Calculated Emissions: Total (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D34,Table_B2B5_Waste[Calculated Emissions: Total (kgCO2e)])","v":0},{"$f":"E34/1000","v":0},{"$f":"F34/1000","v":0},{"$f":"G34/1000","v":0},{"$f":"H34/1000","v":0}]
[null,null,null,"B3 - Repair",{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Materials[Calculated Emissions: Fossil (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Energy[Calculated Emissions: Fossil (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Waste[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Materials[Calculated Emissions: Biogenic (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Energy[Calculated Emissions: Biogenic (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Waste[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Materials[Calculated Emissions: Land Use (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Energy[Calculated Emissions: Land Use (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Waste[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Materials[Calculated Emissions: Total (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Energy[Calculated Emissions: Total (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D35,Table_B2B5_Waste[Calculated Emissions: Total (kgCO2e)])","v":0},{"$f":"E35/1000","v":0},{"$f":"F35/1000","v":0},0,0]
[null,null,null,"B4 - Replacement",{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Materials[Calculated Emissions: Fossil (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Energy[Calculated Emissions: Fossil (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Waste[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Materials[Calculated Emissions: Biogenic (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Energy[Calculated Emissions: Biogenic (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Waste[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Materials[Calculated Emissions: Land Use (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Energy[Calculated Emissions: Land Use (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Waste[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Materials[Calculated Emissions: Total (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Energy[Calculated Emissions: Total (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D36,Table_B2B5_Waste[Calculated Emissions: Total (kgCO2e)])","v":0},0,0,0,0]
[null,null,null,"B5 - Refurbishment",{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Materials[Calculated Emissions: Fossil (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Energy[Calculated Emissions: Fossil (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Waste[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Materials[Calculated Emissions: Biogenic (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Energy[Calculated Emissions: Biogenic (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Waste[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Materials[Calculated Emissions: Land Use (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Energy[Calculated Emissions: Land Use (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Waste[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUMIF(Table_B2B5_Materials[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Materials[Calculated Emissions: Total (kgCO2e)])+SUMIF(Table_B2B5_Energy[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Energy[Calculated Emissions: Total (kgCO2e)])+SUMIF(Table_B2B5_Waste[[GHG Module]:[GHG Module]],$D37,Table_B2B5_Waste[Calculated Emissions: Total (kgCO2e)])","v":0},0,0,0,0]
[null,null,null,"B6 - Operational energy consumption",{"$f":"SUM(Table_B6[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_B6[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_B6[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_B6[Total Emissions (kgCO2e)])","v":0},0,0,0,0]
[null,null,null,"B7 - Operational water consumption",{"$f":"SUM(Table_B7[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_B7[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_B7[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_B7[Total Emissions (kgCO2e)])","v":0},0,0,0,0]
[null,null,null,"B8 - Operational material consumption",{"$f":"SUM(Table_B8[Calculated Emissions: Fossil (kgCO2e)])","v":0},{"$f":"SUM(Table_B8[Calculated Emissions: Biogenic (kgCO2e)])","v":0},{"$f":"SUM(Table_B8[Calculated Emissions: Land Use (kgCO2e)])","v":0},{"$f":"SUM(Table_B8[Total Emissions (kgCO2e)])","v":0},0,0,0,0]
[null,null,null,"B1-B8 Use Total",{"$f":"SUM(E33:E40)","v":0},0,0,0,0,0,0,0]
[]
[null,2,null,"Footprinting Information"]
[]
[null,2.1]
[]
[null,"2.1.1",null,"Module B1 - Use of assets"]
[null,null,null,"Please provide expected direct emissions from the operations of the OSW development over the full lifetime of the development. This may typically include any leakage of insulating gas from transformer equipment in the system boundary, or leakage of refrigerant gas from cooling systems. You may also include any direct removals that occur within the system boundary, technological or biological."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N51*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N51*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N51*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N51*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N52*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N52*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N52*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N52*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N53*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N53*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N53*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N53*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N54*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N54*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N54*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N54*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N55*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N55*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N55*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N55*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N56*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N56*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N56*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N56*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N57*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N57*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N57*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N57*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N58*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N58*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N58*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N58*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N59*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N59*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N59*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N59*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N60*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N60*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N60*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N60*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N61*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N61*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N61*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N61*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N62*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N62*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N62*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N62*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N63*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N63*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N63*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N63*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N64*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N64*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N64*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N64*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N65*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N65*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N65*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N65*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B1 - Use",null,null,null,null,"Direct emissions and removals",null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]]=Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]<>Table_B1_Refrigerants[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES \"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B1_Refrigerants[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B1_Refrigerants[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR($N66*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IFERROR($N66*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],0)","v":0},{"$f":"IFERROR($N66*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],0)","v":0},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR($N66*Table_B1_Refrigerants[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B1_Refrigerants[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B1_Refrigerants[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B1_Refrigerants[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,"2.1.2",null,"Modules B2 - B5 - Maintenance, repair, replacement & refurbishment"]
[null,null,null,"Please provide expected material inputs used in the maintenance, repair, replacement or refurbishment of the assets over the full lifetime of the development.\n\nB2: This module focuses on the routine activities required to maintain the operation of the OSW development during its service life. It typically includes routine inspection and servicing.\n\nB3: This module focuses on the non-routine activities required to restore a product or system back to operational condition after an unexpected failure or damage. It typically includes spare parts.\n\nB4: This module involves replacing major components or parts during the operational life of the system when they reach the end of their service life. It typically includes the replacement of component parts which reach end-of-life before the end of the service life of the OSW development (e.g. replacement blades)\n\nB5: This module involves large-scale upgrades or modifications to the OSW development that may extend its service life, or improve it's performance. "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Materials[[#This Row],[Activity Data: Unit]]=Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Materials[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Materials[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Materials[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Materials[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Materials[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Materials[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Materials[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Materials[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Materials[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,null,null,"Please provide energy consumption, fuel consumption and manufacturing process data from maintenance, repair, replacement or refurbishment of the OSW development over the full lifetime of the development. This typically includes the transportation of equipment and maintenance and repair crews to the site using SOVs, and other vessels."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Energy[[#This Row],[Activity Data: Unit]]=Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Energy[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Energy[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Energy[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Energy[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Energy[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Energy[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Energy[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B2B5_Energy[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Energy[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,null,null,"Please provide expected waste data for maintenance, repair, replacement or refurbishment of the OSW development over the full lifetime of the development."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B2B5_Waste[[#This Row],[Activity Data: Unit]]=Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]<>Table_B2B5_Waste[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B2B5_Waste[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B2B5_Waste[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B2B5_Waste[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]*Table_B2B5_Waste[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B2B5_Waste[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B2B5_Waste[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]]),SUM(Table_B2B5_Waste[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B2B5_Waste[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,"2.1.3",null,"Module B6 - Operational energy consumption"]
[null,null,null,"Please provide the expected energy consumption required for operation over the full lifetime of the development. This includes any electricity imported from the grid during start-up or any planned outage. It may also include any fuels used for back up generators used during operation to support critical systems."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B6 - Operational energy consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B6[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B6[[#This Row],[Activity Data: Unit]]=Table_B6[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B6[[#This Row],[Emissions Factor: Unit]]<>Table_B6[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B6[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B6[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B6[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B6[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B6[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B6[[#This Row],[Activity Data: Quantity]]*Table_B6[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B6[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B6[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B6[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B6[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,"2.1.4",null,"Module B7 - Operational water consumption"]
[null,null,null,"Please provide data for the expected fresh water consumption over the full lifetime of the development."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B7 - Operational water consumption",null,null,null,null,"Electricity, fuels and other utilities","Water consumption",null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B7[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B7[[#This Row],[Activity Data: Unit]]=Table_B7[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B7[[#This Row],[Emissions Factor: Unit]]<>Table_B7[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B7[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B7[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B7[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B7[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B7[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK Entries\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B7[[#This Row],[Activity Data: Quantity]]*Table_B7[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B7[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B7[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_B7[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B7[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[]
[null,"2.1.5",null,"Module B8 - Operational activities not otherwise captured in modules B1-B7"]
[null,null,null,"Please provide data for any other specific activities conducted in the regular operation of the OSW development under study that may not be captured in modules B1-B7."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/UOM)","Emissions Factor: Biogenic (kgCO2e/UOM)","Emissions Factor: Land Use (kgCO2e/UOM)","Emissions Factor: Total (kgCO2e/UOM)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"B8 - Operational material consumption",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_B8[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_B8[[#This Row],[Activity Data: Unit]]=Table_B8[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_B8[[#This Row],[Emissions Factor: Unit]]<>Table_B8[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_B8[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_B8[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_B8[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_B8[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_B8[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Biogenic (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]]=\"Unknown\",\"Unknown\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Land Use (kgCO2e/UOM)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_B8[[#This Row],[Activity Data: Quantity]]*Table_B8[[#This Row],[Emissions Factor: Total (kgCO2e/UOM)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_B8[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_B8[[#This Row],[Emissions Factor: Fossil (kgCO2e/UOM)]:[Emissions Factor: Land Use (kgCO2e/UOM)]])>0,SUM(Table_B8[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_B8[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"}]

{"sheet":"C1-C5 - End-of-Life","index":16,"n_rows":273,"n_cols":30,"rows_kept":273,"cut":false,"hidden":false,"merged":[[64,26,64,29],[91,26,91,29],[47,3,47,5],[27,4,27,7],[47,7,47,9],[83,6,83,12],[8,3,8,10],[9,3,9,10],[10,3,10,10],[11,3,11,10],[12,3,12,10],[112,3,112,9],[63,3,63,9],[56,3,56,9],[84,3,84,9],[180,6,180,12],[159,3,159,9],[134,3,134,9],[135,26,135,29],[113,26,113,29],[254,3,254,9],[182,3,182,9],[204,3,204,9]]}
[]
[]
[null,null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,null,"DATA INPUTS - C1-C5 - End-of-Life of infrastructure"]
[]
[]
[null,null,null,"Lifecycle Stage Description"]
[]
[null,null,null,"Module C1 calculates emissions associated with the deconstruction and demolition of the OSW development at EoL. This should cover all site-based activities required to dismantle, deconstruct and/or demolish the asset being assessed. The carbon emissions arising from any on or off-site deconstruction and demolition activities, including any energy consumption for site accommodation and plant use, must be considered in Module C1."]
[null,null,null,"Module C2 calculates emissions associated with the transportation of deconstruction and demolition arisings to the appropriate disposal site, including any interim stations."]
[null,null,null,"Module C3 calculates emissions associated with the treatment and processing of materials and/or components intended to be recovered and reused or recycled after the end of the life of the OSW development."]
[null,null,null,"Module C4 calculates emissions associated with the disposal of the OSW development materials at their end of life. The two primary forms of disposal are incineration (without energy recovery) or landfill of materials. This is for items not being recovered for reuse and/or recycling."]
[null,null,null,"Module C5 calculates emissions associated with any relandscaping activities at sea or on land after End-of-Life of the OSW development"]
[]
[null,null,null,"READ ME"]
[]
[null,null,null,"This tab calculates the expected emissions from when the infrastructure has reached the end of it's useful life."]
[]
[null,null,null,"Description cell"]
[null,null,null,"Guidance"]
[null,null,null,"Input cell"]
[null,null,null,"Calculation Cell"]
[null,null,null,"Preset Cell"]
[]
[null,1,null,"Results"]
[]
[null,1.1000000000000001,null,"Footprinting results "]
[null,null,null,"Error check:",{"$f":"IF($G$48=\"No data\",IF(COUNTIF($O$163:$Q$230,\"No\"),\"A unit matching error has been detected - please check the quantities and units input into this sheet\",\"No issues with unit\"),IF(COUNTIF($O$54:$Q$132,\"No\"),\"A unit matching error has been detected - please check the quantities and units input into this sheet\",\"No issues with unit\"))","v":"No issues with unit"}]
[]
[null,null,null,"Modules C1-C4 Results"]
[null,null,null,"Lifecycle Stage","Footprinting option selection","Total Fossil Emissions by lifecycle stage","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Emissions by lifecycle stage ","Total Fossil Emissions by lifecycle stage ","Total Biogenic Emissions by lifecycle stage","Total Land Use Emissions by lifecycle stage","Total Project Emissions "]
[null,null,null,"Units",null," kgCO2e"," kgCO2e"," kgCO2e"," kgCO2e","tCO2e","tCO2e","tCO2e","tCO2e"]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"IF($G$48=\"No data\",\"Option B\",\"Option A\")","v":"Option A"},{"$f":"_xlfn.IFS($E33=\"Option A\",SUM(Table_C1_Option_A[Fossil Emissions: Scaled to Capacity of Development (kgCO2e)]),$E33=\"Option B\",SUM(Table_C1_Option_B[Calculated Emissions: Fossil (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E33=\"Option A\",SUM(Table_C1_Option_A[Biogenic Emissions: Scaled to Capacity of Development (kgCO2e)]),$E33=\"Option B\",SUM(Table_C1_Option_B[Calculated Emissions: Biogenic (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E33=\"Option A\",SUM(Table_C1_Option_A[Land Use Emissions: Scaled to Capacity of Development (kgCO2e)]),$E33=\"Option B\",SUM(Table_C1_Option_B[Calculated Emissions: Land Use (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E33=\"Option A\",SUM(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)]),$E33=\"Option B\",SUM(Table_C1_Option_B[Calculated Emissions: Total (kgCO2e)]))","v":0},{"$f":"IFERROR(F33/1000,0)","v":0},{"$f":"IFERROR(G33/1000,0)","v":0},0,0]
[null,null,null,"C2 - Transport to waste processing",{"$f":"IF($G$48=\"No data\",\"Option B\",\"Option A\")","v":"Option A"},{"$f":"_xlfn.IFS($E34=\"Option A\",SUM(Table_C2_Option_A[Fossil Emissions: Scaled to Capacity of Development (kgCO2e)]),$E34=\"Option B\",SUM(Table_C2_Option_B[Calculated Emissions: Fossil (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E34=\"Option A\",SUM(Table_C2_Option_A[Biogenic Emissions: Scaled to Capacity of Development (kgCO2e)]),$E34=\"Option B\",SUM(Table_C2_Option_B[Calculated Emissions: Biogenic (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E34=\"Option A\",SUM(Table_C2_Option_A[Land Use Emissions: Scaled to Capacity of Development (kgCO2e)]),$E34=\"Option B\",SUM(Table_C2_Option_B[Calculated Emissions: Land Use (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E34=\"Option A\",SUM(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)]),$E34=\"Option B\",SUM(Table_C2_Option_B[Calculated Emissions: Total (kgCO2e)]))","v":0},{"$f":"IFERROR(F34/1000,0)","v":0},0,0,{"$f":"IFERROR(I34/1000,0)","v":0}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",{"$f":"IF($G$48=\"No data\",\"Option B\",\"Option A\")","v":"Option A"},{"$f":"_xlfn.IFS($E35=\"Option A\",SUM(Table_C3C4_Option_A[Fossil Emissions: Scaled to Capacity of Development (kgCO2e)]),$E35=\"Option B\",SUM(Table_C3C4_Option_B[Calculated Emissions: Fossil (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E35=\"Option A\",SUM(Table_C3C4_Option_A[Biogenic Emissions: Scaled to Capacity of Development (kgCO2e)]),$E35=\"Option B\",SUM(Table_C3C4_Option_B[Calculated Emissions: Biogenic (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E35=\"Option A\",SUM(Table_C3C4_Option_A[Land Use Emissions: Scaled to Capacity of Development (kgCO2e)]),$E35=\"Option B\",SUM(Table_C3C4_Option_B[Calculated Emissions: Land Use (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E35=\"Option A\",SUM(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)]),$E35=\"Option B\",SUM(Table_C3C4_Option_B[Calculated Emissions: Total (kgCO2e)]))","v":0},{"$f":"IFERROR(F35/1000,0)","v":0},0,0,{"$f":"IFERROR(I35/1000,0)","v":0}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF($G$48=\"No data\",\"Option B\",\"Option A\")","v":"Option A"},{"$f":"_xlfn.IFS($E36=\"Option A\",SUM(Table_C5_Option_A[Fossil Emissions: Scaled to Capacity of Development (kgCO2e)]),$E36=\"Option B\",SUM(Table_C5_Option_B[Calculated Emissions: Fossil (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E36=\"Option A\",SUM(Table_C5_Option_A[Biogenic Emissions: Scaled to Capacity of Development (kgCO2e)]),$E36=\"Option B\",SUM(Table_C5_Option_B[Calculated Emissions: Biogenic (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E36=\"Option A\",SUM(Table_C5_Option_A[Land Use Emissions: Scaled to Capacity of Development (kgCO2e)]),$E36=\"Option B\",SUM(Table_C5_Option_B[Calculated Emissions: Land Use (kgCO2e)]))","v":0},{"$f":"_xlfn.IFS($E36=\"Option A\",SUM(Table_C5_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)]),$E36=\"Option B\",SUM(Table_C5_Option_B[Calculated Emissions: Total (kgCO2e)]))","v":0},{"$f":"IFERROR(F36/1000,0)","v":0},{"$f":"IFERROR(G36/1000,0)","v":0},{"$f":"IFERROR(H36/1000,0)","v":0},{"$f":"IFERROR(I36/1000,0)","v":0}]
[null,null,null,"C1 - C5","Total",{"$f":"SUM(F33:F35)","v":0},0,0,0,0,0,0,0]
[]
[]
[null,null,null,null,"Footprinting option selection","Tonnes","Mass balance check (A1-A3)"]
[null,null,null,"Total quantity of waste processed at End-of-Life (C3-C4)",{"$f":"IF($G$48=\"No data\",\"Option B\",\"Option A\")","v":"Option A"},{"$f":"IF(E41=\"Option A\", SUM(Table_C3C4_Option_A[Activity Data: Quantity]),SUM(Table_C3C4_Option_B[Activity Data: Quantity]))/1000","v":0},{"$f":"IFERROR(IF(('A1-A3 - Production'!E35-F41)/'A1-A3 - Production'!E35<0.001,\"OK\",\"Check material quantities and units (>1% difference)\"),\"Check inputs\")","v":"Check inputs"}]
[]
[null,2,null,"Calculation Methodology Selection"]
[]
[null,2.1,null,"Please answer the prompts below"]
[]
[]
[null,null,null,"Which of the following data types do you have available for the end-of-life emissions calculation?\n - primary data\n - proxy data for EoL activities from another development\n - no data available",null,null,"Primary",{"$f":"_xlfn.IFS(OR(G48=\"Primary\", G48=\"Proxy\"), \"Please follow calculation 3.1 option A\",G48=\"No data\", \"The end-of-life emissions will be calculated in 3.2 option B and are modelled based on the emissions captured in lifecycle module A. Please scroll down to calculation 3.2 to review\")","v":"Please follow calculation 3.1 option A"}]
[]
[]
[null,3,null,"Footprinting Information"]
[]
[null,null,null,"Please use the prompt question in section 2.1 to determine which option is feasible given the data available. "]
[]
[null,3.1,null,"Option A"]
[]
[null,null,null,"If following a proxy methodology (using data from another previously decommissioned site to estimated the required activities for this site) please can you provide details of the proxy site."]
[]
[null,null,null,"Proxy site name","Proxy site location","MW capacity of proxy site","MW capacity of development under calculation"]
[null,null,null,null,null,1000,{"$f":"Installed_capacity__MW","v":880}]
[]
[null,"3.1.1",null,"Module C1 - Deconstruction Demolition"]
[]
[null,null,null,"Please provide energy consumption data for demolition and deconstruction of the site you have data for."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation",null,null,null,null,null,null,null,null,null,null,null,"Relevant if you are using proxy data to estimate the EoL emissions, ignore if using primary data"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)","Fossil Emissions: Scaled to Capacity of Development (kgCO2e)","Biogenic Emissions: Scaled to Capacity of Development (kgCO2e)","Land Use Emissions: Scaled to Capacity of Development (kgCO2e)","Total Emissions: Scaled to Capacity of Development (kgCO2e)"]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C1_Option_A[[#This Row],[Activity Data: Unit]]=Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C1_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C1_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C1_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C1_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C1_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C1_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C1_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,"3.1.2"]
[null,null,null,"Module C2 - Transport Emissions","Emissions due to vehicle, vessel, and aircraft use"]
[null,null,null,"The calculation of the transportation emissions is carried out on a tonne-kilometre basis. Please provide the total weight of transportation journey in tonnes and the total distance in km. If the journey has multiple legs, including overland and sea transportation, you can capture this separately in the input areas for Leg 1 and Leg 2. \n\nPlease provide data on the transportation of assets and waste materials to their disposal sites, covering mode of transport, fuel consumption, OR mode, distance and weight at the site you have data for. Details on assumptions that can be used for transport distances are provided in the table below. "]
[]
[null,null,null,"EoL scenario","Transport scenario"]
[null,null,null,"Reuse / recycling on site","No transport emissions; C2=0"]
[null,null,null,"Reuse / recycling elsewhere","Average between two closest recycling sites"]
[null,null,null,"Landfill / incineration","Average between two closest landfill sites"]
[null,null,null,"Source: RICS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation",null,null,null,null,null,null,null,null,null,null,null,"Relevant if you are using proxy data to estimate the EoL emissions, ignore if using primary data"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)","Fossil Emissions: Scaled to Capacity of Development (kgCO2e)","Biogenic Emissions: Scaled to Capacity of Development (kgCO2e)","Land Use Emissions: Scaled to Capacity of Development (kgCO2e)","Total Emissions: Scaled to Capacity of Development (kgCO2e)"]
[null,null,null,"C2: Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C2 - Transport",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C2_Option_A[[#This Row],[Activity Data: Unit]]=Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C2_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C2_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C2_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C2_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,"3.1.3"]
[null,null,null,"Module C3-C4","Processing, sorting for reuse and recycling and final disposal for non-recyclable waste"]
[]
[null,null,null,"When calculating emissions from recycling, emissions are allocated to either the initial system that provides the material to be recycled, or the resultant recycled product. The OSW footprinting guidance uses the \"recycled content method - cut-off (100/0)\". The cut-off criteria 100/0 allocates recycling emissions to the resultant recycled product. Waste is processed and sorted, before being delivered to a manufacturing (recycling) facility to become an input material for a subsequent product. Under our cut-off criteria, emissions from transportation, processing and sorting of materials from the OSW development must be accounted for but no emissions from subsequent manufacturing (recycling) processes should be included under the end-of-life emissions for the OSW development.. Instead, all emissions are allocated to the resultant recycled product that leaves the processing facility and is used in a different system. Recycling totals may be carried forward for use in the calculation of Module D: Benefits & Loads beyond the system boundary. This means these tables provide no option for recycling. For any products that are expect to be recycled the sorting emission factor should be used."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation",null,null,null,null,null,null,null,null,null,null,null,"Relevant if you are using proxy data to estimate the EoL emissions, ignore if using primary data"]
[null,null,null,"GHG Module","Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)","Fossil Emissions: Scaled to Capacity of Development (kgCO2e)","Biogenic Emissions: Scaled to Capacity of Development (kgCO2e)","Land Use Emissions: Scaled to Capacity of Development (kgCO2e)","Total Emissions: Scaled to Capacity of Development (kgCO2e)"]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(\"Landfill\"=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]), \"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C3C4_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,"3.1.4"]
[null,null,null,"Module C5","Emissions due to vehicle, vessel, and aircraft use and emissions from materials and equipment used in any relandscaping activities for the OSW development post decommissioning"]
[]
[null,null,null,"Please provide the electricity or fuel consumption or distance travelled in vehicles, vessels and aircraft during relandscaping."]
[null,null,null,null,null,null,null,null,null,null,"`",null,null,null,"Note: All Activity Data quantities should be input as a value rather than a formula or calculation",null,null,null,null,null,null,null,null,null,null,null,"Relevant if you are using proxy data to estimate the EoL emissions, ignore if using primary data"]
[null,null,null,"GHG Module","Preconstruction Activity Description","Asset","Component","Supplier","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)","Fossil Emissions: Scaled to Capacity of Development (kgCO2e)","Biogenic Emissions: Scaled to Capacity of Development (kgCO2e)","Land Use Emissions: Scaled to Capacity of Development (kgCO2e)","Total Emissions: Scaled to Capacity of Development (kgCO2e)"]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,"C5 - Relandscaping",null,null,null,null,null,null,null,null,null,null,null,{"$f":"_xlfn.IFS(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C5_Option_A[[#This Row],[Activity Data: Unit]]=Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]<>Table_C5_Option_A[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_A[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_A[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_A[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]]),\"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C1_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Biogenic (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_A[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Land Use (kgCO2e)]]), \"CHECK ENTRIES\")))","v":"-"},{"$f":"IF(ISBLANK(Table_C5_Option_A[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF($G$48=\"Proxy\",(Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]/$G$60)*$F$60,Table_C5_Option_A[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[]
[]
[null,3.2,null,"Option B"]
[]
[null,"3.2.1",null,"Module C1 - Deconstruction/demolition"]
[]
[null,null,null,"Fuel and energy consumption data for demolition and deconstruction has been auto-populated from the data provided in A5 - Construction, assuming that deconstruction fuel consumptions is equivalent to construction fuel consumption. No input is required here."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: All quantities should be input as a final figure rather than a formula or calculation"]
[null,null,null,"GHG Module","Construction Activity Description","Asset","Component","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E66","v":0},{"$f":"'A4-A5 -Transport & Construction'!F66","v":0},{"$f":"'A4-A5 -Transport & Construction'!G66","v":0},{"$f":"'A4-A5 -Transport & Construction'!I66","v":0},{"$f":"'A4-A5 -Transport & Construction'!J66","v":0},{"$f":"'A4-A5 -Transport & Construction'!K66","v":0},{"$f":"'A4-A5 -Transport & Construction'!L66","v":0},{"$f":"'A4-A5 -Transport & Construction'!M66","v":0},{"$f":"'A4-A5 -Transport & Construction'!N66","v":0},{"$f":"'A4-A5 -Transport & Construction'!O66","v":0},{"$f":"'A4-A5 -Transport & Construction'!P66","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y66","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z66","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E67","v":0},{"$f":"'A4-A5 -Transport & Construction'!F67","v":0},{"$f":"'A4-A5 -Transport & Construction'!G67","v":0},{"$f":"'A4-A5 -Transport & Construction'!I67","v":0},{"$f":"'A4-A5 -Transport & Construction'!J67","v":0},{"$f":"'A4-A5 -Transport & Construction'!K67","v":0},{"$f":"'A4-A5 -Transport & Construction'!L67","v":0},{"$f":"'A4-A5 -Transport & Construction'!M67","v":0},{"$f":"'A4-A5 -Transport & Construction'!N67","v":0},{"$f":"'A4-A5 -Transport & Construction'!O67","v":0},{"$f":"'A4-A5 -Transport & Construction'!P67","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y67","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z67","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E68","v":0},{"$f":"'A4-A5 -Transport & Construction'!F68","v":0},{"$f":"'A4-A5 -Transport & Construction'!G68","v":0},{"$f":"'A4-A5 -Transport & Construction'!I68","v":0},{"$f":"'A4-A5 -Transport & Construction'!J68","v":0},{"$f":"'A4-A5 -Transport & Construction'!K68","v":0},{"$f":"'A4-A5 -Transport & Construction'!L68","v":0},{"$f":"'A4-A5 -Transport & Construction'!M68","v":0},{"$f":"'A4-A5 -Transport & Construction'!N68","v":0},{"$f":"'A4-A5 -Transport & Construction'!O68","v":0},{"$f":"'A4-A5 -Transport & Construction'!P68","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y68","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z68","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E69","v":0},{"$f":"'A4-A5 -Transport & Construction'!F69","v":0},{"$f":"'A4-A5 -Transport & Construction'!G69","v":0},{"$f":"'A4-A5 -Transport & Construction'!I69","v":0},{"$f":"'A4-A5 -Transport & Construction'!J69","v":0},{"$f":"'A4-A5 -Transport & Construction'!K69","v":0},{"$f":"'A4-A5 -Transport & Construction'!L69","v":0},{"$f":"'A4-A5 -Transport & Construction'!M69","v":0},{"$f":"'A4-A5 -Transport & Construction'!N69","v":0},{"$f":"'A4-A5 -Transport & Construction'!O69","v":0},{"$f":"'A4-A5 -Transport & Construction'!P69","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y69","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z69","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E70","v":0},{"$f":"'A4-A5 -Transport & Construction'!F70","v":0},{"$f":"'A4-A5 -Transport & Construction'!G70","v":0},{"$f":"'A4-A5 -Transport & Construction'!I70","v":0},{"$f":"'A4-A5 -Transport & Construction'!J70","v":0},{"$f":"'A4-A5 -Transport & Construction'!K70","v":0},{"$f":"'A4-A5 -Transport & Construction'!L70","v":0},{"$f":"'A4-A5 -Transport & Construction'!M70","v":0},{"$f":"'A4-A5 -Transport & Construction'!N70","v":0},{"$f":"'A4-A5 -Transport & Construction'!O70","v":0},{"$f":"'A4-A5 -Transport & Construction'!P70","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y70","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z70","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E71","v":0},{"$f":"'A4-A5 -Transport & Construction'!F71","v":0},{"$f":"'A4-A5 -Transport & Construction'!G71","v":0},{"$f":"'A4-A5 -Transport & Construction'!I71","v":0},{"$f":"'A4-A5 -Transport & Construction'!J71","v":0},{"$f":"'A4-A5 -Transport & Construction'!K71","v":0},{"$f":"'A4-A5 -Transport & Construction'!L71","v":0},{"$f":"'A4-A5 -Transport & Construction'!M71","v":0},{"$f":"'A4-A5 -Transport & Construction'!N71","v":0},{"$f":"'A4-A5 -Transport & Construction'!O71","v":0},{"$f":"'A4-A5 -Transport & Construction'!P71","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y71","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z71","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E72","v":0},{"$f":"'A4-A5 -Transport & Construction'!F72","v":0},{"$f":"'A4-A5 -Transport & Construction'!G72","v":0},{"$f":"'A4-A5 -Transport & Construction'!I72","v":0},{"$f":"'A4-A5 -Transport & Construction'!J72","v":0},{"$f":"'A4-A5 -Transport & Construction'!K72","v":0},{"$f":"'A4-A5 -Transport & Construction'!L72","v":0},{"$f":"'A4-A5 -Transport & Construction'!M72","v":0},{"$f":"'A4-A5 -Transport & Construction'!N72","v":0},{"$f":"'A4-A5 -Transport & Construction'!O72","v":0},{"$f":"'A4-A5 -Transport & Construction'!P72","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y72","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z72","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E73","v":0},{"$f":"'A4-A5 -Transport & Construction'!F73","v":0},{"$f":"'A4-A5 -Transport & Construction'!G73","v":0},{"$f":"'A4-A5 -Transport & Construction'!I73","v":0},{"$f":"'A4-A5 -Transport & Construction'!J73","v":0},{"$f":"'A4-A5 -Transport & Construction'!K73","v":0},{"$f":"'A4-A5 -Transport & Construction'!L73","v":0},{"$f":"'A4-A5 -Transport & Construction'!M73","v":0},{"$f":"'A4-A5 -Transport & Construction'!N73","v":0},{"$f":"'A4-A5 -Transport & Construction'!O73","v":0},{"$f":"'A4-A5 -Transport & Construction'!P73","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y73","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z73","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E74","v":0},{"$f":"'A4-A5 -Transport & Construction'!F74","v":0},{"$f":"'A4-A5 -Transport & Construction'!G74","v":0},{"$f":"'A4-A5 -Transport & Construction'!I74","v":0},{"$f":"'A4-A5 -Transport & Construction'!J74","v":0},{"$f":"'A4-A5 -Transport & Construction'!K74","v":0},{"$f":"'A4-A5 -Transport & Construction'!L74","v":0},{"$f":"'A4-A5 -Transport & Construction'!M74","v":0},{"$f":"'A4-A5 -Transport & Construction'!N74","v":0},{"$f":"'A4-A5 -Transport & Construction'!O74","v":0},{"$f":"'A4-A5 -Transport & Construction'!P74","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y74","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z74","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E75","v":0},{"$f":"'A4-A5 -Transport & Construction'!F75","v":0},{"$f":"'A4-A5 -Transport & Construction'!G75","v":0},{"$f":"'A4-A5 -Transport & Construction'!I75","v":0},{"$f":"'A4-A5 -Transport & Construction'!J75","v":0},{"$f":"'A4-A5 -Transport & Construction'!K75","v":0},{"$f":"'A4-A5 -Transport & Construction'!L75","v":0},{"$f":"'A4-A5 -Transport & Construction'!M75","v":0},{"$f":"'A4-A5 -Transport & Construction'!N75","v":0},{"$f":"'A4-A5 -Transport & Construction'!O75","v":0},{"$f":"'A4-A5 -Transport & Construction'!P75","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y75","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z75","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E76","v":0},{"$f":"'A4-A5 -Transport & Construction'!F76","v":0},{"$f":"'A4-A5 -Transport & Construction'!G76","v":0},{"$f":"'A4-A5 -Transport & Construction'!I76","v":0},{"$f":"'A4-A5 -Transport & Construction'!J76","v":0},{"$f":"'A4-A5 -Transport & Construction'!K76","v":0},{"$f":"'A4-A5 -Transport & Construction'!L76","v":0},{"$f":"'A4-A5 -Transport & Construction'!M76","v":0},{"$f":"'A4-A5 -Transport & Construction'!N76","v":0},{"$f":"'A4-A5 -Transport & Construction'!O76","v":0},{"$f":"'A4-A5 -Transport & Construction'!P76","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y76","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z76","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E77","v":0},{"$f":"'A4-A5 -Transport & Construction'!F77","v":0},{"$f":"'A4-A5 -Transport & Construction'!G77","v":0},{"$f":"'A4-A5 -Transport & Construction'!I77","v":0},{"$f":"'A4-A5 -Transport & Construction'!J77","v":0},{"$f":"'A4-A5 -Transport & Construction'!K77","v":0},{"$f":"'A4-A5 -Transport & Construction'!L77","v":0},{"$f":"'A4-A5 -Transport & Construction'!M77","v":0},{"$f":"'A4-A5 -Transport & Construction'!N77","v":0},{"$f":"'A4-A5 -Transport & Construction'!O77","v":0},{"$f":"'A4-A5 -Transport & Construction'!P77","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y77","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z77","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E78","v":0},{"$f":"'A4-A5 -Transport & Construction'!F78","v":0},{"$f":"'A4-A5 -Transport & Construction'!G78","v":0},{"$f":"'A4-A5 -Transport & Construction'!I78","v":0},{"$f":"'A4-A5 -Transport & Construction'!J78","v":0},{"$f":"'A4-A5 -Transport & Construction'!K78","v":0},{"$f":"'A4-A5 -Transport & Construction'!L78","v":0},{"$f":"'A4-A5 -Transport & Construction'!M78","v":0},{"$f":"'A4-A5 -Transport & Construction'!N78","v":0},{"$f":"'A4-A5 -Transport & Construction'!O78","v":0},{"$f":"'A4-A5 -Transport & Construction'!P78","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y78","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z78","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E79","v":0},{"$f":"'A4-A5 -Transport & Construction'!F79","v":0},{"$f":"'A4-A5 -Transport & Construction'!G79","v":0},{"$f":"'A4-A5 -Transport & Construction'!I79","v":0},{"$f":"'A4-A5 -Transport & Construction'!J79","v":0},{"$f":"'A4-A5 -Transport & Construction'!K79","v":0},{"$f":"'A4-A5 -Transport & Construction'!L79","v":0},{"$f":"'A4-A5 -Transport & Construction'!M79","v":0},{"$f":"'A4-A5 -Transport & Construction'!N79","v":0},{"$f":"'A4-A5 -Transport & Construction'!O79","v":0},{"$f":"'A4-A5 -Transport & Construction'!P79","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y79","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z79","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E80","v":0},{"$f":"'A4-A5 -Transport & Construction'!F80","v":0},{"$f":"'A4-A5 -Transport & Construction'!G80","v":0},{"$f":"'A4-A5 -Transport & Construction'!I80","v":0},{"$f":"'A4-A5 -Transport & Construction'!J80","v":0},{"$f":"'A4-A5 -Transport & Construction'!K80","v":0},{"$f":"'A4-A5 -Transport & Construction'!L80","v":0},{"$f":"'A4-A5 -Transport & Construction'!M80","v":0},{"$f":"'A4-A5 -Transport & Construction'!N80","v":0},{"$f":"'A4-A5 -Transport & Construction'!O80","v":0},{"$f":"'A4-A5 -Transport & Construction'!P80","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y80","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z80","v":"-"}]
[null,null,null,"C1 - Deconstruction and demolition",{"$f":"'A4-A5 -Transport & Construction'!E81","v":0},{"$f":"'A4-A5 -Transport & Construction'!F81","v":0},{"$f":"'A4-A5 -Transport & Construction'!G81","v":0},{"$f":"'A4-A5 -Transport & Construction'!I81","v":0},{"$f":"'A4-A5 -Transport & Construction'!J81","v":0},{"$f":"'A4-A5 -Transport & Construction'!K81","v":0},{"$f":"'A4-A5 -Transport & Construction'!L81","v":0},{"$f":"'A4-A5 -Transport & Construction'!M81","v":0},{"$f":"'A4-A5 -Transport & Construction'!N81","v":0},{"$f":"'A4-A5 -Transport & Construction'!O81","v":0},{"$f":"'A4-A5 -Transport & Construction'!P81","v":""},{"$f":"'A4-A5 -Transport & Construction'!Q81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!R81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!S81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!T81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!U81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!V81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!W81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!X81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Y81","v":"-"},{"$f":"'A4-A5 -Transport & Construction'!Z81","v":"-"}]
[]
[]
[null,"3.2.2",null,"Module C2 - Transport Emissions"]
[]
[null,null,null,"Transportation of assets and waste materials to their processing & disposal sites has been auto-populated based on the data provided in A4. No input is required here.\nIt has been assumed that all materials transported to the site will be removed from the site and taken to a shipyard to be broken down for waste processing at either a landfill or recycling site."]
[]
[null,null,null,"GHG Module","Activity description","Asset","Component","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E45),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F45","v":0},{"$f":"'A4-A5 -Transport & Construction'!G45","v":0},{"$f":"'A4-A5 -Transport & Construction'!I45","v":0},{"$f":"'A4-A5 -Transport & Construction'!J45","v":0},{"$f":"'A4-A5 -Transport & Construction'!K45","v":0},{"$f":"'A4-A5 -Transport & Construction'!L45","v":0},{"$f":"'A4-A5 -Transport & Construction'!M45","v":0},{"$f":"'A4-A5 -Transport & Construction'!N45","v":0},{"$f":"'A4-A5 -Transport & Construction'!O45","v":0},{"$f":"'A4-A5 -Transport & Construction'!P45","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J45),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J45),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J45),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J45),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J45),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L45),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L45),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L45),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L45),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L45),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E46),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F46","v":0},{"$f":"'A4-A5 -Transport & Construction'!G46","v":0},{"$f":"'A4-A5 -Transport & Construction'!I46","v":0},{"$f":"'A4-A5 -Transport & Construction'!J46","v":0},{"$f":"'A4-A5 -Transport & Construction'!K46","v":0},{"$f":"'A4-A5 -Transport & Construction'!L46","v":0},{"$f":"'A4-A5 -Transport & Construction'!M46","v":0},{"$f":"'A4-A5 -Transport & Construction'!N46","v":0},{"$f":"'A4-A5 -Transport & Construction'!O46","v":0},{"$f":"'A4-A5 -Transport & Construction'!P46","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J46),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J46),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J46),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J46),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J46),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L46),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L46),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L46),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L46),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L46),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E47),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F47","v":0},{"$f":"'A4-A5 -Transport & Construction'!G47","v":0},{"$f":"'A4-A5 -Transport & Construction'!I47","v":0},{"$f":"'A4-A5 -Transport & Construction'!J47","v":0},{"$f":"'A4-A5 -Transport & Construction'!K47","v":0},{"$f":"'A4-A5 -Transport & Construction'!L47","v":0},{"$f":"'A4-A5 -Transport & Construction'!M47","v":0},{"$f":"'A4-A5 -Transport & Construction'!N47","v":0},{"$f":"'A4-A5 -Transport & Construction'!O47","v":0},{"$f":"'A4-A5 -Transport & Construction'!P47","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J47),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J47),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J47),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J47),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J47),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L47),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L47),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L47),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L47),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L47),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E48),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F48","v":0},{"$f":"'A4-A5 -Transport & Construction'!G48","v":0},{"$f":"'A4-A5 -Transport & Construction'!I48","v":0},{"$f":"'A4-A5 -Transport & Construction'!J48","v":0},{"$f":"'A4-A5 -Transport & Construction'!K48","v":0},{"$f":"'A4-A5 -Transport & Construction'!L48","v":0},{"$f":"'A4-A5 -Transport & Construction'!M48","v":0},{"$f":"'A4-A5 -Transport & Construction'!N48","v":0},{"$f":"'A4-A5 -Transport & Construction'!O48","v":0},{"$f":"'A4-A5 -Transport & Construction'!P48","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J48),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J48),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J48),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J48),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J48),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L48),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L48),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L48),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L48),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L48),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E49),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F49","v":0},{"$f":"'A4-A5 -Transport & Construction'!G49","v":0},{"$f":"'A4-A5 -Transport & Construction'!I49","v":0},{"$f":"'A4-A5 -Transport & Construction'!J49","v":0},{"$f":"'A4-A5 -Transport & Construction'!K49","v":0},{"$f":"'A4-A5 -Transport & Construction'!L49","v":0},{"$f":"'A4-A5 -Transport & Construction'!M49","v":0},{"$f":"'A4-A5 -Transport & Construction'!N49","v":0},{"$f":"'A4-A5 -Transport & Construction'!O49","v":0},{"$f":"'A4-A5 -Transport & Construction'!P49","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J49),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J49),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J49),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J49),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J49),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L49),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L49),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L49),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L49),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L49),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E50),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F50","v":0},{"$f":"'A4-A5 -Transport & Construction'!G50","v":0},{"$f":"'A4-A5 -Transport & Construction'!I50","v":0},{"$f":"'A4-A5 -Transport & Construction'!J50","v":0},{"$f":"'A4-A5 -Transport & Construction'!K50","v":0},{"$f":"'A4-A5 -Transport & Construction'!L50","v":0},{"$f":"'A4-A5 -Transport & Construction'!M50","v":0},{"$f":"'A4-A5 -Transport & Construction'!N50","v":0},{"$f":"'A4-A5 -Transport & Construction'!O50","v":0},{"$f":"'A4-A5 -Transport & Construction'!P50","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J50),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J50),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J50),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J50),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J50),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L50),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L50),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L50),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L50),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L50),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E51),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F51","v":0},{"$f":"'A4-A5 -Transport & Construction'!G51","v":0},{"$f":"'A4-A5 -Transport & Construction'!I51","v":0},{"$f":"'A4-A5 -Transport & Construction'!J51","v":0},{"$f":"'A4-A5 -Transport & Construction'!K51","v":0},{"$f":"'A4-A5 -Transport & Construction'!L51","v":0},{"$f":"'A4-A5 -Transport & Construction'!M51","v":0},{"$f":"'A4-A5 -Transport & Construction'!N51","v":0},{"$f":"'A4-A5 -Transport & Construction'!O51","v":0},{"$f":"'A4-A5 -Transport & Construction'!P51","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J51),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J51),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J51),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J51),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J51),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L51),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L51),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L51),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L51),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L51),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E52),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F52","v":0},{"$f":"'A4-A5 -Transport & Construction'!G52","v":0},{"$f":"'A4-A5 -Transport & Construction'!I52","v":0},{"$f":"'A4-A5 -Transport & Construction'!J52","v":0},{"$f":"'A4-A5 -Transport & Construction'!K52","v":0},{"$f":"'A4-A5 -Transport & Construction'!L52","v":0},{"$f":"'A4-A5 -Transport & Construction'!M52","v":0},{"$f":"'A4-A5 -Transport & Construction'!N52","v":0},{"$f":"'A4-A5 -Transport & Construction'!O52","v":0},{"$f":"'A4-A5 -Transport & Construction'!P52","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J52),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J52),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J52),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J52),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J52),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L52),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L52),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L52),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L52),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L52),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E53),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F53","v":0},{"$f":"'A4-A5 -Transport & Construction'!G53","v":0},{"$f":"'A4-A5 -Transport & Construction'!I53","v":0},{"$f":"'A4-A5 -Transport & Construction'!J53","v":0},{"$f":"'A4-A5 -Transport & Construction'!K53","v":0},{"$f":"'A4-A5 -Transport & Construction'!L53","v":0},{"$f":"'A4-A5 -Transport & Construction'!M53","v":0},{"$f":"'A4-A5 -Transport & Construction'!N53","v":0},{"$f":"'A4-A5 -Transport & Construction'!O53","v":0},{"$f":"'A4-A5 -Transport & Construction'!P53","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J53),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J53),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J53),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J53),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J53),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L53),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L53),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L53),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L53),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L53),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E54),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F54","v":0},{"$f":"'A4-A5 -Transport & Construction'!G54","v":0},{"$f":"'A4-A5 -Transport & Construction'!I54","v":0},{"$f":"'A4-A5 -Transport & Construction'!J54","v":0},{"$f":"'A4-A5 -Transport & Construction'!K54","v":0},{"$f":"'A4-A5 -Transport & Construction'!L54","v":0},{"$f":"'A4-A5 -Transport & Construction'!M54","v":0},{"$f":"'A4-A5 -Transport & Construction'!N54","v":0},{"$f":"'A4-A5 -Transport & Construction'!O54","v":0},{"$f":"'A4-A5 -Transport & Construction'!P54","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J54),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J54),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J54),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J54),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J54),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L54),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L54),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L54),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L54),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L54),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E55),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F55","v":0},{"$f":"'A4-A5 -Transport & Construction'!G55","v":0},{"$f":"'A4-A5 -Transport & Construction'!I55","v":0},{"$f":"'A4-A5 -Transport & Construction'!J55","v":0},{"$f":"'A4-A5 -Transport & Construction'!K55","v":0},{"$f":"'A4-A5 -Transport & Construction'!L55","v":0},{"$f":"'A4-A5 -Transport & Construction'!M55","v":0},{"$f":"'A4-A5 -Transport & Construction'!N55","v":0},{"$f":"'A4-A5 -Transport & Construction'!O55","v":0},{"$f":"'A4-A5 -Transport & Construction'!P55","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J55),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J55),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J55),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J55),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J55),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L55),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L55),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L55),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L55),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L55),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E56),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F56","v":0},{"$f":"'A4-A5 -Transport & Construction'!G56","v":0},{"$f":"'A4-A5 -Transport & Construction'!I56","v":0},{"$f":"'A4-A5 -Transport & Construction'!J56","v":0},{"$f":"'A4-A5 -Transport & Construction'!K56","v":0},{"$f":"'A4-A5 -Transport & Construction'!L56","v":0},{"$f":"'A4-A5 -Transport & Construction'!M56","v":0},{"$f":"'A4-A5 -Transport & Construction'!N56","v":0},{"$f":"'A4-A5 -Transport & Construction'!O56","v":0},{"$f":"'A4-A5 -Transport & Construction'!P56","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J56),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J56),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J56),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J56),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J56),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L56),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L56),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L56),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L56),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L56),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E57),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F57","v":0},{"$f":"'A4-A5 -Transport & Construction'!G57","v":0},{"$f":"'A4-A5 -Transport & Construction'!I57","v":0},{"$f":"'A4-A5 -Transport & Construction'!J57","v":0},{"$f":"'A4-A5 -Transport & Construction'!K57","v":0},{"$f":"'A4-A5 -Transport & Construction'!L57","v":0},{"$f":"'A4-A5 -Transport & Construction'!M57","v":0},{"$f":"'A4-A5 -Transport & Construction'!N57","v":0},{"$f":"'A4-A5 -Transport & Construction'!O57","v":0},{"$f":"'A4-A5 -Transport & Construction'!P57","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J57),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J57),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J57),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J57),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J57),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L57),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L57),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L57),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L57),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L57),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E58),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F58","v":0},{"$f":"'A4-A5 -Transport & Construction'!G58","v":0},{"$f":"'A4-A5 -Transport & Construction'!I58","v":0},{"$f":"'A4-A5 -Transport & Construction'!J58","v":0},{"$f":"'A4-A5 -Transport & Construction'!K58","v":0},{"$f":"'A4-A5 -Transport & Construction'!L58","v":0},{"$f":"'A4-A5 -Transport & Construction'!M58","v":0},{"$f":"'A4-A5 -Transport & Construction'!N58","v":0},{"$f":"'A4-A5 -Transport & Construction'!O58","v":0},{"$f":"'A4-A5 -Transport & Construction'!P58","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J58),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J58),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J58),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J58),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J58),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L58),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L58),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L58),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L58),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L58),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E59),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F59","v":0},{"$f":"'A4-A5 -Transport & Construction'!G59","v":0},{"$f":"'A4-A5 -Transport & Construction'!I59","v":0},{"$f":"'A4-A5 -Transport & Construction'!J59","v":0},{"$f":"'A4-A5 -Transport & Construction'!K59","v":0},{"$f":"'A4-A5 -Transport & Construction'!L59","v":0},{"$f":"'A4-A5 -Transport & Construction'!M59","v":0},{"$f":"'A4-A5 -Transport & Construction'!N59","v":0},{"$f":"'A4-A5 -Transport & Construction'!O59","v":0},{"$f":"'A4-A5 -Transport & Construction'!P59","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J59),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J59),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J59),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J59),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J59),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L59),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L59),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L59),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L59),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L59),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[null,null,null,{"$f":"Results!$B$50","v":"C2 - Transport"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!E60),\"\",\"To shipyard to be broken down ready for waste processing\")","v":""},{"$f":"'A4-A5 -Transport & Construction'!F60","v":0},{"$f":"'A4-A5 -Transport & Construction'!G60","v":0},{"$f":"'A4-A5 -Transport & Construction'!I60","v":0},{"$f":"'A4-A5 -Transport & Construction'!J60","v":0},{"$f":"'A4-A5 -Transport & Construction'!K60","v":0},{"$f":"'A4-A5 -Transport & Construction'!L60","v":0},{"$f":"'A4-A5 -Transport & Construction'!M60","v":0},{"$f":"'A4-A5 -Transport & Construction'!N60","v":0},{"$f":"'A4-A5 -Transport & Construction'!O60","v":0},{"$f":"'A4-A5 -Transport & Construction'!P60","v":""},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J60),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J60),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J60),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J60),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!J60),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C2_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C2_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C2_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L60),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L60),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L60),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L60),\"-\",IFERROR(Table_C2_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C2_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK('A4-A5 -Transport & Construction'!L60),\"-\",IFERROR(IF(SUM(Table_C2_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C2_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C2_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"-"}]
[]
[]
[null,"3.2.3",null,"Module C3 & C4  - Waste Processing & Disposal"]
[null,null,null,"A list of materials and components for C3 and C4 along with quantities has been in part auto-populated based on data provided in A1-A3 detailing the materials and components that make up the OSW development. Please provide a relevant end-of-life emissions factor selection for each material line. Please use the assumption table below to describe the typical end-of-life fate for materials. The assumptions provided are based on European Commission statistics, with a link to the dataset provided below. If you have a more accurate source for assumptions based on regional statistics where the OSW development is being built, or would like to change the values to make them more regionally specific, please edit he preset assumptions. These % values will combine with the values from the material inventory on A1-A3 to determine the total amount of waste going to landfill, recycling & energy recovery.\n\nWhen calculating emissions from recycling, emissions must be allocated to either the initial product that gets recycled or the resultant recycled product. The OSW footprinting guidance uses the \"recycled content method - cut-off (100/0)\". The cut-off criteria 100/0 allocates all recycling emissions to the resultant recycled product. Waste is delivered to a recycling facility, sorted and then recycled. Under our cut-off criteria, emissions from transport and sorting must be accounted for but no emissions from recycling processes should be included under the end-of-life emissions calculation. Instead, all emissions are allocated to the resultant recycled product that leaves the processing facility and is used in a different system. Recycling totals will be carried forward for use in the calculation of Module D: Benefits & Loads beyond the system boundary. This means these tables provide no option for recycling. For any products that are expect to be recycled the sorting emission factor should be used.\n\nThe quantities for disposal are auto-populated from the total quantities from the material inventory on the A1-A3 Production Tab. The quantities of materials are multiplied by the average % of materials going to landfill. The user shall populate the relevant emission factor for landfilling of the material"]
[]
[null,null,null,"Waste fate statistics by material type"]
[null,null,null,"OSW Activity Taxonomy - Material type","Waste treatment statistics source","Waste region from source","Statistic Year","Waste category from source","Incineration","Landfill","Processing, sorting for recycling and reuse"]
[null,null,null,"Aluminium","European commission","EU27",2020,"Metal wastes, non-ferrous",0,3.8809831824062097E-3,0.99611901681759374]
[null,null,null,"Biogenic materials","European commission","EU27",2020,"Wood wastes",2.7363184079601992E-3,3.2338308457711441E-3,0.99402985074626871]
[null,null,null,"Carbon fibre","European commission","EU27",2020,"Plastic wastes",3.5118525021949078E-3,5.1799824407374892E-2,0.94468832309043016]
[null,null,null,"Concrete","European commission","EU27",2020,"Mineral waste from construction & demolition",0,3.8809831824062097E-3,0.99611901681759374]
[null,null,null,"Copper","European commission","EU27",2020,"Metal wastes, non-ferrous",0,3.8809831824062097E-3,0.99611901681759374]
[null,null,null,"Fibreglass","European commission","EU27",2020,"Plastic wastes",3.5118525021949078E-3,5.1799824407374892E-2,0.94468832309043016]
[null,null,null,"Oils & Lubricants","European commission","EU27",2020,"Used Oils",3.7037037037037035E-2,4.6296296296296294E-3,0.95370370370370372]
[null,null,null,"Other","European commission","EU27",2020,"Mixed and undifferentiated materials",1.1269722013523666E-2,0.20586025544703232,0.78287002253944404]
[null,null,null,"Polymers","European commission","EU27",2020,"Plastic wastes",3.5118525021949078E-3,5.1799824407374892E-2,0.94468832309043016]
[null,null,null,"Steel","European commission","EU27",2020,"Metal wastes, ferrous",0,6.597394029358403E-4,0.99917532574633017]
[]
[null,null,null,"GHG Module","Activity description","Material Type","Asset","Component","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Aluminium","Aluminium","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Biogenic Materials","Biogenic materials","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Carbon fibre","Carbon fibre","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Concrete","Concrete","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Copper","Copper","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Fibreglass","Fibreglass","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Oils & Lubricants","Oils & Lubricants","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":"CHECK ENTRIES"},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Other","Other","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":"CHECK ENTRIES"},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Polymers","Polymers","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Landfill of Steel","Steel","Other","Unassigned","Waste treatment","Landfill",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Aluminium","Aluminium","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Biogenic Materials","Biogenic materials","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Carbon fibre","Carbon fibre","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Concrete","Concrete","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Copper","Copper","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Fibreglass","Fibreglass","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Oils & Lubricants","Oils & Lubricants","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":"CHECK ENTRIES"},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Other","Other","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":"CHECK ENTRIES"},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Polymers","Polymers","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Incineration of Steel","Steel","Other","Unassigned","Waste treatment","Incineration",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Aluminium for recycling, recovery or reuse","Aluminium","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Biogenic materials for recycling, recovery or reuse","Biogenic materials","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Carbon fibre for recycling, recovery or reuse","Carbon fibre","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Concrete for recycling, recovery or reuse","Concrete","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Copper for recycling, recovery or reuse","Copper","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Fibreglass for recycling, recovery or reuse","Fibreglass","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Oils & Lubricants for recycling, recovery or reuse","Oils & Lubricants","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":"CHECK ENTRIES"},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Other for recycling, recovery or reuse","Other","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":"CHECK ENTRIES"},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Polymers for recycling, recovery or reuse","Polymers","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal","Processing and sorting of Steel for recycling, recovery or reuse","Steel","Other","Unassigned","Waste treatment","Processing, sorting for recycling and reuse",null,null,null,{"$f":"IFERROR((INDEX(Material_Inventory[Total material quantities for OSW development in terms of OSW Activity Taxonomy], MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Material_Inventory[Material Type],0)))*INDEX(Waste_Statistics[[Incineration]:[Processing, sorting for recycling and reuse]],MATCH(Table_C3C4_Option_B[[#This Row],[Material Type]],Waste_Statistics[OSW Activity Taxonomy - Material type],0),MATCH(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]],Waste_Statistics[[#Headers],[Incineration]:[Processing, sorting for recycling and reuse]],0)),\"CHECK ENTRIES\")","v":0},"kg",{"$f":"_xlfn.IFS(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=\"\",\"\",Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]]=Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]],\"Yes\",Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]<>Table_C3C4_Option_B[[#This Row],[Activity Data: Unit]],\"No\")","v":""},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C3C4_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C3C4_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"-"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C3C4_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C3C4_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C3C4_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C3C4_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[]
[null,"3.2.4"]
[null,null,null,"Module C5","Emissions due to vehicle, vessel, and aircraft use and emissions from materials and equipment used in any relandscaping activities for the OSW development post decommissioning"]
[]
[null,null,null,"Relandscaping emissions from fuel and energy use in vessels has been auto-populated based on the data provided in A0 for preconstruction activities. No input is required here."]
[null,null,null,null,null,null,null,null,null,null,"`",null,null,null,"Note: All Activity Data quantities should be input as a value rather than a formula or calculation"]
[null,null,null,"GHG Module","Relandscaping Activity Description","Asset","Component","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Emission Factor Name","Emissions Factor: Geography","Emissions Factor: Unit","Activity Data: Quantity","Activity Data: Unit","Unit Match?","Primary, Secondary or Proxy EF?","Emissions Factor: Fossil (kgCO2e/Unit)","Emissions Factor: Biogenic (kgCO2e/Unit)","Emissions Factor: Land Use (kgCO2e/Unit)","Emissions Factor: Total (kgCO2e/Unit)","Calculated Emissions: Fossil (kgCO2e)","Calculated Emissions: Biogenic (kgCO2e)","Calculated Emissions: Land Use (kgCO2e)","Calculated Emissions: Total (kgCO2e)","Total Emissions (kgCO2e)"]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E38),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F38","v":0},{"$f":"'A0 - Preconstruction'!G38","v":0},{"$f":"'A0 - Preconstruction'!I38","v":0},{"$f":"'A0 - Preconstruction'!J38","v":0},{"$f":"'A0 - Preconstruction'!K38","v":0},{"$f":"'A0 - Preconstruction'!L38","v":0},{"$f":"'A0 - Preconstruction'!M38","v":0},{"$f":"'A0 - Preconstruction'!N38","v":0},{"$f":"'A0 - Preconstruction'!O38","v":0},{"$f":"'A0 - Preconstruction'!P38","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E39),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F39","v":0},{"$f":"'A0 - Preconstruction'!G39","v":0},{"$f":"'A0 - Preconstruction'!I39","v":0},{"$f":"'A0 - Preconstruction'!J39","v":0},{"$f":"'A0 - Preconstruction'!K39","v":0},{"$f":"'A0 - Preconstruction'!L39","v":0},{"$f":"'A0 - Preconstruction'!M39","v":0},{"$f":"'A0 - Preconstruction'!N39","v":0},{"$f":"'A0 - Preconstruction'!O39","v":0},{"$f":"'A0 - Preconstruction'!P39","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E40),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F40","v":0},{"$f":"'A0 - Preconstruction'!G40","v":0},{"$f":"'A0 - Preconstruction'!I40","v":0},{"$f":"'A0 - Preconstruction'!J40","v":0},{"$f":"'A0 - Preconstruction'!K40","v":0},{"$f":"'A0 - Preconstruction'!L40","v":0},{"$f":"'A0 - Preconstruction'!M40","v":0},{"$f":"'A0 - Preconstruction'!N40","v":0},{"$f":"'A0 - Preconstruction'!O40","v":0},{"$f":"'A0 - Preconstruction'!P40","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E41),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F41","v":0},{"$f":"'A0 - Preconstruction'!G41","v":0},{"$f":"'A0 - Preconstruction'!I41","v":0},{"$f":"'A0 - Preconstruction'!J41","v":0},{"$f":"'A0 - Preconstruction'!K41","v":0},{"$f":"'A0 - Preconstruction'!L41","v":0},{"$f":"'A0 - Preconstruction'!M41","v":0},{"$f":"'A0 - Preconstruction'!N41","v":0},{"$f":"'A0 - Preconstruction'!O41","v":0},{"$f":"'A0 - Preconstruction'!P41","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E42),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F42","v":0},{"$f":"'A0 - Preconstruction'!G42","v":0},{"$f":"'A0 - Preconstruction'!I42","v":0},{"$f":"'A0 - Preconstruction'!J42","v":0},{"$f":"'A0 - Preconstruction'!K42","v":0},{"$f":"'A0 - Preconstruction'!L42","v":0},{"$f":"'A0 - Preconstruction'!M42","v":0},{"$f":"'A0 - Preconstruction'!N42","v":0},{"$f":"'A0 - Preconstruction'!O42","v":0},{"$f":"'A0 - Preconstruction'!P42","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E43),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F43","v":0},{"$f":"'A0 - Preconstruction'!G43","v":0},{"$f":"'A0 - Preconstruction'!I43","v":0},{"$f":"'A0 - Preconstruction'!J43","v":0},{"$f":"'A0 - Preconstruction'!K43","v":0},{"$f":"'A0 - Preconstruction'!L43","v":0},{"$f":"'A0 - Preconstruction'!M43","v":0},{"$f":"'A0 - Preconstruction'!N43","v":0},{"$f":"'A0 - Preconstruction'!O43","v":0},{"$f":"'A0 - Preconstruction'!P43","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E44),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F44","v":0},{"$f":"'A0 - Preconstruction'!G44","v":0},{"$f":"'A0 - Preconstruction'!I44","v":0},{"$f":"'A0 - Preconstruction'!J44","v":0},{"$f":"'A0 - Preconstruction'!K44","v":0},{"$f":"'A0 - Preconstruction'!L44","v":0},{"$f":"'A0 - Preconstruction'!M44","v":0},{"$f":"'A0 - Preconstruction'!N44","v":0},{"$f":"'A0 - Preconstruction'!O44","v":0},{"$f":"'A0 - Preconstruction'!P44","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E45),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F45","v":0},{"$f":"'A0 - Preconstruction'!G45","v":0},{"$f":"'A0 - Preconstruction'!I45","v":0},{"$f":"'A0 - Preconstruction'!J45","v":0},{"$f":"'A0 - Preconstruction'!K45","v":0},{"$f":"'A0 - Preconstruction'!L45","v":0},{"$f":"'A0 - Preconstruction'!M45","v":0},{"$f":"'A0 - Preconstruction'!N45","v":0},{"$f":"'A0 - Preconstruction'!O45","v":0},{"$f":"'A0 - Preconstruction'!P45","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E46),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F46","v":0},{"$f":"'A0 - Preconstruction'!G46","v":0},{"$f":"'A0 - Preconstruction'!I46","v":0},{"$f":"'A0 - Preconstruction'!J46","v":0},{"$f":"'A0 - Preconstruction'!K46","v":0},{"$f":"'A0 - Preconstruction'!L46","v":0},{"$f":"'A0 - Preconstruction'!M46","v":0},{"$f":"'A0 - Preconstruction'!N46","v":0},{"$f":"'A0 - Preconstruction'!O46","v":0},{"$f":"'A0 - Preconstruction'!P46","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E47),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F47","v":0},{"$f":"'A0 - Preconstruction'!G47","v":0},{"$f":"'A0 - Preconstruction'!I47","v":0},{"$f":"'A0 - Preconstruction'!J47","v":0},{"$f":"'A0 - Preconstruction'!K47","v":0},{"$f":"'A0 - Preconstruction'!L47","v":0},{"$f":"'A0 - Preconstruction'!M47","v":0},{"$f":"'A0 - Preconstruction'!N47","v":0},{"$f":"'A0 - Preconstruction'!O47","v":0},{"$f":"'A0 - Preconstruction'!P47","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E48),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F48","v":0},{"$f":"'A0 - Preconstruction'!G48","v":0},{"$f":"'A0 - Preconstruction'!I48","v":0},{"$f":"'A0 - Preconstruction'!J48","v":0},{"$f":"'A0 - Preconstruction'!K48","v":0},{"$f":"'A0 - Preconstruction'!L48","v":0},{"$f":"'A0 - Preconstruction'!M48","v":0},{"$f":"'A0 - Preconstruction'!N48","v":0},{"$f":"'A0 - Preconstruction'!O48","v":0},{"$f":"'A0 - Preconstruction'!P48","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E49),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F49","v":0},{"$f":"'A0 - Preconstruction'!G49","v":0},{"$f":"'A0 - Preconstruction'!I49","v":0},{"$f":"'A0 - Preconstruction'!J49","v":0},{"$f":"'A0 - Preconstruction'!K49","v":0},{"$f":"'A0 - Preconstruction'!L49","v":0},{"$f":"'A0 - Preconstruction'!M49","v":0},{"$f":"'A0 - Preconstruction'!N49","v":0},{"$f":"'A0 - Preconstruction'!O49","v":0},{"$f":"'A0 - Preconstruction'!P49","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E50),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F50","v":0},{"$f":"'A0 - Preconstruction'!G50","v":0},{"$f":"'A0 - Preconstruction'!I50","v":0},{"$f":"'A0 - Preconstruction'!J50","v":0},{"$f":"'A0 - Preconstruction'!K50","v":0},{"$f":"'A0 - Preconstruction'!L50","v":0},{"$f":"'A0 - Preconstruction'!M50","v":0},{"$f":"'A0 - Preconstruction'!N50","v":0},{"$f":"'A0 - Preconstruction'!O50","v":0},{"$f":"'A0 - Preconstruction'!P50","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E51),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F51","v":0},{"$f":"'A0 - Preconstruction'!G51","v":0},{"$f":"'A0 - Preconstruction'!I51","v":0},{"$f":"'A0 - Preconstruction'!J51","v":0},{"$f":"'A0 - Preconstruction'!K51","v":0},{"$f":"'A0 - Preconstruction'!L51","v":0},{"$f":"'A0 - Preconstruction'!M51","v":0},{"$f":"'A0 - Preconstruction'!N51","v":0},{"$f":"'A0 - Preconstruction'!O51","v":0},{"$f":"'A0 - Preconstruction'!P51","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E52),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F52","v":0},{"$f":"'A0 - Preconstruction'!G52","v":0},{"$f":"'A0 - Preconstruction'!I52","v":0},{"$f":"'A0 - Preconstruction'!J52","v":0},{"$f":"'A0 - Preconstruction'!K52","v":0},{"$f":"'A0 - Preconstruction'!L52","v":0},{"$f":"'A0 - Preconstruction'!M52","v":0},{"$f":"'A0 - Preconstruction'!N52","v":0},{"$f":"'A0 - Preconstruction'!O52","v":0},{"$f":"'A0 - Preconstruction'!P52","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IF(ISBLANK('A0 - Preconstruction'!E53),\"\",\"Relandscaping vessel activities\")","v":""},{"$f":"'A0 - Preconstruction'!F53","v":0},{"$f":"'A0 - Preconstruction'!G53","v":0},{"$f":"'A0 - Preconstruction'!I53","v":0},{"$f":"'A0 - Preconstruction'!J53","v":0},{"$f":"'A0 - Preconstruction'!K53","v":0},{"$f":"'A0 - Preconstruction'!L53","v":0},{"$f":"'A0 - Preconstruction'!M53","v":0},{"$f":"'A0 - Preconstruction'!N53","v":0},{"$f":"'A0 - Preconstruction'!O53","v":0},{"$f":"'A0 - Preconstruction'!P53","v":""},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[OSW EF Category],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: fossil (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: biogenic (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_A[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[climate change: land use (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),0))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Emission Factor Name]]),\"-\",IFERROR(INDEX(EF_Library[Emissions Factor Net (kgCO2e/unit)],MATCH(1,(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L1]]=EF_Library[OSW Activity Taxonomy L1])*(Table_C5_Option_B[[#This Row],[OSW Activity Taxonomy L2]]=EF_Library[OSW Activity Taxonomy L2])*(Table_C5_Option_B[[#This Row],[Emission Factor Name]]=EF_Library[Emission Factor Name])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Geography]]=EF_Library[Geography])*(Table_C5_Option_B[[#This Row],[Emissions Factor: Unit]]=EF_Library[Emissions Factor Unit]),0)),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Biogenic (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IF(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]]=\"Unknown\",\"Unknown\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Land Use (kgCO2e/Unit)]],\"CHECK ENTRIES\")))","v":0},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]*Table_C5_Option_B[[#This Row],[Emissions Factor: Total (kgCO2e/Unit)]],\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"},{"$f":"IF(ISBLANK(Table_C5_Option_B[[#This Row],[Activity Data: Quantity]]),\"-\",IFERROR(IF(SUM(Table_C5_Option_B[[#This Row],[Emissions Factor: Fossil (kgCO2e/Unit)]:[Emissions Factor: Land Use (kgCO2e/Unit)]])>0,SUM(Table_C5_Option_B[[#This Row],[Calculated Emissions: Fossil (kgCO2e)]:[Calculated Emissions: Land Use (kgCO2e)]]),Table_C5_Option_B[[#This Row],[Calculated Emissions: Total (kgCO2e)]]),\"CHECK ENTRIES\"))","v":"CHECK ENTRIES"}]

{"sheet":"Data Quality & Uncertainty","index":17,"n_rows":111,"n_cols":29,"rows_kept":111,"cut":false,"hidden":false,"merged":[[8,3,8,7]]}
[]
[null,null,null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,null,null,"Offshore Wind Footprinting Tool"]
[null,null,null,"DATA INPUTS - DATA QUALITY & PARAMETER UNCERTAINTY"]
[]
[]
[null,null,null,"Data Quality & Parameter Uncertainty"]
[]
[null,null,null,"This tab may be used to assess Data Quality & Parameter Uncertainty. \n\nThe approach follows the guidance set out in the OSW Industry PCF Guidance document, which draws on the requirements of the GHGP Protocol Quantitative Inventory Uncertainty Guidance. The approach taken in this tool is simplified so that the user is only required to assess the aggregated data quality score of full lifecycle module calculation tables, rather than at an activity level. This reduces the granularity of the data quality assessment, uncertainty assessment and the time taken to make the assessment. Due to the inherent limitations of the pedigree matrix approach and the process of translating qualitative DQ assessments into quantitative uncertainty ranges this is deemed the most practical level of granularity. Users should judge the materiality of specific activities within lifecycle modules when assessing. For example, if one activity row represents 90% of the emissions for that module, then the DQ assessment should be weighted towards that activity.\n\nFor each lifecycle module, you must assess the aggregated quality of the activity data and emission factors used in the carbon footprint calculation. Drop-down selections of very good, good, fair and poor are available as assessment options.\n\nTo streamline the assessment, the most relevant sources of data should be assessed on three metrics:\n - Completeness: Does the data provided cover the full scope of relevant activities for the assessment?\n - Source reliability: Where did you get the data from? Was it primary, measured data or did it come from assumptions? Did you have to make conversions?\n\nFor Emission Factors, we assess the following additional sources of uncertainty:\n - Technology: Is the data provided for emission factors representative of the actual technologies used in our activities? For example, \"we use an emission factor for steel produced by blast furnace as it is the only one available, but our steel was produced in an electric arc furnace\".\n - Time: Is the data period for the emissions factors (LCA, PCF, EPD) close in time to the activities we are trying to model? For example, \"we use an EPD that was released in 2018, but our development will be built in 2028, meaning there is quite a long intervening period\".\n - Geography: Is the data region for the emissions factors representative of the region of the OSW development activities? For example, \"we use an EPD for steel produced in Germany, but our steel was produced in the USA\". \n - Basic uncertainty associated with activity type: An additional uncertainty factor acknowledging the inherent uncertainty associated with emission factor data, depending on the activity type. For example, \"material emission factors usually have low uncertainty as they are made according to defined and consistent processes, but freight and transportation emissions can be variable due to vehicle efficiencies under different conditions."]
[]
[null,null,null,"READ ME"]
[]
[null,null,null,"Description cell"]
[null,null,null,"Guidance"]
[null,null,null,"Input cell"]
[null,null,null,"Calculation Cell"]
[null,null,null,"Preset Cell"]
[]
[null,1,null,"Results"]
[]
[]
[null,null,null,"Weighted average DQ score for the assessment","DQ Rating"]
[null,null,null,{"$f":"IFERROR(SUMPRODUCT(DQ_Uncertainty_Assessment[Total contribution to footprint (%)],DQ_Uncertainty_Assessment[Lifecycle Module Average DQ Rating]),\"Complete DQ & Uncertainty Assessment\")","v":0},{"$f":"_xlfn.IFS(ISERROR(DQ_Uncertainty_Results[[#This Row],[Weighted average DQ score for the assessment]]), \"Complete assessment\", DQ_Uncertainty_Results[[#This Row],[Weighted average DQ score for the assessment]]<=0.2, \"Poor\", DQ_Uncertainty_Results[[#This Row],[Weighted average DQ score for the assessment]]<=0.5, \"Fair\",DQ_Uncertainty_Results[[#This Row],[Weighted average DQ score for the assessment]]<=0.7, \"Good\", DQ_Uncertainty_Results[[#This Row],[Weighted average DQ score for the assessment]]<=0.9, \"Very Good\", TRUE, \"Complete DQ Assessment\")","v":"Poor"}]
[]
[null,null,null,"GHG Lifecycle Module"," Calculated (tCO2e)","Weighted average DQ score","Calculated upper error (tCO2e)","Calculated Lower error (tCO2e)"]
[null,null,null,"A0 - Preconstruction",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0.7},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0}]
[null,null,null,"A1-A2 Raw Material and Transport",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0.54411764705882348},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0}]
[null,null,null,"A3 Manufacturing",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"A1-A3 - Production & manufacturing (finished assets & subcomponents)",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"A4 - Transport to site",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"A5 - Construction",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"B1 - Use",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"B2 - Maintenance",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"B3 - Repair",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"B4 - Replacement",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"B5 - Refurbishment",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"B6 - Operational energy consumption",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"B7 - Operational water consumption",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"B8 - Operational activities not otherwise captured in modules B1-B7",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"C1 - Deconstruction Demolition",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"C2 - Transport",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":0},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lifecycle Module Average DQ Rating]:[Lifecycle Module Average DQ Rating]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Upper bound error (tCO2e)]:[Upper bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"},{"$f":"IFERROR(INDEX(DQ_Uncertainty_Assessment[[Lower bound error (tCO2e)]:[Lower bound error (tCO2e)]],MATCH(Results_Lifecycle49[[#This Row],[GHG Lifecycle Module]],DQ_Uncertainty_Assessment[[GHG Lifecycle Module Table]:[GHG Lifecycle Module Table]],0)),\"CHECK ASSESSMENT\")","v":"CHECK RATINGS"}]
[]
[]
[]
[null,2,null,"Data quality & uncertainty assessment information"]
[]
[null,2.1,null,"Data quality assessment"]
[null,null,null,null,null,"You should assess data quality and uncertainty for lifecycle modules that cover at least 90% of total footprint emissions.","In this column, the user should describe the quality of the activity datapoints used to populate the relevant GHG lifecycle module tab. The table requires one description of the aggregated data rather than a description for each activity on the lifecycle tabs for ease of use, please consider materiality within the lifecycle module and weight the assessment towards the most impactful activities.","In this column, the user should rate the activity data quality using the pedigree matrix guidelines below for \"completeness\". This indicates how complete you think the activity data used for the lifecycle module is. If you missed a number of relevant activities based on lack of data availability, you will score this lower.","In this column, the user should rate the activity data quality using the pedigree matrix guidelines below for \"source reliability\". This indicates how good the source data used for the lifecycle module is. If you had to extrapolate from another development instead of using primary data, or had to convert spend to quantities.","This column shows the weighed average DQ score for the lifecycle module activity data.","In this column, the user should attempt to describe the quality of the emission factor datapoints used to populate the relevant GHG lifecycle module tab. The table requires one description of the aggregated data rather than a description for each activity on the lifecycle tabs for ease of use. Please consider materiality within the lifecycle module and weight the assessment towards the most impactful activities.","In this column, the user should rate the emission factors data quality using the pedigree matrix guidelines below for \"technology\". This indicates how well the emission factors used in the lifecycle module represent the technologies of activities (e.g. low-alloyed hot rolled steel, tonnes (good), Steel, average, tonnes (fair)","In this column, the user should rate the emission factors data quality using the pedigree matrix guidelines below for \"time\". This is assessed by estimating how long the period of time is between the calculation and publication of the emission factors used in the lifecycle module, and the occurrence of the activity you are applying it to. (e.g. EF was published in 2019, I'm using it for a footprint in 2023, (fair))","In this column, the user should rate the emission factors data quality using the pedigree matrix guidelines below for \"geography\". This is assessed by comparing the regional specificity of the emission factors used in the lifecycle module to the geographical location where activity is occurring.(e.g. EF for steel making was specific to the relevant country (very good))","In this column, the user should rate the emission factor data quality using the pedigree matrix guidelines below for \"completeness\". This indicates how complete you think the emission factors used are. In general, verified primary emissions factors should be rated very good or good, and secondary or proxy should be rated fair or poor","In this column, the user should rate the activity data quality using the pedigree matrix guidelines below for \"Source reliability\". This indicates how good the emissions factors used are. In general, verified primary emissions factors should be rated Very Good or Good, and Secondary or Proxy should be rated Fair or Poor","This column shows the weighed average DQ score for the lifecycle module emission factors.","Please select an activity category for basic uncertainty. This is an inherent uncertainty related to how emissions are calculated. Some lifecycle modules will have a combination of activities, in this case, select the most material activity type from the lifecycle module on the results tab.","This column shows the weighed average DQ score for the lifecycle module (average of AD and EF)","Uncertainty in the activity data total is assumed to be distributed lognormally (skewed-right, no negative values) in line with typical environmental assessments. The geometric standard distribution shows the distribution around a geometric mean (median), which is the central tendency measure for lognormal distributions","Uncertainty in the emission factor total is assumed to be distributed lognormally (skewed-right, no negative values) in line with typical environmental assessments. The geometric standard distribution shows the distribution around a geometric mean (median), which is the central tendency measure for lognormal distributions","As the emissions calculation is multiplicative, AD * EF, their uncertainties (expressed as GSD2) also multiply to find the total uncertainty for the calculation","The GSD is the typical measure of variability of a lognormal distribution. It is a representation of how much the numbers typically deviate from the geometric mean (calculated emissions total), and can be used to describe our confidence in total.","The uncertainty in a normal distribution is typically defined by % confidence interval. The assumed skewedness of the lognormally distributed parameter means the % coverage of GSD above and below the mean (total emissions) can vary","The uncertainty in a normal distribution is typically defined by % confidence interval. The assumed skewedness of the lognormally distributed parameter means the % coverage of GSD above and below the mean (total emissions) can vary.","The error range is represented by the \"geometric mean + GSD\". In a normal distribution we typically describe this as a confidence interval, or 68% of the data falling within one standard deviation of the mean. This direct correlation doesn’t translate to a lognormal distribution due to its asymmetry.","The error range is represented by the \"geometric mean - GSD\". In a normal distribution we typically describe this as a confidence interval, or 68% of the data falling within one standard deviation of the mean. This direct correlation doesn’t translate to a lognormal distribution due to its asymmetry.","Upper bound error expressed as a %. The upper bound is larger than the lower bound error based on the lognormal distribution (skewed right)","Lower bound error expressed as a %. The upper bound is larger than the lower bound error based on the lognormal distribution (skewed right)"]
[]
[null,null,null,"GHG Lifecycle Module Table","Total calculated emissions (tCO2e)","Total contribution to footprint (%)","Activity Data Qualitative Description","Activity Data DQ rating - Completeness","Activity Data DQ rating - Source reliability","Weighed average DQ score - Activity Data","Emissions Factors Qualitative Description","Emission Factors DQ rating - Technology","Emission Factors DQ rating - Time","Emission Factors DQ rating - Geography","Emission Factors DQ rating - Completeness","Emission Factors DQ rating - Source reliability","Weighed average DQ score - emission factor","Lifecycle module activities basic uncertainty","Lifecycle Module Average DQ Rating","Activity Data Quality Uncertainty: Geometric Standard Deviation^2","Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2","Combined uncertainty for lifecycle module: Geometric Standard Deviation^2","Combined uncertainty: Geometric Standard Deviation","Total Calculated Emissions (tCO2e) - Upper Bound","Total Calculated Emissions (tCO2e) - Lower Bound","Upper bound error (tCO2e)","Lower bound error (tCO2e)","Upper bound error (%)","Lower bound error (%)"]
[null,null,null,"A0 - Preconstruction",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},"e.g.: To populate this table we used data gathered directly from our operations and engineering who have access to primary data related to preconstruction activities, it is of high quality. It was measured in a timely manner and is fully complete with no extrapolation for the OSW development under study or missing activities","Fair","Fair",{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":0.5},"e.g.: The emissions factors used for the A0 calculation are predominately fuel based emission factors taken from a proxy source (UK government).They are based on calorific value and we believe of high quality","Very Good","Very Good","Very Good","Very Good","Very Good",{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":0.9},"Electricity & Fuels",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":0.7},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":1.0432336627876222},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":1},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":1.0432336627876222},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":1.0213881058577206},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"A1-A2 Raw Material and Transport",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},"e.g.: To populate this table we made assumptions about the material composition of the primary materials used in all of the core infrastructure assets. Some were based on old (5 years) technical specification, but most were assumed based on proxies or expert judgement","Good","Good",{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":0.7},"e.g. The emission factors used for A1-A2 are predominantly taken directly from our secondary database and accurately reflect ","Very Good","Poor","Very Good","Poor","Poor",{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":0.38823529411764707},"Materials",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":0.54411764705882348},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":1.0115304798555562},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":1.4362636554664001},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":1.4528244646130231},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":1.2053316824065579},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"A3 Manufacturing",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},"e.g.: To populate this table we made assumptions to allocate the emissions for manufacturing facilities to individual assets",null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Manufacturing processes",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"A1-A3 - Production & manufacturing (finished assets & subcomponents)",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},"For populating this table, we collected EPDs from Siemens Gamesa, which allowed us to ",null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Manufactured Assets",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"A4 - Transport to site",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Electricity & Fuels",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"A5 - Construction",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Electricity & Fuels",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"B1 - Use",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Direct Emissions & removals",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"B2 - Maintenance",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Electricity & Fuels",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"B3 - Repair",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Electricity & Fuels",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"B4 - Replacement",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Materials",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"B5 - Refurbishment",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Materials",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"B6 - Operational energy consumption",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Electricity & Fuels",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"B7 - Operational water consumption",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Electricity & Fuels",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"B8 - Operational activities not otherwise captured in modules B1-B7",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Materials",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"C1 - Deconstruction Demolition",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Freight & Transportation",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"C2 - Transport",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Electricity & Fuels",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"C3-C4 - Waste processing, sorting for recycling & disposal",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},"Waste Treatment",{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"C5 - Relandscaping",{"$f":"IFERROR(INDEX(Results_Lifecycle[[#Data],[#Totals],[Total (tCO2e) ]],MATCH(DQ_Uncertainty_Assessment[[#This Row],[GHG Lifecycle Module Table]],Results_Lifecycle[[#Data],[#Totals],[GHG Lifecycle Module]],0)),\"CHECK ENTRIES\")","v":0},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#Totals],[Total calculated emissions (tCO2e)]:[Total calculated emissions (tCO2e)]],0)","v":0},null,null,null,{"$f":"IFERROR((((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+(INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90)/SUM($H$90:$I$90),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,null,null,null,null,null,{"$f":"IFERROR(((((INDEX(DQ_Indicator_Values[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],DQ_Indicator_Values[Indicator Score],0)))*$E$90)+((INDEX(DQ_Indicator_Values[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],DQ_Indicator_Values[Indicator Score],0)))*$F$90)+((INDEX(DQ_Indicator_Values[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],DQ_Indicator_Values[Indicator Score],0)))*$G$90)+((INDEX(DQ_Indicator_Values[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],DQ_Indicator_Values[Indicator Score],0)))*$H$90)+((INDEX(DQ_Indicator_Values[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],DQ_Indicator_Values[Indicator Score],0)))*$I$90))/SUM($E$90:$I$90)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},null,{"$f":"IFERROR(AVERAGE(DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - Activity Data]],DQ_Uncertainty_Assessment[[#This Row],[Weighed average DQ score - emission factor]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Activity Data DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(EXP(SUM(LN(INDEX(Pedigree_Uncertainty_Scalars[Technology], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Technology]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Time], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Time]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Geography], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Geography]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Completeness], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Completeness]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2,LN(INDEX(Pedigree_Uncertainty_Scalars[Source reliability], MATCH(DQ_Uncertainty_Assessment[[#This Row],[Emission Factors DQ rating - Source reliability]],Pedigree_Uncertainty_Scalars[Indicator Score],0)))^2)),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Activity Data Quality Uncertainty: Geometric Standard Deviation^2]]*DQ_Uncertainty_Assessment[[#This Row],[Emission Factor Data Quality Uncertainty: Geometric Standard Deviation^2]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(SQRT(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty for lifecycle module: Geometric Standard Deviation^2]]),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]*(DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]]^1.96),\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Combined uncertainty: Geometric Standard Deviation]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Upper Bound]]-DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]]-DQ_Uncertainty_Assessment[[#This Row],[Total Calculated Emissions (tCO2e) - Lower Bound]],\"CHECK RATINGS\")","v":"CHECK RATINGS"},{"$f":"IFERROR(DQ_Uncertainty_Assessment[[#This Row],[Upper bound error (tCO2e)]]/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ERROR\")","v":"CHECK ERROR"},{"$f":"IFERROR((-DQ_Uncertainty_Assessment[[#This Row],[Lower bound error (tCO2e)]])/DQ_Uncertainty_Assessment[[#This Row],[Total calculated emissions (tCO2e)]],\"CHECK ENTRIES\")","v":"CHECK ENTRIES"}]
[null,null,null,"Total",{"$f":"SUBTOTAL(109,DQ_Uncertainty_Assessment[Total calculated emissions (tCO2e)])","v":0},{"$f":"SUBTOTAL(109,DQ_Uncertainty_Assessment[Total contribution to footprint (%)])","v":0}]
[]
[null,null,null,"Data quality & uncertainty scoring information: DQ Pedigree matrix & basic uncertainty values"]
[]
[null,null,null,"Data quality pedigree matrix guidance & scalars"]
[]
[null,null,null,"Indicator Score","Technology","Time","Geography","Completeness","Source reliability"]
[null,null,null,"Very Good","Datapoints represent the exact technology used in OSW activity (e.g. EPDs for main assets, primary materials, Steel, aluminium etc))","Datapoints were produced less than 3 years from actual time of OSW activity","Datapoints represent the exact country where in OSW activity took place (e.g., Copper, produced in Germany)","Datapoints represent complete scope of OSW activity for in boundary for the assessment no missing data or extrapolations (e.g., we have primary data for fuel consumption in all vessels, emission factor covers all relevant upstream activities)","Verified, high quality process data based on measurements and other primary data (e.g., Quantity of Aluminium for cables in kg, tonnes, measured by manufacturer)"]
[null,null,null,"Good","Datapoints represents similar technology used in OSW development activity (e.g., Steel, low-alloyed, produced by BOF from generic database)","Datapoints was produced less than 6 years from time of OSW activity","Datapoints represent the region where in OSW activity took place (e.g., Copper, produced in Europe)","Datapoints represents more than half of the activity with minor extrapolation (e.g., we have primary data for fuel consumption for 80% of vessel working days and extrapolate the rest)","Verified process quantity data based partly on assumptions or other secondary data. (e.g., Quantity of aluminium, in kg, tonnes, based on BoM or design)"]
[null,null,null,"Fair","Datapoints represents similar technology used in OSW development activity (e.g., Steel, average produced from generic database)","Datapoints was produced less than 10 years from time of OSW activity","Datapoints represents a different region used as a proxy for OSW activity (Copper produced in Germany, as a proxy for copper produced in Japan, etc.) ","Datapoints represents less than half of total activity significant extrapolation (e.g., we have primary data for fuel consumption for 20% of vessel working days and extrapolate the rest)","Non-verified, low-quality data based on stated assumptions or other qualified estimate (Quantity of aluminium, in kg, tonnes, based on other similar cables)"]
[null,null,null,"Poor","Datapoints does not represent a specific technology (e.g., Metals, unknown, from assumptions)","Datapoints was produced more than 10 years from time of OSW activity or has not yet occurred (prospective)","Datapoints does not describe a geographical area, or area is unknown (Copper, unknown production geography)","Datapoints represents less than 5% of total activity (we have we have primary data for fuel consumption for 1% of vessel working days and extrapolate the rest)","Non-verified data based on unqualified estimates (Quantity of aluminium, converted from financial cost, based on guess for average cable)"]
[]
[null,null,null,"Data quality indicator values and data quality weighting factors (OSW Industry PCF Guidance -  GHG Protocol Quantitative Uncertainty Guidance)"]
[]
[null,null,null,"Indicator Score","Technology","Time","Geography","Completeness","Source reliability","Weighted average DQ score"]
[null,null,null,"Very Good",0.9,0.9,0.9,0.9,0.9,0.9]
[null,null,null,"Good",0.7,0.7,0.7,0.7,0.7,0.7]
[null,null,null,"Fair",0.5,0.5,0.5,0.5,0.5,0.5]
[null,null,null,"Poor",0.17499999999999999,0.17499999999999999,0.17499999999999999,0.17499999999999999,0.17499999999999999,0.2]
[null,null,null,"DQ Weighting Factor",1.5,2,1,2,2,"NA"]
[]
[null,null,null,"Uncertainty scaling factors for pedigree matrix (GHGP)"]
[null,null,null,"Source: Quantitative Inventory Uncertainty - Greenhouse Gas Protocol"]
[null,null,null,"Indicator Score","Technology","Time","Geography","Completeness","Source reliability"]
[null,null,null,"Very Good",1,1,1,1,1]
[null,null,null,"Good",1.2,1.1000000000000001,1.02,1.05,1.1000000000000001]
[null,null,null,"Fair",1.5,1.2,1.05,1.1000000000000001,1.2]
[null,null,null,"Poor",2,1.5,1.1000000000000001,1.2,1.5]
[]
[]
[null,null,null,"Basic uncertainty scalars for activity type - Emission Factors"]
[null,null,null,"Source: Quantitative Inventory Uncertainty - Greenhouse Gas Protocol"]
[null,null,null,"Activity Category","Basic uncertainty scaling factor"]
[null,null,null,"Direct Emissions & removals",1.05]
[null,null,null,"Freight & Transportation",2]
[null,null,null,"Electricity & Fuels",1.05]
[null,null,null,"Manufactured Assets",1.05]
[null,null,null,"Manufactured Sub-components",1.05]
[null,null,null,"Manufacturing processes",1.05]
[null,null,null,"Materials",1.05]
[null,null,null,"Waste Treatment",1.05]

{"sheet":"Conversions","index":18,"n_rows":219,"n_cols":45,"rows_kept":219,"cut":false,"hidden":false,"merged":[[8,1,8,5]]}
[]
[null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,"Offshore Wind Footprinting Tool"]
[null,"UNIT CONVERSION CALCULATOR"]
[]
[]
[null,"Tab description"]
[]
[null,"The Unit Conversion tab provides conversion factors for various units of measurement commonly used for activity data in the OSW development system. These may  be applied to convert data to the correct unit required for an emission factor when performing calculations on tabs A1-C5. "]
[]
[]
[null,"Unit conversion calculator"]
[]
[null,"Measurement type","Quantity ","From","To","Converted quantity"]
[null,null,null,null,null,{"$f":"IFERROR(IF(E15=\"\",\"\",INDEX(E20:E220,MATCH(1,(D15=C20:C220)*(E15=D20:D220),0))*C15), \"Check units\")","v":""}]
[]
[]
[null,"Conversion data",null,null,null,null,"Do not modify - used for 'From' dependant drop-down",null,null,null,null,null,"Do not modify - used for 'To' dependant drop-down"]
[null,"Measurement Type","from_unit_name","to_unit_name","value",null,{"$f":"TRANSPOSE(_xlfn._xlws.SORT(_xlfn.UNIQUE(B20:B219)))","v":"Area"},"Distance","Energy","Mass","Volume",null,{"$f":"TRANSPOSE(_xlfn._xlws.SORT(_xlfn.UNIQUE(C20:C219)))","v":"acre"},"centimetre","cubic foot","cubic metre","foot","gallon","gigajoule","gigawatt-hour","gram","hectare","inch","joule","kilogram","kilometre","kilowatt-hour","litre","long ton","megawatt-hour","metre","mile","millimetre","nautical mile","short ton","square foot","square inch","square kilometre","square metre","square mile","square yard","terawatt-hour","tonne","watt-hour","yard"]
[null,"Distance","kilometre","metre",1000,null,{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($C$20:$C$220,$B$20:$B$220=G19))),\"No selection\")","v":"acre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($C$20:$C$220,$B$20:$B$220=H19))),\"No selection\")","v":"centimetre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($C$20:$C$220,$B$20:$B$220=I19))),\"No selection\")","v":"gigajoule"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($C$20:$C$220,$B$20:$B$220=J19))),\"No selection\")","v":"gram"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($C$20:$C$220,$B$20:$B$220=K19))),\"No selection\")","v":"cubic foot"},null,{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=M19))),\"No selection\")","v":"hectare"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=N19))),\"No selection\")","v":"foot"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=O19))),\"No selection\")","v":"cubic metre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=P19))),\"No selection\")","v":"cubic foot"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=Q19))),\"No selection\")","v":"centimetre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=R19))),\"No selection\")","v":"cubic foot"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=S19))),\"No selection\")","v":"gigawatt-hour"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=T19))),\"No selection\")","v":"gigajoule"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=U19))),\"No selection\")","v":"kilogram"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=V19))),\"No selection\")","v":"acre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=W19))),\"No selection\")","v":"centimetre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=X19))),\"No selection\")","v":"gigajoule"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=Y19))),\"No selection\")","v":"gram"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=Z19))),\"No selection\")","v":"centimetre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AA19))),\"No selection\")","v":"gigajoule"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AB19))),\"No selection\")","v":"cubic foot"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AC19))),\"No selection\")","v":"gram"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AD19))),\"No selection\")","v":"gigajoule"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AE19))),\"No selection\")","v":"centimetre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AF19))),\"No selection\")","v":"centimetre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AG19))),\"No selection\")","v":"centimetre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AH19))),\"No selection\")","v":"centimetre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AI19))),\"No selection\")","v":"gram"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AJ19))),\"No selection\")","v":"acre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AK19))),\"No selection\")","v":"acre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AL19))),\"No selection\")","v":"acre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AM19))),\"No selection\")","v":"acre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AN19))),\"No selection\")","v":"acre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AO19))),\"No selection\")","v":"acre"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AP19))),\"No selection\")","v":"gigajoule"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AQ19))),\"No selection\")","v":"gram"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AR19))),\"No selection\")","v":"gigajoule"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER($D$20:$D$220,$C$20:$C$220=AS19))),\"No selection\")","v":"centimetre"}]
[null,"Distance","kilometre","centimetre",100000,null,"hectare","foot","gigawatt-hour","kilogram","cubic metre",null,"square foot","inch","gallon","gallon","inch","cubic metre","joule","joule","long ton","square foot","foot","gigawatt-hour","long ton","foot","gigawatt-hour","cubic metre","kilogram","gigawatt-hour","foot","foot","foot","foot","kilogram","hectare","hectare","hectare","hectare","hectare","hectare","gigawatt-hour","kilogram","gigawatt-hour","foot"]
[null,"Distance","kilometre","mile",0.62137100000000001,null,"square foot","inch","joule","long ton","gallon",null,"square inch","kilometre","litre","litre","kilometre","litre","kilowatt-hour","kilowatt-hour","short ton","square inch","kilometre","kilowatt-hour","short ton","inch","joule","gallon","short ton","joule","inch","inch","inch","inch","long ton","square inch","square foot","square foot","square foot","square foot","square foot","joule","long ton","joule","inch"]
[null,"Distance","kilometre","yard",1093.6099999999999,null,"square inch","kilometre","kilowatt-hour","short ton","litre",null,"square kilometre","metre",null,null,"metre",null,"megajoule","megajoule","tonne","square kilometre","metre","megajoule","tonne","metre","megajoule",null,"tonne","kilowatt-hour","kilometre","kilometre","kilometre","metre","ounce","square kilometre","square metre","square inch","square inch","square inch","square inch","kilowatt-hour","short ton","kilowatt-hour","kilometre"]
[null,"Distance","kilometre","foot",3280.84,null,"square kilometre","metre","megawatt-hour","tonne",null,null,"square metre","mile",null,null,"mile",null,"megawatt-hour","megawatt-hour",null,"square metre","mile","megawatt-hour",null,"mile","megawatt-hour",null,null,"megajoule","mile","metre","metre","mile","tonne","square metre","square mile","square metre","square kilometre","square kilometre","square kilometre","megajoule",null,"megajoule","metre"]
[null,"Distance","kilometre","inch",39370.1,null,"square metre","mile","terawatt-hour",null,null,null,"square mile","nautical mile",null,null,"nautical mile",null,"terawatt-hour","terawatt-hour",null,"square mile","nautical mile","terawatt-hour",null,"nautical mile","terawatt-hour",null,null,"terawatt-hour","nautical mile","nautical mile","mile","yard",null,"square mile","square yard","square mile","square mile","square metre","square metre","megawatt-hour",null,"megawatt-hour","mile"]
[null,"Distance","kilometre","nautical mile",0.53995700000000002,null,"square mile","millimetre","watt-hour",null,null,null,"square yard","yard",null,null,"yard",null,"watt-hour","watt-hour",null,"square yard","yard","watt-hour",null,"yard","watt-hour",null,null,"watt-hour","yard","yard","nautical mile",null,null,"square yard",null,"square yard","square yard","square yard","square mile","watt-hour",null,"terawatt-hour","nautical mile"]
[null,"Distance","metre","kilometre",1E-3,null,"square yard","nautical mile",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yard"]
[null,"Distance","metre","centimetre",100,null,null,"yard"]
[null,"Distance","metre","mile",6.2137100000000001E-4]
[null,"Distance","metre","yard",1.09361]
[null,"Distance","metre","foot",3.28084]
[null,"Distance","metre","inch",39.370100000000001]
[null,"Distance","metre","nautical mile",5.3995699999999998E-4]
[null,"Distance","centimetre","kilometre",1.0000000000000001E-5]
[null,"Distance","centimetre","metre",0.01]
[null,"Distance","centimetre","mile",6.2137000000000003E-6]
[null,"Distance","centimetre","yard",1.0936100000000001E-2]
[null,"Distance","centimetre","foot",3.2808400000000001E-2]
[null,"Distance","centimetre","inch",0.39370100000000002]
[null,"Distance","centimetre","nautical mile",5.3995999999999999E-6]
[null,"Distance","millimetre","kilometre",9.9999999999999995E-7]
[null,"Distance","millimetre","metre",1E-3]
[null,"Distance","millimetre","centimetre",0.1]
[null,"Distance","millimetre","mile",6.2137000000000001E-7]
[null,"Distance","millimetre","yard",1.0936100000000001E-3]
[null,"Distance","millimetre","foot",3.2808400000000001E-3]
[null,"Distance","millimetre","inch",3.9370099999999998E-2]
[null,"Distance","millimetre","nautical mile",5.3995999999999997E-7]
[null,"Distance","mile","kilometre",1.6093440000000001]
[null,"Distance","mile","metre",1609.3440000000001]
[null,"Distance","mile","centimetre",1609344]
[null,"Distance","mile","yard",1760]
[null,"Distance","mile","foot",5280]
[null,"Distance","mile","inch",63360]
[null,"Distance","mile","nautical mile",0.86897599999999997]
[null,"Distance","yard","kilometre",9.144E-4]
[null,"Distance","yard","metre",0.91439999999999999]
[null,"Distance","yard","centimetre",91.44]
[null,"Distance","yard","mile",5.6818199999999998E-4]
[null,"Distance","yard","foot",3]
[null,"Distance","yard","inch",36]
[null,"Distance","yard","nautical mile",4.9373699999999995E-4]
[null,"Distance","foot","kilometre",3.0479999999999998E-4]
[null,"Distance","foot","metre",0.30480000000000002]
[null,"Distance","foot","centimetre",30.48]
[null,"Distance","foot","mile",1.8939400000000001E-4]
[null,"Distance","foot","yard",0.33333299999999999]
[null,"Distance","foot","inch",12]
[null,"Distance","foot","nautical mile",1.6457900000000001E-4]
[null,"Distance","inch","kilometre",2.5400000000000001E-5]
[null,"Distance","inch","metre",2.5399999999999999E-2]
[null,"Distance","inch","centimetre",2.54]
[null,"Distance","inch","mile",1.5783000000000001E-5]
[null,"Distance","inch","yard",2.7777799999999998E-2]
[null,"Distance","inch","foot",8.3333299999999999E-2]
[null,"Distance","inch","nautical mile",1.3715E-5]
[null,"Distance","nautical mile","inch",72913.399999999994]
[null,"Distance","nautical mile","metre",1852]
[null,"Distance","nautical mile","centimetre",185200]
[null,"Distance","nautical mile","mile",1.1507799999999999]
[null,"Distance","nautical mile","yard",2025.37]
[null,"Distance","nautical mile","foot",6076.12]
[null,"Mass","tonne","kilogram",1000]
[null,"Mass","tonne","gram",1000000]
[null,"Mass","kilogram","tonne",1E-3]
[null,"Mass","kilogram","gram",1000]
[null,"Mass","gram","tonne",9.9999999999999995E-7]
[null,"Mass","gram","kilogram",1E-3]
[null,"Volume","cubic metre","litre",1000]
[null,"Volume","cubic metre","gallon",219.96899999999999]
[null,"Volume","cubic metre","cubic foot",35.314700000000002]
[null,"Volume","litre","cubic metre",1E-3]
[null,"Volume","litre","gallon",0.219969]
[null,"Volume","litre","cubic foot",3.5314699999999997E-2]
[null,"Volume","gallon","cubic metre",4.54609E-3]
[null,"Volume","gallon","litre",4.5460900000000004]
[null,"Volume","gallon","cubic foot",0.16054399999999999]
[null,"Volume","cubic foot","cubic metre",2.83168E-2]
[null,"Volume","cubic foot","litre",28.316800000000001]
[null,"Volume","cubic foot","gallon",6.2288300000000003]
[null,"Area","square kilometre","hectare",100]
[null,"Area","square kilometre","square metre",1000000]
[null,"Area","square kilometre","square mile",0.386102]
[null,"Area","square kilometre","acre",247.10499999999999]
[null,"Area","square kilometre","square yard",1196000]
[null,"Area","square kilometre","square foot",10760000]
[null,"Area","square kilometre","square inch",1550000000]
[null,"Area","hectare","square kilometre",0.01]
[null,"Area","hectare","square metre",10000]
[null,"Area","hectare","square mile",3.8610200000000002E-3]
[null,"Area","hectare","acre",2.47105]
[null,"Area","hectare","square yard",11959.9]
[null,"Area","hectare","square foot",107639]
[null,"Area","hectare","square inch",15500000]
[null,"Area","square metre","square kilometre",9.9999999999999995E-7]
[null,"Area","square metre","hectare",1E-4]
[null,"Area","square metre","square mile",3.861E-7]
[null,"Area","square metre","acre",2.4710500000000001E-4]
[null,"Area","square metre","square yard",1.1959900000000001]
[null,"Area","square metre","square foot",10.7639]
[null,"Area","square metre","square inch",1550]
[null,"Area","square mile","square kilometre",2.5899899999999998]
[null,"Area","square mile","hectare",258.99900000000002]
[null,"Area","square mile","square metre",2590000]
[null,"Area","square mile","acre",640]
[null,"Area","square mile","square yard",3098000]
[null,"Area","square mile","square foot",27880000]
[null,"Area","square mile","square inch",4014000000]
[null,"Area","acre","square kilometre",4.0468600000000002E-3]
[null,"Area","acre","hectare",0.40468599999999999]
[null,"Area","acre","square metre",4046.86]
[null,"Area","acre","square mile",1.5625000000000001E-3]
[null,"Area","acre","square yard",4840]
[null,"Area","acre","square foot",43560]
[null,"Area","acre","square inch",6273000]
[null,"Area","square yard","square kilometre",8.3613000000000001E-7]
[null,"Area","square yard","hectare",8.3613000000000001E-5]
[null,"Area","square yard","square metre",0.83612699999999995]
[null,"Area","square yard","square mile",3.2282999999999999E-7]
[null,"Area","square yard","acre",2.0661200000000001E-4]
[null,"Area","square yard","square foot",9]
[null,"Area","square yard","square inch",1296]
[null,"Area","square foot","square kilometre",9.2902999999999995E-8]
[null,"Area","square foot","hectare",9.2902999999999998E-6]
[null,"Area","square foot","square metre",9.2902999999999999E-2]
[null,"Area","square foot","square mile",3.5870000000000003E-8]
[null,"Area","square foot","acre",2.2957000000000001E-5]
[null,"Area","square foot","square yard",0.111111]
[null,"Area","square foot","square inch",144]
[null,"Area","square inch","square foot",6.9444399999999996E-3]
[null,"Area","square inch","hectare",6.4515999999999994E-8]
[null,"Area","square inch","square metre",6.4515999999999998E-4]
[null,"Area","square inch","square mile",2.491E-10]
[null,"Area","square inch","acre",1.5942000000000001E-7]
[null,"Area","square inch","square yard",7.7160499999999997E-4]
[null,"Energy","gigajoule","joule",1000000000]
[null,"Energy","gigajoule","watt-hour",2.7778E+105]
[null,"Energy","gigajoule","kilowatt-hour",277.77780000000001]
[null,"Energy","gigajoule","megawatt-hour",0.27779999999999999]
[null,"Energy","gigajoule","gigawatt-hour",2.7777999999999999E-4]
[null,"Energy","gigajoule","terawatt-hour",2.7777999999999999E-7]
[null,"Energy","gigajoule","megajoule",1000]
[null,"Energy","watt-hour","joule",3600]
[null,"Energy","watt-hour","gigajoule",3600000]
[null,"Energy","watt-hour","kilowatt-hour",1E-3]
[null,"Energy","watt-hour","megawatt-hour",9.9999999999999995E-7]
[null,"Energy","watt-hour","gigawatt-hour",1.0000000000000001E-9]
[null,"Energy","watt-hour","terawatt-hour",9.9999999999999998E-13]
[null,"Energy","watt-hour","megajoule",3.5999999999999999E-3]
[null,"Energy","kilowatt-hour","joule",3600000]
[null,"Energy","kilowatt-hour","gigajoule",3.5999999999999999E-3]
[null,"Energy","kilowatt-hour","watt-hour",1000]
[null,"Energy","kilowatt-hour","megawatt-hour",1E-3]
[null,"Energy","kilowatt-hour","gigawatt-hour",9.9999999999999995E-7]
[null,"Energy","kilowatt-hour","terawatt-hour",1.0000000000000001E-9]
[null,"Energy","kilowatt-hour","megajoule",3.6]
[null,"Energy","megawatt-hour","joule",3600000000]
[null,"Energy","megawatt-hour","gigajoule",3.6]
[null,"Energy","megawatt-hour","watt-hour",1000000]
[null,"Energy","megawatt-hour","kilowatt-hour",1000]
[null,"Energy","megawatt-hour","gigawatt-hour",1E-3]
[null,"Energy","megawatt-hour","terawatt-hour",9.9999999999999995E-7]
[null,"Energy","megawatt-hour","megajoule",3600]
[null,"Energy","gigawatt-hour","joule",3600000000000]
[null,"Energy","gigawatt-hour","gigajoule",3600]
[null,"Energy","gigawatt-hour","watt-hour",1000000000]
[null,"Energy","gigawatt-hour","kilowatt-hour",1000000]
[null,"Energy","gigawatt-hour","megawatt-hour",1000]
[null,"Energy","gigawatt-hour","terawatt-hour",1E-3]
[null,"Energy","gigawatt-hour","megajoule",3600000]
[null,"Energy","terawatt-hour","joule",3600000000000000]
[null,"Energy","terawatt-hour","gigajoule",3600000]
[null,"Energy","terawatt-hour","watt-hour",1000000000000]
[null,"Energy","terawatt-hour","kilowatt-hour",1000000000]
[null,"Energy","terawatt-hour","megawatt-hour",1000000]
[null,"Energy","terawatt-hour","gigawatt-hour",1000]
[null,"Energy","terawatt-hour","megajoule",3600000]
[null,"Energy","joule","gigajoule",1.0000000000000001E-9]
[null,"Energy","joule","megajoule",9.9999999999999995E-7]
[null,"Energy","joule","watt-hour",2.7777800000000001E-4]
[null,"Energy","joule","kilowatt-hour",2.7777799999999999E-7]
[null,"Energy","joule","megawatt-hour",2.7777799999999998E-10]
[null,"Energy","joule","gigawatt-hour",2.7777800000000001E-13]
[null,"Energy","joule","terawatt-hour",2.7777800000000001E-16]
[null,"Mass","long ton","tonne",1.0160499999999999]
[null,"Mass","long ton","kilogram",1016.05]
[null,"Mass","long ton","gram",1016000]
[null,"Mass","short ton","tonne",0.90718500000000002]
[null,"Mass","short ton","kilogram",907.18499999999995]
[null,"Mass","short ton","gram",907185]
[null,"Mass","short ton","ounce",32000]
[null,"Mass","tonne","long ton",0.98420700000000005]
[null,"Mass","tonne","short ton",1.1023099999999999]
[null,"Mass","kilogram","long ton",9.8420699999999996E-4]
[null,"Mass","kilogram","short ton",1.10231E-3]
[null,"Mass","gram","long ton",9.842100000000001E-7]
[null,"Mass","gram","short ton",1.1023E-6]
[null,"Mass","long ton","short ton",1.1200000000000001]
[null,"Mass","short ton","long ton",0.89285700000000001]

{"sheet":"Results","index":19,"n_rows":234,"n_cols":10,"rows_kept":234,"cut":false,"hidden":false,"merged":[[21,1,21,5]]}
[]
[]
[null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,"RESULTS"]
[]
[]
[null,"Description cell"]
[null,"Calculation Cell"]
[]
[null,"Reporting emissions per reference unit and other selected intensity metrics"]
[]
[null,"GHG Lifecycle Module","Unit","Assessor defined reference flow","Sensitivity analysis (default reference flow parameters)"]
[null,"Installed capacity","MW",{"$f":"IFERROR(Installed_capacity__MW,0)","v":880},{"$f":"Installed_capacity__MW","v":880}]
[null,"Reference flow (expected lifetime electricity delivered to grid)","kWh",{"$f":"IFERROR(Reference_flow_kWh,0)","v":94432800000},{"$f":"Reference_flow_kWh_SA","v":91542000000}]
[null,"Absolute emissions from OSW development lifecycle (A1-C4)","tCO2e",{"$f":"IFERROR(Results_Lifecycle[[#Totals],[Total (tCO2e) ]],0)","v":0},{"$f":"IFERROR(Results_Lifecycle[[#Totals],[Total (tCO2e) ]],0)","v":0}]
[null,"Emissions per kWh, net, delivered to the grid","gCO2e/kWh delivered",{"$f":"IFERROR((D$15*1000000)/(D$14),0)","v":0},{"$f":"IFERROR((E$15*1000000)/(E$14),0)","v":0}]
[null,"Emissions per MW installed capacity","tCO2e/MW installed",{"$f":"IFERROR((D$15)/(D$13),0)","v":0},{"$f":"IFERROR((E$15)/(E$13),0)","v":0}]
[null,"Emissions per operational year","tCO2e/year of operation",{"$f":"IFERROR(D$15/Assumed_service_life_Years,0)","v":0},{"$f":"IFERROR(E$15/Assumed_service_life_Years_SA,0)","v":0}]
[]
[]
[null,"Absolute emissions by lifecycle stage, module & emissions type"]
[null,"This table shows the full breakdown of emissions by lifecycle module, and where possible, emissions type. Where an Emission Factor did not have a breakdown including Fossil, Biogenic or Land-use Change emissions, and reported a single net emissions total, this appears directly in the Total column."]
[]
[]
[null,"GHG Lifecycle Module","Fossil (tCO2e)","Biogenic (tCO2e)","Land Use Change (tCO2e)","Total (tCO2e) ","% of total emissions by information module and lifecyle stage (green bar)"]
[null,"A0 - Preconstruction "]
[null,"A0 - Preconstruction",{"$f":"'A0 - Preconstruction'!I29","v":0},{"$f":"'A0 - Preconstruction'!J29","v":0},{"$f":"'A0 - Preconstruction'!K29","v":0},{"$f":"'A0 - Preconstruction'!L29","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"TOTAL (A0)",{"$f":"SUM(C27)","v":0},{"$f":"SUM(D27)","v":0},{"$f":"SUM(E27)","v":0},{"$f":"SUM(F27)","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"A1-A3 - Production & manufacturing "]
[null,"A1-A2 Raw Material and Transport",{"$f":"'A1-A3 - Production'!I29","v":0},{"$f":"'A1-A3 - Production'!J29","v":0},{"$f":"'A1-A3 - Production'!K29","v":0},{"$f":"'A1-A3 - Production'!L29","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"A3 Manufacturing",{"$f":"'A1-A3 - Production'!I30","v":0},{"$f":"'A1-A3 - Production'!J30","v":0},{"$f":"'A1-A3 - Production'!K30","v":0},{"$f":"'A1-A3 - Production'!L30","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"A1-A3 - Production & manufacturing (finished assets & subcomponents)",{"$f":"'A1-A3 - Production'!I31","v":0},{"$f":"'A1-A3 - Production'!J31","v":0},{"$f":"'A1-A3 - Production'!K31","v":0},{"$f":"'A1-A3 - Production'!L31","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"TOTAL Production & manufacturing (A1-A3)",{"$f":"SUM(C30:C32)","v":0},{"$f":"SUM(D30:D32)","v":0},{"$f":"SUM(E30:E32)","v":0},{"$f":"SUM(F30:F32)","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"A4 -A5 - Construction & Installation "]
[null,"A4 - Transport to site",{"$f":"'A4-A5 -Transport & Construction'!I30","v":0},{"$f":"'A4-A5 -Transport & Construction'!J30","v":0},{"$f":"'A4-A5 -Transport & Construction'!K30","v":0},{"$f":"'A4-A5 -Transport & Construction'!L30","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"A5 - Construction",{"$f":"'A4-A5 -Transport & Construction'!I31","v":0},{"$f":"'A4-A5 -Transport & Construction'!J31","v":0},{"$f":"'A4-A5 -Transport & Construction'!K31","v":0},{"$f":"'A4-A5 -Transport & Construction'!L31","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"TOTAL Construction & Installation (A4-A5)",{"$f":"SUM(C35:C36)","v":0},{"$f":"SUM(D35:D36)","v":0},{"$f":"SUM(E35:E36)","v":0},{"$f":"SUM(F35:F36)","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"B1-B8 - Use "]
[null,"B1 - Use",{"$f":"'B1-B8 - Use'!I33","v":0},{"$f":"'B1-B8 - Use'!J33","v":0},{"$f":"'B1-B8 - Use'!K33","v":0},{"$f":"'B1-B8 - Use'!L33","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"B2 - Maintenance",{"$f":"'B1-B8 - Use'!I34","v":0},{"$f":"'B1-B8 - Use'!J34","v":0},{"$f":"'B1-B8 - Use'!K34","v":0},{"$f":"'B1-B8 - Use'!L34","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"B3 - Repair",{"$f":"'B1-B8 - Use'!I35","v":0},{"$f":"'B1-B8 - Use'!J35","v":0},{"$f":"'B1-B8 - Use'!K35","v":0},{"$f":"'B1-B8 - Use'!L35","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"B4 - Replacement",{"$f":"'B1-B8 - Use'!I36","v":0},{"$f":"'B1-B8 - Use'!J36","v":0},{"$f":"'B1-B8 - Use'!K36","v":0},{"$f":"'B1-B8 - Use'!L36","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"B5 - Refurbishment",{"$f":"'B1-B8 - Use'!I37","v":0},{"$f":"'B1-B8 - Use'!J37","v":0},{"$f":"'B1-B8 - Use'!K37","v":0},{"$f":"'B1-B8 - Use'!L37","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"B6 - Operational energy consumption",{"$f":"'B1-B8 - Use'!I38","v":0},{"$f":"'B1-B8 - Use'!J38","v":0},{"$f":"'B1-B8 - Use'!K38","v":0},{"$f":"'B1-B8 - Use'!L38","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"B7 - Operational water consumption",{"$f":"'B1-B8 - Use'!I39","v":0},{"$f":"'B1-B8 - Use'!J39","v":0},{"$f":"'B1-B8 - Use'!K39","v":0},{"$f":"'B1-B8 - Use'!L39","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"B8 - Operational activities not otherwise captured in modules B1-B7",{"$f":"'B1-B8 - Use'!I40","v":0},{"$f":"'B1-B8 - Use'!J40","v":0},{"$f":"'B1-B8 - Use'!K40","v":0},{"$f":"'B1-B8 - Use'!L40","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"TOTAL Use (B1-B8)",{"$f":"SUM(C39:C46)","v":0},{"$f":"SUM(D39:D46)","v":0},{"$f":"SUM(E39:E46)","v":0},{"$f":"SUM(F39:F46)","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"C1-C4 - End of Life "]
[null,"C1 - Deconstruction Demolition",{"$f":"'C1-C5 - End-of-Life'!J33","v":0},{"$f":"'C1-C5 - End-of-Life'!K33","v":0},{"$f":"'C1-C5 - End-of-Life'!L33","v":0},{"$f":"'C1-C5 - End-of-Life'!M33","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"C2 - Transport",{"$f":"'C1-C5 - End-of-Life'!J34","v":0},{"$f":"'C1-C5 - End-of-Life'!K34","v":0},{"$f":"'C1-C5 - End-of-Life'!L34","v":0},{"$f":"'C1-C5 - End-of-Life'!M34","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"C3-C4 - Waste processing, sorting for recycling & disposal",{"$f":"'C1-C5 - End-of-Life'!J35","v":0},{"$f":"'C1-C5 - End-of-Life'!K35","v":0},{"$f":"'C1-C5 - End-of-Life'!L35","v":0},{"$f":"'C1-C5 - End-of-Life'!M35","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"C5 - Relandscaping",{"$f":"'C1-C5 - End-of-Life'!J36","v":0},{"$f":"'C1-C5 - End-of-Life'!K36","v":0},{"$f":"'C1-C5 - End-of-Life'!L36","v":0},{"$f":"'C1-C5 - End-of-Life'!M36","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"TOTAL End-of-life (C1-C5)",{"$f":"SUM(C49:C52)","v":0},0,0,{"$f":"SUM(F49:F52)","v":0},{"$f":"IFERROR(Results_Lifecycle[[#This Row],[Total (tCO2e) ]]/Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"-\")","v":"-"}]
[null,"Total"]
[null,"Total Lifecycle Emissions (tCO2e)",{"$f":"SUBTOTAL(109,C27,C30:C32,C35:C36,C39:C46,C49:C51)","v":0},{"$f":"SUBTOTAL(109,D27,D30:D32,D35:D36,D39:D46,D49:D51)","v":0},{"$f":"SUBTOTAL(109,E27,E30:E32,E35:E36,E39:E46,E49:E51)","v":0},{"$f":"SUBTOTAL(109,F27,F30:F32,F35:F36,F39:F46,F49:F52)","v":0},"---------------------------"]
[]
[]
[null,"Reporting emissions and removals by Asset and Component "]
[]
[null,"Assets & sub-components","A0 emissions (kgCO2e)","A1-A3 emissions (kgCO2e)","A4 Emissions (kgCO2e)","A5 Emissions (kgCO2e)","B1-B8 Emissions (kgCO2e)","C1-C5 Emissions (kgCO2e)","Total Asset Emissions (kgCO2e)","% of Emissions by asset (green) and subasset (blue)"]
[null,"Wind turbine generators (WTG)"]
[null,"Nacelle and internals",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$61,Table_A0[Component],$B62)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$61,Table_A1_Module_A1A2[Component],$B62)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$61,Table_A1_Module_A3[Component],$B62)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$61,Table_A1_Module_A1A3[Component],$B62)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$61,Table_A4[Component],$B62)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$61,Table_A5_Fuel[Component],$B62)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$61,Table_A5_Waste[Component],$B62)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$61,Table_B1_Refrigerants[Component],$B62)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$61,Table_B2B5_Materials[Component],$B62)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$61,Table_B2B5_Energy[Component],$B62)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$61,Table_B2B5_Waste[Component],$B62)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$61,Table_B6[Component],$B62)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$61,Table_B7[Component],$B62)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$61,Table_B8[Component],$B62)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$61,Table_C1_Option_B[Component],$B62)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$61,Table_C2_Option_B[Component],$B62)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$61,Table_C3C4_Option_B[Component],$B62)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$61,Table_C5_Option_B[Component],$B62),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$61,Table_C1_Option_A[Component],$B62)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$61,Table_C2_Option_A[Component],$B62)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$61,Table_C3C4_Option_A[Component],$B62)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$61,Table_C5_Option_A[Component],$B62))","v":0},{"$f":"SUM(C62:H62)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Blades, hub, and rotor system",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$61,Table_A0[Component],$B63)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$61,Table_A1_Module_A1A2[Component],$B63)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$61,Table_A1_Module_A3[Component],$B63)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$61,Table_A1_Module_A1A3[Component],$B63)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$61,Table_A4[Component],$B63)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$61,Table_A5_Fuel[Component],$B63)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$61,Table_A5_Waste[Component],$B63)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$61,Table_B1_Refrigerants[Component],$B63)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$61,Table_B2B5_Materials[Component],$B63)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$61,Table_B2B5_Energy[Component],$B63)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$61,Table_B2B5_Waste[Component],$B63)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$61,Table_B6[Component],$B63)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$61,Table_B7[Component],$B63)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$61,Table_B8[Component],$B63)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$61,Table_C1_Option_B[Component],$B63)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$61,Table_C2_Option_B[Component],$B63)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$61,Table_C3C4_Option_B[Component],$B63)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$61,Table_C5_Option_B[Component],$B63),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$61,Table_C1_Option_A[Component],$B63)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$61,Table_C2_Option_A[Component],$B63)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$61,Table_C3C4_Option_A[Component],$B63)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$61,Table_C5_Option_A[Component],$B63))","v":0},{"$f":"SUM(C63:H63)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Tower",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$61,Table_A0[Component],$B64)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$61,Table_A1_Module_A1A2[Component],$B64)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$61,Table_A1_Module_A3[Component],$B64)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$61,Table_A1_Module_A1A3[Component],$B64)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$61,Table_A4[Component],$B64)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$61,Table_A5_Fuel[Component],$B64)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$61,Table_A5_Waste[Component],$B64)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$61,Table_B1_Refrigerants[Component],$B64)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$61,Table_B2B5_Materials[Component],$B64)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$61,Table_B2B5_Energy[Component],$B64)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$61,Table_B2B5_Waste[Component],$B64)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$61,Table_B6[Component],$B64)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$61,Table_B7[Component],$B64)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$61,Table_B8[Component],$B64)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$61,Table_C1_Option_B[Component],$B64)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$61,Table_C2_Option_B[Component],$B64)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$61,Table_C3C4_Option_B[Component],$B64)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$61,Table_C5_Option_B[Component],$B64),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$61,Table_C1_Option_A[Component],$B64)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$61,Table_C2_Option_A[Component],$B64)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$61,Table_C3C4_Option_A[Component],$B64)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$61,Table_C5_Option_A[Component],$B64))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Transformer",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$61,Table_A0[Component],$B65)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$61,Table_A1_Module_A1A2[Component],$B65)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$61,Table_A1_Module_A3[Component],$B65)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$61,Table_A1_Module_A1A3[Component],$B65)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$61,Table_A4[Component],$B65)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$61,Table_A5_Fuel[Component],$B65)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$61,Table_A5_Waste[Component],$B65)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$61,Table_B1_Refrigerants[Component],$B65)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$61,Table_B2B5_Materials[Component],$B65)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$61,Table_B2B5_Energy[Component],$B65)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$61,Table_B2B5_Waste[Component],$B65)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$61,Table_B6[Component],$B65)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$61,Table_B7[Component],$B65)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$61,Table_B8[Component],$B65)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$61,Table_C1_Option_B[Component],$B65)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$61,Table_C2_Option_B[Component],$B65)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$61,Table_C3C4_Option_B[Component],$B65)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$61,Table_C5_Option_B[Component],$B65),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$61,Table_C1_Option_A[Component],$B65)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$61,Table_C2_Option_A[Component],$B65)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$61,Table_C3C4_Option_A[Component],$B65)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$61,Table_C5_Option_A[Component],$B65))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$61,Table_A0[Component],$B66)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$61,Table_A1_Module_A1A2[Component],$B66)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$61,Table_A1_Module_A3[Component],$B66)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$61,Table_A1_Module_A1A3[Component],$B66)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$61,Table_A4[Component],$B66)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$61,Table_A5_Fuel[Component],$B66)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$61,Table_A5_Waste[Component],$B66)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$61,Table_B1_Refrigerants[Component],$B66)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$61,Table_B2B5_Materials[Component],$B66)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$61,Table_B2B5_Energy[Component],$B66)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$61,Table_B2B5_Waste[Component],$B66)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$61,Table_B6[Component],$B66)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$61,Table_B7[Component],$B66)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$61,Table_B8[Component],$B66)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$61,Table_C1_Option_B[Component],$B66)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$61,Table_C2_Option_B[Component],$B66)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$61,Table_C3C4_Option_B[Component],$B66)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$61,Table_C5_Option_B[Component],$B66),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$61,Table_C1_Option_A[Component],$B66)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$61,Table_C2_Option_A[Component],$B66)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$61,Table_C3C4_Option_A[Component],$B66)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$61,Table_C5_Option_A[Component],$B66))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Wind turbine generators)",{"$f":"SUM(C62:C66)","v":0},{"$f":"SUM(D62:D66)","v":0},{"$f":"SUM(E62:E66)","v":0},{"$f":"SUM(F62:F66)","v":0},0,0,{"$f":"SUM(C67:H67)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Fixed foundations"]
[null,"Monopile",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$68,Table_A0[Component],$B69)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$68,Table_A1_Module_A1A2[Component],B69)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$68,Table_A1_Module_A3[Component],B69)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$68,Table_A1_Module_A1A3[Component],B69)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$68,Table_A4[Component],$B69)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$68,Table_A5_Fuel[Component],$B69)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$68,Table_A5_Waste[Component],$B69)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$68,Table_B1_Refrigerants[Component],$B69)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$68,Table_B2B5_Materials[Component],$B69)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$68,Table_B2B5_Energy[Component],$B69)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$68,Table_B2B5_Waste[Component],$B69)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$68,Table_B6[Component],$B69)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$68,Table_B7[Component],$B69)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$68,Table_B8[Component],$B69)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$68,Table_C1_Option_B[Component],$B69)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$68,Table_C2_Option_B[Component],$B69)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$68,Table_C3C4_Option_B[Component],$B69)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$68,Table_C5_Option_B[Component],$B69),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$68,Table_C1_Option_A[Component],$B69)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$68,Table_C2_Option_A[Component],$B69)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$68,Table_C3C4_Option_A[Component],$B69)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$68,Table_C5_Option_A[Component],$B69))","v":0},{"$f":"SUM(C69:H69)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Jacket",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$68,Table_A0[Component],$B70)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$68,Table_A1_Module_A1A2[Component],B70)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$68,Table_A1_Module_A3[Component],B70)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$68,Table_A1_Module_A1A3[Component],B70)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$68,Table_A4[Component],$B70)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$68,Table_A5_Fuel[Component],$B70)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$68,Table_A5_Waste[Component],$B70)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$68,Table_B1_Refrigerants[Component],$B70)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$68,Table_B2B5_Materials[Component],$B70)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$68,Table_B2B5_Energy[Component],$B70)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$68,Table_B2B5_Waste[Component],$B70)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$68,Table_B6[Component],$B70)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$68,Table_B7[Component],$B70)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$68,Table_B8[Component],$B70)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$68,Table_C1_Option_B[Component],$B70)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$68,Table_C2_Option_B[Component],$B70)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$68,Table_C3C4_Option_B[Component],$B70)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$68,Table_C5_Option_B[Component],$B70),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$68,Table_C1_Option_A[Component],$B70)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$68,Table_C2_Option_A[Component],$B70)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$68,Table_C3C4_Option_A[Component],$B70)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$68,Table_C5_Option_A[Component],$B70))","v":0},{"$f":"SUM(C70:H70)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Transition piece",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$68,Table_A0[Component],$B71)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$68,Table_A1_Module_A1A2[Component],B71)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$68,Table_A1_Module_A3[Component],B71)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$68,Table_A1_Module_A1A3[Component],B71)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$68,Table_A4[Component],$B71)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$68,Table_A5_Fuel[Component],$B71)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$68,Table_A5_Waste[Component],$B71)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$68,Table_B1_Refrigerants[Component],$B71)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$68,Table_B2B5_Materials[Component],$B71)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$68,Table_B2B5_Energy[Component],$B71)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$68,Table_B2B5_Waste[Component],$B71)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$68,Table_B6[Component],$B71)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$68,Table_B7[Component],$B71)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$68,Table_B8[Component],$B71)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$68,Table_C1_Option_B[Component],$B71)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$68,Table_C2_Option_B[Component],$B71)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$68,Table_C3C4_Option_B[Component],$B71)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$68,Table_C5_Option_B[Component],$B71),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$68,Table_C1_Option_A[Component],$B71)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$68,Table_C2_Option_A[Component],$B71)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$68,Table_C3C4_Option_A[Component],$B71)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$68,Table_C5_Option_A[Component],$B71))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other fixed foundation technologies",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$68,Table_A0[Component],$B72)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$68,Table_A1_Module_A1A2[Component],B72)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$68,Table_A1_Module_A3[Component],B72)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$68,Table_A1_Module_A1A3[Component],B72)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$68,Table_A4[Component],$B72)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$68,Table_A5_Fuel[Component],$B72)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$68,Table_A5_Waste[Component],$B72)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$68,Table_B1_Refrigerants[Component],$B72)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$68,Table_B2B5_Materials[Component],$B72)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$68,Table_B2B5_Energy[Component],$B72)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$68,Table_B2B5_Waste[Component],$B72)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$68,Table_B6[Component],$B72)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$68,Table_B7[Component],$B72)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$68,Table_B8[Component],$B72)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$68,Table_C1_Option_B[Component],$B72)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$68,Table_C2_Option_B[Component],$B72)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$68,Table_C3C4_Option_B[Component],$B72)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$68,Table_C5_Option_B[Component],$B72),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$68,Table_C1_Option_A[Component],$B72)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$68,Table_C2_Option_A[Component],$B72)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$68,Table_C3C4_Option_A[Component],$B72)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$68,Table_C5_Option_A[Component],$B72))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$68,Table_A0[Component],$B73)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$68,Table_A1_Module_A1A2[Component],B73)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$68,Table_A1_Module_A3[Component],B73)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$68,Table_A1_Module_A1A3[Component],B73)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$68,Table_A4[Component],$B73)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$68,Table_A5_Fuel[Component],$B73)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$68,Table_A5_Waste[Component],$B73)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$68,Table_B1_Refrigerants[Component],$B73)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$68,Table_B2B5_Materials[Component],$B73)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$68,Table_B2B5_Energy[Component],$B73)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$68,Table_B2B5_Waste[Component],$B73)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$68,Table_B6[Component],$B73)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$68,Table_B7[Component],$B73)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$68,Table_B8[Component],$B73)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$68,Table_C1_Option_B[Component],$B73)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$68,Table_C2_Option_B[Component],$B73)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$68,Table_C3C4_Option_B[Component],$B73)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$68,Table_C5_Option_B[Component],$B73),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$68,Table_C1_Option_A[Component],$B73)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$68,Table_C2_Option_A[Component],$B73)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$68,Table_C3C4_Option_A[Component],$B73)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$68,Table_C5_Option_A[Component],$B73))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Fixed foundations)",{"$f":"SUM(C69:C73)","v":0},0,0,0,0,0,{"$f":"SUM(C74:H74)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Floating foundations"]
[null,"Platform",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$75,Table_A0[Component],$B76)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$75,Table_A1_Module_A1A2[Component],B76)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$75,Table_A1_Module_A3[Component],B76)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$75,Table_A1_Module_A1A3[Component],B76)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$75,Table_A4[Component],$B76)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$75,Table_A5_Fuel[Component],$B76)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$75,Table_A5_Waste[Component],$B76)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$75,Table_B1_Refrigerants[Component],$B76)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$75,Table_B2B5_Materials[Component],$B76)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$75,Table_B2B5_Energy[Component],$B76)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$75,Table_B2B5_Waste[Component],$B76)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$75,Table_B6[Component],$B76)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$75,Table_B7[Component],$B76)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$75,Table_B8[Component],$B76)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$75,Table_C1_Option_B[Component],$B76)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$75,Table_C2_Option_B[Component],$B76)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$75,Table_C3C4_Option_B[Component],$B76)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$75,Table_C5_Option_B[Component],$B76),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$75,Table_C1_Option_A[Component],$B76)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$75,Table_C2_Option_A[Component],$B76)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$75,Table_C3C4_Option_A[Component],$B76)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$75,Table_C5_Option_A[Component],$B76))","v":0},{"$f":"SUM(C76:H76)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Mooring",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$75,Table_A0[Component],$B77)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$75,Table_A1_Module_A1A2[Component],B77)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$75,Table_A1_Module_A3[Component],B77)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$75,Table_A1_Module_A1A3[Component],B77)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$75,Table_A4[Component],$B77)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$75,Table_A5_Fuel[Component],$B77)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$75,Table_A5_Waste[Component],$B77)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$75,Table_B1_Refrigerants[Component],$B77)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$75,Table_B2B5_Materials[Component],$B77)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$75,Table_B2B5_Energy[Component],$B77)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$75,Table_B2B5_Waste[Component],$B77)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$75,Table_B6[Component],$B77)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$75,Table_B7[Component],$B77)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$75,Table_B8[Component],$B77)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$75,Table_C1_Option_B[Component],$B77)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$75,Table_C2_Option_B[Component],$B77)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$75,Table_C3C4_Option_B[Component],$B77)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$75,Table_C5_Option_B[Component],$B77),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$75,Table_C1_Option_A[Component],$B77)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$75,Table_C2_Option_A[Component],$B77)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$75,Table_C3C4_Option_A[Component],$B77)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$75,Table_C5_Option_A[Component],$B77))","v":0},{"$f":"SUM(C77:H77)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Anchor",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$75,Table_A0[Component],$B78)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$75,Table_A1_Module_A1A2[Component],B78)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$75,Table_A1_Module_A3[Component],B78)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$75,Table_A1_Module_A1A3[Component],B78)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$75,Table_A4[Component],$B78)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$75,Table_A5_Fuel[Component],$B78)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$75,Table_A5_Waste[Component],$B78)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$75,Table_B1_Refrigerants[Component],$B78)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$75,Table_B2B5_Materials[Component],$B78)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$75,Table_B2B5_Energy[Component],$B78)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$75,Table_B2B5_Waste[Component],$B78)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$75,Table_B6[Component],$B78)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$75,Table_B7[Component],$B78)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$75,Table_B8[Component],$B78)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$75,Table_C1_Option_B[Component],$B78)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$75,Table_C2_Option_B[Component],$B78)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$75,Table_C3C4_Option_B[Component],$B78)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$75,Table_C5_Option_B[Component],$B78),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$75,Table_C1_Option_A[Component],$B78)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$75,Table_C2_Option_A[Component],$B78)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$75,Table_C3C4_Option_A[Component],$B78)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$75,Table_C5_Option_A[Component],$B78))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other floating foundation technologies",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$87,Table_A0[Component],$B79)","v":0},null,null,null,{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$75,Table_B1_Refrigerants[Component],$B79)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$75,Table_B2B5_Materials[Component],$B79)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$75,Table_B2B5_Energy[Component],$B79)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$75,Table_B2B5_Waste[Component],$B79)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$75,Table_B6[Component],$B79)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$75,Table_B7[Component],$B79)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$75,Table_B8[Component],$B79)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$75,Table_C1_Option_B[Component],$B79)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$75,Table_C2_Option_B[Component],$B79)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$75,Table_C3C4_Option_B[Component],$B79)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$75,Table_C5_Option_B[Component],$B79),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$75,Table_C1_Option_A[Component],$B79)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$75,Table_C2_Option_A[Component],$B79)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$75,Table_C3C4_Option_A[Component],$B79)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$75,Table_C5_Option_A[Component],$B79))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$75,Table_A0[Component],$B80)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$75,Table_A1_Module_A1A2[Component],B80)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$75,Table_A1_Module_A3[Component],B80)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$75,Table_A1_Module_A1A3[Component],B80)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$75,Table_A4[Component],$B80)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$75,Table_A5_Fuel[Component],$B80)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$75,Table_A5_Waste[Component],$B80)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$75,Table_B1_Refrigerants[Component],$B80)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$75,Table_B2B5_Materials[Component],$B80)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$75,Table_B2B5_Energy[Component],$B80)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$75,Table_B2B5_Waste[Component],$B80)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$75,Table_B6[Component],$B80)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$75,Table_B7[Component],$B80)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$75,Table_B8[Component],$B80)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$75,Table_C1_Option_B[Component],$B80)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$75,Table_C2_Option_B[Component],$B80)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$75,Table_C3C4_Option_B[Component],$B80)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$75,Table_C5_Option_B[Component],$B80),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$75,Table_C1_Option_A[Component],$B80)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$75,Table_C2_Option_A[Component],$B80)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$75,Table_C3C4_Option_A[Component],$B80)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$75,Table_C5_Option_A[Component],$B80))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Floating foundations)",{"$f":"SUM(C76:C80)","v":0},{"$f":"SUM(D76:D80)","v":0},{"$f":"SUM(E76:E78)","v":0},{"$f":"SUM(F76:F78)","v":0},{"$f":"SUM(G76:G78)","v":0},{"$f":"SUM(H76:H78)","v":0},{"$f":"SUM(C81:H81)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Cables"]
[null,"Inter array cables",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$82,Table_A0[Component],$B83)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$82,Table_A1_Module_A1A2[Component],B83)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$82,Table_A1_Module_A3[Component],B83)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$82,Table_A1_Module_A1A3[Component],B83)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$82,Table_A4[Component],$B83)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$82,Table_A5_Fuel[Component],$B83)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$82,Table_A5_Waste[Component],$B83)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$82,Table_B1_Refrigerants[Component],$B83)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$82,Table_B2B5_Materials[Component],$B83)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$82,Table_B2B5_Energy[Component],$B83)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$82,Table_B2B5_Waste[Component],$B83)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$82,Table_B6[Component],$B83)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$82,Table_B7[Component],$B83)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$82,Table_B8[Component],$B83)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$82,Table_C1_Option_B[Component],$B83)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$82,Table_C2_Option_B[Component],$B83)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$82,Table_C3C4_Option_B[Component],$B83)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$82,Table_C5_Option_B[Component],$B83),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$82,Table_C1_Option_A[Component],$B83)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$82,Table_C2_Option_A[Component],$B83)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$82,Table_C3C4_Option_A[Component],$B83)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$82,Table_C5_Option_A[Component],$B83))","v":0},{"$f":"SUM(C83:H83)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Export cables",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$82,Table_A0[Component],$B84)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$82,Table_A1_Module_A1A2[Component],B84)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$82,Table_A1_Module_A3[Component],B84)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$82,Table_A1_Module_A1A3[Component],B84)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$82,Table_A4[Component],$B84)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$82,Table_A5_Fuel[Component],$B84)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$82,Table_A5_Waste[Component],$B84)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$82,Table_B1_Refrigerants[Component],$B84)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$82,Table_B2B5_Materials[Component],$B84)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$82,Table_B2B5_Energy[Component],$B84)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$82,Table_B2B5_Waste[Component],$B84)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$82,Table_B6[Component],$B84)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$82,Table_B7[Component],$B84)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$82,Table_B8[Component],$B84)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$82,Table_C1_Option_B[Component],$B84)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$82,Table_C2_Option_B[Component],$B84)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$82,Table_C3C4_Option_B[Component],$B84)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$82,Table_C5_Option_B[Component],$B84),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$82,Table_C1_Option_A[Component],$B84)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$82,Table_C2_Option_A[Component],$B84)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$82,Table_C3C4_Option_A[Component],$B84)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$82,Table_C5_Option_A[Component],$B84))","v":0},{"$f":"SUM(C84:H84)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$82,Table_A0[Component],$B85)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$82,Table_A1_Module_A1A2[Component],B85)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$82,Table_A1_Module_A3[Component],B85)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$82,Table_A1_Module_A1A3[Component],B85)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$82,Table_A4[Component],$B85)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$82,Table_A5_Fuel[Component],$B85)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$82,Table_A5_Waste[Component],$B85)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$82,Table_B1_Refrigerants[Component],$B85)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$82,Table_B2B5_Materials[Component],$B85)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$82,Table_B2B5_Energy[Component],$B85)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$82,Table_B2B5_Waste[Component],$B85)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$82,Table_B6[Component],$B85)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$82,Table_B7[Component],$B85)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$82,Table_B8[Component],$B85)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$82,Table_C1_Option_B[Component],$B85)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$82,Table_C2_Option_B[Component],$B85)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$82,Table_C3C4_Option_B[Component],$B85)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$82,Table_C5_Option_B[Component],$B85),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$82,Table_C1_Option_A[Component],$B85)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$82,Table_C2_Option_A[Component],$B85)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$82,Table_C3C4_Option_A[Component],$B85)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$82,Table_C5_Option_A[Component],$B85))","v":0},{"$f":"SUM(C85:H85)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Cables)",{"$f":"SUM(C83:C85)","v":0},{"$f":"SUM(D83:D85)","v":0},{"$f":"SUM(E83:E85)","v":0},{"$f":"SUM(F83:F85)","v":0},0,0,{"$f":"SUM(C86:H86)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Offshore substation"]
[null,"Transformers",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$87,Table_A0[Component],$B88)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$87,Table_A1_Module_A1A2[Component],B88)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$87,Table_A1_Module_A3[Component],B88)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$87,Table_A1_Module_A1A3[Component],B88)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$87,Table_A4[Component],$B88)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$87,Table_A5_Fuel[Component],$B88)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$87,Table_A5_Waste[Component],$B88)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$87,Table_B1_Refrigerants[Component],$B88)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$87,Table_B2B5_Materials[Component],$B88)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$87,Table_B2B5_Energy[Component],$B88)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$87,Table_B2B5_Waste[Component],$B88)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$87,Table_B6[Component],$B88)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$87,Table_B7[Component],$B88)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$87,Table_B8[Component],$B88)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$87,Table_C1_Option_B[Component],$B88)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$87,Table_C2_Option_B[Component],$B88)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$87,Table_C3C4_Option_B[Component],$B88)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$87,Table_C5_Option_B[Component],$B88),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$87,Table_C1_Option_A[Component],$B88)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$87,Table_C2_Option_A[Component],$B88)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$87,Table_C3C4_Option_A[Component],$B88)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$87,Table_C5_Option_A[Component],$B88))","v":0},{"$f":"SUM(C88:H88)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Switchgear",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$87,Table_A0[Component],$B89)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$87,Table_A1_Module_A1A2[Component],B89)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$87,Table_A1_Module_A3[Component],B89)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$87,Table_A1_Module_A1A3[Component],B89)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$87,Table_A4[Component],$B89)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$87,Table_A5_Fuel[Component],$B89)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$87,Table_A5_Waste[Component],$B89)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$87,Table_B1_Refrigerants[Component],$B89)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$87,Table_B2B5_Materials[Component],$B89)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$87,Table_B2B5_Energy[Component],$B89)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$87,Table_B2B5_Waste[Component],$B89)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$87,Table_B6[Component],$B89)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$87,Table_B7[Component],$B89)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$87,Table_B8[Component],$B89)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$87,Table_C1_Option_B[Component],$B89)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$87,Table_C2_Option_B[Component],$B89)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$87,Table_C3C4_Option_B[Component],$B89)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$87,Table_C5_Option_B[Component],$B89),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$87,Table_C1_Option_A[Component],$B89)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$87,Table_C2_Option_A[Component],$B89)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$87,Table_C3C4_Option_A[Component],$B89)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$87,Table_C5_Option_A[Component],$B89))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Facilities",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$87,Table_A0[Component],$B90)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$87,Table_A1_Module_A1A2[Component],B90)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$87,Table_A1_Module_A3[Component],B90)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$87,Table_A1_Module_A1A3[Component],B90)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$87,Table_A4[Component],$B90)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$87,Table_A5_Fuel[Component],$B90)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$87,Table_A5_Waste[Component],$B90)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$87,Table_B1_Refrigerants[Component],$B90)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$87,Table_B2B5_Materials[Component],$B90)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$87,Table_B2B5_Energy[Component],$B90)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$87,Table_B2B5_Waste[Component],$B90)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$87,Table_B6[Component],$B90)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$87,Table_B7[Component],$B90)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$87,Table_B8[Component],$B90)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$87,Table_C1_Option_B[Component],$B90)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$87,Table_C2_Option_B[Component],$B90)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$87,Table_C3C4_Option_B[Component],$B90)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$87,Table_C5_Option_B[Component],$B90),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$87,Table_C1_Option_A[Component],$B90)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$87,Table_C2_Option_A[Component],$B90)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$87,Table_C3C4_Option_A[Component],$B90)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$87,Table_C5_Option_A[Component],$B90))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Structure",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$87,Table_A0[Component],$B91)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$87,Table_A1_Module_A1A2[Component],B91)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$87,Table_A1_Module_A3[Component],B91)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$87,Table_A1_Module_A1A3[Component],B91)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$87,Table_A4[Component],$B91)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$87,Table_A5_Fuel[Component],$B91)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$87,Table_A5_Waste[Component],$B91)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$87,Table_B1_Refrigerants[Component],$B91)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$87,Table_B2B5_Materials[Component],$B91)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$87,Table_B2B5_Energy[Component],$B91)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$87,Table_B2B5_Waste[Component],$B91)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$87,Table_B6[Component],$B91)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$87,Table_B7[Component],$B91)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$87,Table_B8[Component],$B91)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$87,Table_C1_Option_B[Component],$B91)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$87,Table_C2_Option_B[Component],$B91)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$87,Table_C3C4_Option_B[Component],$B91)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$87,Table_C5_Option_B[Component],$B91),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$87,Table_C1_Option_A[Component],$B91)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$87,Table_C2_Option_A[Component],$B91)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$87,Table_C3C4_Option_A[Component],$B91)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$87,Table_C5_Option_A[Component],$B91))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$87,Table_A0[Component],$B92)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$87,Table_A1_Module_A1A2[Component],B92)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$87,Table_A1_Module_A3[Component],B92)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$87,Table_A1_Module_A1A3[Component],B92)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$87,Table_A4[Component],$B92)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$87,Table_A5_Fuel[Component],$B92)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$87,Table_A5_Waste[Component],$B92)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$87,Table_B1_Refrigerants[Component],$B92)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$87,Table_B2B5_Materials[Component],$B92)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$87,Table_B2B5_Energy[Component],$B92)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$87,Table_B2B5_Waste[Component],$B92)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$87,Table_B6[Component],$B92)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$87,Table_B7[Component],$B92)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$87,Table_B8[Component],$B92)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$87,Table_C1_Option_B[Component],$B92)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$87,Table_C2_Option_B[Component],$B92)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$87,Table_C3C4_Option_B[Component],$B92)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$87,Table_C5_Option_B[Component],$B92),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$87,Table_C1_Option_A[Component],$B92)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$87,Table_C2_Option_A[Component],$B92)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$87,Table_C3C4_Option_A[Component],$B92)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$87,Table_C5_Option_A[Component],$B92))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Offshore substation)",{"$f":"SUM(C88:C92)","v":0},{"$f":"SUM(D88:D92)","v":0},0,0,0,0,0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Onshore substation"]
[null,"Transformers",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$94,Table_A0[Component],$B95)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$94,Table_A1_Module_A1A2[Component],B95)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$94,Table_A1_Module_A3[Component],B95)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$94,Table_A1_Module_A1A3[Component],B95)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$94,Table_A4[Component],$B95)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$94,Table_A5_Fuel[Component],$B95)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$94,Table_A5_Waste[Component],$B95)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$94,Table_B1_Refrigerants[Component],$B95)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$94,Table_B2B5_Materials[Component],$B95)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$94,Table_B2B5_Energy[Component],$B95)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$94,Table_B2B5_Waste[Component],$B95)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$94,Table_B6[Component],$B95)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$94,Table_B7[Component],$B95)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$94,Table_B8[Component],$B95)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$94,Table_C1_Option_B[Component],$B95)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$94,Table_C2_Option_B[Component],$B95)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$94,Table_C3C4_Option_B[Component],$B95)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$94,Table_C5_Option_B[Component],$B95),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$94,Table_C1_Option_A[Component],$B95)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$94,Table_C2_Option_A[Component],$B95)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$94,Table_C3C4_Option_A[Component],$B95)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$94,Table_C5_Option_A[Component],$B95))","v":0},{"$f":"SUM(C95:H95)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Switchgear",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$94,Table_A0[Component],$B96)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$94,Table_A1_Module_A1A2[Component],B96)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$94,Table_A1_Module_A3[Component],B96)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$94,Table_A1_Module_A1A3[Component],B96)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$94,Table_A4[Component],$B96)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$94,Table_A5_Fuel[Component],$B96)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$94,Table_A5_Waste[Component],$B96)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$94,Table_B1_Refrigerants[Component],$B96)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$94,Table_B2B5_Materials[Component],$B96)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$94,Table_B2B5_Energy[Component],$B96)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$94,Table_B2B5_Waste[Component],$B96)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$94,Table_B6[Component],$B96)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$94,Table_B7[Component],$B96)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$94,Table_B8[Component],$B96)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$94,Table_C1_Option_B[Component],$B96)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$94,Table_C2_Option_B[Component],$B96)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$94,Table_C3C4_Option_B[Component],$B96)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$94,Table_C5_Option_B[Component],$B96),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$94,Table_C1_Option_A[Component],$B96)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$94,Table_C2_Option_A[Component],$B96)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$94,Table_C3C4_Option_A[Component],$B96)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$94,Table_C5_Option_A[Component],$B96))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Facilities",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$94,Table_A0[Component],$B97)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$94,Table_A1_Module_A1A2[Component],B97)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$94,Table_A1_Module_A3[Component],B97)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$94,Table_A1_Module_A1A3[Component],B97)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$94,Table_A4[Component],$B97)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$94,Table_A5_Fuel[Component],$B97)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$94,Table_A5_Waste[Component],$B97)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$94,Table_B1_Refrigerants[Component],$B97)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$94,Table_B2B5_Materials[Component],$B97)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$94,Table_B2B5_Energy[Component],$B97)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$94,Table_B2B5_Waste[Component],$B97)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$94,Table_B6[Component],$B97)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$94,Table_B7[Component],$B97)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$94,Table_B8[Component],$B97)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$94,Table_C1_Option_B[Component],$B97)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$94,Table_C2_Option_B[Component],$B97)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$94,Table_C3C4_Option_B[Component],$B97)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$94,Table_C5_Option_B[Component],$B97),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$94,Table_C1_Option_A[Component],$B97)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$94,Table_C2_Option_A[Component],$B97)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$94,Table_C3C4_Option_A[Component],$B97)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$94,Table_C5_Option_A[Component],$B97))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Structure",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$94,Table_A0[Component],$B98)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$94,Table_A1_Module_A1A2[Component],B98)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$94,Table_A1_Module_A3[Component],B98)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$94,Table_A1_Module_A1A3[Component],B98)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$94,Table_A4[Component],$B98)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$94,Table_A5_Fuel[Component],$B98)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$94,Table_A5_Waste[Component],$B98)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$94,Table_B1_Refrigerants[Component],$B98)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$94,Table_B2B5_Materials[Component],$B98)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$94,Table_B2B5_Energy[Component],$B98)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$94,Table_B2B5_Waste[Component],$B98)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$94,Table_B6[Component],$B98)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$94,Table_B7[Component],$B98)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$94,Table_B8[Component],$B98)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$94,Table_C1_Option_B[Component],$B98)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$94,Table_C2_Option_B[Component],$B98)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$94,Table_C3C4_Option_B[Component],$B98)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$94,Table_C5_Option_B[Component],$B98),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$94,Table_C1_Option_A[Component],$B98)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$94,Table_C2_Option_A[Component],$B98)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$94,Table_C3C4_Option_A[Component],$B98)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$94,Table_C5_Option_A[Component],$B98))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$94,Table_A0[Component],$B99)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$94,Table_A1_Module_A1A2[Component],B99)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$94,Table_A1_Module_A3[Component],B99)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$94,Table_A1_Module_A1A3[Component],B99)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$94,Table_A4[Component],$B99)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$94,Table_A5_Fuel[Component],$B99)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$94,Table_A5_Waste[Component],$B99)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$94,Table_B1_Refrigerants[Component],$B99)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$94,Table_B2B5_Materials[Component],$B99)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$94,Table_B2B5_Energy[Component],$B99)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$94,Table_B2B5_Waste[Component],$B99)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$94,Table_B6[Component],$B99)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$94,Table_B7[Component],$B99)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$94,Table_B8[Component],$B99)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$94,Table_C1_Option_B[Component],$B99)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$94,Table_C2_Option_B[Component],$B99)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$94,Table_C3C4_Option_B[Component],$B99)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$94,Table_C5_Option_B[Component],$B99),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$94,Table_C1_Option_A[Component],$B99)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$94,Table_C2_Option_A[Component],$B99)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$94,Table_C3C4_Option_A[Component],$B99)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$94,Table_C5_Option_A[Component],$B99))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Onshore substation)",{"$f":"SUM(C95:C99)","v":0},0,0,0,0,0,0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Operations base"]
[null,"Site buildings",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$101,Table_A0[Component],$B102)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$101,Table_A1_Module_A1A2[Component],B102)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$101,Table_A1_Module_A3[Component],B102)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$101,Table_A1_Module_A1A3[Component],B102)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$101,Table_A4[Component],$B102)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$101,Table_A5_Fuel[Component],$B102)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$101,Table_A5_Waste[Component],$B102)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$101,Table_B1_Refrigerants[Component],$B102)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$101,Table_B2B5_Materials[Component],$B102)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$101,Table_B2B5_Energy[Component],$B102)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$101,Table_B2B5_Waste[Component],$B102)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$101,Table_B6[Component],$B102)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$101,Table_B7[Component],$B102)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$101,Table_B8[Component],$B102)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$101,Table_C1_Option_B[Component],$B102)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$101,Table_C2_Option_B[Component],$B102)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$101,Table_C3C4_Option_B[Component],$B102)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$101,Table_C5_Option_B[Component],$B102),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$101,Table_C1_Option_A[Component],$B102)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$101,Table_C2_Option_A[Component],$B102)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$101,Table_C3C4_Option_A[Component],$B102)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$101,Table_C5_Option_A[Component],$B102))","v":0},{"$f":"SUM(C102:H102)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Roads",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$101,Table_A0[Component],$B103)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$101,Table_A1_Module_A1A2[Component],B103)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$101,Table_A1_Module_A3[Component],B103)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$101,Table_A1_Module_A1A3[Component],B103)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$101,Table_A4[Component],$B103)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$101,Table_A5_Fuel[Component],$B103)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$101,Table_A5_Waste[Component],$B103)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$101,Table_B1_Refrigerants[Component],$B103)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$101,Table_B2B5_Materials[Component],$B103)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$101,Table_B2B5_Energy[Component],$B103)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$101,Table_B2B5_Waste[Component],$B103)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$101,Table_B6[Component],$B103)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$101,Table_B7[Component],$B103)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$101,Table_B8[Component],$B103)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$101,Table_C1_Option_B[Component],$B103)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$101,Table_C2_Option_B[Component],$B103)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$101,Table_C3C4_Option_B[Component],$B103)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$101,Table_C5_Option_B[Component],$B103),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$101,Table_C1_Option_A[Component],$B103)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$101,Table_C2_Option_A[Component],$B103)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$101,Table_C3C4_Option_A[Component],$B103)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$101,Table_C5_Option_A[Component],$B103))","v":0},{"$f":"SUM(C103:H103)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Vessel berths",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$101,Table_A0[Component],$B104)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$101,Table_A1_Module_A1A2[Component],B104)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$101,Table_A1_Module_A3[Component],B104)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$101,Table_A1_Module_A1A3[Component],B104)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$101,Table_A4[Component],$B104)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$101,Table_A5_Fuel[Component],$B104)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$101,Table_A5_Waste[Component],$B104)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$101,Table_B1_Refrigerants[Component],$B104)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$101,Table_B2B5_Materials[Component],$B104)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$101,Table_B2B5_Energy[Component],$B104)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$101,Table_B2B5_Waste[Component],$B104)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$101,Table_B6[Component],$B104)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$101,Table_B7[Component],$B104)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$101,Table_B8[Component],$B104)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$101,Table_C1_Option_B[Component],$B104)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$101,Table_C2_Option_B[Component],$B104)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$101,Table_C3C4_Option_B[Component],$B104)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$101,Table_C5_Option_B[Component],$B104),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$101,Table_C1_Option_A[Component],$B104)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$101,Table_C2_Option_A[Component],$B104)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$101,Table_C3C4_Option_A[Component],$B104)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$101,Table_C5_Option_A[Component],$B104))","v":0},{"$f":"SUM(C104:H104)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$101,Table_A0[Component],$B105)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$101,Table_A1_Module_A1A2[Component],B105)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$101,Table_A1_Module_A3[Component],B105)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$101,Table_A1_Module_A1A3[Component],B105)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$101,Table_A4[Component],$B105)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$101,Table_A5_Fuel[Component],$B105)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$101,Table_A5_Waste[Component],$B105)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$101,Table_B1_Refrigerants[Component],$B105)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$101,Table_B2B5_Materials[Component],$B105)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$101,Table_B2B5_Energy[Component],$B105)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$101,Table_B2B5_Waste[Component],$B105)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$101,Table_B6[Component],$B105)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$101,Table_B7[Component],$B105)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$101,Table_B8[Component],$B105)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$101,Table_C1_Option_B[Component],$B105)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$101,Table_C2_Option_B[Component],$B105)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$101,Table_C3C4_Option_B[Component],$B105)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$101,Table_C5_Option_B[Component],$B105),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$101,Table_C1_Option_A[Component],$B105)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$101,Table_C2_Option_A[Component],$B105)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$101,Table_C3C4_Option_A[Component],$B105)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$101,Table_C5_Option_A[Component],$B105))","v":0},{"$f":"SUM(C105:H105)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Operations base)",{"$f":"SUM(C102:C105)","v":0},0,0,0,0,0,{"$f":"SUM(C106:H106)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Construction and installation assets"]
[null,"Turbine Installation vessel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$107,Table_A0[Component],$B108)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$107,Table_A1_Module_A1A2[Component],B108)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$107,Table_A1_Module_A3[Component],B108)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$107,Table_A1_Module_A1A3[Component],B108)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$107,Table_A4[Component],$B108)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$107,Table_A5_Fuel[Component],$B108)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$107,Table_A5_Waste[Component],$B108)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$107,Table_B1_Refrigerants[Component],$B108)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$107,Table_B2B5_Materials[Component],$B108)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$107,Table_B2B5_Energy[Component],$B108)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$107,Table_B2B5_Waste[Component],$B108)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$107,Table_B6[Component],$B108)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$107,Table_B7[Component],$B108)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$107,Table_B8[Component],$B108)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$107,Table_C1_Option_B[Component],$B108)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$107,Table_C2_Option_B[Component],$B108)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$107,Table_C3C4_Option_B[Component],$B108)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$107,Table_C5_Option_B[Component],$B108),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$107,Table_C1_Option_A[Component],$B108)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$107,Table_C2_Option_A[Component],$B108)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$107,Table_C3C4_Option_A[Component],$B108)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$107,Table_C5_Option_A[Component],$B108))","v":0},{"$f":"SUM(C108:H108)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Foundation installation vessel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$107,Table_A0[Component],$B109)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$107,Table_A1_Module_A1A2[Component],B109)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$107,Table_A1_Module_A3[Component],B109)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$107,Table_A1_Module_A1A3[Component],B109)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$107,Table_A4[Component],$B109)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$107,Table_A5_Fuel[Component],$B109)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$107,Table_A5_Waste[Component],$B109)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$107,Table_B1_Refrigerants[Component],$B109)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$107,Table_B2B5_Materials[Component],$B109)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$107,Table_B2B5_Energy[Component],$B109)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$107,Table_B2B5_Waste[Component],$B109)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$107,Table_B6[Component],$B109)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$107,Table_B7[Component],$B109)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$107,Table_B8[Component],$B109)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$107,Table_C1_Option_B[Component],$B109)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$107,Table_C2_Option_B[Component],$B109)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$107,Table_C3C4_Option_B[Component],$B109)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$107,Table_C5_Option_B[Component],$B109),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$107,Table_C1_Option_A[Component],$B109)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$107,Table_C2_Option_A[Component],$B109)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$107,Table_C3C4_Option_A[Component],$B109)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$107,Table_C5_Option_A[Component],$B109))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Substation installation vessel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$107,Table_A0[Component],$B110)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$107,Table_A1_Module_A1A2[Component],B110)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$107,Table_A1_Module_A3[Component],B110)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$107,Table_A1_Module_A1A3[Component],B110)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$107,Table_A4[Component],$B110)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$107,Table_A5_Fuel[Component],$B110)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$107,Table_A5_Waste[Component],$B110)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$107,Table_B1_Refrigerants[Component],$B110)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$107,Table_B2B5_Materials[Component],$B110)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$107,Table_B2B5_Energy[Component],$B110)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$107,Table_B2B5_Waste[Component],$B110)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$107,Table_B6[Component],$B110)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$107,Table_B7[Component],$B110)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$107,Table_B8[Component],$B110)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$107,Table_C1_Option_B[Component],$B110)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$107,Table_C2_Option_B[Component],$B110)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$107,Table_C3C4_Option_B[Component],$B110)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$107,Table_C5_Option_B[Component],$B110),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$107,Table_C1_Option_A[Component],$B110)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$107,Table_C2_Option_A[Component],$B110)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$107,Table_C3C4_Option_A[Component],$B110)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$107,Table_C5_Option_A[Component],$B110))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Cable installation vessel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$107,Table_A0[Component],$B111)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$107,Table_A1_Module_A1A2[Component],B111)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$107,Table_A1_Module_A3[Component],B111)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$107,Table_A1_Module_A1A3[Component],B111)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$107,Table_A4[Component],$B111)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$107,Table_A5_Fuel[Component],$B111)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$107,Table_A5_Waste[Component],$B111)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$107,Table_B1_Refrigerants[Component],$B111)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$107,Table_B2B5_Materials[Component],$B111)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$107,Table_B2B5_Energy[Component],$B111)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$107,Table_B2B5_Waste[Component],$B111)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$107,Table_B6[Component],$B111)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$107,Table_B7[Component],$B111)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$107,Table_B8[Component],$B111)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$107,Table_C1_Option_B[Component],$B111)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$107,Table_C2_Option_B[Component],$B111)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$107,Table_C3C4_Option_B[Component],$B111)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$107,Table_C5_Option_B[Component],$B111),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$107,Table_C1_Option_A[Component],$B111)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$107,Table_C2_Option_A[Component],$B111)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$107,Table_C3C4_Option_A[Component],$B111)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$107,Table_C5_Option_A[Component],$B111))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Onshore plant and machinery",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$107,Table_A0[Component],$B112)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$107,Table_A1_Module_A1A2[Component],B112)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$107,Table_A1_Module_A3[Component],B112)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$107,Table_A1_Module_A1A3[Component],B112)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$107,Table_A4[Component],$B112)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$107,Table_A5_Fuel[Component],$B112)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$107,Table_A5_Waste[Component],$B112)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$107,Table_B1_Refrigerants[Component],$B112)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$107,Table_B2B5_Materials[Component],$B112)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$107,Table_B2B5_Energy[Component],$B112)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$107,Table_B2B5_Waste[Component],$B112)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$107,Table_B6[Component],$B112)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$107,Table_B7[Component],$B112)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$107,Table_B8[Component],$B112)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$107,Table_C1_Option_B[Component],$B112)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$107,Table_C2_Option_B[Component],$B112)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$107,Table_C3C4_Option_B[Component],$B112)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$107,Table_C5_Option_B[Component],$B112),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$107,Table_C1_Option_A[Component],$B112)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$107,Table_C2_Option_A[Component],$B112)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$107,Table_C3C4_Option_A[Component],$B112)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$107,Table_C5_Option_A[Component],$B112))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$107,Table_A0[Component],$B113)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$107,Table_A1_Module_A1A2[Component],B113)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$107,Table_A1_Module_A3[Component],B113)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$107,Table_A1_Module_A1A3[Component],B113)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$107,Table_A4[Component],$B113)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$107,Table_A5_Fuel[Component],$B113)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$107,Table_A5_Waste[Component],$B113)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$107,Table_B1_Refrigerants[Component],$B113)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$107,Table_B2B5_Materials[Component],$B113)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$107,Table_B2B5_Energy[Component],$B113)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$107,Table_B2B5_Waste[Component],$B113)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$107,Table_B6[Component],$B113)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$107,Table_B7[Component],$B113)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$107,Table_B8[Component],$B113)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$107,Table_C1_Option_B[Component],$B113)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$107,Table_C2_Option_B[Component],$B113)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$107,Table_C3C4_Option_B[Component],$B113)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$107,Table_C5_Option_B[Component],$B113),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$107,Table_C1_Option_A[Component],$B113)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$107,Table_C2_Option_A[Component],$B113)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$107,Table_C3C4_Option_A[Component],$B113)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$107,Table_C5_Option_A[Component],$B113))","v":0},0,{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Construction & Installation assets)",{"$f":"SUM(C108:C113)","v":0},0,0,0,0,0,{"$f":"SUM(C114:H114)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Operations and maintenance assets"]
[null,"Service operations vessels",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$115,Table_A0[Component],$B116)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$115,Table_A1_Module_A1A2[Component],B116)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$115,Table_A1_Module_A3[Component],B116)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$115,Table_A1_Module_A1A3[Component],B116)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$115,Table_A4[Component],$B116)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$115,Table_A5_Fuel[Component],$B116)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$115,Table_A5_Waste[Component],$B116)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$115,Table_B1_Refrigerants[Component],$B116)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$115,Table_B2B5_Materials[Component],$B116)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$115,Table_B2B5_Energy[Component],$B116)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$115,Table_B2B5_Waste[Component],$B116)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$115,Table_B6[Component],$B116)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$115,Table_B7[Component],$B116)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$115,Table_B8[Component],$B116)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$115,Table_C1_Option_B[Component],$B116)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$115,Table_C2_Option_B[Component],$B116)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$115,Table_C3C4_Option_B[Component],$B116)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$115,Table_C5_Option_B[Component],$B116),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$115,Table_C1_Option_A[Component],$B116)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$115,Table_C2_Option_A[Component],$B116)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$115,Table_C3C4_Option_A[Component],$B116)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$115,Table_C5_Option_A[Component],$B116))","v":0},{"$f":"SUM(C116:H116)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Crew transfer vessels",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$115,Table_A0[Component],$B117)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$115,Table_A1_Module_A1A2[Component],B117)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$115,Table_A1_Module_A3[Component],B117)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$115,Table_A1_Module_A1A3[Component],B117)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$115,Table_A4[Component],$B117)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$115,Table_A5_Fuel[Component],$B117)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$115,Table_A5_Waste[Component],$B117)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$115,Table_B1_Refrigerants[Component],$B117)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$115,Table_B2B5_Materials[Component],$B117)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$115,Table_B2B5_Energy[Component],$B117)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$115,Table_B2B5_Waste[Component],$B117)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$115,Table_B6[Component],$B117)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$115,Table_B7[Component],$B117)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$115,Table_B8[Component],$B117)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$115,Table_C1_Option_B[Component],$B117)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$115,Table_C2_Option_B[Component],$B117)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$115,Table_C3C4_Option_B[Component],$B117)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$115,Table_C5_Option_B[Component],$B117),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$115,Table_C1_Option_A[Component],$B117)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$115,Table_C2_Option_A[Component],$B117)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$115,Table_C3C4_Option_A[Component],$B117)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$115,Table_C5_Option_A[Component],$B117))","v":0},{"$f":"SUM(C117:H117)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Helicopters, drones or other aerial vehicle",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$115,Table_A0[Component],$B118)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$115,Table_A1_Module_A1A2[Component],B118)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$115,Table_A1_Module_A3[Component],B118)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$115,Table_A1_Module_A1A3[Component],B118)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$115,Table_A4[Component],$B118)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$115,Table_A5_Fuel[Component],$B118)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$115,Table_A5_Waste[Component],$B118)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$115,Table_B1_Refrigerants[Component],$B118)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$115,Table_B2B5_Materials[Component],$B118)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$115,Table_B2B5_Energy[Component],$B118)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$115,Table_B2B5_Waste[Component],$B118)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$115,Table_B6[Component],$B118)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$115,Table_B7[Component],$B118)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$115,Table_B8[Component],$B118)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$115,Table_C1_Option_B[Component],$B118)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$115,Table_C2_Option_B[Component],$B118)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$115,Table_C3C4_Option_B[Component],$B118)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$115,Table_C5_Option_B[Component],$B118),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$115,Table_C1_Option_A[Component],$B118)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$115,Table_C2_Option_A[Component],$B118)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$115,Table_C3C4_Option_A[Component],$B118)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$115,Table_C5_Option_A[Component],$B118))","v":0},{"$f":"SUM(C118:H118)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$115,Table_A0[Component],$B119)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$115,Table_A1_Module_A1A2[Component],B119)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$115,Table_A1_Module_A3[Component],B119)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$115,Table_A1_Module_A1A3[Component],B119)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$115,Table_A4[Component],$B119)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$115,Table_A5_Fuel[Component],$B119)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$115,Table_A5_Waste[Component],$B119)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$115,Table_B1_Refrigerants[Component],$B119)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$115,Table_B2B5_Materials[Component],$B119)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$115,Table_B2B5_Energy[Component],$B119)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$115,Table_B2B5_Waste[Component],$B119)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$115,Table_B6[Component],$B119)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$115,Table_B7[Component],$B119)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$115,Table_B8[Component],$B119)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$115,Table_C1_Option_B[Component],$B119)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$115,Table_C2_Option_B[Component],$B119)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$115,Table_C3C4_Option_B[Component],$B119)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$115,Table_C5_Option_B[Component],$B119),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$115,Table_C1_Option_A[Component],$B119)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$115,Table_C2_Option_A[Component],$B119)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$115,Table_C3C4_Option_A[Component],$B119)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$115,Table_C5_Option_A[Component],$B119))","v":0},{"$f":"SUM(C119:H119)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Operations & Maintenance Assets)",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$87,Table_A0[Component],$B120)","v":0},{"$f":"SUM(D116:D119)","v":0},{"$f":"SUM(E116:E119)","v":0},{"$f":"SUM(F116:F119)","v":0},{"$f":"SUM(G116:G119)","v":0},{"$f":"SUM(H116:H119)","v":0},{"$f":"SUM(C120:H120)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other"]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[Asset],$B$121,Table_A0[Component],$B122)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[Asset],$B$121,Table_A1_Module_A1A2[Component],B122)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[Asset],$B$121,Table_A1_Module_A3[Component],B122)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[Asset],$B$121,Table_A1_Module_A1A3[Component],B122)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[Asset],$B$121,Table_A4[Component],$B122)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[Asset],$B$121,Table_A5_Fuel[Component],$B122)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[Asset],$B$121,Table_A5_Waste[Component],$B122)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[Asset],$B$121,Table_B1_Refrigerants[Component],$B122)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[Asset],$B$121,Table_B2B5_Materials[Component],$B122)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[Asset],$B$121,Table_B2B5_Energy[Component],$B122)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[Asset],$B$121,Table_B2B5_Waste[Component],$B122)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[Asset],$B$121,Table_B6[Component],$B122)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[Asset],$B$121,Table_B7[Component],$B122)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[Asset],$B$121,Table_B8[Component],$B122)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[Asset],$B$121,Table_C1_Option_B[Component],$B122)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[Asset],$B$121,Table_C2_Option_B[Component],$B122)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[Asset],$B$121,Table_C3C4_Option_B[Component],$B122)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[Asset],$B$121,Table_C5_Option_B[Component],$B122),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[Asset],$B$121,Table_C1_Option_A[Component],$B122)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[Asset],$B$121,Table_C2_Option_A[Component],$B122)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[Asset],$B$121,Table_C3C4_Option_A[Component],$B122)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[Asset],$B$121,Table_C5_Option_A[Component],$B122))","v":0},{"$f":"SUM(C122:H122)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Other)",{"$f":"SUM(C122)","v":0},0,0,0,0,0,{"$f":"SUM(C123:H123)","v":0},{"$f":"IFERROR(Results_Asset[[#This Row],[Total Asset Emissions (kgCO2e)]]/Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Total Asset Emissions by Lifecycle Stage",{"$f":"SUBTOTAL(109,C62:C66,C69:C73,C76:C80,C83:C85,C88:C92,C95:C99,C102:C105,C108:C113,C116:C119,C122)","v":0},0,0,0,0,{"$f":"SUBTOTAL(109,H62:H66,H69:H73,H76:H80,H83:H85,H88:H92,H95:H99,H102:H105,H108:H113,H116:H119,H122)","v":0},{"$f":"SUBTOTAL(109,I62:I66,I69:I73,I76:I80,I83:I85,I88:I92,I95:I99,I102:I105,I108:I113,I116:I119,I122)","v":0}]
[null,"ERROR CHECK - Do totals match?",{"$f":"IF(ROUND(Results_Asset[[#Totals],[A0 emissions (kgCO2e)]]/1000,2)=ROUND(F28,2),\"Yes\",\"CHECK ASSET LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Asset[[#Totals],[A1-A3 emissions (kgCO2e)]]/1000,2)=ROUND(F33,2),\"Yes\",\"CHECK ASSET LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Asset[[#Totals],[A4 Emissions (kgCO2e)]]/1000,2)=ROUND(F35,2),\"Yes\",\"CHECK ASSET LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Asset[[#Totals],[A5 Emissions (kgCO2e)]]/1000,2)=ROUND(F36,2),\"Yes\",\"CHECK ASSET LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Asset[[#Totals],[B1-B8 Emissions (kgCO2e)]]/1000,2)=ROUND(F47,2),\"Yes\",\"CHECK ASSET LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Asset[[#Totals],[C1-C5 Emissions (kgCO2e)]]/1000,2)=ROUND(F53,2),\"Yes\",\"CHECK ASSET LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]]/1000,2)=ROUND(F55,2),\"Yes\",\"CHECK ASSET LABELLING\")","v":"Yes"}]
[]
[null,"Reporting emissions and removals by Activity and Sub-category"]
[]
[null,"Activities L1, L2","A0 emissions (kgCO2e)","A1-A3 emissions (kgCO2e)","A4 Emissions (kgCO2e)","A5 Emissions (kgCO2e)","B1-B8 Emissions (kgCO2e)","C1-C5 Emissions (kgCO2e)","Total Activity Emissions (kgCO2e)","% of Emissions by L1 (green) and L2 (blue) activity"]
[null,"Direct emissions and removals"]
[null,"Emissions",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$130,Table_A0[OSW Activity Taxonomy L2],$B131)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$130,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$130,Table_A1_Module_A3[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$130,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],$B131)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$130,Table_A4[OSW Activity Taxonomy L2],$B131)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$61,Table_A5_Fuel[OSW Activity Taxonomy L2],$B62)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$61,Table_A5_Waste[OSW Activity Taxonomy L2],$B62)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$130,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$130,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$130,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$130,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$130,Table_B6[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$130,Table_B7[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$130,Table_B8[OSW Activity Taxonomy L2],$B131)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$130,Table_C1_Option_B[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$130,Table_C2_Option_B[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$130,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$130,Table_C5_Option_B[OSW Activity Taxonomy L2],$B131),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$130,Table_C1_Option_A[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$130,Table_C2_Option_A[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$130,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B131)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$130,Table_C5_Option_A[OSW Activity Taxonomy L2],$B131))","v":0},{"$f":"SUM(C131:H131)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Removals",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$130,Table_A0[OSW Activity Taxonomy L2],$B132)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$130,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$130,Table_A1_Module_A3[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$130,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],$B132)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$130,Table_A4[OSW Activity Taxonomy L2],$B132)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$61,Table_A5_Fuel[OSW Activity Taxonomy L2],$B63)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$61,Table_A5_Waste[OSW Activity Taxonomy L2],$B63)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$130,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$130,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$130,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$130,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$130,Table_B6[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$130,Table_B7[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$130,Table_B8[OSW Activity Taxonomy L2],$B132)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$130,Table_C1_Option_B[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$130,Table_C2_Option_B[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$130,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$130,Table_C5_Option_B[OSW Activity Taxonomy L2],$B132),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$130,Table_C1_Option_A[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$130,Table_C2_Option_A[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$130,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B132)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$130,Table_C5_Option_A[OSW Activity Taxonomy L2],$B132))","v":0},{"$f":"SUM(C132:H132)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Direct emissions and removals)",{"$f":"SUM(C131:C132)","v":0},{"$f":"SUM(D131:D132)","v":0},0,0,0,0,0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Electricity, fuels and other utilities"]
[null,"Biofuels lifecycle",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$134,Table_A0[OSW Activity Taxonomy L2],$B135)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B135)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A3[OSW Activity Taxonomy L2],B135)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B135)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$134,Table_A4[OSW Activity Taxonomy L2],$B135)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$134,Table_A5_Fuel[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$134,Table_A5_Waste[OSW Activity Taxonomy L2],$B135)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$134,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$134,Table_B6[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$134,Table_B7[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$134,Table_B8[OSW Activity Taxonomy L2],$B135)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_B[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_B[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_B[OSW Activity Taxonomy L2],$B135),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_A[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_A[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B135)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_A[OSW Activity Taxonomy L2],$B135))","v":0},{"$f":"SUM(C135:H135)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Electricity lifecycle",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$134,Table_A0[OSW Activity Taxonomy L2],$B136)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B136)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A3[OSW Activity Taxonomy L2],B136)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B136)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$134,Table_A4[OSW Activity Taxonomy L2],$B136)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$134,Table_A5_Fuel[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$134,Table_A5_Waste[OSW Activity Taxonomy L2],$B136)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$134,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$134,Table_B6[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$134,Table_B7[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$134,Table_B8[OSW Activity Taxonomy L2],$B136)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_B[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_B[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_B[OSW Activity Taxonomy L2],$B136),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_A[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_A[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B136)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_A[OSW Activity Taxonomy L2],$B136))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Gaseous fuels lifecycle",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$134,Table_A0[OSW Activity Taxonomy L2],$B137)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B137)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A3[OSW Activity Taxonomy L2],B137)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B137)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$134,Table_A4[OSW Activity Taxonomy L2],$B137)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$134,Table_A5_Fuel[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$134,Table_A5_Waste[OSW Activity Taxonomy L2],$B137)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$134,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$134,Table_B6[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$134,Table_B7[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$134,Table_B8[OSW Activity Taxonomy L2],$B137)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_B[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_B[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_B[OSW Activity Taxonomy L2],$B137),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_A[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_A[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B137)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_A[OSW Activity Taxonomy L2],$B137))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Liquid fuels lifecycle",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$134,Table_A0[OSW Activity Taxonomy L2],$B138)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B138)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A3[OSW Activity Taxonomy L2],B138)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B138)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$134,Table_A4[OSW Activity Taxonomy L2],$B138)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$134,Table_A5_Fuel[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$134,Table_A5_Waste[OSW Activity Taxonomy L2],$B138)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$134,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$134,Table_B6[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$134,Table_B7[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$134,Table_B8[OSW Activity Taxonomy L2],$B138)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_B[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_B[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_B[OSW Activity Taxonomy L2],$B138),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_A[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_A[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B138)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_A[OSW Activity Taxonomy L2],$B138))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Solid fuels lifecycle",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$134,Table_A0[OSW Activity Taxonomy L2],$B139)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B139)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A3[OSW Activity Taxonomy L2],B139)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B139)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$134,Table_A4[OSW Activity Taxonomy L2],$B139)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$134,Table_A5_Fuel[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$134,Table_A5_Waste[OSW Activity Taxonomy L2],$B139)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$134,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$134,Table_B6[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$134,Table_B7[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$134,Table_B8[OSW Activity Taxonomy L2],$B139)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_B[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_B[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_B[OSW Activity Taxonomy L2],$B139),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_A[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_A[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B139)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_A[OSW Activity Taxonomy L2],$B139))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Water consumption",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$134,Table_A0[OSW Activity Taxonomy L2],$B140)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B140)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A3[OSW Activity Taxonomy L2],B140)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$134,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B140)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$134,Table_A4[OSW Activity Taxonomy L2],$B140)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$134,Table_A5_Fuel[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$134,Table_A5_Waste[OSW Activity Taxonomy L2],$B140)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$134,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$134,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$134,Table_B6[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$134,Table_B7[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$134,Table_B8[OSW Activity Taxonomy L2],$B140)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_B[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_B[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_B[OSW Activity Taxonomy L2],$B140),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C1_Option_A[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C2_Option_A[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B140)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$134,Table_C5_Option_A[OSW Activity Taxonomy L2],$B140))","v":0},{"$f":"SUM(C140:H140)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Electricity & Fuels)",{"$f":"SUM(C135:C139)","v":0},0,0,0,0,0,0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Fully manufactured assets"]
[null,"Wind turbine generators (WTG)",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B143)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B143)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B143)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B143)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B143)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B143)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B143)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B143),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B143)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B143))","v":0},{"$f":"SUM(C143:H143)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Fixed foundation",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B144)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B144)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B144)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B144)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B144)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B144)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B144)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B144),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B144)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B144))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Floating foundation",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B145)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B145)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B145)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B145)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B145)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B145)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B145)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B145),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B145)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B145))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Cables",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B146)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B146)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B146)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B146)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B146)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B146)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B146)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B146),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B146)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B146))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Offshore substation",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B147)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B147)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B147)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B147)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B147)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B147)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B147)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B147),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B147)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B147))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Onshore substation",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B148)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B148)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B148)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B148)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B148)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B148)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B148)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B148),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B148)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B148))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Operations base",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B149)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B149)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B149)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B149)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B149)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B149)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B149)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B149),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B149)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B149))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Construction and installation assets",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B150)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B150)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B150)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B150)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B150)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B150)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B150)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B150),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B150)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B150))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Operations and maintenance assets",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B151)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B151)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B151)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B151)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B151)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B151)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B151)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B151),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B151)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B151))","v":0},{"$f":"SUM(C151:H151)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$142,Table_A0[OSW Activity Taxonomy L2],$B152)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B152)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A3[OSW Activity Taxonomy L2],B152)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$142,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B152)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$142,Table_A4[OSW Activity Taxonomy L2],$B152)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$142,Table_A5_Fuel[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$142,Table_A5_Waste[OSW Activity Taxonomy L2],$B152)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$142,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$142,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$142,Table_B6[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$142,Table_B7[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$142,Table_B8[OSW Activity Taxonomy L2],$B152)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_B[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_B[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_B[OSW Activity Taxonomy L2],$B152),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C1_Option_A[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C2_Option_A[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B152)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$142,Table_C5_Option_A[OSW Activity Taxonomy L2],$B152))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Manufactured Assets)",{"$f":"SUM(C143:C150)","v":0},0,0,0,0,0,0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Fully manufactured components"]
[null,"Nacelle and internals",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B155)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B155)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B155)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B155)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B155)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B155)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B155)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B155),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B155)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B155))","v":0},{"$f":"SUM(C155:H155)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Blades, hub, and rotor system",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B156)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B156)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B156)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B156)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B156)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B156)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B156)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B156),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B156)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B156))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Tower",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B157)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B157)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B157)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B157)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B157)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B157)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B157)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B157),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B157)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B157))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Transformer",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B158)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B158)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B158)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B158)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B158)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B158)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B158)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B158),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B158)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B158))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Monopile",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B159)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B159)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B159)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B159)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B159)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B159)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B159)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B159),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B159)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B159))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Jacket",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B160)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B160)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B160)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B160)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B160)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B160)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B160)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B160),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B160)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B160))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Transition piece",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B161)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B161)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B161)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B161)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B161)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B161)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B161)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B161),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B161)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B161))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other fixed foundation technologies",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B162)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B162)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B162)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B162)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B162)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B162)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B162)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B162),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B162)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B162))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Platform",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B163)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B163)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B163)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B163)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B163)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B163)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B163)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B163),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B163)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B163))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Mooring",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B164)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B164)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B164)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B164)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B164)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B164)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B164)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B164),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B164)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B164))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Anchors",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B165)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B165)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B165)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B165)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B165)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B165)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B165)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B165),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B165)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B165))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other floating foundation technologies",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B166)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B166)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B166)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B166)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B166)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B166)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B166)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B166),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B166)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B166))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Inter array cables",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B167)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B167)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B167)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B167)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B167)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B167)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B167)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B167),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B167)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B167))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Export cables",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B168)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B168)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B168)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B168)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B168)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B168)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B168)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B168),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B168)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B168))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Transformers",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B169)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B169)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B169)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B169)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B169)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B169)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B169)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B169),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B169)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B169))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Switchgear",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B170)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B170)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B170)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B170)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B170)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B170)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B170)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B170),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B170)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B170))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Facilities",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B171)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B171)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B171)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B171)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B171)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B171)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B171)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B171),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B171)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B171))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Structure",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B172)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B172)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B172)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B172)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B172)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B172)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B172)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B172),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B172)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B172))","v":0},{"$f":"SUM(C172:H172)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Transformers",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B173)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B173)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B173)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B173)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B173)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B173)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B173)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B173),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B173)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B173))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Switchgear",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B174)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B174)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B174)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B174)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B174)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B174)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B174)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B174),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B174)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B174))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Facilities",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B175)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B175)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B175)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B175)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B175)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B175)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B175)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B175),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B175)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B175))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Structure",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B176)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B176)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B176)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B176)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B176)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B176)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B176)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B176),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B176)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B176))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Site buildings",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B177)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B177)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B177)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B177)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B177)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B177)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B177)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B177),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B177)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B177))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Roads",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B178)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B178)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B178)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B178)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B178)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B178)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B178)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B178),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B178)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B178))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Vessel berths",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B179)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B179)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B179)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B179)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B179)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B179)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B179)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B179),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B179)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B179))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Turbine Installation vessel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B180)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B180)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B180)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B180)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B180)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B180)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B180)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B180),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B180)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B180))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Foundation installation vessel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B181)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B181)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B181)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B181)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B181)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B181)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B181)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B181),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B181)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B181))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Substation installation vessel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B182)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B182)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B182)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B182)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B182)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B182)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B182)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B182),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B182)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B182))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Cable installation vessel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B183)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B183)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B183)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B183)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B183)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B183)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B183)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B183),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B183)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B183))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Onshore plant and machinery",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B184)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B184)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B184)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B184)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B184)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B184)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B184)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B184),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B184)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B184))","v":0},{"$f":"SUM(C184:H184)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Service operations vessels",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B185)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B185)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B185)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B185)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B185)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B185)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B185)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B185),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B185)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B185))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Crew transfer vessels",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B186)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B186)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B186)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B186)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B186)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B186)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B186)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B186),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B186)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B186))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Helicopters, drones or other",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B187)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B187)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B187)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B187)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B187)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B187)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B187)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B187),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B187)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B187))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$154,Table_A0[OSW Activity Taxonomy L2],$B188)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B188)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A3[OSW Activity Taxonomy L2],B188)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$154,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B188)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$154,Table_A4[OSW Activity Taxonomy L2],$B188)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$154,Table_A5_Fuel[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$154,Table_A5_Waste[OSW Activity Taxonomy L2],$B188)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$154,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$154,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$154,Table_B6[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$154,Table_B7[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$154,Table_B8[OSW Activity Taxonomy L2],$B188)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_B[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_B[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_B[OSW Activity Taxonomy L2],$B188),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C1_Option_A[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C2_Option_A[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B188)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$154,Table_C5_Option_A[OSW Activity Taxonomy L2],$B188))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Cables)",{"$f":"SUM(C155:C171)","v":0},0,0,0,0,0,0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Manufacturing processes"]
[null,"Coating and galvanising processes",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$190,Table_A0[OSW Activity Taxonomy L2],$B191)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B191)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A3[OSW Activity Taxonomy L2],B191)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B191)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$190,Table_A4[OSW Activity Taxonomy L2],$B191)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$190,Table_A5_Fuel[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$190,Table_A5_Waste[OSW Activity Taxonomy L2],$B191)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$190,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$190,Table_B6[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$190,Table_B7[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$190,Table_B8[OSW Activity Taxonomy L2],$B191)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C1_Option_B[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C2_Option_B[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C5_Option_B[OSW Activity Taxonomy L2],$B191),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C1_Option_A[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C2_Option_A[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B191)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C5_Option_A[OSW Activity Taxonomy L2],$B191))","v":0},{"$f":"SUM(C191:H191)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Joining and welding processes",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$190,Table_A0[OSW Activity Taxonomy L2],$B192)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B192)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A3[OSW Activity Taxonomy L2],B192)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B192)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$190,Table_A4[OSW Activity Taxonomy L2],$B192)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$190,Table_A5_Fuel[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$190,Table_A5_Waste[OSW Activity Taxonomy L2],$B192)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$190,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$190,Table_B6[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$190,Table_B7[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$190,Table_B8[OSW Activity Taxonomy L2],$B192)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C1_Option_B[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C2_Option_B[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C5_Option_B[OSW Activity Taxonomy L2],$B192),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C1_Option_A[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C2_Option_A[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B192)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C5_Option_A[OSW Activity Taxonomy L2],$B192))","v":0},{"$f":"SUM(C192:H192)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Material processing",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$190,Table_A0[OSW Activity Taxonomy L2],$B193)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B193)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A3[OSW Activity Taxonomy L2],B193)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B193)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$190,Table_A4[OSW Activity Taxonomy L2],$B193)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$190,Table_A5_Fuel[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$190,Table_A5_Waste[OSW Activity Taxonomy L2],$B193)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$190,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$190,Table_B6[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$190,Table_B7[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$190,Table_B8[OSW Activity Taxonomy L2],$B193)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C1_Option_B[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C2_Option_B[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C5_Option_B[OSW Activity Taxonomy L2],$B193),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C1_Option_A[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C2_Option_A[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B193)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C5_Option_A[OSW Activity Taxonomy L2],$B193))","v":0},{"$f":"SUM(C193:H193)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other manufacturing processes",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$190,Table_A0[OSW Activity Taxonomy L2],$B194)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B194)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A3[OSW Activity Taxonomy L2],B194)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$190,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B194)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$190,Table_A4[OSW Activity Taxonomy L2],$B194)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$190,Table_A5_Fuel[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$190,Table_A5_Waste[OSW Activity Taxonomy L2],$B194)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$190,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$190,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$190,Table_B6[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$190,Table_B7[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$190,Table_B8[OSW Activity Taxonomy L2],$B194)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C1_Option_B[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C2_Option_B[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$190,Table_C5_Option_B[OSW Activity Taxonomy L2],$B194),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C1_Option_A[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C2_Option_A[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B194)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$190,Table_C5_Option_A[OSW Activity Taxonomy L2],$B194))","v":0},{"$f":"SUM(C194:H194)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Manufacturing processes)",{"$f":"SUM(C191:C194)","v":0},0,0,0,0,0,{"$f":"SUM(C195:H195)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Materials"]
[null,"Aluminium",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B197)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B197)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B197)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B197)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B197)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B197)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B197)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B197),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B197)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B197))","v":0},{"$f":"SUM(C197:H197)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Biogenic materials",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B198)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B198)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B198)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B198)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B198)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B198)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B198)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B198),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B198)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B198))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Carbon fibre",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B199)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B199)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B199)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B199)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B199)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B199)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B199)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B199),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B199)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B199))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Concrete",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B200)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B200)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B200)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B200)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B200)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B200)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B200)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B200),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B200)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B200))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Copper",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B201)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B201)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B201)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B201)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B201)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B201)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B201)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B201),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B201)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B201))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Fibreglass",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B202)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B202)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B202)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B202)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B202)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B202)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B202)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B202),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B202)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B202))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Oils and Lubricants",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B203)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B203)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B203)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B203)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B203)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B203)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B203)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B203),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B203)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B203))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other materials",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B204)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B204)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B204)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B204)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B204)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B204)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B204)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B204),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B204)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B204))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Polymers",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B205)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B205)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B205)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B205)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B205)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B205)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B205)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B205),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B205)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B205))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Steel",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$196,Table_A0[OSW Activity Taxonomy L2],$B206)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B206)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A3[OSW Activity Taxonomy L2],B206)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$196,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B206)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$196,Table_A4[OSW Activity Taxonomy L2],$B206)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$196,Table_A5_Fuel[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$196,Table_A5_Waste[OSW Activity Taxonomy L2],$B206)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$196,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$196,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$196,Table_B6[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$196,Table_B7[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$196,Table_B8[OSW Activity Taxonomy L2],$B206)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_B[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_B[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_B[OSW Activity Taxonomy L2],$B206),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C1_Option_A[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C2_Option_A[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B206)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$196,Table_C5_Option_A[OSW Activity Taxonomy L2],$B206))","v":0},0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Materials)",{"$f":"SUM(C197:C206)","v":0},0,0,0,0,0,0,{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Freight and transportation"]
[null,"Air freight and transportation",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$208,Table_A0[OSW Activity Taxonomy L2],$B209)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B209)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A3[OSW Activity Taxonomy L2],B209)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B209)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$208,Table_A4[OSW Activity Taxonomy L2],$B209)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$208,Table_A5_Fuel[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$208,Table_A5_Waste[OSW Activity Taxonomy L2],$B209)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$208,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$208,Table_B6[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$208,Table_B7[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$208,Table_B8[OSW Activity Taxonomy L2],$B209)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C1_Option_B[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C2_Option_B[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C5_Option_B[OSW Activity Taxonomy L2],$B209),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C1_Option_A[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C2_Option_A[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B209)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C5_Option_A[OSW Activity Taxonomy L2],$B209))","v":0},{"$f":"SUM(C209:H209)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Rail freight and transportation",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$208,Table_A0[OSW Activity Taxonomy L2],$B210)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B210)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A3[OSW Activity Taxonomy L2],B210)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B210)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$208,Table_A4[OSW Activity Taxonomy L2],$B210)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$208,Table_A5_Fuel[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$208,Table_A5_Waste[OSW Activity Taxonomy L2],$B210)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$208,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$208,Table_B6[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$208,Table_B7[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$208,Table_B8[OSW Activity Taxonomy L2],$B210)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C1_Option_B[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C2_Option_B[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C5_Option_B[OSW Activity Taxonomy L2],$B210),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C1_Option_A[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C2_Option_A[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B210)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C5_Option_A[OSW Activity Taxonomy L2],$B210))","v":0},{"$f":"SUM(C210:H210)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Road freight and transportation",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$208,Table_A0[OSW Activity Taxonomy L2],$B211)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B211)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A3[OSW Activity Taxonomy L2],B211)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B211)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$208,Table_A4[OSW Activity Taxonomy L2],$B211)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$208,Table_A5_Fuel[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$208,Table_A5_Waste[OSW Activity Taxonomy L2],$B211)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$208,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$208,Table_B6[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$208,Table_B7[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$208,Table_B8[OSW Activity Taxonomy L2],$B211)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C1_Option_B[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C2_Option_B[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C5_Option_B[OSW Activity Taxonomy L2],$B211),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C1_Option_A[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C2_Option_A[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B211)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C5_Option_A[OSW Activity Taxonomy L2],$B211))","v":0},{"$f":"SUM(C211:H211)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Sea freight and transportation",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$208,Table_A0[OSW Activity Taxonomy L2],$B212)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B212)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A3[OSW Activity Taxonomy L2],B212)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$208,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B212)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$208,Table_A4[OSW Activity Taxonomy L2],$B212)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$208,Table_A5_Fuel[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$208,Table_A5_Waste[OSW Activity Taxonomy L2],$B212)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$208,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$208,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$208,Table_B6[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$208,Table_B7[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$208,Table_B8[OSW Activity Taxonomy L2],$B212)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C1_Option_B[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C2_Option_B[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$208,Table_C5_Option_B[OSW Activity Taxonomy L2],$B212),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C1_Option_A[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C2_Option_A[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B212)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$208,Table_C5_Option_A[OSW Activity Taxonomy L2],$B212))","v":0},{"$f":"SUM(C212:H212)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Freight and transportation)",{"$f":"SUM(C209:C212)","v":0},0,0,0,0,0,{"$f":"SUM(C213:H213)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Waste treatment"]
[null,"Incineration",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$214,Table_A0[OSW Activity Taxonomy L2],$B215)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B215)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A3[OSW Activity Taxonomy L2],B215)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B215)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$214,Table_A4[OSW Activity Taxonomy L2],$B215)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$214,Table_A5_Fuel[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$214,Table_A5_Waste[OSW Activity Taxonomy L2],$B215)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$214,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$214,Table_B6[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$214,Table_B7[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$214,Table_B8[OSW Activity Taxonomy L2],$B215)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C1_Option_B[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C2_Option_B[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C5_Option_B[OSW Activity Taxonomy L2],$B215),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C1_Option_A[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C2_Option_A[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B215)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C5_Option_A[OSW Activity Taxonomy L2],$B215))","v":0},{"$f":"SUM(C215:H215)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Landfill",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$214,Table_A0[OSW Activity Taxonomy L2],$B216)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B216)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A3[OSW Activity Taxonomy L2],B216)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B216)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$214,Table_A4[OSW Activity Taxonomy L2],$B216)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$214,Table_A5_Fuel[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$214,Table_A5_Waste[OSW Activity Taxonomy L2],$B216)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$214,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$214,Table_B6[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$214,Table_B7[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$214,Table_B8[OSW Activity Taxonomy L2],$B216)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C1_Option_B[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C2_Option_B[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C5_Option_B[OSW Activity Taxonomy L2],$B216),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C1_Option_A[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C2_Option_A[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B216)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C5_Option_A[OSW Activity Taxonomy L2],$B216))","v":0},{"$f":"SUM(C216:H216)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Processing, sorting for recycling and reuse",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$214,Table_A0[OSW Activity Taxonomy L2],$B217)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B217)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A3[OSW Activity Taxonomy L2],B217)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B217)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$214,Table_A4[OSW Activity Taxonomy L2],$B217)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$214,Table_A5_Fuel[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$214,Table_A5_Waste[OSW Activity Taxonomy L2],$B217)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$214,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$214,Table_B6[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$214,Table_B7[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$214,Table_B8[OSW Activity Taxonomy L2],$B217)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C1_Option_B[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C2_Option_B[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C5_Option_B[OSW Activity Taxonomy L2],$B217),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C1_Option_A[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C2_Option_A[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B217)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C5_Option_A[OSW Activity Taxonomy L2],$B217))","v":0},{"$f":"SUM(C217:H217)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$214,Table_A0[OSW Activity Taxonomy L2],$B218)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B218)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A3[OSW Activity Taxonomy L2],B218)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$214,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B218)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$214,Table_A4[OSW Activity Taxonomy L2],$B218)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$214,Table_A5_Fuel[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$214,Table_A5_Waste[OSW Activity Taxonomy L2],$B218)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$214,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$214,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$214,Table_B6[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$214,Table_B7[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$214,Table_B8[OSW Activity Taxonomy L2],$B218)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C1_Option_B[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C2_Option_B[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$214,Table_C5_Option_B[OSW Activity Taxonomy L2],$B218),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C1_Option_A[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C2_Option_A[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B218)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$214,Table_C5_Option_A[OSW Activity Taxonomy L2],$B218))","v":0},{"$f":"SUM(C218:H218)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Waste treatment)",{"$f":"SUM(C215:C218)","v":0},0,0,0,0,{"$f":"SUM(H215:H218)","v":0},{"$f":"SUM(C219:H219)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Water"]
[null,"Water consumption",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$220,Table_A0[OSW Activity Taxonomy L2],$B221)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$220,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B221)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$220,Table_A1_Module_A3[OSW Activity Taxonomy L2],B221)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$220,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B221)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$220,Table_A4[OSW Activity Taxonomy L2],$B221)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$220,Table_A5_Fuel[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$220,Table_A5_Waste[OSW Activity Taxonomy L2],$B221)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$220,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$220,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$220,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$220,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$220,Table_B6[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$220,Table_B7[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$220,Table_B8[OSW Activity Taxonomy L2],$B221)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$220,Table_C1_Option_B[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$220,Table_C2_Option_B[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$220,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$220,Table_C5_Option_B[OSW Activity Taxonomy L2],$B221),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$220,Table_C1_Option_A[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$220,Table_C2_Option_A[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$220,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B221)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$220,Table_C5_Option_A[OSW Activity Taxonomy L2],$B221))","v":0},{"$f":"SUM(C221:H221)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Water)",{"$f":"SUM(C221:C221)","v":0},0,0,0,0,0,{"$f":"SUM(C222:H222)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Other"]
[null,"Unassigned",{"$f":"SUMIFS(Table_A0[Total Emissions (kgCO2e)],Table_A0[OSW Activity Taxonomy L1],$B$223,Table_A0[OSW Activity Taxonomy L2],$B224)","v":0},{"$f":"SUMIFS(Table_A1_Module_A1A2[Total Emissions (kgCO2e)],Table_A1_Module_A1A2[OSW Activity Taxonomy L1],$B$223,Table_A1_Module_A1A2[OSW Activity Taxonomy L2],B224)+SUMIFS(Table_A1_Module_A3[Total Emissions (kgCO2e)],Table_A1_Module_A3[OSW Activity Taxonomy L1],$B$223,Table_A1_Module_A3[OSW Activity Taxonomy L2],B224)+SUMIFS(Table_A1_Module_A1A3[Total Emissions (kgCO2e)],Table_A1_Module_A1A3[OSW Activity Taxonomy L1],$B$223,Table_A1_Module_A1A3[OSW Activity Taxonomy L2],B224)","v":0},{"$f":"SUMIFS(Table_A4[Total Emissions (kgCO2e)],Table_A4[OSW Activity Taxonomy L1],$B$223,Table_A4[OSW Activity Taxonomy L2],$B224)","v":0},{"$f":"SUMIFS(Table_A5_Fuel[Total Emissions (kgCO2e)],Table_A5_Fuel[OSW Activity Taxonomy L1],$B$223,Table_A5_Fuel[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_A5_Waste[Total Emissions (kgCO2e)],Table_A5_Waste[OSW Activity Taxonomy L1],$B$223,Table_A5_Waste[OSW Activity Taxonomy L2],$B224)","v":0},{"$f":"SUMIFS(Table_B1_Refrigerants[Total Emissions (kgCO2e)],Table_B1_Refrigerants[OSW Activity Taxonomy L1],$B$223,Table_B1_Refrigerants[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_B2B5_Materials[Total Emissions (kgCO2e)],Table_B2B5_Materials[OSW Activity Taxonomy L1],$B$223,Table_B2B5_Materials[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_B2B5_Energy[Total Emissions (kgCO2e)],Table_B2B5_Energy[OSW Activity Taxonomy L1],$B$223,Table_B2B5_Energy[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_B2B5_Waste[Total Emissions (kgCO2e)],Table_B2B5_Waste[OSW Activity Taxonomy L1],$B$223,Table_B2B5_Waste[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_B6[Total Emissions (kgCO2e)],Table_B6[OSW Activity Taxonomy L1],$B$223,Table_B6[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_B7[Total Emissions (kgCO2e)],Table_B7[OSW Activity Taxonomy L1],$B$223,Table_B7[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_B8[Total Emissions (kgCO2e)],Table_B8[OSW Activity Taxonomy L1],$B$223,Table_B8[OSW Activity Taxonomy L2],$B224)","v":0},{"$f":"IF('C1-C5 - End-of-Life'!$G$48=\"No data\",SUMIFS(Table_C1_Option_B[Total Emissions (kgCO2e)],Table_C1_Option_B[OSW Activity Taxonomy L1],$B$223,Table_C1_Option_B[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_C2_Option_B[Total Emissions (kgCO2e)],Table_C2_Option_B[OSW Activity Taxonomy L1],$B$223,Table_C2_Option_B[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_C3C4_Option_B[Total Emissions (kgCO2e)],Table_C3C4_Option_B[OSW Activity Taxonomy L1],$B$223,Table_C3C4_Option_B[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_C5_Option_B[Total Emissions (kgCO2e)],Table_C5_Option_B[OSW Activity Taxonomy L1],$B$223,Table_C5_Option_B[OSW Activity Taxonomy L2],$B224),SUMIFS(Table_C1_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C1_Option_A[OSW Activity Taxonomy L1],$B$223,Table_C1_Option_A[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_C2_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C2_Option_A[OSW Activity Taxonomy L1],$B$223,Table_C2_Option_A[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_C3C4_Option_A[Total Emissions: Scaled to Capacity of Development (kgCO2e)],Table_C3C4_Option_A[OSW Activity Taxonomy L1],$B$223,Table_C3C4_Option_A[OSW Activity Taxonomy L2],$B224)+SUMIFS(Table_C5_Option_A[Total Emissions (kgCO2e)],Table_C5_Option_A[OSW Activity Taxonomy L1],$B$223,Table_C5_Option_A[OSW Activity Taxonomy L2],$B224))","v":0},{"$f":"SUM(C224:H224)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"TOTAL (Other)",{"$f":"SUM(C224:C224)","v":0},0,0,0,0,0,{"$f":"SUM(C225:H225)","v":0},{"$f":"IFERROR(Results_Activities[[#This Row],[Total Activity Emissions (kgCO2e)]]/Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],\"-\")","v":"-"}]
[null,"Total",{"$f":"SUBTOTAL(109,C131:C132,C135:C140,C143:C152,C155:C188,C191:C194,C197:C206,C209:C212,C215:C218,C221,C224:C224)","v":0},0,0,0,0,{"$f":"SUBTOTAL(109,H131:H132,H135:H140,H143:H152,H155:H188,H191:H194,H197:H206,H209:H212,H215:H218,H221,H224:H224)","v":0},{"$f":"SUBTOTAL(109,I131:I132,I135:I140,I143:I152,I155:I188,I191:I194,I197:I206,I209:I212,I215:I218,I221,I224:I224)","v":0}]
[null,"ERROR CHECK - do totals match?",{"$f":"IF(ROUND(Results_Activities[[#Totals],[A0 emissions (kgCO2e)]],2)=ROUND(Results_Asset[[#Totals],[A0 emissions (kgCO2e)]],2),\"Yes\",\"CHECK ACTIVITY LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Activities[[#Totals],[A1-A3 emissions (kgCO2e)]],2)=ROUND(Results_Asset[[#Totals],[A1-A3 emissions (kgCO2e)]],2),\"Yes\",\"CHECK ACTIVITY LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Activities[[#Totals],[A4 Emissions (kgCO2e)]],2)=ROUND(Results_Asset[[#Totals],[A4 Emissions (kgCO2e)]],2),\"Yes\",\"CHECK ACTIVITY LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Activities[[#Totals],[A5 Emissions (kgCO2e)]],2)=ROUND(Results_Asset[[#Totals],[A5 Emissions (kgCO2e)]],2),\"Yes\",\"CHECK ACTIVITY LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Activities[[#Totals],[B1-B8 Emissions (kgCO2e)]],2)=ROUND(Results_Asset[[#Totals],[B1-B8 Emissions (kgCO2e)]],2),\"Yes\",\"CHECK ACTIVITY LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Activities[[#Totals],[C1-C5 Emissions (kgCO2e)]],2)=ROUND(Results_Asset[[#Totals],[C1-C5 Emissions (kgCO2e)]],2),\"Yes\",\"CHECK ACTIVITY LABELLING\")","v":"Yes"},{"$f":"IF(ROUND(Results_Activities[[#Totals],[Total Activity Emissions (kgCO2e)]],2)=ROUND(Results_Asset[[#Totals],[Total Asset Emissions (kgCO2e)]],2),\"Yes\",\"CHECK ACTIVITY LABELLING\")","v":"Yes"}]
[]
[]
[]
[null,null,null,null,null,null,{"$f":"Results_Activities[[#Totals],[B1-B8 Emissions (kgCO2e)]]-Results_Asset[[#Totals],[B1-B8 Emissions (kgCO2e)]]","v":0}]
[]
[]
[null,null,null,{"$f":"Results_Asset[[#Totals],[A1-A3 emissions (kgCO2e)]]-Results_Activities[[#Totals],[A1-A3 emissions (kgCO2e)]]","v":0}]

{"sheet":"Graphs","index":20,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"SUS-JIP   |  Offshore Wind Footprinting Tool"]
[null,"GRAPHS"]
[]
[]
[null,"Footprint results graphs"]

{"sheet":"PER Export","index":21,"n_rows":27,"n_cols":3,"rows_kept":27,"cut":false,"hidden":false,"merged":[[2,1,2,2]]}
[]
[]
[]
[]
[]
["Date:"]
[{"$f":"TODAY()","v":"2024-10-02"}]
[]
["Assessment  Details"]
[]
["Assessor name:",{"$f":"IF(ISBLANK(Assessor_name),\"Please complete project summary tab\",Assessor_name)","v":"Please complete project summary tab"}]
["Assessor email: ",{"$f":"IF(ISBLANK(Assessor_email),\"Please complete project summary tab\",Assessor_email)","v":"Please complete project summary tab"}]
["Development name:",{"$f":"IF(ISBLANK(Development_name),\"Please complete project summary tab\",Development_name)","v":"Please complete project summary tab"}]
["Development location:",{"$f":"IF(ISBLANK(Development_location),\"Please complete project summary tab\",Development_location)","v":"Please complete project summary tab"}]
["Assessment type:",{"$f":"IF(ISBLANK(Assessment_type),\"Please complete project summary tab\",Assessment_type)","v":"Please complete project summary tab"}]
["Installed capacity:",{"$f":"IF(ISBLANK(Installed_capacity__MW),\"Please complete project summary tab\",Installed_capacity__MW)","v":880},"MW"]
["Assumed capacity factor:",{"$f":"IF(ISBLANK(Assumed_capacity_factor),\"Please complete project summary tab\",Assumed_capacity_factor)","v":0.5}]
["Assumed service life:",{"$f":"IF(ISBLANK(Assumed_service_life_Years),\"Please complete project summary tab\",Assumed_service_life_Years)","v":25},"Years"]
["Assumed electrical losses in system boundary:",{"$f":"IF(ISBLANK(Assumed_electrical_losses_in_system_boundary),\"Please complete project summary tab\",Assumed_electrical_losses_in_system_boundary)","v":0.02}]
[]
["OSW PCF Results"]
[]
["Absolute emissions for the development:",{"$f":"IFERROR(Results_Lifecycle[[#Totals],[Total (tCO2e) ]],\"Check results\")","v":0},"tCO2e"]
["Emissions per declared unit (kWh delivered to grid):",{"$f":"IFERROR(Results!D16, \"Check results\")","v":0},"gCO2e / kWh delivered to grid"]
["Emissions per MW installed:",{"$f":"IFERROR(B23/B16,\"Check results\")","v":0},"tCO2e / MW installed"]
["Annual emissions:",{"$f":"IFERROR(B23/B18,\"Check results\")","v":0},"tCO2e / Year in operation"]
["Data quality rating for the assessment:",{"$f":"IFERROR(DQ_Uncertainty_Results[DQ Rating],\"Check DQ Assessment\")","v":"Poor"}]

{"sheet":"Lists","index":22,"n_rows":55,"n_cols":19,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["Assessment Type","Background Data Used","Impact Method Used","Impact Indicator Used","Reporting Standard","Verified","OSW Activity Taxonomy L1","OSW Activity Taxonomy L2","Options","Preconstruction Modules","Production Modules","Construction & Installation Modules","Use of infrastructure Modules","End-of-life of infrastructure Modules","Transport Journey Leg","Assessment","Cut-off","IEA Scenarios","IEA Energy Region"]
["PCF","Ecoinvent","IPCC 2021","GWP100","ISO 14067","Yes","Direct Emissions","Fugitive emissions","Option A","A0 - Preconstruction","A1: Raw Material Supply","A4: Transport","B1: Use","C1: De-construction Demolition","Transport to onshore site","Operational development","Operational assessment:\n\n•\tNon-material contributors may be excluded for practical reasons (data availability, data quality, or other stated justification) if the highest reasonable estimate for that source of emissions does not exceed 0.2% of the total footprint. Aggregate exclusions should not exceed 2% of estimated the total footprint. \n•\tPlease refer to Appendix 1 for a list of activities for mandatory inclusion for an assessment of an operational development.\n•\tExclusions shall be stated clearly in the assumptions along with their GHG emissions estimates. The organisation shall document a simple justification for these exclusions. If exclusion exceed the thresholds listed above due to practical limitations the assessor shall clearly describe the exclusions and justify the approach footprint. Aggregate exclusions should not exceed 2% of estimated the total footprint. ","stated policies scenario","World"]
["LCA","Sphera MCL (fka GaBi)","IPCC 2021 no LT","GWP100 no LT","GHGP Product Standard","No","Freight & Transportation","Process emissions","Option B",null,"A2: Transport","A5: Construction installation process","B2: Maintenance","C2: Transport","Transport from onshore to offshore site","Prospective development","Prospective assessment:\n\n•\tNon-material contributors may be excluded for practical reasons (data availability, data quality, or other stated justification) if the highest reasonable estimate does not exceed 1% of the total footprint. Aggregate exclusions should not exceed 5% of the total footprint.\n•\tPlease refer to Appendix 1 for a list of activities for mandatory inclusion for an assessment of an operational development.\n•\tExclusions shall be stated clearly in the assumptions and listed the Product Emissions Report, along with their GHG emissions estimates. The organisation shall document a simple justification for these exclusions. If exclusion exceed the thresholds listed above, this shall be clearly documented and disclosed.","announced pledges scenario","North America"]
["EPD","Other","CML v4.8 2016 no LT",null,"ISO 14040/14044",null,"Electricity & Fuels","Sea freight & transport",null,null,"A3: Manufacturing",null,"B3: Repair","C3: Waste Processing",null,null,null,null,"United States"]
[null,null,"CML v4.8 2016",null,"EN 15804",null,"Manufactured Assets","Road freight & transportation",null,null,"A1-A3: Production",null,"B4: Replacement","C4: Disposal",null,null,null,null,"Central and South America"]
[null,null,"Ecological Scarcity 2021 no LT",null,null,null,"Manufactured Sub-components","Air freight & transportation",null,null,null,null,"B5: Refurbishment","C5: Relandscaping",null,null,null,null,"Brazil"]
[null,null,"Ecological Scarcity 2021",null,null,null,"Manufacturing processes","Biofuels lifecycle",null,null,null,null,"B6-B8: Operational energy, material consumption, waste and water treatment",null,null,null,null,null,"Europe"]
[null,null,"EF v3.0 no LT",null,null,null,"Materials","Electricity lifecycle",null,null,null,null,null,null,null,null,null,null,"European Union"]
[null,null,"EF v3.0",null,null,null,"Waste Treatment","Gaseous fuels lifecycle",null,null,null,null,null,null,null,null,null,null,"Africa"]
[null,null,"EF v3.1 no LT",null,null,null,"Other","Liquid fuels lifecycle",null,null,null,null,null,null,null,null,null,null,"Middle East"]
[null,null,"EF v3.1",null,null,null,null,"Solid fuels lifecycle",null,null,null,null,null,null,null,null,null,null,"Eurasia"]
[null,null,"IPCC 2013 no LT",null,null,null,null,"Wind turbine generators (WTG)",null,null,null,null,null,null,null,null,null,null,"Russia"]
[null,null,"IPCC 2013",null,null,null,null,"Fixed foundation",null,null,null,null,null,null,null,null,null,null,"Asia Pacific"]
[null,null,"ReCiPe 2016 v1.03, midpoint (H) no LT",null,null,null,null,"Floating foundation",null,null,null,null,null,null,null,null,null,null,"China"]
[null,null,"ReCiPe 2016 v1.03, midpoint (H)",null,null,null,null,"Cables",null,null,null,null,null,null,null,null,null,null,"India"]
[null,null,"TRACI v2.1 no LT",null,null,null,null,"Offshore substation",null,null,null,null,null,null,null,null,null,null,"Japan"]
[null,null,"TRACI v2.1",null,null,null,null,"Onshore substation",null,null,null,null,null,null,null,null,null,null,"Southeast Asia"]
[null,null,"EF v3.0 EN15804",null,null,null,null,"Operations base",null,null,null,null,null,null,null,null,null,null,"OECD"]
[null,null,"EF v3.1 EN15804",null,null,null,null,"Other Assets",null,null,null,null,null,null,null,null,null,null,"Non-OECD"]
[null,null,null,null,null,null,null,"Nacelle",null,null,null,null,null,null,null,null,null,null,"Advanced economies"]
[null,null,null,null,null,null,null,"Rotor",null,null,null,null,null,null,null,null,null,null,"Emerging market and developing economies"]
[null,null,null,null,null,null,null,"Tower"]
[null,null,null,null,null,null,null,"Monopile"]
[null,null,null,null,null,null,null,"Jacket"]
[null,null,null,null,null,null,null,"Transition piece"]
[null,null,null,null,null,null,null,"Gravity base"]
[null,null,null,null,null,null,null,"Platform"]
[null,null,null,null,null,null,null,"Mooring"]
[null,null,null,null,null,null,null,"Anchor"]
[null,null,null,null,null,null,null,"Inter Array cables"]
[null,null,null,null,null,null,null,"Export cables"]
[null,null,null,null,null,null,null,"Transformers"]
[null,null,null,null,null,null,null,"Switchgear"]
[null,null,null,null,null,null,null,"Facilities"]
[null,null,null,null,null,null,null,"Structure"]
[null,null,null,null,null,null,null,"Site buildings"]
[null,null,null,null,null,null,null,"Roads"]
[null,null,null,null,null,null,null,"Vessel berths"]
[null,null,null,null,null,null,null,"Material processing"]
[null,null,null,null,null,null,null,"Joining & welding processes"]
[null,null,null,null,null,null,null,"Coating & galvanising processes"]
[null,null,null,null,null,null,null,"Other manufacturing processes"]
[null,null,null,null,null,null,null,"Aluminium"]
[null,null,null,null,null,null,null,"Biogenic materials"]
[null,null,null,null,null,null,null,"Carbon fibre"]
[null,null,null,null,null,null,null,"Concrete"]
[null,null,null,null,null,null,null,"Copper"]
[null,null,null,null,null,null,null,"Fibreglass"]
[null,null,null,null,null,null,null,"Oils & Lubricants"]
[null,null,null,null,null,null,null,"Other materials"]
[null,null,null,null,null,null,null,"Polymers"]
[null,null,null,null,null,null,null,"Steel "]
[null,null,null,null,null,null,null,"Landfill"]
[null,null,null,null,null,null,null,"Recycling"]
[null,null,null,null,null,null,null,"Energy recovery"]

{"sheet":"Taxonomies","index":23,"n_rows":75,"n_cols":5,"rows_kept":75,"cut":false,"hidden":true,"merged":[]}
["L1: Assets","L2: Subcomponents",null,"L1: Activity Category","L2: Activity Subcategory"]
["Wind turbine generators (WTG)","Nacelle and internals",null,"Direct emissions and removals","Emissions"]
["Wind turbine generators (WTG)","Blades, hub, and rotor system",null,"Direct emissions and removals","Removals"]
["Wind turbine generators (WTG)","Tower",null,"Freight and transportation","Air freight and transportation"]
["Wind turbine generators (WTG)","Transformer",null,"Freight and transportation","Rail freight and transportation"]
["Wind turbine generators (WTG)","Unassigned",null,"Freight and transportation","Road freight and transportation"]
["Fixed foundations","Monopile",null,"Freight and transportation","Sea freight and transportation"]
["Fixed foundations","Jacket",null,"Electricity, fuels and other utilities","Biofuels lifecycle"]
["Fixed foundations","Transition piece",null,"Electricity, fuels and other utilities","Electricity lifecycle"]
["Fixed foundations","Other fixed foundation technologies",null,"Electricity, fuels and other utilities","Gaseous fuels lifecycle"]
["Fixed foundations","Unassigned",null,"Electricity, fuels and other utilities","Liquid fuels lifecycle"]
["Floating foundations","Platform",null,"Electricity, fuels and other utilities","Solid fuels lifecycle"]
["Floating foundations","Mooring",null,"Electricity, fuels and other utilities","Water consumption"]
["Floating foundations","Anchors",null,"Fully manufactured assets","Wind turbine generators (WTG)"]
["Floating foundations","Other floating foundation technologies",null,"Fully manufactured assets","Fixed foundations"]
["Floating foundations","Unassigned",null,"Fully manufactured assets","Floating foundations"]
["Cables","Inter array cables",null,"Fully manufactured assets","Cables"]
["Cables","Export cables",null,"Fully manufactured assets","Offshore substation"]
["Cables","Unassigned",null,"Fully manufactured assets","Onshore substation"]
["Offshore substation","Transformers",null,"Fully manufactured assets","Operations base"]
["Offshore substation","Switchgear",null,"Fully manufactured assets","Construction and installation assets"]
["Offshore substation","Facilities",null,"Fully manufactured assets","Operations and maintenance assets"]
["Offshore substation","Structure",null,"Fully manufactured assets","Other"]
["Offshore substation","Unassigned",null,"Fully manufactured components","Nacelle and internals"]
["Onshore substation","Transformers",null,"Fully manufactured components","Blades, hub, and rotor system"]
["Onshore substation","Switchgear",null,"Fully manufactured components","Tower"]
["Onshore substation","Facilities",null,"Fully manufactured components","Transformer"]
["Onshore substation","Structure",null,"Fully manufactured components","Monopile"]
["Onshore substation","Unassigned",null,"Fully manufactured components","Jacket"]
["Operations base","Site buildings",null,"Fully manufactured components","Transition piece"]
["Operations base","Roads",null,"Fully manufactured components","Other fixed foundation technologies"]
["Operations base","Vessel berths",null,"Fully manufactured components","Platform"]
["Operations base","Unassigned",null,"Fully manufactured components","Mooring"]
["Construction and installation assets","Turbine Installation vessel",null,"Fully manufactured components","Anchors"]
["Construction and installation assets","Foundation installation vessel",null,"Fully manufactured components","Other floating foundation technologies"]
["Construction and installation assets","Substation installation vessel",null,"Fully manufactured components","Inter array cables"]
["Construction and installation assets","Cable installation vessel",null,"Fully manufactured components","Export cables"]
["Construction and installation assets","Onshore plant and machinery",null,"Fully manufactured components","Transformers"]
["Construction and installation assets","Unassigned",null,"Fully manufactured components","Switchgear"]
["Operations and maintenance assets","Service operations vessels",null,"Fully manufactured components","Facilities"]
["Operations and maintenance assets","Crew transfer vessels",null,"Fully manufactured components","Structure"]
["Operations and maintenance assets","Helicopters, drones or other aerial vehicle",null,"Fully manufactured components","Transformers"]
["Other","Unassigned",null,"Fully manufactured components","Switchgear"]
[null,null,null,"Fully manufactured components","Facilities"]
[null,null,null,"Fully manufactured components","Structure"]
[null,null,null,"Fully manufactured components","Site buildings"]
[null,null,null,"Fully manufactured components","Roads"]
[null,null,null,"Fully manufactured components","Vessel berths"]
[null,null,null,"Fully manufactured components","Turbine Installation vessel"]
[null,null,null,"Fully manufactured components","Foundation installation vessel"]
[null,null,null,"Fully manufactured components","Substation installation vessel"]
[null,null,null,"Fully manufactured components","Cable installation vessel"]
[null,null,null,"Fully manufactured components","Onshore plant and machinery"]
[null,null,null,"Fully manufactured components","Service operations vessels"]
[null,null,null,"Fully manufactured components","Crew transfer vessels"]
[null,null,null,"Fully manufactured components","Helicopters, drones or other aerial vehicle"]
[null,null,null,"Fully manufactured components","Other"]
[null,null,null,"Manufacturing processes","Coating and galvanising processes"]
[null,null,null,"Manufacturing processes","Joining and welding processes"]
[null,null,null,"Manufacturing processes","Material processing"]
[null,null,null,"Manufacturing processes","Other manufacturing processes"]
[null,null,null,"Materials","Aluminium"]
[null,null,null,"Materials","Biogenic materials"]
[null,null,null,"Materials","Carbon fibre"]
[null,null,null,"Materials","Concrete"]
[null,null,null,"Materials","Copper"]
[null,null,null,"Materials","Fibreglass"]
[null,null,null,"Materials","Oils and Lubricants"]
[null,null,null,"Materials","Other materials"]
[null,null,null,"Materials","Polymers"]
[null,null,null,"Materials","Steel"]
[null,null,null,"Waste treatment","Incineration"]
[null,null,null,"Waste treatment","Landfill"]
[null,null,null,"Waste treatment","Processing, sorting for recycling and reuse"]
[null,null,null,"Other","Unassigned"]

{"sheet":"Dynamic Dropdowns>>","index":24,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["This sheet is inentionally left blank"]

{"sheet":"EF L1 List","index":25,"n_rows":9,"n_cols":5,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
[null,"Do not modify this sheet, dropdowns will update automatically as you add to the Emissions factor database"]
[null,{"$f":"TRANSPOSE(_xlfn._xlws.SORT(_xlfn.UNIQUE(EF_Library[OSW EF Category])))","v":"Characterisation Factors"},"Secondary: Ecoinvent","Secondary: Proxy"]
[null,{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(EF_Library[[OSW Activity Taxonomy L1]:[OSW Activity Taxonomy L1]],EF_Library[[OSW EF Category]:[OSW EF Category]]=B2))),\"No selection\")","v":"Direct emissions and removals"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(EF_Library[[OSW Activity Taxonomy L1]:[OSW Activity Taxonomy L1]],EF_Library[[OSW EF Category]:[OSW EF Category]]=C2))),\"No selection\")","v":"Electricity, fuels and other utilitites"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(EF_Library[[OSW Activity Taxonomy L1]:[OSW Activity Taxonomy L1]],EF_Library[[OSW EF Category]:[OSW EF Category]]=D2))),\"No selection\")","v":"Electricity, fuels and other utilitites"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(EF_Library[[OSW Activity Taxonomy L1]:[OSW Activity Taxonomy L1]],EF_Library[[OSW EF Category]:[OSW EF Category]]=E2))),\"No selection\")","v":"No selection"}]
[null,null,"Freight and transportation","Fully manufactured assets"]
[null,null,"Fully manufactured assets","Fully manufactured components"]
[null,null,"Fully manufactured components","Materials"]
[null,null,"Manufacturing processes"]
[null,null,"Materials"]
[null,null,"Waste treatment"]

{"sheet":"EF L2 List","index":26,"n_rows":11,"n_cols":16384,"rows_kept":11,"cut":false,"hidden":true,"merged":[],"flags":["row_too_large"]}
[null,"Do not modify this sheet, dropdowns will update automatically as you add to the Emissions factor database"]
[null,{"$f":"TRANSPOSE(_xlfn._xlws.SORT(_xlfn.UNIQUE(EF_Library[OSW Activity Taxonomy L1])))","v":"Direct emissions and removals"},"Electricity, fuels and other utilitites","Freight and transportation","Fully manufactured assets","Fully manufactured components","Manufacturing processes","Materials","Waste treatment"]
[{"$cut":{"chars":2170714,"head":""}}]
[null,"Removals","Electricity lifecycle","Rail freight and transportation","Wind turbine generators (WTG)","Nacelle and internals","Joining and welding processes","Concrete","Landfill"]
[null,null,"Gaseous fuels lifecycle","Road freight and transportation",null,"Tower","Material processing","Copper","Processing, sorting for recycling and reuse"]
[null,null,"Liquid fuels lifecycle","Sea freight and transportation",null,"Transformer",null,"Epoxy resin"]
[null,null,"Solid fuels lifecycle",null,null,null,null,"Fibreglass"]
[null,null,"Water consumption",null,null,null,null,"Oils and lubricants"]
[null,null,null,null,null,null,null,"Other materials"]
[null,null,null,null,null,null,null,"Polymers"]
[null,null,null,null,null,null,null,"Steel"]

{"sheet":"EF L3 List","index":27,"n_rows":48,"n_cols":153,"rows_kept":48,"cut":false,"hidden":true,"merged":[]}
[null,"Do not modify this sheet, dropdowns will update automatically as you add to the Emissions factor database"]
[null,{"$f":"TRANSPOSE(_xlfn.UNIQUE(EF_Library[OSW Activity Taxonomy L2]))","v":"Electricity lifecycle"},"Gaseous fuels lifecycle","Liquid fuels lifecycle","Water consumption","Air freight and transportation","Rail freight and transportation","Road freight and transportation","Sea freight and transportation","Cables","Wind turbine generators (WTG)","Nacelle and internals","Transformer","Coating and galvanising processes","Joining and welding processes","Material processing","Aluminium","Concrete","Copper","Oils and lubricants","Other materials","Polymers","Steel","Incineration","Landfill","Processing, sorting for recycling and reuse","Biofuels lifecycle","Solid fuels lifecycle","Epoxy resin","Fibreglass","Blades, hub, and rotor system","Tower","Emissions","Removals"]
[null,{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!B2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!C2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!D2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!E2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!F2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!G2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!H2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!I2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!J2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!K2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!L2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!M2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!N2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!O2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!P2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!Q2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!R2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!S2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!T2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!U2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!V2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!W2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!X2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!Y2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!Z2)),\"No selection\")","v":0},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AA2)),\"No selection\")","v":"Bio Petrol"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AB2)),\"No selection\")","v":"Coal (domestic)"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AC2)),\"No selection\")","v":"Products based on epoxy-resin, group 1"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AD2)),\"No selection\")","v":"Polyamide profiles reinforced with 25% fibreglass"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AE2)),\"No selection\")","v":"Hub (Siemens Gamesa 11-200 (11 MW))"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AF2)),\"No selection\")","v":"Tower (Siemens Gamesa 11-200 (11 MW))"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AG2)),\"No selection\")","v":"Bromopropane"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AH2)),\"No selection\")","v":"Carbon dioxide, removal from atmosphere"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AI2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AJ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AK2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AL2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AM2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AN2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AO2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AP2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AQ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AR2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AS2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AT2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AU2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AV2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AW2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AX2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AY2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!AZ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BA2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BB2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BC2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BD2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BE2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BF2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BG2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BH2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BI2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BJ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BK2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BL2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BM2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BN2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BO2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BP2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BQ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BR2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BS2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BT2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BU2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BV2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BW2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BX2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BY2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!BZ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CA2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CB2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CC2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CD2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CE2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CF2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CG2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CH2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CI2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CJ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CK2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CL2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CM2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CN2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CO2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CP2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CQ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CR2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CS2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CT2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CU2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CV2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CW2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CX2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CY2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!CZ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DA2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DB2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DC2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DD2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DE2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DF2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DG2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DH2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DI2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DJ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DK2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DL2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DM2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DN2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DO2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DP2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DQ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DR2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DS2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DT2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DU2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DV2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DW2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DX2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DY2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!DZ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EA2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EB2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EC2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!ED2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EE2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EF2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EG2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EH2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EI2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EJ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EK2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EL2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EM2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EN2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EO2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EP2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EQ2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!ER2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!ES2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!ET2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EU2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EV2)),\"No selection\")","v":"No selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.FILTER(EF_Library[[Emission Factor Name]:[Emission Factor Name]],EF_Library[[OSW Activity Taxonomy L2]:[OSW Activity Taxonomy L2]]='EF L3 List'!EW2)),\"No selection\")","v":"No selection"}]
[null,null,"Butane","Aviation spirit",null,null,null,null,null,null,"WTG (Siemens Gamesa 11-200 (11 MW))","Backend (Siemens Gamesa 11-200 (11 MW))",null,null,null,null,null,null,"Copper wire rod",null,null,null,"Heavy steel plates",null,null,null,"Biodiesel HVO","Coal (electricity generation - home produced coal only)","Products based on epoxy-resin, group 2","Mesh","Blades (Siemens Gamesa 11-200 (11 MW))","Tower (Siemens Gamesa 14-222 (14 MW))","Butane"]
[null,null,"CNG","Aviation turbine fuel",null,null,null,null,null,null,"WTG (Siemens Gamesa 14-222 (14 MW))","Generator (Siemens Gamesa 11-200 (11 MW))",null,null,null,null,null,null,null,null,null,null,"Hot rolled steel plates",null,null,null,"Biodiesel ME","Coal (electricity generation)","Products based on epoxy-resin, group 3",null,"Hub (Siemens Gamesa 14-222 (14 MW))","Tower (Siemens Gamesa 14-236 (14 MW))","Carbon dioxide, fossil"]
[null,null,"LNG","Burning oil",null,null,null,null,null,null,"WTG (Siemens Gamesa 14-236 (14 MW))","Backend assembly (Siemens Gamesa 11-200 (11 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biodiesel ME (from tallow)","Coal (industrial)","Products based on epoxy-resin, group 4",null,"Blades (Siemens Gamesa 14-222 (14 MW))",null,"Carbon dioxide, from soil or biomass stock"]
[null,null,"LPG","Diesel (100% mineral diesel)",null,null,null,null,null,null,null,"Electric components (Siemens Gamesa 11-200 (11 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biodiesel ME (from used cooking oil)","Coking coal","Products based on epoxy-resin, group 5",null,"Hub (Siemens Gamesa 14-236 (14 MW))",null,"Chloroform"]
[null,null,"Natural gas","Diesel (average biofuel blend)",null,null,null,null,null,null,null,"Backend (Siemens Gamesa 14-222 (14 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bioethanol","Petroleum coke",null,null,"Blades (Siemens Gamesa 14-236 (14 MW))",null,"Dinitrogen monoxide"]
[null,null,"Natural gas (100% mineral blend)","Fuel oil",null,null,null,null,null,null,null,"Generator (Siemens Gamesa 14-222 (14 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biomethane (compressed)",null,null,null,null,null,"Ethane"]
[null,null,"Other petroleum gas","Gas oil",null,null,null,null,null,null,null,"Backend assembly (Siemens Gamesa 14-222 (14 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biomethane (liquified)",null,null,null,null,null,"Ethane, 1,1,1,2-tetrafluoro-, HFC-134a"]
[null,null,"Propane","Lubricants",null,null,null,null,null,null,null,"Electric components (Siemens Gamesa 14-222 (14 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biopropane",null,null,null,null,null,"Ethane, 1,1,1-trichloro-, HCFC-140"]
[null,null,null,"Marine fuel oil",null,null,null,null,null,null,null,"Backend (Siemens Gamesa 14-236 (14 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methanol (bio)",null,null,null,null,null,"Ethane, 1,1,1-trifluoro-, HFC-143a"]
[null,null,null,"Marine gas oil",null,null,null,null,null,null,null,"Generator (Siemens Gamesa 14-236 (14 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Off road biodiesel",null,null,null,null,null,"Ethane, 1,1,2-trichloro-1,2,2-trifluoro-, CFC-113"]
[null,null,null,"Naphtha",null,null,null,null,null,null,null,"Backend assembly (Siemens Gamesa 14-236 (14 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Renewable petrol",null,null,null,null,null,"Ethane, 1,1-dichloro-1-fluoro-, HCFC-141b"]
[null,null,null,"Petrol (100% mineral petrol)",null,null,null,null,null,null,null,"Electric components (Siemens Gamesa 14-236 (14 MW))",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biogas",null,null,null,null,null,"Ethane, 1,1-difluoro-, HFC-152a"]
[null,null,null,"Petrol (average biofuel blend)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Landfill gas",null,null,null,null,null,"Ethane, 1,2-dichloro-"]
[null,null,null,"Processed fuel oils - distillate oil",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Grass/straw",null,null,null,null,null,"Ethane, 1,2-dichloro-1,1,2,2-tetrafluoro-, CFC-114"]
[null,null,null,"Processed fuel oils - residual oil",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wood chips",null,null,null,null,null,"Ethane, 1-chloro-1,1-difluoro-, HCFC-142b"]
[null,null,null,"Refinery miscellaneous",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wood logs",null,null,null,null,null,"Ethane, 2,2-dichloro-1,1,1-trifluoro-, HCFC-123"]
[null,null,null,"Waste oils",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wood pellets",null,null,null,null,null,"Ethane, 2-chloro-1,1,1,2-tetrafluoro-, HCFC-124"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ethane, chloropentafluoro-, CFC-115"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ethane, hexafluoro-, HFC-116"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ethane, pentafluoro-, HFC-125"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, bromo-, Halon 1001"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, bromochlorodifluoro-, Halon 1211"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, bromotrifluoro-, Halon 1301"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, chlorodifluoro-, HCFC-22"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, chloro-fluoro-, HCFC-31"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, chlorotrifluoro-, CFC-13"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, dichloro-, HCC-30"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, dichlorodifluoro-, CFC-12"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, dichlorofluoro-, HCFC-21"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, difluoro-, HFC-32"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, fossil"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, from soil or biomass stock"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, monochloro-, R-40"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, non-fossil"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, tetrachloro-, R-10"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, tetrafluoro-, R-14"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, trichlorofluoro-, CFC-11"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Methane, trifluoro-, HFC-23"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Monochloroethane"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nitrogen fluoride"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Perfluoropentane"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Propane"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sulfur hexafluoride"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tetrachloroethylene"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Trichloroethylene"]

{"sheet":"EF L4 List","index":28,"n_rows":5,"n_cols":16384,"rows_kept":5,"cut":false,"hidden":true,"merged":[],"flags":["row_too_large"]}
[null,"Do not modify this sheet, dropdowns will update automatically as you add to the Emissions factor database"]
[null,{"$f":"TRANSPOSE(_xlfn.UNIQUE(EF_Library[Emission Factor Name]))","v":0},"Bio Petrol","Biodiesel HVO","Biodiesel ME","Biodiesel ME (from tallow)","Biodiesel ME (from used cooking oil)","Bioethanol","Biomethane (compressed)","Biomethane (liquified)","Biopropane","Methanol (bio)","Off road biodiesel","Renewable petrol","Biogas","Landfill gas","Grass/straw","Wood chips","Wood logs","Wood pellets","Butane","CNG","LNG","LPG","Natural gas","Natural gas (100% mineral blend)","Other petroleum gas","Propane","Aviation spirit","Aviation turbine fuel","Burning oil","Diesel (100% mineral diesel)","Diesel (average biofuel blend)","Fuel oil","Gas oil","Lubricants","Marine fuel oil","Marine gas oil","Naphtha","Petrol (100% mineral petrol)","Petrol (average biofuel blend)","Processed fuel oils - distillate oil","Processed fuel oils - residual oil","Refinery miscellaneous","Waste oils","Coal (domestic)","Coal (electricity generation - home produced coal only)","Coal (electricity generation)","Coal (industrial)","Coking coal","Petroleum coke","Copper wire rod","Products based on epoxy-resin, group 1","Products based on epoxy-resin, group 2","Products based on epoxy-resin, group 3","Products based on epoxy-resin, group 4","Products based on epoxy-resin, group 5","Polyamide profiles reinforced with 25% fibreglass","Mesh","Heavy steel plates","Hot rolled steel plates","WTG (Siemens Gamesa 11-200 (11 MW))","Backend (Siemens Gamesa 11-200 (11 MW))","Generator (Siemens Gamesa 11-200 (11 MW))","Hub (Siemens Gamesa 11-200 (11 MW))","Backend assembly (Siemens Gamesa 11-200 (11 MW))","Electric components (Siemens Gamesa 11-200 (11 MW))","Blades (Siemens Gamesa 11-200 (11 MW))","Tower (Siemens Gamesa 11-200 (11 MW))","WTG (Siemens Gamesa 14-222 (14 MW))","Backend (Siemens Gamesa 14-222 (14 MW))","Generator (Siemens Gamesa 14-222 (14 MW))","Hub (Siemens Gamesa 14-222 (14 MW))","Backend assembly (Siemens Gamesa 14-222 (14 MW))","Electric components (Siemens Gamesa 14-222 (14 MW))","Blades (Siemens Gamesa 14-222 (14 MW))","Tower (Siemens Gamesa 14-222 (14 MW))","WTG (Siemens Gamesa 14-236 (14 MW))","Backend (Siemens Gamesa 14-236 (14 MW))","Generator (Siemens Gamesa 14-236 (14 MW))","Hub (Siemens Gamesa 14-236 (14 MW))","Backend assembly (Siemens Gamesa 14-236 (14 MW))","Electric components (Siemens Gamesa 14-236 (14 MW))","Blades (Siemens Gamesa 14-236 (14 MW))","Tower (Siemens Gamesa 14-236 (14 MW))","Bromopropane","Carbon dioxide, fossil","Carbon dioxide, from soil or biomass stock","Carbon dioxide, removal from atmosphere","Chloroform","Dinitrogen monoxide","Ethane","Ethane, 1,1,1,2-tetrafluoro-, HFC-134a","Ethane, 1,1,1-trichloro-, HCFC-140","Ethane, 1,1,1-trifluoro-, HFC-143a","Ethane, 1,1,2-trichloro-1,2,2-trifluoro-, CFC-113","Ethane, 1,1-dichloro-1-fluoro-, HCFC-141b","Ethane, 1,1-difluoro-, HFC-152a","Ethane, 1,2-dichloro-","Ethane, 1,2-dichloro-1,1,2,2-tetrafluoro-, CFC-114","Ethane, 1-chloro-1,1-difluoro-, HCFC-142b","Ethane, 2,2-dichloro-1,1,1-trifluoro-, HCFC-123","Ethane, 2-chloro-1,1,1,2-tetrafluoro-, HCFC-124","Ethane, chloropentafluoro-, CFC-115","Ethane, hexafluoro-, HFC-116","Ethane, pentafluoro-, HFC-125","Methane, bromo-, Halon 1001","Methane, bromochlorodifluoro-, Halon 1211","Methane, bromotrifluoro-, Halon 1301","Methane, chlorodifluoro-, HCFC-22","Methane, chloro-fluoro-, HCFC-31","Methane, chlorotrifluoro-, CFC-13","Methane, dichloro-, HCC-30","Methane, dichlorodifluoro-, CFC-12","Methane, dichlorofluoro-, HCFC-21","Methane, difluoro-, HFC-32","Methane, fossil","Methane, from soil or biomass stock","Methane, monochloro-, R-40","Methane, non-fossil","Methane, tetrachloro-, R-10","Methane, tetrafluoro-, R-14","Methane, trichlorofluoro-, CFC-11","Methane, trifluoro-, HFC-23","Monochloroethane","Nitrogen fluoride","Perfluoropentane","Sulfur hexafluoride","Tetrachloroethylene","Trichloroethylene"]
[{"$cut":{"chars":2166997,"head":""}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GLO",null,null,null,null,null,null,"GLO",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GLO",null,null,null,null,null,null,null,null,"Unreported"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EUR"]

{"sheet":"EF Unit List","index":29,"n_rows":7,"n_cols":16384,"rows_kept":7,"cut":false,"hidden":true,"merged":[],"flags":["row_too_large"]}
[null,"Do not modify this sheet, dropdowns will update automatically as you add to the Emissions factor database"]
[null,{"$f":"TRANSPOSE(_xlfn.UNIQUE(EF_Library[Emission Factor Name]))","v":0},"Bio Petrol","Biodiesel HVO","Biodiesel ME","Biodiesel ME (from tallow)","Biodiesel ME (from used cooking oil)","Bioethanol","Biomethane (compressed)","Biomethane (liquified)","Biopropane","Methanol (bio)","Off road biodiesel","Renewable petrol","Biogas","Landfill gas","Grass/straw","Wood chips","Wood logs","Wood pellets","Butane","CNG","LNG","LPG","Natural gas","Natural gas (100% mineral blend)","Other petroleum gas","Propane","Aviation spirit","Aviation turbine fuel","Burning oil","Diesel (100% mineral diesel)","Diesel (average biofuel blend)","Fuel oil","Gas oil","Lubricants","Marine fuel oil","Marine gas oil","Naphtha","Petrol (100% mineral petrol)","Petrol (average biofuel blend)","Processed fuel oils - distillate oil","Processed fuel oils - residual oil","Refinery miscellaneous","Waste oils","Coal (domestic)","Coal (electricity generation - home produced coal only)","Coal (electricity generation)","Coal (industrial)","Coking coal","Petroleum coke","Copper wire rod","Products based on epoxy-resin, group 1","Products based on epoxy-resin, group 2","Products based on epoxy-resin, group 3","Products based on epoxy-resin, group 4","Products based on epoxy-resin, group 5","Polyamide profiles reinforced with 25% fibreglass","Mesh","Heavy steel plates","Hot rolled steel plates","WTG (Siemens Gamesa 11-200 (11 MW))","Backend (Siemens Gamesa 11-200 (11 MW))","Generator (Siemens Gamesa 11-200 (11 MW))","Hub (Siemens Gamesa 11-200 (11 MW))","Backend assembly (Siemens Gamesa 11-200 (11 MW))","Electric components (Siemens Gamesa 11-200 (11 MW))","Blades (Siemens Gamesa 11-200 (11 MW))","Tower (Siemens Gamesa 11-200 (11 MW))","WTG (Siemens Gamesa 14-222 (14 MW))","Backend (Siemens Gamesa 14-222 (14 MW))","Generator (Siemens Gamesa 14-222 (14 MW))","Hub (Siemens Gamesa 14-222 (14 MW))","Backend assembly (Siemens Gamesa 14-222 (14 MW))","Electric components (Siemens Gamesa 14-222 (14 MW))","Blades (Siemens Gamesa 14-222 (14 MW))","Tower (Siemens Gamesa 14-222 (14 MW))","WTG (Siemens Gamesa 14-236 (14 MW))","Backend (Siemens Gamesa 14-236 (14 MW))","Generator (Siemens Gamesa 14-236 (14 MW))","Hub (Siemens Gamesa 14-236 (14 MW))","Backend assembly (Siemens Gamesa 14-236 (14 MW))","Electric components (Siemens Gamesa 14-236 (14 MW))","Blades (Siemens Gamesa 14-236 (14 MW))","Tower (Siemens Gamesa 14-236 (14 MW))","Bromopropane","Carbon dioxide, fossil","Carbon dioxide, from soil or biomass stock","Carbon dioxide, removal from atmosphere","Chloroform","Dinitrogen monoxide","Ethane","Ethane, 1,1,1,2-tetrafluoro-, HFC-134a","Ethane, 1,1,1-trichloro-, HCFC-140","Ethane, 1,1,1-trifluoro-, HFC-143a","Ethane, 1,1,2-trichloro-1,2,2-trifluoro-, CFC-113","Ethane, 1,1-dichloro-1-fluoro-, HCFC-141b","Ethane, 1,1-difluoro-, HFC-152a","Ethane, 1,2-dichloro-","Ethane, 1,2-dichloro-1,1,2,2-tetrafluoro-, CFC-114","Ethane, 1-chloro-1,1-difluoro-, HCFC-142b","Ethane, 2,2-dichloro-1,1,1-trifluoro-, HCFC-123","Ethane, 2-chloro-1,1,1,2-tetrafluoro-, HCFC-124","Ethane, chloropentafluoro-, CFC-115","Ethane, hexafluoro-, HFC-116","Ethane, pentafluoro-, HFC-125","Methane, bromo-, Halon 1001","Methane, bromochlorodifluoro-, Halon 1211","Methane, bromotrifluoro-, Halon 1301","Methane, chlorodifluoro-, HCFC-22","Methane, chloro-fluoro-, HCFC-31","Methane, chlorotrifluoro-, CFC-13","Methane, dichloro-, HCC-30","Methane, dichlorodifluoro-, CFC-12","Methane, dichlorofluoro-, HCFC-21","Methane, difluoro-, HFC-32","Methane, fossil","Methane, from soil or biomass stock","Methane, monochloro-, R-40","Methane, non-fossil","Methane, tetrachloro-, R-10","Methane, tetrafluoro-, R-14","Methane, trichlorofluoro-, CFC-11","Methane, trifluoro-, HFC-23","Monochloroethane","Nitrogen fluoride","Perfluoropentane","Sulfur hexafluoride","Tetrachloroethylene","Trichloroethylene"]
[{"$cut":{"chars":2168513,"head":""}}]
[null,null,"kg","kg","kg","kg","kg","kg","kg","kg","kg","kg","kg","kg","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Gross CV)","kWh (Gross CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)","kWh (Net CV)"]
[null,null,"litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres",null,null,null,null,null,null,"litres","litres","litres","litres","kWh (Net CV)","kWh (Net CV)","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","litres","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes","tonnes"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kg",null,null,null,null,null,null,"kg"]

{"sheet":"Asset Taxonomy","index":30,"n_rows":8,"n_cols":15,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
[null,"Do not modify this sheet, dropdowns will update automatically as you add to the Emissions factor database"]
[null,{"$f":"TRANSPOSE(_xlfn._xlws.SORT(_xlfn.UNIQUE(AssetTaxonomy[L1: Assets])))","v":"Cables"},"Construction and installation assets","Fixed foundations","Floating foundations","Offshore substation","Onshore substation","Operations and maintenance assets","Operations base","Other","Wind turbine generators (WTG)"]
[null,{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=B2))),\"No Selection\")","v":"Export cables"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=C2))),\"No Selection\")","v":"Cable installation vessel"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=D2))),\"No Selection\")","v":"Jacket"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=E2))),\"No Selection\")","v":"Anchors"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=F2))),\"No Selection\")","v":"Facilities"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=G2))),\"No Selection\")","v":"Facilities"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[L2: Subcomponents],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=H2))),\"No Selection\")","v":"Crew transfer vessels"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=I2))),\"No Selection\")","v":"Roads"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=J2))),\"No Selection\")","v":"Unassigned"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=K2))),\"No Selection\")","v":"Blades, hub, and rotor system"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=L2))),\"No Selection\")","v":"No Selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=M2))),\"No Selection\")","v":"No Selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=N2))),\"No Selection\")","v":"No Selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[L1: Assets],AssetTaxonomy[L2: Subcomponents]=O2))),\"No Selection\")","v":"No Selection"}]
[null,"Inter array cables","Foundation installation vessel","Monopile","Mooring","Structure","Structure","Helicopters, drones or other aerial vehicle","Site buildings",null,"Nacelle and internals"]
[null,"Unassigned","Onshore plant and machinery","Other fixed foundation technologies","Other floating foundation technologies","Switchgear","Switchgear","Service operations vessels","Unassigned",null,"Tower"]
[null,null,"Substation installation vessel","Transition piece","Platform","Transformers","Transformers",null,"Vessel berths",null,"Transformer"]
[null,null,"Turbine Installation vessel","Unassigned","Unassigned","Unassigned","Unassigned",null,null,null,"Unassigned"]
[null,null,"Unassigned"]

{"sheet":"Geographies","index":31,"n_rows":352,"n_cols":2,"rows_kept":352,"cut":false,"hidden":true,"merged":[]}
["Country or Region","Shortcut"]
["Andorra","AD"]
["United Arab Emirates","AE"]
["Afghanistan","AF"]
["Antigua and Barbuda","AG"]
["Anguilla","AI"]
["Albania","AL"]
["IAl producing Area 2, North America","Al producing Area 2, North America"]
["Armenia","AM"]
["Angola","AO"]
["Antarctica","AQ"]
["Argentina","AR"]
["American Samoa","AS"]
["Alaska Systems Coordinating Council","ASCC"]
["Asia without China","Asia without China"]
["Austria","AT"]
["Australia","AU"]
["Australian Capital Territory","AUS-ACT"]
["New South Wales","AUS-NSW"]
["Northern Territory","AUS-NTR"]
["Queensland","AUS-QNS"]
["South Australia","AUS-SAS"]
["Tasmania","AUS-TSM"]
["Victoria","AUS-VCT"]
["Western Australia","AUS-WAS"]
["Aruba","AW"]
["Åland Islands","AX"]
["Azerbaijan","AZ"]
["Bosnia and Herzegovina","BA"]
["Baltic System Operator","BALTSO"]
["Barbados","BB"]
["Bangladesh","BD"]
["Belgium","BE"]
["Burkina Faso","BF"]
["Bulgaria","BG"]
["Bahrain","BH"]
["Burundi","BI"]
["Benin","BJ"]
["Saint Barthelemy","BL"]
["Bermuda","BM"]
["Brunei Darussalam","BN"]
["Bolivia, Plurinational State of","BO"]
["Bonaire, Sint Eustatius, and Saba","BQ"]
["Brazil","BR"]
["Bahamas","BS"]
["Bhutan","BT"]
["Bouvet Island","BV"]
["Botswana","BW"]
["Belarus","BY"]
["Belize","BZ"]
["Canada","CA"]
["Alberta","CA-AB"]
["British Columbia","CA-BC"]
["Manitoba","CA-MB"]
["Canada without Alberta","Canada without Alberta"]
["Canada without Alberta and Quebec","Canada without Alberta and Quebec"]
["Canary Islands","Canary Islands"]
["New Brunswick","CA-NB"]
["Newfoundland and Labrador","CA-NF"]
["Nova Scotia","CA-NS"]
["Northwest Territories","CA-NT"]
["Nunavut","CA-NU"]
["Ontario","CA-ON"]
["Prince Edward Island","CA-PE"]
["Québec","CA-QC"]
["Saskatchewan","CA-SK"]
["Yukon Territory","CA-YK"]
["Cocos (Keeling) Islands","CC"]
["Congo, Democratic Republic of the","CD"]
["Central Asia","Central Asia"]
["Central European Power Association","CENTREL"]
["Central African Republic","CF"]
["Congo","CG"]
["Switzerland","CH"]
["Churchill Falls Generating Station","Churchill Falls"]
["Cote d'Ivoire","CI"]
["Cook Islands","CK"]
["Chile","CL"]
["Cameroon","CM"]
["China","CN"]
["Colombia","CO"]
["Costa Rica","CR"]
["Serbia and Montenegro","CS"]
["Cuba","CU"]
["Cape Verde","CV"]
["Curaçao","CW"]
["Christmas Island","CX"]
["Cyprus","CY"]
["Czech Republic","CZ"]
["Germany","DE"]
["Djibouti","DJ"]
["Denmark","DK"]
["Dominica","DM"]
["Dominican Republic","DO"]
["Algeria","DZ"]
["Ecuador","EC"]
["Estonia","EE"]
["Central and Eastern Europe","EEU"]
["Egypt","EG"]
["Western Sahara","EH"]
["European Network of Transmission Systems Operators for Electricity","ENTSO-E"]
["Eritrea","ER"]
["Spain","ES"]
["Ethiopia","ET"]
["Europe without NORDEL (NCPA)","Europe without NORDEL (NCPA)"]
["Europe without Switzerland","Europe without Switzerland"]
["Europe, without Russia and Turkey","Europe, without Russia and Turkey"]
["Finland","FI"]
["Fiji","FJ"]
["Falkland Islands (Malvinas)","FK"]
["Micronesia, Federated States of","FM"]
["Faroe Islands","FO"]
["France","FR"]
["France, including overseas territories","France, including overseas territories"]
["Florida Reliability Coordinating Council","FRCC"]
["Commonwealth of Independent States","FSU"]
["Gabon","GA"]
["United Kingdom","GB"]
["Grenada","GD"]
["Georgia","GE"]
["French Guiana","GF"]
["Guernsey","GG"]
["Ghana","GH"]
["Gibraltar","GI"]
["Greenland","GL"]
["Global","GLO"]
["Gambia","GM"]
["Guinea","GN"]
["Guadeloupe","GP"]
["Equatorial Guinea","GQ"]
["Greece","GR"]
["South Georgia and the South Sandwich Islands","GS"]
["Guatemala","GT"]
["Guam","GU"]
["Guinea-Bissau","GW"]
["Guyana","GY"]
["HICC","HICC"]
["Hong Kong","HK"]
["Heard Island and McDonald Islands","HM"]
["Honduras","HN"]
["Croatia","HR"]
["Haiti","HT"]
["Hungary","HU"]
["IAl producing Area 1, Africa","IAI Area 1"]
["IAI producing Area 2, North America, without Quebec","IAI Area 2, without Quebec"]
["IAl producing Area 3, South America","IAI Area 3"]
["IAI producing Area 4 and 5, South and East Asia, without China","IAI Area 4&5 without China"]
["IAl producing Area 6A, West Europe","IAI Area 6A"]
["IAl producing Area 6B, East/Central Europe","IAI Area 6B"]
["IAl producing Area 8, Gulf-Aluminium Council/Gulf Region","IAI Area 8"]
["Aluminium producing area, EU27 and EFTA countries","IAI Area, EU27 & EFTA"]
["Aluminium producing area, Europe outside EU27 and EFTA","IAI Area, Europe outside EU & EFTA"]
["Indonesia","ID"]
["Ireland","IE"]
["Israel","IL"]
["Isle of Man","IM"]
["India","IN"]
["British Indian Ocean Territory","IO"]
["Iraq","IQ"]
["Iran (Islamic Republic of)","IR"]
["Iceland","IS"]
["Italy","IT"]
["Jersey","JE"]
["Jamaica","JM"]
["Jordan","JO"]
["Japan","JP"]
["Kenya","KE"]
["Kyrgyzstan","KG"]
["Cambodia","KH"]
["Kiribati","KI"]
["Comoros","KM"]
["Saint Kitts and Nevis","KN"]
["Korea, Democratic People's Republic of","KP"]
["Korea, Republic of","KR"]
["Kuwait","KW"]
["Cayman Islands","KY"]
["Kazakhstan","KZ"]
["Lao People's Democratic Republic","LA"]
["Lebanon","LB"]
["Saint Lucia","LC"]
["Liechtenstein","LI"]
["Sri Lanka","LK"]
["Liberia","LR"]
["Lesotho","LS"]
["Lithuania","LT"]
["Luxembourg","LU"]
["Latvia","LV"]
["Libya","LY"]
["Morocco","MA"]
["Monaco","MC"]
["Moldova, Republic of","MD"]
["Montenegro","ME"]
["Saint Martin","MF"]
["Madagascar","MG"]
["Marshall Islands","MH"]
["Macedonia, the Former Yugoslav Republic of","MK"]
["Mali","ML"]
["Myanmar","MM"]
["Mongolia","MN"]
["Macau","MO"]
["Northern Mariana Islands","MP"]
["Martinique","MQ"]
["Mauritania","MR"]
["Midwest Reliability Organization","MRO"]
["Midwest Reliability Organization, US part only","MRO, US only"]
["Montserrat","MS"]
["Malta","MT"]
["Mauritius","MU"]
["Maldives","MV"]
["Malawi","MW"]
["Mexico","MX"]
["Malaysia","MY"]
["Mozambique","MZ"]
["Namibia","NA"]
["North American Free Trade Agreement","NAFTA"]
["New Caledonia","NC"]
["Niger","NE"]
["Norfolk Island","NF"]
["Nigeria","NG"]
["Nicaragua","NI"]
["Netherlands","NL"]
["Norway","NO"]
["Nordic Countries Power Association","NORDEL"]
["Nepal","NP"]
["Northeast Power Coordinating Council","NPCC"]
["Northeast Power Coordinating Council, US part only","NPCC, US only"]
["Nauru","NR"]
["Niue","NU"]
["New Zealand","NZ"]
["Oman","OM"]
["Panama","PA"]
["Peru","PE"]
["French Polynesia","PF"]
["Papua New Guinea","PG"]
["Philippines","PH"]
["Pakistan","PK"]
["Poland","PL"]
["Saint Pierre and Miquelon","PM"]
["Pitcairn","PN"]
["Puerto Rico","PR"]
["Palestinian Territory, Occupied","PS"]
["Portugal","PT"]
["Palau","PW"]
["Paraguay","PY"]
["Qatar","QA"]
["Québec, Hydro-Québec distribution network","Québec, HQ distribution network"]
["Africa","RAF"]
["Asia","RAS"]
["Reunion","RE"]
["Europe","RER"]
["Europe without Austria, Belgium, France, Germany, Italy, Liechtenstein, Monaco, San Marino, Switzerland, and the Vatican","RER w/o AT+BE+CH+DE+FR+IT"]
["Europe without Germany and Switzerland","RER w/o CH+DE"]
["Europe without Germany, the Netherlands, and Norway","RER w/o DE+NL+NO"]
["ReliabilityFirst Corporation","RFC"]
["Latin America and the Caribbean","RLA"]
["Middle East","RME"]
["Northern America","RNA"]
["Romania","RO"]
["Rest-of-World","RoW"]
["Serbia","RS"]
["Russian Federation","RU"]
["Rwanda","RW"]
["Saudi Arabia","SA"]
["South Asia","SAS"]
["Solomon Islands","SB"]
["Seychelles","SC"]
["Sudan","SD"]
["Sweden","SE"]
["SERC Reliability Corporation","SERC"]
["Singapore","SG"]
["Saint Helena","SH"]
["Slovenia","SI"]
["Svalbard and Jan Mayen","SJ"]
["Slovakia","SK"]
["Sierra Leone","SL"]
["San Marino","SM"]
["Senegal","SN"]
["Somalia","SO"]
["Spain, including overseas territories","Spain, including overseas territories"]
["Southwest Power Pool","SPP"]
["Suriname","SR"]
["South Sudan","SS"]
["Sao Tome and Principe","ST"]
["El Salvador","SV"]
["Sint Maarten, Dutch part","SX"]
["Syrian Arab Republic","SY"]
["Swaziland","SZ"]
["Turks and Caicos Islands","TC"]
["Chad","TD"]
["French Southern Territories","TF"]
["Togo","TG"]
["Thailand","TH"]
["Tajikistan","TJ"]
["Tokelau","TK"]
["Timor-Leste","TL"]
["Turkmenistan","TM"]
["Tunisia","TN"]
["Tonga","TO"]
["Turkey","TR"]
["Texas Regional Entity","TRE"]
["Trinidad and Tobago","TT"]
["Tuvalu","TV"]
["Taiwan, Province of China","TW"]
["Tanzania, United Republic Of","TZ"]
["Ukraine","UA"]
["Union for the Co-ordination of Transmission of Electricity","UCTE"]
["UCTE without France","UCTE without France"]
["UCTE without Germany","UCTE without Germany"]
["UCTE without Germany and France","UCTE without Germany and France"]
["Uganda","UG"]
["United States Minor Outlying Islands","UM"]
["Americas","UN-AMERICAS"]
["Asia, UN Region","UN-ASIA"]
["Australia and New Zealand","UN-AUSTRALIANZ"]
["Central America","UN-CAMERICA"]
["Eastern Africa","UN-EAFRICA"]
["Eastern Asia","UN-EASIA"]
["Eastern Europe","UN-EEUROPE"]
["Europe, UN Region","UN-EUROPE"]
["Middle Africa","UN-MAFRICA"]
["Melanesia","UN-MELANESIA"]
["Micronesia","UN-MICRONESIA"]
["Northern Africa","UN-NAFRICA"]
["Northern Europe","UN-NEUROPE"]
["Oceania","UN-OCEANIA"]
["Polynesia","UN-POLYNESIA"]
["South America","UN-SAMERICA"]
["Southern Africa","UN-SASIA"]
["South-Eastern Asia","UN-SEASIA"]
["Southern Europe","UN-SEUROPE"]
["Western Africa","UN-WAFRICA"]
["Western Asia","UN-WASIA"]
["United States","US"]
["Uruguay","UY"]
["Uzbekistan","UZ"]
["Holy See (Vatican City State)","VA"]
["Saint Vincent and the Grenadines","VC"]
["Venezuela","VE"]
["Virgin Islands, British","VG"]
["Virgin Islands, U.S.","VI"]
["Viet Nam","VN"]
["Vanuatu","VU"]
["Western Electricity Coordinating Council","WECC"]
["Western Electricity Coordinating Council, US part only","WECC, US only"]
["Western Europe","WEU"]
["Wallis and Futuna","WF"]
["Samoa","WS"]
["Yemen","YE"]
["Mayotte","YT"]
["South Africa","ZA"]
["Zambia","ZM"]
["Zimbabwe","ZW"]

{"sheet":"Activity Taxonomy","index":32,"n_rows":32,"n_cols":12,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
[null,"Do not modify this sheet, dropdowns will update automatically as you add to the Emissions factor database"]
[null,{"$f":"TRANSPOSE(_xlfn._xlws.SORT(_xlfn.UNIQUE(ActivityTaxonomy[L1: Activity Category])))","v":"Direct emissions and removals"},"Electricity, fuels and other utilities","Freight and transportation","Fully manufactured assets","Fully manufactured components","Manufacturing processes","Materials","Other","Waste treatment"]
[null,{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=B2))),\"No Selection\")","v":"Emissions"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=C2))),\"No Selection\")","v":"Biofuels lifecycle"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=D2))),\"No Selection\")","v":"Air freight and transportation"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=E2))),\"No Selection\")","v":"Cables"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=F2))),\"No Selection\")","v":"Anchors"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=G2))),\"No Selection\")","v":"Coating and galvanising processes"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=H2))),\"No Selection\")","v":"Aluminium"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=I2))),\"No Selection\")","v":"Unassigned"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(ActivityTaxonomy[[L2: Activity Subcategory]:[L2: Activity Subcategory]],ActivityTaxonomy[[L1: Activity Category]:[L1: Activity Category]]=J2))),\"No Selection\")","v":"Incineration"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=K2))),\"No Selection\")","v":"No Selection"},{"$f":"IFERROR(_xlfn.UNIQUE(_xlfn._xlws.SORT(_xlfn._xlws.FILTER(AssetTaxonomy[[L2: Subcomponents]:[L2: Subcomponents]],AssetTaxonomy[[L1: Assets]:[L1: Assets]]=L2))),\"No Selection\")","v":"No Selection"}]
[null,"Removals","Electricity lifecycle","Rail freight and transportation","Construction and installation assets","Blades, hub, and rotor system","Joining and welding processes","Biogenic materials",null,"Landfill"]
[null,null,"Gaseous fuels lifecycle","Road freight and transportation","Fixed foundations","Cable installation vessel","Material processing","Carbon fibre",null,"Processing, sorting for recycling and reuse"]
[null,null,"Liquid fuels lifecycle","Sea freight and transportation","Floating foundations","Crew transfer vessels","Other manufacturing processes","Concrete"]
[null,null,"Solid fuels lifecycle",null,"Offshore substation","Export cables",null,"Copper"]
[null,null,"Water consumption",null,"Onshore substation","Facilities",null,"Fibreglass"]
[null,null,null,null,"Operations and maintenance assets","Foundation installation vessel",null,"Oils and Lubricants"]
[null,null,null,null,"Operations base","Helicopters, drones or other aerial vehicle",null,"Other materials"]
[null,null,null,null,"Other","Inter array cables",null,"Polymers"]
[null,null,null,null,"Wind turbine generators (WTG)","Jacket",null,"Steel"]
[null,null,null,null,null,"Monopile"]
[null,null,null,null,null,"Mooring"]
[null,null,null,null,null,"Nacelle and internals"]
[null,null,null,null,null,"Onshore plant and machinery"]
[null,null,null,null,null,"Other"]
[null,null,null,null,null,"Other fixed foundation technologies"]
[null,null,null,null,null,"Other floating foundation technologies"]
[null,null,null,null,null,"Platform"]
[null,null,null,null,null,"Roads"]
[null,null,null,null,null,"Service operations vessels"]
[null,null,null,null,null,"Site buildings"]
[null,null,null,null,null,"Structure"]
[null,null,null,null,null,"Substation installation vessel"]
[null,null,null,null,null,"Switchgear"]
[null,null,null,null,null,"Tower"]
[null,null,null,null,null,"Transformer"]
[null,null,null,null,null,"Transformers"]
[null,null,null,null,null,"Transition piece"]
[null,null,null,null,null,"Turbine Installation vessel"]
[null,null,null,null,null,"Vessel berths"]